<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>C:/Users/Vince/Documents/websvn/trunk/Eagle/projects/DEC/Mxxx/M908/M908Bbackfb.bmp</text>
<text>CONNECTOR W908B</text>
<text>6-73P</text>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="EDGE-CON2">
<description>Single-Height DEC edge connector</description>
</package>
<package name="SINGLE">
<description>Single-Height DEC board</description>
</package>
<package name="FLIPCHIP">
</package>
</packages>
</library>
<library name="wirepad">
<packages>
<package name="2,54/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dec-con" package="EDGE-CON2" value=""/>
<element name="U$2" library="dec-con" package="SINGLE" value="OUTLINE-SINGLE"/>
<element name="A1" library="wirepad" package="2,54/1,0" value=""/>
<element name="B1" library="wirepad" package="2,54/1,0" value=""/>
<element name="C1" library="wirepad" package="2,54/1,0" value=""/>
<element name="D1" library="wirepad" package="2,54/1,0" value=""/>
<element name="E1" library="wirepad" package="2,54/1,0" value=""/>
<element name="F1" library="wirepad" package="2,54/1,0" value=""/>
<element name="H1" library="wirepad" package="2,54/1,0" value=""/>
<element name="J1" library="wirepad" package="2,54/1,0" value=""/>
<element name="K1" library="wirepad" package="2,54/1,0" value=""/>
<element name="L1" library="wirepad" package="2,54/1,0" value=""/>
<element name="M1" library="wirepad" package="2,54/1,0" value=""/>
<element name="N1" library="wirepad" package="2,54/1,0" value=""/>
<element name="P1" library="wirepad" package="2,54/1,0" value=""/>
<element name="R1" library="wirepad" package="2,54/1,0" value=""/>
<element name="S1" library="wirepad" package="2,54/1,0" value=""/>
<element name="T1" library="wirepad" package="2,54/1,0" value=""/>
<element name="U1" library="wirepad" package="2,54/1,0" value=""/>
<element name="V1" library="wirepad" package="2,54/1,0" value=""/>
<element name="A2" library="wirepad" package="2,54/1,0" value=""/>
<element name="B2" library="wirepad" package="2,54/1,0" value=""/>
<element name="C2" library="wirepad" package="2,54/1,0" value=""/>
<element name="D2" library="wirepad" package="2,54/1,0" value=""/>
<element name="E2" library="wirepad" package="2,54/1,0" value=""/>
<element name="F2" library="wirepad" package="2,54/1,0" value=""/>
<element name="H2" library="wirepad" package="2,54/1,0" value=""/>
<element name="J2" library="wirepad" package="2,54/1,0" value=""/>
<element name="K2" library="wirepad" package="2,54/1,0" value=""/>
<element name="L2" library="wirepad" package="2,54/1,0" value=""/>
<element name="M2" library="wirepad" package="2,54/1,0" value=""/>
<element name="N2" library="wirepad" package="2,54/1,0" value=""/>
<element name="P2" library="wirepad" package="2,54/1,0" value=""/>
<element name="R2" library="wirepad" package="2,54/1,0" value=""/>
<element name="S2" library="wirepad" package="2,54/1,0" value=""/>
<element name="T2" library="wirepad" package="2,54/1,0" value=""/>
<element name="U2" library="wirepad" package="2,54/1,0" value=""/>
<element name="V2" library="wirepad" package="2,54/1,0" value=""/>
<element name="RN3" library="rcl" package="0207/10" value="10"/>
<element name="RN4" library="rcl" package="0207/10" value="10"/>
<element name="RN1" library="rcl" package="0207/10" value="10"/>
<element name="RN2" library="rcl" package="0207/10" value="10"/>
<element name="U$3" library="dec-con" package="FLIPCHIP" value=""/>
</elements>
<signals>
<signal name="N$4">
<contactref element="U$1" pad="D1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="E1"/>
<contactref element="E1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="F1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="H1"/>
<contactref element="H1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="J1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="K1"/>
<contactref element="K1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="L1"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="M1"/>
<contactref element="M1" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="N1"/>
<contactref element="N1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="P1"/>
<contactref element="P1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="R1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="S1"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="T1"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="U1"/>
<contactref element="RN2" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="V1"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="A2" pad="1"/>
<contactref element="RN4" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="B2" pad="1"/>
<contactref element="RN3" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="C2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="D2"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="E2"/>
<contactref element="E2" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="F2"/>
<contactref element="F2" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="H2"/>
<contactref element="H2" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="J2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="K2"/>
<contactref element="K2" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="U$1" pad="L2"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="U$1" pad="M2"/>
<contactref element="M2" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="U$1" pad="N2"/>
<contactref element="N2" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="U$1" pad="P2"/>
<contactref element="P2" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="U$1" pad="R2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="U$1" pad="S2"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="U$1" pad="T2"/>
<contactref element="T2" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="U$1" pad="U2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="U$1" pad="V2"/>
<contactref element="V2" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="V1" pad="1"/>
<contactref element="RN1" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="U1" pad="1"/>
<contactref element="RN2" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="U$1" pad="B2"/>
<contactref element="RN3" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="U$1" pad="A2"/>
<contactref element="RN4" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="U$1" pad="A1"/>
<contactref element="A1" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="U$1" pad="B1"/>
<contactref element="B1" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="U$1" pad="C1"/>
<contactref element="C1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
