<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="18.415" y1="132.08" x2="125.73" y2="132.08" width="0" layer="20"/>
<wire x1="125.73" y1="132.08" x2="125.73" y2="0" width="0" layer="20"/>
<wire x1="125.73" y1="0" x2="15.875" y2="0" width="0" layer="20"/>
<text>PDP 8I POWER CABLE CONNECTOR</text>
<text>G792A</text>
<text>2-70</text>
<hole x="20.32" y="4.1275" drill="3.175"/>
<hole x="30.48" y="4.1275" drill="3.175"/>
<hole x="120.65" y="75.565" drill="3.175"/>
<hole x="120.65" y="126.365" drill="3.175"/>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="EDGE-CON4">
<description>Double-Height DEC edge connector</description>
</package>
<package name="SPADELUG">
<description>Spade Lug Mounting Hole</description>
</package>
<package name="FLIPCHIP">
</package>
<package name="FLEX19W">
<description>19 SMT pads on 0.1" centers</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="E25-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 9 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="dec-con" package="EDGE-CON4" value=""/>
<element name="-30V" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="GND" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="FLEX1" library="dec-con" package="FLEX19W" value="FLEX19W"/>
<element name="FLEX2" library="dec-con" package="FLEX19W" value="FLEX19W"/>
<element name="C1" library="rcl" package="E25-9" value="150uF"/>
<element name="C2" library="rcl" package="E25-9" value="10uF"/>
<element name="C3" library="rcl" package="E25-9" value="10uF"/>
<element name="U$3" library="dec-con" package="FLIPCHIP" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="GND" pad="1"/>
<contactref element="U$2" pad="AV1"/>
<contactref element="U$2" pad="AU1"/>
<contactref element="U$2" pad="AT1"/>
<contactref element="U$2" pad="AS1"/>
<contactref element="U$2" pad="AR1"/>
<contactref element="U$2" pad="AP1"/>
<contactref element="U$2" pad="AN1"/>
<contactref element="U$2" pad="AM1"/>
<contactref element="U$2" pad="AL1"/>
<contactref element="U$2" pad="AK1"/>
<contactref element="U$2" pad="AJ1"/>
<contactref element="U$2" pad="AD1"/>
<contactref element="U$2" pad="AE1"/>
<contactref element="U$2" pad="AF1"/>
<contactref element="U$2" pad="AH1"/>
<contactref element="U$2" pad="BV1"/>
<contactref element="U$2" pad="BU1"/>
<contactref element="U$2" pad="BT1"/>
<contactref element="U$2" pad="BS1"/>
<contactref element="U$2" pad="BR1"/>
<contactref element="U$2" pad="BP1"/>
<contactref element="U$2" pad="BN1"/>
<contactref element="U$2" pad="BM1"/>
<contactref element="U$2" pad="BL1"/>
<contactref element="U$2" pad="BK1"/>
<contactref element="U$2" pad="BJ1"/>
<contactref element="U$2" pad="BH1"/>
<contactref element="U$2" pad="BF1"/>
<contactref element="U$2" pad="BE1"/>
<contactref element="U$2" pad="BD1"/>
<contactref element="C3" pad="+"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="+"/>
<contactref element="FLEX1" pad="18"/>
<contactref element="FLEX1" pad="17"/>
<contactref element="FLEX1" pad="2"/>
<contactref element="FLEX1" pad="3"/>
<contactref element="FLEX1" pad="4"/>
<contactref element="FLEX1" pad="5"/>
<contactref element="FLEX1" pad="6"/>
<contactref element="FLEX1" pad="7"/>
<contactref element="FLEX1" pad="8"/>
<contactref element="FLEX1" pad="9"/>
<contactref element="FLEX1" pad="10"/>
<contactref element="FLEX1" pad="11"/>
<contactref element="FLEX1" pad="12"/>
<contactref element="FLEX1" pad="13"/>
<contactref element="FLEX1" pad="14"/>
<contactref element="FLEX1" pad="15"/>
<contactref element="FLEX1" pad="16"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="+"/>
<contactref element="U$2" pad="AV2"/>
<contactref element="U$2" pad="AD2"/>
<contactref element="U$2" pad="AU2"/>
<contactref element="U$2" pad="AT2"/>
<contactref element="U$2" pad="AS2"/>
<contactref element="U$2" pad="AR2"/>
<contactref element="U$2" pad="AP2"/>
<contactref element="U$2" pad="AN2"/>
<contactref element="U$2" pad="AM2"/>
<contactref element="U$2" pad="AL2"/>
<contactref element="U$2" pad="AK2"/>
<contactref element="U$2" pad="AJ2"/>
<contactref element="U$2" pad="AH2"/>
<contactref element="U$2" pad="AE2"/>
<contactref element="U$2" pad="AF2"/>
<contactref element="U$2" pad="BD2"/>
<contactref element="U$2" pad="BJ2"/>
<contactref element="U$2" pad="BH2"/>
<contactref element="U$2" pad="BF2"/>
<contactref element="U$2" pad="BE2"/>
<contactref element="FLEX2" pad="16"/>
<contactref element="FLEX2" pad="4"/>
<contactref element="FLEX2" pad="5"/>
<contactref element="FLEX2" pad="6"/>
<contactref element="FLEX2" pad="7"/>
<contactref element="FLEX2" pad="8"/>
<contactref element="FLEX2" pad="9"/>
<contactref element="FLEX2" pad="10"/>
<contactref element="FLEX2" pad="15"/>
<contactref element="FLEX2" pad="14"/>
<contactref element="FLEX2" pad="13"/>
<contactref element="FLEX2" pad="12"/>
<contactref element="FLEX2" pad="11"/>
</signal>
<signal name="-15V">
<contactref element="C2" pad="-"/>
<contactref element="C3" pad="-"/>
<contactref element="U$2" pad="BV2"/>
<contactref element="U$2" pad="BK2"/>
<contactref element="U$2" pad="BL2"/>
<contactref element="U$2" pad="BM2"/>
<contactref element="U$2" pad="BN2"/>
<contactref element="U$2" pad="BP2"/>
<contactref element="U$2" pad="BR2"/>
<contactref element="U$2" pad="BS2"/>
<contactref element="U$2" pad="BT2"/>
<contactref element="U$2" pad="BU2"/>
<contactref element="FLEX2" pad="17"/>
<contactref element="FLEX2" pad="18"/>
</signal>
<signal name="-30V">
<contactref element="FLEX2" pad="3"/>
<contactref element="-30V" pad="1"/>
<contactref element="FLEX2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
