<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>SERIAL PORT CARD</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>M837</text>
</plain>
<libraries>
<library name="dec-con">
<description>DEC Edge Connectors and Parts</description>
<packages>
<package name="EDGE-CON8">
<description>Quad-Height DEC edge connector</description>
</package>
<package name="E12-8">
<description>A 0.8 inch electrolytic.</description>
</package>
<package name="NC1">
<description>NC Jumper, circular lobes</description>
</package>
<package name="C063-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="OMNIBUS">
<description>Quad-Height DEC board</description>
</package>
</packages>
</library>
<library name="atmel-cpld">
<description>5V CPLD w/ISP 

32 Macrocell, low power w/ISP, 5V</description>
<packages>
<package name="S84">
<description>&lt;b&gt;84 Pin PLCC Socket&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-harting-ml">
<packages>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="alan_common">
<description>Alan's frequently used manually inputted parts</description>
<packages>
<package name="AMP_DB-9RA">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08S">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor-sil">
<description>&lt;b&gt;Resistors in Single Inline Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SIL11">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-dil">
<description>&lt;b&gt;DIL Switches and Code Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DP-06">
<description>&lt;b&gt;DIL/CODE SWITCH&lt;/b&gt;&lt;p&gt;
distributor Buerklin, 17G572</description>
</package>
</packages>
</library>
<library name="switch">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="9070-1W">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
 Marquardt</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C33" library="dec-con" package="E12-8" value="6.8uF"/>
<element name="C34" library="dec-con" package="E12-8" value="6.8uF"/>
<element name="C35" library="dec-con" package="E12-8" value="6.8uF"/>
<element name="VCCINT" library="dec-con" package="NC1" value="JUMPER-NC1"/>
<element name="VCCIO" library="dec-con" package="NC1" value="JUMPER-NC1"/>
<element name="C1" library="dec-con" package="C063-025X075" value=".22uF"/>
<element name="C2" library="dec-con" package="C063-025X075" value=".22uF"/>
<element name="C3" library="dec-con" package="C063-025X075" value=".22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="dec-con" package="C063-025X075" value=".22uF"/>
<element name="U$1" library="dec-con" package="EDGE-CON8" value="QUAD"/>
<element name="SV2" library="con-harting-ml" package="ML10" value=" ">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$2" library="dec-con" package="OMNIBUS" value="OUTLINE-OMNIBUS"/>
<element name="E2" library="atmel-cpld" package="S84" value="ATF150X84"/>
<element name="SERIAL" library="switch-dil" package="DP-06" value="CONF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="26M1097"/>
<attribute name="MPN" value="MCDP06"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9471618"/>
</element>
<element name="USB" library="alan_common" package="AMP_DB-9RA" value="USB-DB9-D5-F">
<attribute name="MOUSER#" value="571-1734352-1"/>
<attribute name="MANF#" value="1734352-1"/>
<attribute name="MANF" value="TE/AMP"/>
</element>
<element name="C5" library="dec-con" package="C063-025X075" value=".22uF"/>
<element name="RN2" library="resistor-sil" package="SIL11" value="47K">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="OSC" library="crystal" package="DIL08S" value="19.661 MHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="TS_DISABLE" library="switch" package="9070-1W" value="M837"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C35" pad="-"/>
<contactref element="C33" pad="-"/>
<contactref element="C34" pad="-"/>
<contactref element="U$1" pad="AN2"/>
<contactref element="U$1" pad="AT2"/>
<contactref element="U$1" pad="AF2"/>
<contactref element="U$1" pad="AC2"/>
<contactref element="U$1" pad="AN1"/>
<contactref element="U$1" pad="AT1"/>
<contactref element="U$1" pad="AF1"/>
<contactref element="U$1" pad="BT1"/>
<contactref element="U$1" pad="BN1"/>
<contactref element="U$1" pad="BF1"/>
<contactref element="U$1" pad="BC1"/>
<contactref element="U$1" pad="BF2"/>
<contactref element="U$1" pad="BC2"/>
<contactref element="U$1" pad="CN1"/>
<contactref element="U$1" pad="CC1"/>
<contactref element="U$1" pad="DT1"/>
<contactref element="U$1" pad="DN1"/>
<contactref element="U$1" pad="DF1"/>
<contactref element="U$1" pad="DC1"/>
<contactref element="U$1" pad="CC2"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="SV2" pad="2"/>
<contactref element="SV2" pad="10"/>
<contactref element="E2" pad="7"/>
<contactref element="E2" pad="19"/>
<contactref element="E2" pad="32"/>
<contactref element="E2" pad="42"/>
<contactref element="E2" pad="47"/>
<contactref element="E2" pad="59"/>
<contactref element="E2" pad="72"/>
<contactref element="E2" pad="82"/>
<contactref element="SERIAL" pad="6"/>
<contactref element="SERIAL" pad="5"/>
<contactref element="SERIAL" pad="4"/>
<contactref element="SERIAL" pad="3"/>
<contactref element="SERIAL" pad="2"/>
<contactref element="SERIAL" pad="1"/>
<contactref element="USB" pad="G2"/>
<contactref element="USB" pad="5"/>
<contactref element="USB" pad="G1"/>
<contactref element="C5" pad="2"/>
<contactref element="OSC" pad="4"/>
<contactref element="TS_DISABLE" pad="B"/>
<contactref element="TS_DISABLE" pad="B1"/>
<contactref element="TS_DISABLE" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="C35" pad="+"/>
<contactref element="C33" pad="+"/>
<contactref element="C34" pad="+"/>
<contactref element="U$1" pad="AA2"/>
<contactref element="U$1" pad="BA2"/>
<contactref element="U$1" pad="CA2"/>
<contactref element="VCCIO" pad="1"/>
<contactref element="VCCINT" pad="1"/>
<contactref element="SV2" pad="4"/>
<contactref element="C5" pad="1"/>
<contactref element="RN2" pad="1"/>
<contactref element="OSC" pad="8"/>
</signal>
<signal name="D_L">
<contactref element="U$1" pad="DK2"/>
<contactref element="E2" pad="11"/>
</signal>
<signal name="INT_RQST_L">
<contactref element="U$1" pad="CP1"/>
<contactref element="E2" pad="25"/>
</signal>
<signal name="IO_PAUSE_L">
<contactref element="U$1" pad="CD1"/>
<contactref element="E2" pad="36"/>
</signal>
<signal name="CPMA_DISABLE_L">
<contactref element="U$1" pad="CU1"/>
<contactref element="E2" pad="21"/>
</signal>
<signal name="IR01_L">
<contactref element="U$1" pad="DE2"/>
<contactref element="E2" pad="16"/>
</signal>
<signal name="DF_ENABLE">
<contactref element="U$1" pad="CA1"/>
<contactref element="E2" pad="37"/>
</signal>
<signal name="IR00_L">
<contactref element="U$1" pad="DD2"/>
<contactref element="E2" pad="17"/>
</signal>
<signal name="IND1_L">
<contactref element="U$1" pad="CU2"/>
<contactref element="E2" pad="20"/>
</signal>
<signal name="SKIP_L">
<contactref element="U$1" pad="CS1"/>
<contactref element="E2" pad="22"/>
</signal>
<signal name="IND2_L">
<contactref element="U$1" pad="CV2"/>
<contactref element="E2" pad="18"/>
</signal>
<signal name="MD10_L">
<contactref element="U$1" pad="DM1"/>
<contactref element="E2" pad="9"/>
</signal>
<signal name="MD08_L">
<contactref element="U$1" pad="DK1"/>
<contactref element="E2" pad="12"/>
</signal>
<signal name="MD09_L">
<contactref element="U$1" pad="DL1"/>
<contactref element="E2" pad="10"/>
</signal>
<signal name="TP2">
<contactref element="U$1" pad="CE2"/>
<contactref element="E2" pad="34"/>
</signal>
<signal name="C1_L">
<contactref element="U$1" pad="CH1"/>
<contactref element="E2" pad="33"/>
</signal>
<signal name="F_L">
<contactref element="U$1" pad="DJ2"/>
<contactref element="E2" pad="15"/>
</signal>
<signal name="INITIALIZE">
<contactref element="U$1" pad="CR1"/>
<contactref element="E2" pad="24"/>
</signal>
<signal name="TP3">
<contactref element="U$1" pad="CH2"/>
<contactref element="E2" pad="31"/>
</signal>
<signal name="DATA11_L">
<contactref element="U$1" pad="DV1"/>
<contactref element="E2" pad="77"/>
</signal>
<signal name="KEY_CTL_L">
<contactref element="U$1" pad="DU2"/>
<contactref element="E2" pad="79"/>
</signal>
<signal name="LOAD_ADDR">
<contactref element="U$1" pad="DR2"/>
<contactref element="E2" pad="2"/>
</signal>
<signal name="F_SET_L">
<contactref element="U$1" pad="DP2"/>
<contactref element="E2" pad="5"/>
</signal>
<signal name="DATA08_L">
<contactref element="U$1" pad="DR1"/>
<contactref element="E2" pad="4"/>
</signal>
<signal name="MD11_L">
<contactref element="U$1" pad="DP1"/>
<contactref element="E2" pad="6"/>
</signal>
<signal name="DATA09_L">
<contactref element="U$1" pad="DS1"/>
<contactref element="E2" pad="81"/>
</signal>
<signal name="DATA10_L">
<contactref element="U$1" pad="DU1"/>
<contactref element="E2" pad="80"/>
</signal>
<signal name="VCCINT">
<contactref element="VCCINT" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="E2" pad="3"/>
<contactref element="E2" pad="43"/>
</signal>
<signal name="VCCIO">
<contactref element="VCCIO" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="E2" pad="13"/>
<contactref element="E2" pad="26"/>
<contactref element="E2" pad="38"/>
<contactref element="E2" pad="53"/>
<contactref element="E2" pad="66"/>
<contactref element="E2" pad="78"/>
</signal>
<signal name="TMS2">
<contactref element="SV2" pad="5"/>
<contactref element="E2" pad="23"/>
</signal>
<signal name="MD02_L">
<contactref element="U$1" pad="AM1"/>
<contactref element="E2" pad="64"/>
</signal>
<signal name="TP4">
<contactref element="U$1" pad="CJ2"/>
<contactref element="E2" pad="30"/>
</signal>
<signal name="TDI2">
<contactref element="SV2" pad="9"/>
<contactref element="E2" pad="14"/>
</signal>
<signal name="TDO2">
<contactref element="SV2" pad="3"/>
<contactref element="E2" pad="71"/>
</signal>
<signal name="TCK2">
<contactref element="SV2" pad="1"/>
<contactref element="E2" pad="62"/>
</signal>
<signal name="TP_AA1">
<contactref element="U$1" pad="AA1"/>
<contactref element="E2" pad="74"/>
<contactref element="SERIAL" pad="10"/>
<contactref element="RN2" pad="4"/>
</signal>
<signal name="TP_AB1">
<contactref element="U$1" pad="AB1"/>
<contactref element="E2" pad="73"/>
<contactref element="SERIAL" pad="9"/>
<contactref element="RN2" pad="5"/>
</signal>
<signal name="EMA0_L">
<contactref element="U$1" pad="AD2"/>
<contactref element="E2" pad="70"/>
</signal>
<signal name="EMA1_L">
<contactref element="U$1" pad="AE2"/>
<contactref element="E2" pad="69"/>
</signal>
<signal name="MD00_L">
<contactref element="U$1" pad="AK1"/>
<contactref element="E2" pad="67"/>
</signal>
<signal name="MD01_L">
<contactref element="U$1" pad="AL1"/>
<contactref element="E2" pad="65"/>
</signal>
<signal name="MD03_L">
<contactref element="U$1" pad="AP1"/>
<contactref element="E2" pad="63"/>
</signal>
<signal name="TP_BA1">
<contactref element="U$1" pad="BA1"/>
<contactref element="E2" pad="56"/>
<contactref element="SERIAL" pad="8"/>
<contactref element="RN2" pad="6"/>
</signal>
<signal name="TP_BB1">
<contactref element="U$1" pad="BB1"/>
<contactref element="E2" pad="55"/>
<contactref element="SERIAL" pad="7"/>
<contactref element="RN2" pad="7"/>
</signal>
<signal name="LOAD_CNTL">
<contactref element="U$1" pad="BH2"/>
<contactref element="E2" pad="54"/>
</signal>
<signal name="DATA03_L">
<contactref element="U$1" pad="AV1"/>
<contactref element="E2" pad="57"/>
</signal>
<signal name="MD04_L">
<contactref element="U$1" pad="BK1"/>
<contactref element="E2" pad="52"/>
</signal>
<signal name="MD05_L">
<contactref element="U$1" pad="BL1"/>
<contactref element="E2" pad="51"/>
</signal>
<signal name="MD06_L">
<contactref element="U$1" pad="BM1"/>
<contactref element="E2" pad="50"/>
</signal>
<signal name="MD07_L">
<contactref element="U$1" pad="BP1"/>
<contactref element="E2" pad="49"/>
</signal>
<signal name="INT_IN_PROGRESS_L">
<contactref element="U$1" pad="BP2"/>
<contactref element="E2" pad="48"/>
</signal>
<signal name="DATA05_L">
<contactref element="U$1" pad="BS1"/>
<contactref element="E2" pad="45"/>
</signal>
<signal name="DATA06_L">
<contactref element="U$1" pad="BU1"/>
<contactref element="E2" pad="44"/>
</signal>
<signal name="RUN_L">
<contactref element="U$1" pad="BU2"/>
<contactref element="E2" pad="41"/>
</signal>
<signal name="DATA07_L">
<contactref element="U$1" pad="BV1"/>
<contactref element="E2" pad="40"/>
</signal>
<signal name="POWER_OK">
<contactref element="U$1" pad="BV2"/>
<contactref element="E2" pad="39"/>
</signal>
<signal name="TS1_L">
<contactref element="U$1" pad="CK2"/>
<contactref element="E2" pad="29"/>
</signal>
<signal name="INTERNAL_IO_L">
<contactref element="U$1" pad="CL1"/>
<contactref element="E2" pad="28"/>
</signal>
<signal name="EMA2_L">
<contactref element="U$1" pad="AH2"/>
<contactref element="E2" pad="68"/>
</signal>
<signal name="USER_MODE_L">
<contactref element="U$1" pad="DM2"/>
<contactref element="E2" pad="8"/>
</signal>
<signal name="SW">
<contactref element="U$1" pad="DV2"/>
</signal>
<signal name="DATA00_L">
<contactref element="U$1" pad="AR1"/>
<contactref element="E2" pad="61"/>
</signal>
<signal name="DATA02_L">
<contactref element="U$1" pad="AU1"/>
<contactref element="E2" pad="58"/>
</signal>
<signal name="DATA01_L">
<contactref element="U$1" pad="AS1"/>
<contactref element="E2" pad="60"/>
</signal>
<signal name="DATA04_L">
<contactref element="U$1" pad="BR1"/>
<contactref element="E2" pad="46"/>
</signal>
<signal name="C0_L">
<contactref element="U$1" pad="CE1"/>
<contactref element="E2" pad="35"/>
</signal>
<signal name="TS3_L">
<contactref element="U$1" pad="CM2"/>
<contactref element="E2" pad="27"/>
</signal>
<signal name="CF1">
<contactref element="SERIAL" pad="11"/>
<contactref element="RN2" pad="3"/>
<contactref element="E2" pad="84"/>
</signal>
<signal name="CF0">
<contactref element="SERIAL" pad="12"/>
<contactref element="RN2" pad="2"/>
<contactref element="E2" pad="1"/>
<contactref element="TS_DISABLE" pad="2"/>
</signal>
<signal name="CLK">
<contactref element="E2" pad="83"/>
<contactref element="OSC" pad="5"/>
</signal>
<signal name="DCD">
<contactref element="USB" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="USB" pad="4"/>
</signal>
<signal name="TXD">
<contactref element="USB" pad="2"/>
<contactref element="E2" pad="76"/>
</signal>
<signal name="RXD">
<contactref element="USB" pad="3"/>
<contactref element="E2" pad="75"/>
</signal>
<signal name="CTS">
<contactref element="USB" pad="8"/>
</signal>
<signal name="DSR">
<contactref element="USB" pad="6"/>
</signal>
<signal name="RTS">
<contactref element="USB" pad="7"/>
</signal>
<signal name="RI">
<contactref element="USB" pad="9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
