<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="18.415" x2="0.635" y2="18.415" width="0" layer="20"/>
<text>MEMORY EXTENSION AND TIME SHARE</text>
<text>KM8E</text>
<text>+</text>
<text>+</text>
<text>CS*A B C D E F H J K L M N P R S T U V W X Y Z</text>
<text>+</text>
<text>M837</text>
</plain>
<libraries>
<library name="dec-con">
<description>DEC Edge Connectors and Parts</description>
<packages>
<package name="EDGE-CON8">
<description>Quad-Height DEC edge connector</description>
</package>
<package name="E12-8">
<description>A 0.8 inch electrolytic.</description>
</package>
<package name="NC1">
<description>NC Jumper, circular lobes</description>
</package>
<package name="C063-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="OMNIBUS">
<description>Quad-Height DEC board</description>
</package>
</packages>
</library>
<library name="atmel-cpld">
<description>5V CPLD w/ISP 

32 Macrocell, low power w/ISP, 5V</description>
<packages>
<package name="TH100B">
<description>Experimental 100 pin PQFP "pachage".</description>
</package>
</packages>
</library>
<library name="con-harting-ml">
<packages>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="02P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C33" library="dec-con" package="E12-8" value="6.8uF"/>
<element name="C34" library="dec-con" package="E12-8" value="6.8uF"/>
<element name="C35" library="dec-con" package="E12-8" value="6.8uF"/>
<element name="VCCINT" library="dec-con" package="NC1" value="JUMPER-NC1"/>
<element name="VCCIO" library="dec-con" package="NC1" value="JUMPER-NC1"/>
<element name="C1" library="dec-con" package="C063-025X075" value=".22uF"/>
<element name="C2" library="dec-con" package="C063-025X075" value=".22uF"/>
<element name="C3" library="dec-con" package="C063-025X075" value=".22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="dec-con" package="C063-025X075" value=".22uF"/>
<element name="E1" library="atmel-cpld" package="TH100B" value="ATF150X100X"/>
<element name="U$1" library="dec-con" package="EDGE-CON8" value="QUAD"/>
<element name="SV2" library="con-harting-ml" package="ML10" value=" ">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$2" library="dec-con" package="OMNIBUS" value="OUTLINE-OMNIBUS"/>
<element name="!TS" library="con-amp-quick" package="02P" value="Disable">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C35" pad="-"/>
<contactref element="C33" pad="-"/>
<contactref element="C34" pad="-"/>
<contactref element="U$1" pad="AN2"/>
<contactref element="U$1" pad="AT2"/>
<contactref element="U$1" pad="AF2"/>
<contactref element="U$1" pad="AC2"/>
<contactref element="U$1" pad="AN1"/>
<contactref element="U$1" pad="AT1"/>
<contactref element="U$1" pad="AF1"/>
<contactref element="U$1" pad="BT1"/>
<contactref element="U$1" pad="BN1"/>
<contactref element="U$1" pad="BF1"/>
<contactref element="U$1" pad="BC1"/>
<contactref element="U$1" pad="BF2"/>
<contactref element="U$1" pad="BC2"/>
<contactref element="U$1" pad="CN1"/>
<contactref element="U$1" pad="CC1"/>
<contactref element="U$1" pad="DT1"/>
<contactref element="U$1" pad="DN1"/>
<contactref element="U$1" pad="DF1"/>
<contactref element="U$1" pad="DC1"/>
<contactref element="U$1" pad="CC2"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="E1" pad="13"/>
<contactref element="E1" pad="28"/>
<contactref element="E1" pad="40"/>
<contactref element="E1" pad="45"/>
<contactref element="E1" pad="61"/>
<contactref element="E1" pad="76"/>
<contactref element="E1" pad="88"/>
<contactref element="E1" pad="97"/>
<contactref element="E1" pad="27"/>
<contactref element="SV2" pad="2"/>
<contactref element="SV2" pad="10"/>
<contactref element="E1" pad="P$26"/>
<contactref element="E1" pad="P$30"/>
<contactref element="E1" pad="P$24"/>
<contactref element="E1" pad="P$28"/>
<contactref element="!TS" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="C35" pad="+"/>
<contactref element="C33" pad="+"/>
<contactref element="C34" pad="+"/>
<contactref element="U$1" pad="AA2"/>
<contactref element="U$1" pad="BA2"/>
<contactref element="U$1" pad="CA2"/>
<contactref element="VCCIO" pad="1"/>
<contactref element="VCCINT" pad="1"/>
<contactref element="SV2" pad="4"/>
</signal>
<signal name="D_L">
<contactref element="E1" pad="70"/>
<contactref element="U$1" pad="DK2"/>
</signal>
<signal name="INT_RQST_L">
<contactref element="E1" pad="83"/>
<contactref element="U$1" pad="CP1"/>
</signal>
<signal name="IO_PAUSE_L">
<contactref element="E1" pad="92"/>
<contactref element="U$1" pad="CD1"/>
</signal>
<signal name="CPMA_DISABLE_L">
<contactref element="E1" pad="80"/>
<contactref element="U$1" pad="CU1"/>
</signal>
<signal name="IR01_L">
<contactref element="E1" pad="73"/>
<contactref element="U$1" pad="DE2"/>
</signal>
<signal name="DF_ENABLE">
<contactref element="E1" pad="94"/>
<contactref element="U$1" pad="CA1"/>
</signal>
<signal name="IR00_L">
<contactref element="E1" pad="74"/>
<contactref element="U$1" pad="DD2"/>
</signal>
<signal name="IND1_L">
<contactref element="E1" pad="79"/>
<contactref element="U$1" pad="CU2"/>
</signal>
<signal name="SKIP_L">
<contactref element="E1" pad="81"/>
<contactref element="U$1" pad="CS1"/>
</signal>
<signal name="IND2_L">
<contactref element="E1" pad="78"/>
<contactref element="U$1" pad="CV2"/>
</signal>
<signal name="MD10_L">
<contactref element="E1" pad="67"/>
<contactref element="U$1" pad="DM1"/>
</signal>
<signal name="MD08_L">
<contactref element="E1" pad="71"/>
<contactref element="U$1" pad="DK1"/>
</signal>
<signal name="MD09_L">
<contactref element="E1" pad="69"/>
<contactref element="U$1" pad="DL1"/>
</signal>
<signal name="TP2">
<contactref element="U$1" pad="CE2"/>
<contactref element="E1" pad="91"/>
</signal>
<signal name="C1_L">
<contactref element="E1" pad="90"/>
<contactref element="U$1" pad="CH1"/>
</signal>
<signal name="F_L">
<contactref element="E1" pad="72"/>
<contactref element="U$1" pad="DJ2"/>
</signal>
<signal name="INITIALIZE">
<contactref element="E1" pad="82"/>
<contactref element="U$1" pad="CR1"/>
</signal>
<signal name="TP3">
<contactref element="U$1" pad="CH2"/>
<contactref element="E1" pad="89"/>
</signal>
<signal name="DATA11_L">
<contactref element="E1" pad="56"/>
<contactref element="U$1" pad="DV1"/>
</signal>
<signal name="KEY_CTL_L">
<contactref element="E1" pad="57"/>
<contactref element="U$1" pad="DU2"/>
</signal>
<signal name="LOAD_ADDR">
<contactref element="E1" pad="60"/>
<contactref element="U$1" pad="DR2"/>
</signal>
<signal name="TS_DISABLE_L">
<contactref element="E1" pad="54"/>
<contactref element="!TS" pad="1"/>
</signal>
<signal name="F_SET_L">
<contactref element="E1" pad="63"/>
<contactref element="U$1" pad="DP2"/>
</signal>
<signal name="DATA08_L">
<contactref element="E1" pad="62"/>
<contactref element="U$1" pad="DR1"/>
</signal>
<signal name="MD11_L">
<contactref element="E1" pad="65"/>
<contactref element="U$1" pad="DP1"/>
</signal>
<signal name="DATA09_L">
<contactref element="E1" pad="59"/>
<contactref element="U$1" pad="DS1"/>
</signal>
<signal name="DATA10_L">
<contactref element="E1" pad="58"/>
<contactref element="U$1" pad="DU1"/>
</signal>
<signal name="VCCINT">
<contactref element="VCCINT" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="E1" pad="41"/>
<contactref element="E1" pad="93"/>
<contactref element="E1" pad="P$25"/>
<contactref element="E1" pad="P$23"/>
</signal>
<signal name="VCCIO">
<contactref element="VCCIO" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="E1" pad="20"/>
<contactref element="E1" pad="36"/>
<contactref element="E1" pad="53"/>
<contactref element="E1" pad="68"/>
<contactref element="E1" pad="84"/>
<contactref element="E1" pad="5"/>
<contactref element="E1" pad="P$27"/>
<contactref element="E1" pad="VCCIO@1"/>
<contactref element="E1" pad="P$29"/>
<contactref element="E1" pad="VCCIO@2"/>
</signal>
<signal name="TMS2">
<contactref element="E1" pad="17"/>
<contactref element="SV2" pad="5"/>
</signal>
<signal name="MD02_L">
<contactref element="U$1" pad="AM1"/>
<contactref element="E1" pad="16"/>
</signal>
<signal name="TP4">
<contactref element="U$1" pad="CJ2"/>
<contactref element="E1" pad="87"/>
</signal>
<signal name="TDI2">
<contactref element="SV2" pad="9"/>
<contactref element="E1" pad="6"/>
</signal>
<signal name="TDO2">
<contactref element="SV2" pad="3"/>
<contactref element="E1" pad="75"/>
</signal>
<signal name="TCK2">
<contactref element="SV2" pad="1"/>
<contactref element="E1" pad="64"/>
</signal>
<signal name="TP_AA1">
<contactref element="E1" pad="25"/>
<contactref element="U$1" pad="AA1"/>
</signal>
<signal name="TP_AB1">
<contactref element="E1" pad="24"/>
<contactref element="U$1" pad="AB1"/>
</signal>
<signal name="EMA0_L">
<contactref element="E1" pad="23"/>
<contactref element="U$1" pad="AD2"/>
</signal>
<signal name="EMA1_L">
<contactref element="E1" pad="22"/>
<contactref element="U$1" pad="AE2"/>
</signal>
<signal name="MD00_L">
<contactref element="E1" pad="19"/>
<contactref element="U$1" pad="AK1"/>
</signal>
<signal name="MD01_L">
<contactref element="E1" pad="18"/>
<contactref element="U$1" pad="AL1"/>
</signal>
<signal name="MD03_L">
<contactref element="E1" pad="15"/>
<contactref element="U$1" pad="AP1"/>
</signal>
<signal name="TP_BA1">
<contactref element="E1" pad="11"/>
<contactref element="U$1" pad="BA1"/>
</signal>
<signal name="TP_BB1">
<contactref element="E1" pad="10"/>
<contactref element="U$1" pad="BB1"/>
</signal>
<signal name="LOAD_CNTL">
<contactref element="E1" pad="9"/>
<contactref element="U$1" pad="BH2"/>
</signal>
<signal name="DATA03_L">
<contactref element="E1" pad="14"/>
<contactref element="U$1" pad="AV1"/>
</signal>
<signal name="MD04_L">
<contactref element="E1" pad="8"/>
<contactref element="U$1" pad="BK1"/>
</signal>
<signal name="MD05_L">
<contactref element="E1" pad="7"/>
<contactref element="U$1" pad="BL1"/>
</signal>
<signal name="MD06_L">
<contactref element="E1" pad="4"/>
<contactref element="U$1" pad="BM1"/>
</signal>
<signal name="MD07_L">
<contactref element="E1" pad="3"/>
<contactref element="U$1" pad="BP1"/>
</signal>
<signal name="INT_IN_PROGRESS_L">
<contactref element="E1" pad="2"/>
<contactref element="U$1" pad="BP2"/>
</signal>
<signal name="DATA05_L">
<contactref element="E1" pad="1"/>
<contactref element="U$1" pad="BS1"/>
</signal>
<signal name="DATA06_L">
<contactref element="E1" pad="100"/>
<contactref element="U$1" pad="BU1"/>
</signal>
<signal name="RUN_L">
<contactref element="E1" pad="99"/>
<contactref element="U$1" pad="BU2"/>
</signal>
<signal name="DATA07_L">
<contactref element="E1" pad="98"/>
<contactref element="U$1" pad="BV1"/>
</signal>
<signal name="POWER_OK">
<contactref element="E1" pad="96"/>
<contactref element="U$1" pad="BV2"/>
</signal>
<signal name="TS1_L">
<contactref element="U$1" pad="CK2"/>
<contactref element="E1" pad="86"/>
</signal>
<signal name="INTERNAL_IO_L">
<contactref element="U$1" pad="CL1"/>
<contactref element="E1" pad="85"/>
</signal>
<signal name="EMA2_L">
<contactref element="U$1" pad="AH2"/>
<contactref element="E1" pad="21"/>
</signal>
<signal name="USER_MODE_L">
<contactref element="U$1" pad="DM2"/>
<contactref element="E1" pad="66"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
