<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20"/>
<wire x1="1.27" y1="0" x2="49.53" y2="0" width="0" layer="20"/>
<wire x1="49.53" y1="0" x2="50.8" y2="1.27" width="0" layer="20"/>
<wire x1="50.8" y1="72.39" x2="49.53" y2="73.66" width="0" layer="20"/>
<wire x1="49.53" y1="73.66" x2="1.27" y2="73.66" width="0" layer="20"/>
<wire x1="1.27" y1="73.66" x2="0" y2="72.39" width="0" layer="20"/>
<wire x1="0" y1="72.39" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="50.8" y1="1.27" x2="50.8" y2="72.39" width="0" layer="20"/>
</plain>
<libraries>
<library name="dec-con">
<description>DEC Edge Connectors and Parts</description>
<packages>
<package name="DEC40PINH">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-thomas-betts">
<description>&lt;b&gt;Thomas &amp; Betts Connectors&lt;/b&gt;&lt;p&gt;
Based on Thomas &amp; Betts Catalog &lt;i&gt;Electronioc Interconnects European Edition 1998&lt;/i&gt;.&lt;p&gt;
Created 10.06.1999&lt;br&gt;
Packages changed/corrected 22.02.2006 librarian@cadsoft.de&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="H2M09RA">
<description>&lt;b&gt;THOMAS&amp;BETTS&lt;/b&gt; H2M09RA29A</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="dec-con" package="DEC40PINH" value="Digital In"/>
<element name="X1" library="con-thomas-betts" package="H2M09RA" value="D-SUB9-H2M09RA">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="D1" library="diode" package="DO35-10" value="1N4148"/>
<element name="D2" library="diode" package="DO35-10" value="1N4148"/>
<element name="X2" library="con-thomas-betts" package="H2M09RA" value="D-SUB9-H2M09RA">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="D3" library="diode" package="DO35-10" value="1N4148"/>
<element name="D4" library="diode" package="DO35-10" value="1N4148"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="A"/>
<contactref element="J2" pad="C"/>
<contactref element="J2" pad="E"/>
<contactref element="J2" pad="H"/>
<contactref element="J2" pad="K"/>
<contactref element="J2" pad="M"/>
<contactref element="J2" pad="P"/>
<contactref element="J2" pad="U"/>
<contactref element="J2" pad="S"/>
<contactref element="J2" pad="W"/>
<contactref element="J2" pad="Y"/>
<contactref element="J2" pad="AA"/>
<contactref element="J2" pad="CC"/>
<contactref element="J2" pad="EE"/>
<contactref element="J2" pad="MM"/>
<contactref element="J2" pad="KK"/>
<contactref element="J2" pad="HH"/>
<contactref element="J2" pad="PP"/>
<contactref element="X1" pad="8"/>
<contactref element="X2" pad="8"/>
</signal>
<signal name="VCC">
<contactref element="J2" pad="SS"/>
<contactref element="J2" pad="UU"/>
</signal>
<signal name="P1THRST">
<contactref element="J2" pad="J"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="P2THRST">
<contactref element="J2" pad="BB"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="P1DOWN">
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="P1LEFT">
<contactref element="X1" pad="3"/>
<contactref element="D2" pad="A"/>
<contactref element="J2" pad="F"/>
</signal>
<signal name="P1RIGHT">
<contactref element="X1" pad="4"/>
<contactref element="D1" pad="A"/>
<contactref element="J2" pad="D"/>
</signal>
<signal name="P1FIRE">
<contactref element="X1" pad="6"/>
<contactref element="J2" pad="B"/>
</signal>
<signal name="P2DOWN">
<contactref element="D4" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="P2LEFT">
<contactref element="X2" pad="3"/>
<contactref element="D4" pad="A"/>
<contactref element="J2" pad="Z"/>
</signal>
<signal name="P2RIGHT">
<contactref element="X2" pad="4"/>
<contactref element="D3" pad="A"/>
<contactref element="J2" pad="X"/>
</signal>
<signal name="P2FIRE">
<contactref element="X2" pad="6"/>
<contactref element="J2" pad="V"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
