<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="48.26" y1="48.26" x2="50.8" y2="48.26" width="0" layer="20"/>
<wire x1="50.8" y1="48.26" x2="50.8" y2="15.24" width="0" layer="20"/>
<wire x1="50.8" y1="15.24" x2="48.26" y2="15.24" width="0" layer="20"/>
<wire x1="48.26" y1="15.24" x2="48.26" y2="48.26" width="0" layer="20"/>
<text>CABLE CONNECTOR M901B</text>
<text>C:/Users/Vince/Documents/websvn/trunk/Eagle/projects/DEC/Mxxx/M901/M901Bfrontb.bmp</text>
<text>C:/Users/Vince/Documents/websvn/trunk/Eagle/projects/DEC/Mxxx/M901/M901Bbackfb.bmp</text>
<hole x="74.93" y="5.715" drill="3.175"/>
<hole x="74.93" y="56.515" drill="3.175"/>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="EDGE-CON2">
<description>Single-Height DEC edge connector</description>
</package>
<package name="SINGLE">
<description>Single-Height DEC board</description>
</package>
<package name="FLEX19">
<description>19 SMT pads on 0.0625" centers</description>
</package>
<package name="FLIPCHIP">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dec-con" package="EDGE-CON2" value=""/>
<element name="U$2" library="dec-con" package="SINGLE" value="OUTLINE-SINGLE"/>
<element name="BFLEX" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="TFLEX" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="R1" library="rcl" package="0207/10" value="10"/>
<element name="R2" library="rcl" package="0207/10" value="10"/>
<element name="R3" library="rcl" package="0207/10" value="10"/>
<element name="R4" library="rcl" package="0207/10" value="10"/>
<element name="U$3" library="dec-con" package="FLIPCHIP" value=""/>
</elements>
<signals>
<signal name="N$4">
<contactref element="U$1" pad="D1"/>
<contactref element="TFLEX" pad="16"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="E1"/>
<contactref element="TFLEX" pad="15"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="H1"/>
<contactref element="TFLEX" pad="13"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="J1"/>
<contactref element="TFLEX" pad="12"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="L1"/>
<contactref element="TFLEX" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="M1"/>
<contactref element="TFLEX" pad="9"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="P1"/>
<contactref element="TFLEX" pad="7"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="S1"/>
<contactref element="TFLEX" pad="5"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="D2"/>
<contactref element="BFLEX" pad="16"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="E2"/>
<contactref element="BFLEX" pad="15"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="H2"/>
<contactref element="BFLEX" pad="13"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="K2"/>
<contactref element="BFLEX" pad="11"/>
</signal>
<signal name="N$29">
<contactref element="U$1" pad="M2"/>
<contactref element="BFLEX" pad="9"/>
</signal>
<signal name="N$31">
<contactref element="U$1" pad="P2"/>
<contactref element="BFLEX" pad="7"/>
</signal>
<signal name="N$33">
<contactref element="U$1" pad="S2"/>
<contactref element="BFLEX" pad="5"/>
</signal>
<signal name="N$34">
<contactref element="U$1" pad="T2"/>
<contactref element="BFLEX" pad="4"/>
</signal>
<signal name="N$36">
<contactref element="U$1" pad="V2"/>
<contactref element="BFLEX" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="U$1" pad="B1"/>
<contactref element="TFLEX" pad="18"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="T1"/>
<contactref element="TFLEX" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="A1"/>
<contactref element="TFLEX" pad="19"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="C1"/>
<contactref element="TFLEX" pad="17"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="F1"/>
<contactref element="TFLEX" pad="14"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="K1"/>
<contactref element="TFLEX" pad="11"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="N1"/>
<contactref element="TFLEX" pad="8"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="R1"/>
<contactref element="TFLEX" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="U2"/>
<contactref element="BFLEX" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="R2"/>
<contactref element="BFLEX" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="N2"/>
<contactref element="BFLEX" pad="8"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="L2"/>
<contactref element="BFLEX" pad="10"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="J2"/>
<contactref element="BFLEX" pad="12"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="F2"/>
<contactref element="BFLEX" pad="14"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="C2"/>
<contactref element="BFLEX" pad="17"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="A2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="BFLEX" pad="19"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="R4" pad="2"/>
<contactref element="BFLEX" pad="18"/>
</signal>
<signal name="N$32">
<contactref element="U$1" pad="B2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="TFLEX" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="TFLEX" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="U$1" pad="U1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="V1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
