<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="60.96" y1="48.26" x2="63.5" y2="48.26" width="0" layer="20"/>
<wire x1="63.5" y1="48.26" x2="63.5" y2="15.24" width="0" layer="20"/>
<wire x1="63.5" y1="15.24" x2="60.96" y2="15.24" width="0" layer="20"/>
<wire x1="60.96" y1="15.24" x2="60.96" y2="48.26" width="0" layer="20"/>
<text>M903B</text>
<text>C:/Users/Vince/Documents/websvn/trunk/Eagle/projects/DEC/Mxxx/M903/M903Bfrontb.bmp</text>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="EDGE-CON2">
<description>Single-Height DEC edge connector</description>
</package>
<package name="SINGLE">
<description>Single-Height DEC board</description>
</package>
<package name="FLEX19">
<description>19 SMT pads on 0.0625" centers</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dec-con" package="EDGE-CON2" value=""/>
<element name="U$2" library="dec-con" package="SINGLE" value="OUTLINE-SINGLE"/>
<element name="BFLEX" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="TFLEX" library="dec-con" package="FLEX19" value="FLEX19"/>
</elements>
<signals>
<signal name="N$4">
<contactref element="U$1" pad="D1"/>
<contactref element="TFLEX" pad="16"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="E1"/>
<contactref element="TFLEX" pad="14"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="H1"/>
<contactref element="TFLEX" pad="12"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="J1"/>
<contactref element="TFLEX" pad="10"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="L1"/>
<contactref element="TFLEX" pad="8"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="M1"/>
<contactref element="TFLEX" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="P1"/>
<contactref element="TFLEX" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="S1"/>
<contactref element="TFLEX" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="D2"/>
<contactref element="BFLEX" pad="18"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="E2"/>
<contactref element="BFLEX" pad="16"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="H2"/>
<contactref element="BFLEX" pad="14"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="K2"/>
<contactref element="BFLEX" pad="12"/>
</signal>
<signal name="N$29">
<contactref element="U$1" pad="M2"/>
<contactref element="BFLEX" pad="10"/>
</signal>
<signal name="N$31">
<contactref element="U$1" pad="P2"/>
<contactref element="BFLEX" pad="8"/>
</signal>
<signal name="N$33">
<contactref element="U$1" pad="S2"/>
<contactref element="BFLEX" pad="6"/>
</signal>
<signal name="N$34">
<contactref element="U$1" pad="T2"/>
<contactref element="BFLEX" pad="4"/>
</signal>
<signal name="N$36">
<contactref element="U$1" pad="V2"/>
<contactref element="BFLEX" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="U$1" pad="B1"/>
<contactref element="TFLEX" pad="18"/>
</signal>
<signal name="GND1">
<contactref element="U$1" pad="A1"/>
<contactref element="TFLEX" pad="19"/>
<contactref element="U$1" pad="C1"/>
<contactref element="TFLEX" pad="17"/>
<contactref element="U$1" pad="F1"/>
<contactref element="TFLEX" pad="13"/>
<contactref element="U$1" pad="K1"/>
<contactref element="TFLEX" pad="9"/>
<contactref element="U$1" pad="N1"/>
<contactref element="TFLEX" pad="5"/>
<contactref element="U$1" pad="R1"/>
<contactref element="TFLEX" pad="3"/>
<contactref element="U$1" pad="T1"/>
<contactref element="TFLEX" pad="1"/>
</signal>
<signal name="GND2">
<contactref element="U$1" pad="C2"/>
<contactref element="BFLEX" pad="19"/>
<contactref element="U$1" pad="F2"/>
<contactref element="BFLEX" pad="15"/>
<contactref element="U$1" pad="J2"/>
<contactref element="BFLEX" pad="13"/>
<contactref element="U$1" pad="L2"/>
<contactref element="BFLEX" pad="11"/>
<contactref element="U$1" pad="N2"/>
<contactref element="BFLEX" pad="9"/>
<contactref element="U$1" pad="R2"/>
<contactref element="BFLEX" pad="7"/>
<contactref element="U$1" pad="U2"/>
<contactref element="BFLEX" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
