<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 14:34:29</description>
<packages>
<package name="SOIC127P600X175-16N">
</package>
<package name="QFP80P900X900X160-32N">
</package>
<package name="SOP65P640X120-24N">
</package>
<package name="SOP65P490X110-8N">
</package>
<package name="SOIC127P600X175-8N">
</package>
<package name="QFN50P500X500X100-32N">
</package>
<package name="SOP63P600X175-24N">
</package>
<package name="SOP63P600X175-16N">
</package>
<package name="SOIC127P1021X265-20N">
</package>
<package name="SOIC127P1030X265-20N">
</package>
<package name="DIP254P762X533-8">
</package>
<package name="SOIC127P1031X265-24N">
</package>
<package name="DIP254P762X444-16">
</package>
<package name="SOIC127P600X173-16N">
</package>
<package name="DIP254P762X445-8">
</package>
<package name="SOIC127P600X175-14N">
</package>
<package name="DIP254P762X469-14">
</package>
<package name="SOP65P640X120-14N">
</package>
<package name="SOT65P210X110-5N">
</package>
<package name="SOT95P275X110-5N">
</package>
<package name="SOT95P240X110-3N">
</package>
<package name="SOT95P240X111-3N">
</package>
<package name="PLCC127P1257X1257X457-28N">
</package>
<package name="PLCC127P1244X1244X457-28N">
</package>
<package name="SOP65P640X120-20N">
</package>
<package name="SOP65P640X120-16N">
</package>
<package name="SOIC127P1030X265-24N">
</package>
<package name="SOIC127P1030X265-16N">
</package>
<package name="DIP254P762X457-18">
</package>
<package name="DIP254P762X469-16">
</package>
<package name="DIP254P762X457-20">
</package>
<package name="SOP50P810X110-48N">
</package>
<package name="SOT95P275X110-6N">
</package>
<package name="SOP65P640X110-8N">
</package>
<package name="QFN50P300X300X100-17N">
</package>
<package name="SOIC127P600X172-8N">
</package>
<package name="SOT95P280X110-5N">
</package>
<package name="DFN200X200X55-7N">
</package>
<package name="SOP95P275X110-6N">
</package>
<package name="BGA12C50P4X3_150X200X60">
</package>
<package name="BGA9C50P3X3_145X145X66">
</package>
<package name="DFN600X500X100-19N">
</package>
<package name="SOP95P275X110-5N">
</package>
<package name="DFN120X120X40-6N">
</package>
<package name="DFN300X330X90-6N">
</package>
<package name="DFN300X300X55-13N">
</package>
<package name="SOIC127P600X175-9N">
</package>
<package name="DFN300X300X100-10N">
</package>
<package name="SOP50P310X90-8N">
</package>
<package name="SOT65P210X110-6N">
</package>
</packages>
<symbols>
<symbol name="74HC595DG">
<pin name="VCC" direction="pwr"/>
<pin name="OUT_EN" direction="in"/>
<pin name="A" direction="in"/>
<pin name="SQH" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="LATCH_CLOCK" direction="in"/>
<pin name="SHIFT_CLOCK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QH" direction="out"/>
</symbol>
<symbol name="A5191HRTLG-XTD">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="TXD" direction="in"/>
<pin name="RXA" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="RXAFI" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="CDREF" direction="in"/>
<pin name="AREF" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="TEST1" direction="in"/>
<pin name="TEST2" direction="nc"/>
<pin name="TEST3" direction="nc"/>
<pin name="TEST4" direction="nc"/>
<pin name="TEST5" direction="in"/>
<pin name="TEST7" direction="in"/>
<pin name="TEST8" direction="in"/>
<pin name="TEST9" direction="in"/>
<pin name="TEST10" direction="in"/>
<pin name="TEST11" direction="nc"/>
<pin name="TEST12" direction="nc"/>
<pin name="VSS_2" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="VSSA_2" direction="pas"/>
<pin name="VSSA" direction="pas"/>
<pin name="CD" direction="out"/>
<pin name="RXD" direction="out"/>
<pin name="TXA" direction="out"/>
<pin name="RXAF" direction="out"/>
<pin name="XOUT" direction="out"/>
<pin name="CBIAS" direction="out"/>
</symbol>
<symbol name="ADM1024ARUZ">
<pin name="VCCP2/D2-" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="+VCCP1" direction="pwr"/>
<pin name="+2.5VIN/D2+" direction="in"/>
<pin name="+5.0VIN" direction="in"/>
<pin name="+12VIN" direction="in"/>
<pin name="~RESET"/>
<pin name="FAN1/AIN1" direction="in"/>
<pin name="FAN2/AIN2" direction="in"/>
<pin name="D1-" direction="in"/>
<pin name="D1+" direction="in"/>
<pin name="VID0/IRQ0" direction="in"/>
<pin name="VID1/IRQ1" direction="in"/>
<pin name="VID2/IRQ2" direction="in"/>
<pin name="VID3/IRQ3" direction="in"/>
<pin name="VID4/IRQ4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="NTEST_OUT/ADD"/>
<pin name="NTEST_IN/AOUT"/>
<pin name="SDA"/>
<pin name="SCL" direction="out"/>
<pin name="~INT" direction="out"/>
<pin name="~THERM"/>
<pin name="CI"/>
</symbol>
<symbol name="ADM1032ARMZ">
<pin name="VDD" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="D+" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~ALERT" direction="out"/>
<pin name="~THERM" direction="out"/>
<pin name="SDATA"/>
</symbol>
<symbol name="ADM1032ARZ">
<pin name="VDD" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="D+" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~ALERT" direction="out"/>
<pin name="~THERM" direction="out"/>
<pin name="SDATA"/>
</symbol>
<symbol name="ADT7461ARMZ">
<pin name="VDD" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="SDATA"/>
<pin name="D+" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~ALERT/~THERM2" direction="out"/>
<pin name="~THERM" direction="out"/>
</symbol>
<symbol name="ADT7462ACPZ-5RL7">
<pin name="VCC" direction="pwr"/>
<pin name="VCCP1/+1.5V/+1.8V/+2.5V" direction="pwr"/>
<pin name="VCCP2/+1.5V/+1.8V/+2.5V" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="ADD" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="D1-/SCSI_TERM1" direction="in"/>
<pin name="D1+/+2.5V/+1.8V_15" direction="in"/>
<pin name="D2-" direction="in"/>
<pin name="D2+" direction="in"/>
<pin name="D3+/+1.25V/+0.9V" direction="in"/>
<pin name="D3-/SCSI_TERM2" direction="in"/>
<pin name="~FAN2MAX/CI" direction="pwr"/>
<pin name="TACH5/+12V1" direction="in"/>
<pin name="TACH6/+12V2" direction="in"/>
<pin name="TACH7/+5V" direction="in"/>
<pin name="TACH8/+12V3" direction="in"/>
<pin name="VID0/GPIO1/TACH1" direction="in"/>
<pin name="VID1/GPIO2/TACH2" direction="in"/>
<pin name="VID2/GPIO3/TACH3" direction="in"/>
<pin name="VID3/GPIO4/TACH4" direction="in"/>
<pin name="VID4/GPIO5/PWM1" direction="in"/>
<pin name="VID5/GPIO6/PWM2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SDA"/>
<pin name="~ALERT" direction="out"/>
<pin name="PWM3" direction="out"/>
<pin name="PWM4/+3.3V" direction="out"/>
<pin name="~THERM1/+1.5V1/GPIO7/VID6" direction="out"/>
<pin name="~THERM2/+1.5V2/GPIO8" direction="out"/>
<pin name="VR_HOT1/+1.2V1/+3.3V" direction="out"/>
<pin name="VR_HOT2/+1.2V2/V_BATT" direction="out"/>
</symbol>
<symbol name="ADT7463ARQZ">
<pin name="VCCP" direction="pwr"/>
<pin name="+12VIN/VID5" direction="pwr"/>
<pin name="+5VIN/~THERM" direction="pwr"/>
<pin name="+2.5VIN/~SMBALERT" direction="pwr"/>
<pin name="VID0" direction="in"/>
<pin name="VID1" direction="in"/>
<pin name="VID2" direction="in"/>
<pin name="VID3" direction="in"/>
<pin name="VID4" direction="in"/>
<pin name="D1-" direction="in"/>
<pin name="D1+" direction="in"/>
<pin name="D2+" direction="in"/>
<pin name="D2-" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="TACH1" direction="in"/>
<pin name="TACH2" direction="in"/>
<pin name="TACH3" direction="in"/>
<pin name="TACH4/ADDRESS_SELECT/~THERM" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="SDA"/>
<pin name="PWM1/XTO"/>
<pin name="PWM2/~SMBALERT" direction="in"/>
<pin name="PWM3/~ADDRESS_ENABLE"/>
</symbol>
<symbol name="ADT7467ARQZ">
<pin name="VCC" direction="pwr"/>
<pin name="VCCP" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="D1+" direction="in"/>
<pin name="D1-" direction="in"/>
<pin name="D2+" direction="in"/>
<pin name="D2-" direction="in"/>
<pin name="TACH1" direction="in"/>
<pin name="TACH2" direction="in"/>
<pin name="TACH3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="PWM1/XTO" direction="out"/>
<pin name="PWM2/~SMBALERT" direction="out"/>
<pin name="PWM3"/>
<pin name="TACH4/GPIO/~THERM/~SMBALERT"/>
</symbol>
<symbol name="AMIS30624C6244RG">
<pin name="VDD" direction="pwr"/>
<pin name="VBB_2" direction="pwr"/>
<pin name="VBB" direction="pwr"/>
<pin name="VCP" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="TST1" direction="in"/>
<pin name="TST2" direction="in"/>
<pin name="CPN" direction="pas"/>
<pin name="CPP" direction="pas"/>
<pin name="HW" direction="in"/>
<pin name="SWI" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="MOTYN" direction="out"/>
<pin name="MOTYP" direction="out"/>
<pin name="MOTXN" direction="out"/>
<pin name="MOTXP" direction="out"/>
</symbol>
<symbol name="AMIS30660CANH2G">
<pin name="VCC" direction="pwr"/>
<pin name="CANL" direction="in"/>
<pin name="CANH" direction="in"/>
<pin name="TXD" direction="in"/>
<pin name="S" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
<pin name="RXD" direction="out"/>
</symbol>
<symbol name="AMIS30663CANG2G">
<pin name="VCC" direction="pwr"/>
<pin name="TXD" direction="in"/>
<pin name="V33" direction="in"/>
<pin name="CANL" direction="in"/>
<pin name="CANH" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
<pin name="RXD" direction="out"/>
</symbol>
<symbol name="AMIS42770ICAW1RG">
<pin name="VCC" direction="pwr"/>
<pin name="~EN1" direction="in"/>
<pin name="~EN2" direction="in"/>
<pin name="TEXT" direction="in"/>
<pin name="TX0" direction="in"/>
<pin name="VREF1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="CANL1"/>
<pin name="CANL2"/>
<pin name="CANH1"/>
<pin name="CANH2"/>
<pin name="RX0" direction="out"/>
<pin name="RINT" direction="out"/>
</symbol>
<symbol name="CAT24C04LI-G">
<pin name="VCC" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="WP" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="SDA"/>
</symbol>
<symbol name="CAT24C16LI-G">
<pin name="VCC" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="WP" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="SDA"/>
</symbol>
<symbol name="CAT24C44LI">
<pin name="VCC" direction="pwr"/>
<pin name="~RECALL" direction="in"/>
<pin name="~STORE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="SK" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="CAT25020LI-G">
<pin name="VCC" direction="pwr"/>
<pin name="SCK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="~WP" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="~HOLD" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="SO" direction="out"/>
</symbol>
<symbol name="CAT25256LI-G">
<pin name="VCC" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="~WP" direction="in"/>
<pin name="~HOLD" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="~SO" direction="out"/>
</symbol>
<symbol name="CAT93C56LI-G">
<pin name="VCC" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="ORG" direction="in"/>
<pin name="SK" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="CAT9532WI">
<pin name="VCC" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="VSS" direction="in"/>
<pin name="LED0" direction="out"/>
<pin name="LED1" direction="out"/>
<pin name="LED2" direction="out"/>
<pin name="LED3" direction="out"/>
<pin name="LED4" direction="out"/>
<pin name="LED5" direction="out"/>
<pin name="LED6" direction="out"/>
<pin name="LED7" direction="out"/>
<pin name="LED8" direction="out"/>
<pin name="LED9" direction="out"/>
<pin name="LED10" direction="out"/>
<pin name="LED11" direction="out"/>
<pin name="LED12" direction="out"/>
<pin name="LED13" direction="out"/>
<pin name="LED14" direction="out"/>
<pin name="LED15" direction="out"/>
</symbol>
<symbol name="CS5171ED8G">
<pin name="VCC" direction="pwr"/>
<pin name="VC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="pas"/>
<pin name="TEST" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="CS8182YDFR8G">
<pin name="VIN" direction="pwr"/>
<pin name="ADJ" direction="in"/>
<pin name="VREF/ENABLE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="CS8190EDWFR20G">
<pin name="VCC" direction="pwr"/>
<pin name="CP+" direction="in"/>
<pin name="CP-" direction="in"/>
<pin name="FREQIN" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SQOUT" direction="out"/>
<pin name="COS+" direction="out"/>
<pin name="COS-" direction="out"/>
<pin name="SIN-" direction="out"/>
<pin name="SIN+" direction="out"/>
<pin name="VREG" direction="out"/>
<pin name="F/VOUT" direction="out"/>
</symbol>
<symbol name="CS8190ENF16G">
<pin name="VCC" direction="pwr"/>
<pin name="CP-" direction="in"/>
<pin name="CP+" direction="in"/>
<pin name="BIAS" direction="pas"/>
<pin name="FREQIN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SINE+" direction="out"/>
<pin name="SINE-" direction="out"/>
<pin name="F/VOUT" direction="out"/>
<pin name="SQOUT" direction="out"/>
<pin name="VREG" direction="out"/>
<pin name="COS+" direction="out"/>
<pin name="COS-" direction="out"/>
</symbol>
<symbol name="FS6370-01G-XTD">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="XIN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="SEL_CD" direction="in"/>
<pin name="PD/SCL" direction="in"/>
<pin name="OE/SDA"/>
<pin name="VSS_2" direction="pas"/>
<pin name="VSS_3" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="XOUT" direction="out"/>
<pin name="CLK_A" direction="out"/>
<pin name="CLK_B" direction="out"/>
<pin name="CLK_C" direction="out"/>
<pin name="CLK_D" direction="out"/>
</symbol>
<symbol name="FS6377-01G-XTD">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="XIN" direction="in"/>
<pin name="SEL_CD" direction="in"/>
<pin name="ADDR" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="VSS_2" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="XOUT" direction="out"/>
<pin name="OE" direction="out"/>
<pin name="CLK_D" direction="out"/>
<pin name="CLK_C" direction="out"/>
<pin name="CLK_B" direction="out"/>
<pin name="CLK_A" direction="out"/>
<pin name="SDA"/>
</symbol>
<symbol name="FS7140-01G-XTD">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="XIN" direction="in"/>
<pin name="ADDR0" direction="in"/>
<pin name="ADDR1" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="IPRG" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="VSS_2" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="XOUT" direction="out"/>
<pin name="CLKP" direction="out"/>
<pin name="CLKN" direction="out"/>
<pin name="SDA"/>
</symbol>
<symbol name="LM201ANG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_2" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="OFS_2" direction="pas"/>
<pin name="OFS" direction="pas"/>
<pin name="COMP" direction="pas"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM211DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="BALANCE/STROBE" direction="in"/>
<pin name="BALANCE" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM224DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE,_GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM224DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE,_GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM224NG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="LM239DG">
<pin name="VCC" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM239NG">
<pin name="VCC" direction="pwr"/>
<pin name="-IN_1" direction="in"/>
<pin name="+IN_1" direction="in"/>
<pin name="-IN_2" direction="in"/>
<pin name="+IN_2" direction="in"/>
<pin name="-IN_3" direction="in"/>
<pin name="+IN_3" direction="in"/>
<pin name="-IN_4" direction="in"/>
<pin name="+IN_4" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="LM2574N-5G">
<pin name="VIN" direction="pwr"/>
<pin name="FB"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="SIG_GND" direction="pas"/>
<pin name="PWR_GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM258DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_A" direction="in"/>
<pin name="POS_IN_A" direction="in"/>
<pin name="NEG_IN_B" direction="in"/>
<pin name="POS_IN_B" direction="in"/>
<pin name="VEE/GND" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM2901DTBR2G">
<pin name="VCC" direction="pwr"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT3" direction="out"/>
</symbol>
<symbol name="LM2901NG">
<pin name="VCC" direction="pwr"/>
<pin name="-IN_1" direction="in"/>
<pin name="+IN_1" direction="in"/>
<pin name="+IN_2" direction="in"/>
<pin name="-IN_2" direction="in"/>
<pin name="-IN_3" direction="in"/>
<pin name="+IN_3" direction="in"/>
<pin name="-IN_4" direction="in"/>
<pin name="+IN_4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="LM2901VDTBR2G">
<pin name="VCC" direction="pwr"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT3" direction="out"/>
</symbol>
<symbol name="LM2902DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE,_GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM2902NG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="LM2903VDG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_A" direction="in"/>
<pin name="POS_IN_A" direction="in"/>
<pin name="NEG_IN_B" direction="in"/>
<pin name="POS_IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM2903VDR2G">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_A" direction="in"/>
<pin name="POS_IN_A" direction="in"/>
<pin name="NEG_IN_B" direction="in"/>
<pin name="POS_IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM2904NG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_A_2" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_B_2" direction="in"/>
<pin name="VEE/GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM2931ACDG">
<pin name="IN" direction="pwr"/>
<pin name="ADJUST" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="OUT_INHIBIT" direction="out"/>
</symbol>
<symbol name="LM2931AD-5.0G">
<pin name="IN" direction="pwr"/>
<pin name="ADJUST" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="OUT_INHIBIT" direction="out"/>
</symbol>
<symbol name="LM2931CDG">
<pin name="IN" direction="pwr"/>
<pin name="ADJUST" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="OUT_INHIBIT" direction="out"/>
</symbol>
<symbol name="LM2931CDR2G">
<pin name="IN" direction="pwr"/>
<pin name="ADJUST" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="OUT_INHIBIT" direction="out"/>
</symbol>
<symbol name="LM2931D-5.0G">
<pin name="IN" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM301ADG">
<pin name="VCC" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="BALANCE_2" direction="in"/>
<pin name="BALANCE" direction="in"/>
<pin name="NEG_IN" direction="in"/>
<pin name="POS_IN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM301ANG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_2" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="OFS_2" direction="pas"/>
<pin name="OFS" direction="pas"/>
<pin name="COMP" direction="pas"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM311DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN" direction="in"/>
<pin name="POS_IN" direction="in"/>
<pin name="BALANCE/STROBE" direction="in"/>
<pin name="BALANCE" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM311NG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_2" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="OFS" direction="pas"/>
<pin name="OFS/STRB" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM317LBDG">
<pin name="VIN" direction="pwr"/>
<pin name="ADJUST" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT_3" direction="out"/>
<pin name="VOUT_4" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM317LDG">
<pin name="VIN" direction="pwr"/>
<pin name="ADJUST" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT_3" direction="out"/>
<pin name="VOUT_4" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM317LDR2G">
<pin name="VIN" direction="pwr"/>
<pin name="ADJUST" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT_3" direction="out"/>
<pin name="VOUT_4" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM324ANG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE,GND" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="LM324DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE,_GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM324DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE,_GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM339DR2G">
<pin name="VCC" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM339NG">
<pin name="VCC" direction="pwr"/>
<pin name="+IN_1" direction="in"/>
<pin name="-IN_1" direction="in"/>
<pin name="-IN_2" direction="in"/>
<pin name="+IN_2" direction="in"/>
<pin name="-IN_3" direction="in"/>
<pin name="+IN_3" direction="in"/>
<pin name="-IN_4" direction="in"/>
<pin name="+IN_4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="LM358DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_A" direction="in"/>
<pin name="POS_IN_A" direction="in"/>
<pin name="NEG_IN_B" direction="in"/>
<pin name="POS_IN_B" direction="in"/>
<pin name="VEE/GND" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM358DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_A" direction="in"/>
<pin name="POS_IN_A" direction="in"/>
<pin name="NEG_IN_B" direction="in"/>
<pin name="POS_IN_B" direction="in"/>
<pin name="VEE/GND" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM358NG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_A_2" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_B_2" direction="in"/>
<pin name="VEE/GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM385BD-1.2G">
<pin name="ANODE" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C._6" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="CATHODE" direction="out"/>
</symbol>
<symbol name="LM393DG.">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_A_2" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_B_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM393DG">
<pin name="VCC" direction="pwr"/>
<pin name="+IN_A" direction="in"/>
<pin name="-IN_A" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM393DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_A_2" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_B_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM393NG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_A_2" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_B_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM833NG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="LP2951ACDG">
<pin name="IN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="VO_TAP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="~ERROR_OUT" direction="out"/>
</symbol>
<symbol name="LP2951ACDR2G">
<pin name="IN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="VO_TAP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="~ERROR_OUT" direction="out"/>
</symbol>
<symbol name="LP2951ACNG">
<pin name="INPUT" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="VO_TAP" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="SHUTDOWN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~ERROR_OUTPUT" direction="out"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2951CD-3.3R2G">
<pin name="IN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="VO_TAP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="~ERROR_OUT" direction="out"/>
</symbol>
<symbol name="LP2951CDG">
<pin name="IN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="VO_TAP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="~ERROR_OUT" direction="out"/>
</symbol>
<symbol name="M74VHC1G125DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="M74VHC1G132DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y" direction="out"/>
</symbol>
<symbol name="M74VHC1GT00DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="M74VHC1GT04DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y" direction="out"/>
</symbol>
<symbol name="M74VHC1GT08DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="M74VHC1GT125DF1G">
<pin name="VCC" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="M74VHC1GT126DF1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="M74VHC1GT126DT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="M74VHC1GT14DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y" direction="out"/>
</symbol>
<symbol name="M74VHC1GT32DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="M74VHC1GT50DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="M74VHC1GT50DTT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="M74VHC1GT86DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MAX809JTRG">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="MAX809STRG">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="MAX809TTRG">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="MAX810MTRG">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="RESET" direction="out"/>
</symbol>
<symbol name="MAX810RTRG">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="RESET" direction="out"/>
</symbol>
<symbol name="MC100E016FNG">
<pin name="VCC" direction="pwr"/>
<pin name="VCCO_2" direction="pwr"/>
<pin name="VCCO_3" direction="pwr"/>
<pin name="VCCO" direction="pwr"/>
<pin name="~CE" direction="in"/>
<pin name="~PE" direction="in"/>
<pin name="MR" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="TCLD" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="~TC" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC100E111FNG">
<pin name="VCC" direction="pwr"/>
<pin name="VCCO_2" direction="pwr"/>
<pin name="VCCO_3" direction="pwr"/>
<pin name="VCCO" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="VBB" direction="out"/>
<pin name="~EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="~Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="~Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="~Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="~Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="~Q8" direction="out"/>
</symbol>
<symbol name="MC100EL11DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC100EL14DWG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="pwr"/>
<pin name="~CLK" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SEL" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="~Q4" direction="out"/>
</symbol>
<symbol name="MC100EL15DG">
<pin name="VCC" direction="pwr"/>
<pin name="~EN" direction="in"/>
<pin name="SEL" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
<pin name="VBB" direction="in"/>
</symbol>
<symbol name="MC100EL1648DG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="TANK" direction="in"/>
<pin name="AGC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="VEE_2" direction="out"/>
<pin name="VEE" direction="out"/>
</symbol>
<symbol name="MC100EL16DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="VBB" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EL31DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="S" direction="in"/>
<pin name="R" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="~Q" direction="out"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC100EL32DG">
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100EL57DG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="~D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="~D3" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="~Q" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="VBB1" direction="out"/>
<pin name="VBB2" direction="out"/>
</symbol>
<symbol name="MC100EL91DWG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="~D2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PECLVBB_2" direction="out"/>
<pin name="PECLVBB" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q2" direction="out"/>
</symbol>
<symbol name="MC100ELT20DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~Q" direction="out"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC100ELT20DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~Q" direction="out"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC100ELT21DG">
<pin name="VCC" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="D0" direction="out"/>
<pin name="~D0" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100ELT21DTG">
<pin name="VCC" direction="pwr"/>
<pin name="Q0" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~DO" direction="out"/>
<pin name="D0" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100ELT24DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100ELT24DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100ELT25DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D1" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="pwr"/>
<pin name="VBB" direction="pwr"/>
</symbol>
<symbol name="MC100EP01DG">
<pin name="VCC" direction="pwr"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EP01DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EP05DG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EP05DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EP08DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EP11DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
</symbol>
<symbol name="MC100EP11DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
</symbol>
<symbol name="MC100EP131FAG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="out"/>
<pin name="VCC" direction="in"/>
<pin name="C0" direction="in"/>
<pin name="~C0" direction="in"/>
<pin name="C1" direction="in"/>
<pin name="~C1" direction="in"/>
<pin name="C2" direction="in"/>
<pin name="~C2" direction="in"/>
<pin name="C3" direction="in"/>
<pin name="~C3" direction="in"/>
<pin name="CC" direction="in"/>
<pin name="~CC" direction="in"/>
<pin name="R0" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="R3" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="SET" direction="in"/>
<pin name="VEE_2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
</symbol>
<symbol name="MC100EP139DTG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~EN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="DIVSELB0" direction="in"/>
<pin name="DIVSELB1" direction="in"/>
<pin name="DIVSELA" direction="in"/>
<pin name="MR" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="~Q0" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q3" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100EP140DG">
<pin name="VCC" direction="pwr"/>
<pin name="R" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="~U" direction="out"/>
<pin name="U" direction="out"/>
<pin name="D" direction="out"/>
<pin name="~D" direction="out"/>
</symbol>
<symbol name="MC100EP142FAG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="~CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="~CLK1" direction="in"/>
<pin name="S-IN" direction="in"/>
<pin name="~S-IN" direction="in"/>
<pin name="SEL" direction="in"/>
<pin name="MR" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="out"/>
<pin name="VEE_2" direction="pas"/>
<pin name="VEE" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="~Q7" direction="out"/>
</symbol>
<symbol name="MC100EP14DTG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="~CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="~CLK1" direction="in"/>
<pin name="CLK_SEL" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="~Q4" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100EP16DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100EP16DTG">
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="~Q" direction="out"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC100EP16DTR2G">
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="~Q" direction="out"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC100EP195BFAG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="SETMIN" direction="in"/>
<pin name="SETMAX" direction="in"/>
<pin name="VBB" direction="out"/>
<pin name="~EN" direction="out"/>
<pin name="VCF" direction="in"/>
<pin name="LEN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEF" direction="in"/>
<pin name="VEE_2" direction="out"/>
<pin name="VEE_3" direction="pas"/>
<pin name="VEE" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
<pin name="~CASCADE" direction="out"/>
<pin name="CASCADE" direction="out"/>
</symbol>
<symbol name="MC100EP195FAG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~EN" direction="out"/>
<pin name="VCF" direction="in"/>
<pin name="LEN" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="SETMAX" direction="in"/>
<pin name="SETMIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEF" direction="out"/>
<pin name="VEE_2" direction="in"/>
<pin name="VEE_3" direction="pas"/>
<pin name="VEE" direction="in"/>
<pin name="VBB" direction="out"/>
<pin name="CASCADE" direction="out"/>
<pin name="~CASCADE" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
</symbol>
<symbol name="MC100EP196FAG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="VBB" direction="out"/>
<pin name="VCF" direction="in"/>
<pin name="LEN" direction="in"/>
<pin name="~EN" direction="out"/>
<pin name="SETMIN" direction="in"/>
<pin name="SETMAX" direction="in"/>
<pin name="FTUNE" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="VEF" direction="in"/>
<pin name="VEE_2" direction="out"/>
<pin name="VEE_3" direction="pas"/>
<pin name="VEE" direction="pas"/>
<pin name="~CASCADE" direction="out"/>
<pin name="CASCADE" direction="out"/>
<pin name="~Q" direction="out"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC100EP210SFAG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VTA" direction="in"/>
<pin name="VTB" direction="in"/>
<pin name="CLKA" direction="in"/>
<pin name="~CLKA" direction="in"/>
<pin name="CLKB" direction="in"/>
<pin name="~CLKB" direction="in"/>
<pin name="VEE_2" direction="pas"/>
<pin name="VEE" direction="pas"/>
<pin name="QA0" direction="out"/>
<pin name="~QA0" direction="out"/>
<pin name="QA1" direction="out"/>
<pin name="~QA1" direction="out"/>
<pin name="QA2" direction="out"/>
<pin name="~QA2" direction="out"/>
<pin name="QA3" direction="out"/>
<pin name="~QA3" direction="out"/>
<pin name="QA4" direction="out"/>
<pin name="~QA4" direction="out"/>
<pin name="QB0" direction="out"/>
<pin name="~QB0" direction="out"/>
<pin name="QB1" direction="out"/>
<pin name="~QB1" direction="out"/>
<pin name="QB2" direction="out"/>
<pin name="~QB2" direction="out"/>
<pin name="QB3" direction="pwr"/>
<pin name="~QB3" direction="out"/>
<pin name="QB4" direction="out"/>
<pin name="~QB4" direction="out"/>
</symbol>
<symbol name="MC100EP29DTG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="~CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="~CLK1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="~DO" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="R0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100EP31DG">
<pin name="VCC" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="D" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EP31DTG">
<pin name="VCC" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EP32DG">
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100EP32DTG">
<pin name="VCC" direction="pwr"/>
<pin name="~CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100EP33DTG">
<pin name="VCC" direction="pwr"/>
<pin name="~CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100EP40DTG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VTFB" direction="in"/>
<pin name="~VTFB" direction="in"/>
<pin name="VTR" direction="in"/>
<pin name="~VTR" direction="in"/>
<pin name="R" direction="in"/>
<pin name="~R" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~FB" direction="in"/>
<pin name="PLD" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="~U" direction="out"/>
<pin name="U" direction="out"/>
<pin name="D" direction="out"/>
<pin name="~D" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100EP445FAG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VBB0" direction="out"/>
<pin name="VBB1" direction="out"/>
<pin name="SINSEL" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="~PCLK" direction="out"/>
<pin name="PCLK" direction="out"/>
<pin name="~CKEN" direction="in"/>
<pin name="CKSEL" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="SINA" direction="in"/>
<pin name="~SINA" direction="in"/>
<pin name="SINB" direction="in"/>
<pin name="~SINB" direction="in"/>
<pin name="VEE_2" direction="pas"/>
<pin name="VEE" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC100EP446FAG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~CKEN" direction="in"/>
<pin name="CKEN" direction="in"/>
<pin name="CKSEL" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="VCF" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="VEF" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="VEE_2" direction="pas"/>
<pin name="VEE_3" direction="pas"/>
<pin name="VEE" direction="pas"/>
<pin name="VBB1" direction="out"/>
<pin name="VBB2" direction="out"/>
<pin name="SOUT" direction="out"/>
<pin name="~SOUT" direction="out"/>
<pin name="PCLK" direction="out"/>
<pin name="~PCLK" direction="out"/>
</symbol>
<symbol name="MC100EP451FAG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="MR" direction="out"/>
<pin name="D0" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="~D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="~D3" direction="in"/>
<pin name="D4" direction="pwr"/>
<pin name="~D4" direction="in"/>
<pin name="D5" direction="out"/>
<pin name="~D5" direction="out"/>
<pin name="VEE_2" direction="pas"/>
<pin name="VEE" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="~Q4" direction="out"/>
<pin name="Q5" direction="pwr"/>
<pin name="~Q5" direction="out"/>
</symbol>
<symbol name="MC100EP51DG">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="D" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EP51DTG">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EP56DTG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="D0A" direction="in"/>
<pin name="~D0A" direction="in"/>
<pin name="D0B" direction="in"/>
<pin name="~D0B" direction="in"/>
<pin name="D1A" direction="in"/>
<pin name="~D1A" direction="in"/>
<pin name="D1B" direction="in"/>
<pin name="~D1B" direction="in"/>
<pin name="COM_SEL" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="VBB0" direction="out"/>
<pin name="VBB1" direction="out"/>
</symbol>
<symbol name="MC100EP56DWG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="COM_SEL" direction="in"/>
<pin name="D0A" direction="in"/>
<pin name="~D0A" direction="in"/>
<pin name="D0B" direction="in"/>
<pin name="~D0B" direction="in"/>
<pin name="D1A" direction="in"/>
<pin name="~D1A" direction="in"/>
<pin name="D1B" direction="in"/>
<pin name="~D1B" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="VBBO" direction="out"/>
<pin name="VBB1" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC100EP57DTG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="~D2" direction="in"/>
<pin name="~D3" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="VBB1" direction="out"/>
<pin name="VBB2" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EP58DG">
<pin name="VCC" direction="pwr"/>
<pin name="DA" direction="in"/>
<pin name="DB" direction="in"/>
<pin name="SEL" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EP58DTG">
<pin name="VCC" direction="pwr"/>
<pin name="DB" direction="in"/>
<pin name="DA" direction="in"/>
<pin name="SEL" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EPT20DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EPT20DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EPT22DG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC100EPT22DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC100EPT24DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EPT24DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="NC_2" direction="in"/>
<pin name="NC" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100EPT25DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100EPT25DTG">
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="pas"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC100EPT26DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VBB" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
</symbol>
<symbol name="MC100EPT26DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VBB" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
</symbol>
<symbol name="MC100LVEL11DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC100LVEL11DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC100LVEL11DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC100LVEL14DWG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SEL" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="~Q3" direction="out"/>
<pin name="~Q4" direction="out"/>
</symbol>
<symbol name="MC100LVEL16DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="~Q" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100LVEL16DTG">
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100LVEL29DWG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="R0" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="~CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="~CLK1" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100LVEL51DG">
<pin name="VCC" direction="pwr"/>
<pin name="R" direction="in"/>
<pin name="D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC100LVEL90DWG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="ECLVBB_2" direction="pwr"/>
<pin name="ECLVBB" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="~D2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="Q0_2" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="Q1_2" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2_2" direction="out"/>
<pin name="Q2" direction="out"/>
</symbol>
<symbol name="MC100LVEL91DWG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="~D2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~Q0" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="PECLVBB_2" direction="out"/>
<pin name="PECLVBB" direction="out"/>
</symbol>
<symbol name="MC100LVEL92DWG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LVCC_2" direction="pwr"/>
<pin name="LVCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="~D2" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="in"/>
<pin name="~Q1" direction="in"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="VBB_PECL" direction="out"/>
<pin name="VBB_PECL_2" direction="out"/>
</symbol>
<symbol name="MC100LVELT22DG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC100LVELT22DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC100LVELT23DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
</symbol>
<symbol name="MC100LVEP111FAG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="~CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="~CLK1" direction="in"/>
<pin name="CLK_SEL" direction="in"/>
<pin name="VBB" direction="out"/>
<pin name="VEE" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="~Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="~Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="~Q6" direction="out"/>
<pin name="~Q7" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="~Q8" direction="out"/>
<pin name="~Q9" direction="out"/>
<pin name="Q9" direction="out"/>
</symbol>
<symbol name="MC100LVEP11DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC100LVEP11DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC100LVEP14DTG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK0" direction="in"/>
<pin name="~CLK0" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="~CLK1" direction="in"/>
<pin name="CLK_SEL" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="~Q4" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC100LVEP16DTG">
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="pas"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10E016FNG">
<pin name="VCC" direction="pwr"/>
<pin name="VCCO_2" direction="pwr"/>
<pin name="VCCO_3" direction="pwr"/>
<pin name="VCCO" direction="pwr"/>
<pin name="~CE" direction="in"/>
<pin name="~PE" direction="in"/>
<pin name="MR" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="TCLD" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="~TC" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC10EL01DG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10EL04DG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10EL16DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="VBB" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10EL16DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="VBB" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10EL31DG">
<pin name="VCC" direction="pwr"/>
<pin name="S" direction="in"/>
<pin name="D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="R" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10EL89DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC10ELT20DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10ELT21DG">
<pin name="VCC" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="D0" direction="out"/>
<pin name="~D0" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC10ELT22DG">
<pin name="VCC" direction="pwr"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="MC10ELT24DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10ELT25DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC10ELT25DTG">
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC10ELT28DG">
<pin name="VCC" direction="pwr"/>
<pin name="DECL" direction="in"/>
<pin name="~DECL" direction="in"/>
<pin name="QTTL" direction="in"/>
<pin name="DTTL" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="QECL" direction="out"/>
<pin name="~QECL" direction="out"/>
</symbol>
<symbol name="MC10EP05DG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10EP16DG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
<pin name="VBB" direction="out"/>
</symbol>
<symbol name="MC10EP16DTG">
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="~Q" direction="out"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC10EP195FAG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="LEN" direction="in"/>
<pin name="~EN" direction="out"/>
<pin name="VBB" direction="out"/>
<pin name="VEF" direction="out"/>
<pin name="VCF" direction="in"/>
<pin name="SETMIN" direction="in"/>
<pin name="SETMAX" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE_2" direction="in"/>
<pin name="VEE_3" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="CASCADE" direction="out"/>
<pin name="~CASCADE" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10EP31DG">
<pin name="VCC" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="D" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10EP32DTG">
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="MC10H101PG">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="AIN" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="COM_IN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="AOUT" direction="out"/>
<pin name="~AOUT" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="~BOUT" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="~COUT" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="~DOUT" direction="out"/>
</symbol>
<symbol name="MC10H102PG">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="AIN_2" direction="in"/>
<pin name="AIN" direction="in"/>
<pin name="BIN_2" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="CIN_2" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="DIN_2" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="~AOUT" direction="out"/>
<pin name="~BOUT" direction="out"/>
<pin name="~COUT" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="~DOUT" direction="out"/>
</symbol>
<symbol name="MC10H105PG">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="AIN_2" direction="in"/>
<pin name="AIN" direction="in"/>
<pin name="BIN_2" direction="in"/>
<pin name="BIN_3" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="CIN_2" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="AOUT" direction="out"/>
<pin name="~AOUT" direction="out"/>
<pin name="BOUT_2" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="~COUT" direction="out"/>
<pin name="COUT" direction="out"/>
</symbol>
<symbol name="MC10H116DG">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="AIN" direction="in"/>
<pin name="~AIN" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="~BIN" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="~CIN" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="VBB" direction="out"/>
<pin name="AOUT" direction="out"/>
<pin name="~AOUT" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="~BOUT" direction="out"/>
<pin name="~COUT" direction="out"/>
<pin name="COUT" direction="out"/>
</symbol>
<symbol name="MC10H124PG">
<pin name="VCC" direction="pwr"/>
<pin name="COMMON_STROBE" direction="pas"/>
<pin name="AIN" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AOUT" direction="out"/>
<pin name="~AOUT" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="~BOUT" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="~COUT" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="~DOUT" direction="out"/>
</symbol>
<symbol name="MC10H125PG">
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="pas"/>
<pin name="AIN" direction="in"/>
<pin name="~AIN" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="~BIN" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="~CIN" direction="in"/>
<pin name="~DIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="AOUT" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="MC10H131PG">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="~CE1" direction="in"/>
<pin name="~CE2" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="CC" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
</symbol>
<symbol name="MC10H136PG">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="~CIN" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~COUT" direction="out"/>
</symbol>
<symbol name="MC12026ADG">
<pin name="VCC" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="MC" direction="in"/>
<pin name="SW" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC12080DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="SW1" direction="in"/>
<pin name="SW2" direction="in"/>
<pin name="SW3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC12093DG">
<pin name="VCC" direction="pwr"/>
<pin name="~IN" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="SW1" direction="in"/>
<pin name="SW2" direction="in"/>
<pin name="SB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC12095DG">
<pin name="VCC" direction="pwr"/>
<pin name="~IN" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="SW" direction="in"/>
<pin name="SB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC14001BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="MC14001BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14001UBCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="MC14001UBDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14007UBDG">
<pin name="VDD" direction="pwr"/>
<pin name="D-PA" direction="in"/>
<pin name="D-PB" direction="in"/>
<pin name="D-NA" direction="in"/>
<pin name="D-NB" direction="in"/>
<pin name="S-PB" direction="in"/>
<pin name="S-PC" direction="out"/>
<pin name="S-NB" direction="out"/>
<pin name="S-NC" direction="in"/>
<pin name="GATEA" direction="in"/>
<pin name="GATEB" direction="out"/>
<pin name="GATEC" direction="out"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTC" direction="in"/>
</symbol>
<symbol name="MC14008BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="COUT" direction="out"/>
<pin name="S1" direction="out"/>
<pin name="S2" direction="out"/>
<pin name="S3" direction="out"/>
<pin name="S4" direction="out"/>
</symbol>
<symbol name="MC14011BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14011BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14011BDR2G">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14011UBCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14011UBDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14012BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN1A" direction="in"/>
<pin name="IN1B" direction="in"/>
<pin name="IN2A" direction="in"/>
<pin name="IN2B" direction="in"/>
<pin name="IN3A" direction="in"/>
<pin name="IN3B" direction="in"/>
<pin name="IN4A" direction="in"/>
<pin name="IN4B" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="MC14012BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_3A" direction="in"/>
<pin name="IN_3B" direction="in"/>
<pin name="IN_4A" direction="in"/>
<pin name="IN_4B" direction="in"/>
<pin name="NC_2" direction="in"/>
<pin name="NC" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="MC14013BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="SA" direction="in"/>
<pin name="SB" direction="in"/>
<pin name="RA" direction="in"/>
<pin name="RB" direction="in"/>
<pin name="DA" direction="in"/>
<pin name="DB" direction="in"/>
<pin name="CA" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="QA" direction="out"/>
<pin name="~QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="~QB" direction="out"/>
</symbol>
<symbol name="MC14013BDG">
<pin name="VDD" direction="pwr"/>
<pin name="SA" direction="in"/>
<pin name="SB" direction="in"/>
<pin name="CA" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="DA" direction="in"/>
<pin name="DB" direction="in"/>
<pin name="RA" direction="in"/>
<pin name="RB" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="QA" direction="out"/>
<pin name="~QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="~QB" direction="out"/>
</symbol>
<symbol name="MC14014BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="C" direction="in"/>
<pin name="P/S" direction="in"/>
<pin name="DS" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="P8" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
</symbol>
<symbol name="MC14016BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="CONTROL_1" direction="in"/>
<pin name="CONTROL_2" direction="in"/>
<pin name="CONTROL_3" direction="in"/>
<pin name="CONTROL_4" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC14016BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="CONTROL1" direction="in"/>
<pin name="CONTROL2" direction="in"/>
<pin name="CONTROL3" direction="in"/>
<pin name="CONTROL4" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC14017BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="~CE" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="COUT" direction="out"/>
</symbol>
<symbol name="MC14017BDG">
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="~CE" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="COUT" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
</symbol>
<symbol name="MC14020BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="C" direction="in"/>
<pin name="R" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q1" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q11" direction="out"/>
<pin name="Q12" direction="out"/>
<pin name="Q13" direction="out"/>
<pin name="Q14" direction="out"/>
</symbol>
<symbol name="MC14020BDG">
<pin name="VDD" direction="pwr"/>
<pin name="C" direction="in"/>
<pin name="R" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q11" direction="out"/>
<pin name="Q12" direction="out"/>
<pin name="Q13" direction="out"/>
<pin name="Q14" direction="out"/>
</symbol>
<symbol name="MC14022BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="~CE" direction="in"/>
<pin name="C" direction="pas"/>
<pin name="R" direction="in"/>
<pin name="NC_2" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="COUT" direction="out"/>
</symbol>
<symbol name="MC14022BDG">
<pin name="VDD" direction="pwr"/>
<pin name="C" direction="in"/>
<pin name="R" direction="in"/>
<pin name="~CE" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="COUT" direction="out"/>
</symbol>
<symbol name="MC14023BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_3A" direction="in"/>
<pin name="IN_3B" direction="in"/>
<pin name="IN_3C" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
</symbol>
<symbol name="MC14023BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_3A" direction="in"/>
<pin name="IN_3B" direction="in"/>
<pin name="IN_3C" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
</symbol>
<symbol name="MC14024BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC14025BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_3A" direction="in"/>
<pin name="IN_3B" direction="in"/>
<pin name="IN_3C" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
</symbol>
<symbol name="MC14025BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_3A" direction="in"/>
<pin name="IN_3B" direction="in"/>
<pin name="IN_3C" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
</symbol>
<symbol name="MC14027BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="CA" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="SA" direction="in"/>
<pin name="SB" direction="in"/>
<pin name="RA" direction="in"/>
<pin name="RB" direction="in"/>
<pin name="JA" direction="in"/>
<pin name="JB" direction="in"/>
<pin name="KA" direction="in"/>
<pin name="KB" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="~QA" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="~QB" direction="out"/>
<pin name="QB" direction="out"/>
</symbol>
<symbol name="MC14027BDG">
<pin name="VDD" direction="pwr"/>
<pin name="SA" direction="in"/>
<pin name="SB" direction="in"/>
<pin name="RA" direction="in"/>
<pin name="RB" direction="in"/>
<pin name="JA" direction="in"/>
<pin name="JB" direction="in"/>
<pin name="CA" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="KA" direction="in"/>
<pin name="KB" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="~QA" direction="out"/>
<pin name="~QB" direction="out"/>
</symbol>
<symbol name="MC14028BDG">
<pin name="VDD" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
</symbol>
<symbol name="MC14029BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="~CIN" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="U/D" direction="in"/>
<pin name="B/D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~COUT" direction="out"/>
</symbol>
<symbol name="MC14029BDR2G">
<pin name="VDD" direction="pwr"/>
<pin name="~CIN" direction="in"/>
<pin name="B/D" direction="in"/>
<pin name="U/D" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="~COUT" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
</symbol>
<symbol name="MC14040BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="C" direction="in"/>
<pin name="R" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q11" direction="out"/>
<pin name="Q12" direction="out"/>
</symbol>
<symbol name="MC14040BDG">
<pin name="VDD" direction="pwr"/>
<pin name="C" direction="in"/>
<pin name="R" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q11" direction="out"/>
<pin name="Q12" direction="out"/>
</symbol>
<symbol name="MC14040BDR2G">
<pin name="VDD" direction="pwr"/>
<pin name="C" direction="in"/>
<pin name="R" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q11" direction="out"/>
<pin name="Q12" direction="out"/>
</symbol>
<symbol name="MC14042BDG">
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="POLARITY" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
</symbol>
<symbol name="MC14043BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="S0" direction="in"/>
<pin name="R0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="S3" direction="in"/>
<pin name="R3" direction="in"/>
<pin name="E" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
</symbol>
<symbol name="MC14043BDG">
<pin name="VDD" direction="pwr"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S3" direction="in"/>
<pin name="R0" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="R3" direction="in"/>
<pin name="E" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
</symbol>
<symbol name="MC14044BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="~R0" direction="in"/>
<pin name="~S0" direction="in"/>
<pin name="~R1" direction="in"/>
<pin name="~S1" direction="in"/>
<pin name="~R2" direction="in"/>
<pin name="~S2" direction="in"/>
<pin name="~R3" direction="in"/>
<pin name="~S3" direction="in"/>
<pin name="E" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
</symbol>
<symbol name="MC14046BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="INH" direction="in"/>
<pin name="LD" direction="pas"/>
<pin name="PCAIN" direction="in"/>
<pin name="PCBIN" direction="in"/>
<pin name="VCOIN" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VCOOUT" direction="out"/>
<pin name="SFOUT" direction="out"/>
<pin name="PC1OUT" direction="out"/>
<pin name="PC2OUT" direction="out"/>
<pin name="C1A" direction="pas"/>
<pin name="C1B" direction="pas"/>
<pin name="R1" direction="pas"/>
<pin name="R2" direction="pas"/>
<pin name="ZENER" direction="pas"/>
</symbol>
<symbol name="MC14049BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="INF" direction="in"/>
<pin name="INE" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTE" direction="out"/>
<pin name="OUTF" direction="out"/>
</symbol>
<symbol name="MC14049BDG">
<pin name="VDD" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="INE" direction="in"/>
<pin name="INF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTE" direction="out"/>
<pin name="OUTF" direction="out"/>
</symbol>
<symbol name="MC14049UBCPG">
<pin name="VDD" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="INE" direction="in"/>
<pin name="INF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTE" direction="out"/>
<pin name="OUTF" direction="out"/>
</symbol>
<symbol name="MC14049UBDG">
<pin name="VDD" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="INE" direction="in"/>
<pin name="INF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTE" direction="out"/>
<pin name="OUTF" direction="out"/>
</symbol>
<symbol name="MC14049UBDR2G">
<pin name="VDD" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="INE" direction="in"/>
<pin name="INF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTE" direction="out"/>
<pin name="OUTF" direction="out"/>
</symbol>
<symbol name="MC14050BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="INE" direction="in"/>
<pin name="INF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTE" direction="out"/>
<pin name="OUTF" direction="out"/>
</symbol>
<symbol name="MC14050BDG">
<pin name="VDD" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="INE" direction="in"/>
<pin name="INF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTE" direction="out"/>
<pin name="OUTF" direction="out"/>
</symbol>
<symbol name="MC14050BDR2G">
<pin name="VDD" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="INE" direction="in"/>
<pin name="INF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTE" direction="out"/>
<pin name="OUTF" direction="out"/>
</symbol>
<symbol name="MC14051BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="INH" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="X3"/>
<pin name="X4"/>
<pin name="X5"/>
<pin name="X6"/>
<pin name="X7"/>
<pin name="VEE" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="X" direction="out"/>
</symbol>
<symbol name="MC14051BDG">
<pin name="VDD" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="INH" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="X" direction="out"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="X3"/>
<pin name="X4"/>
<pin name="X5"/>
<pin name="X6"/>
<pin name="X7"/>
</symbol>
<symbol name="MC14051BDTR2G">
<pin name="VDD" direction="pwr"/>
<pin name="INH" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="X3"/>
<pin name="X4"/>
<pin name="X5"/>
<pin name="X6"/>
<pin name="X7"/>
<pin name="VEE" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="X"/>
</symbol>
<symbol name="MC14052BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="INH" direction="pas"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y0" direction="in"/>
<pin name="Y1" direction="in"/>
<pin name="Y2" direction="in"/>
<pin name="Y3" direction="in"/>
<pin name="X0" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="X3" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="Y" direction="out"/>
<pin name="X" direction="out"/>
</symbol>
<symbol name="MC14053BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="INH" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="X1"/>
<pin name="X0"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Z1"/>
<pin name="Z0"/>
<pin name="VEE" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="X"/>
<pin name="Y"/>
<pin name="Z"/>
</symbol>
<symbol name="MC14053BDG">
<pin name="VDD" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="INH" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="X" direction="out"/>
<pin name="Y" direction="out"/>
<pin name="Z" direction="out"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Z0"/>
<pin name="Z1"/>
</symbol>
<symbol name="MC14053BDTR2G">
<pin name="VDD" direction="pwr"/>
<pin name="INH" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="Y1"/>
<pin name="Y0"/>
<pin name="Z0"/>
<pin name="Z1"/>
<pin name="VEE" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="X"/>
<pin name="Y"/>
<pin name="Z"/>
</symbol>
<symbol name="MC14060BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q12" direction="out"/>
<pin name="Q13" direction="out"/>
<pin name="Q14" direction="out"/>
</symbol>
<symbol name="MC14060BDG">
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q12" direction="out"/>
<pin name="Q13" direction="out"/>
<pin name="Q14" direction="out"/>
</symbol>
<symbol name="MC14066BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="CONTROL_1" direction="in"/>
<pin name="CONTROL_2" direction="in"/>
<pin name="CONTROL_3" direction="in"/>
<pin name="CONTROL_4" direction="in"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC14066BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="CONTROL_1" direction="in"/>
<pin name="CONTROL_2" direction="in"/>
<pin name="CONTROL_3" direction="in"/>
<pin name="CONTROL_4" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC14066BDR2G">
<pin name="VDD" direction="pwr"/>
<pin name="CNTR1" direction="in"/>
<pin name="CNTR2" direction="in"/>
<pin name="CNTR3" direction="in"/>
<pin name="CNTR4" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC14066BDTR2G">
<pin name="VDD" direction="pwr"/>
<pin name="IN1" direction="in"/>
<pin name="CONTROL1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="CONTROL2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="CONTROL3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="CONTROL4" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC14067BDWG">
<pin name="VDD" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="X3"/>
<pin name="X5_2"/>
<pin name="X5"/>
<pin name="X6"/>
<pin name="X7"/>
<pin name="X8"/>
<pin name="X9"/>
<pin name="X10"/>
<pin name="X11"/>
<pin name="X12"/>
<pin name="X13"/>
<pin name="X14"/>
<pin name="X15"/>
<pin name="INHIBIT" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="X"/>
</symbol>
<symbol name="MC14069UBCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT_6" direction="out"/>
<pin name="OUT_3" direction="out"/>
</symbol>
<symbol name="MC14069UBDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT_6" direction="out"/>
</symbol>
<symbol name="MC14070BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="MC14070BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14071BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="MC14071BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14073BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_3A" direction="in"/>
<pin name="IN_3B" direction="in"/>
<pin name="IN_3C" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
</symbol>
<symbol name="MC14077BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14081BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="MC14081BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14093BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="MC14093BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1A" direction="in"/>
<pin name="IN_1B" direction="in"/>
<pin name="IN_1C" direction="in"/>
<pin name="IN_1D" direction="in"/>
<pin name="IN_2A" direction="in"/>
<pin name="IN_2B" direction="in"/>
<pin name="IN_2C" direction="in"/>
<pin name="IN_2D" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="MC14094BDG">
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DATA" direction="in"/>
<pin name="STROBE" direction="pwr"/>
<pin name="VSS" direction="pas"/>
<pin name="OUT_EN" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="QS" direction="out"/>
<pin name="QS_2" direction="out"/>
</symbol>
<symbol name="MC14099BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="DATA" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="WRITE_DISABLE" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC14106BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT_6" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC14175BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="C" direction="in"/>
<pin name="~R" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
</symbol>
<symbol name="MC14490DWG">
<pin name="VDD" direction="pwr"/>
<pin name="OSCIN" direction="in"/>
<pin name="FIN" direction="in"/>
<pin name="AIN" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="EIN" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OSCOUT" direction="out"/>
<pin name="AOUT" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="EOUT" direction="out"/>
<pin name="FOUT" direction="out"/>
</symbol>
<symbol name="MC14490PG">
<pin name="VDD" direction="pwr"/>
<pin name="OSCIN" direction="in"/>
<pin name="AIN" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="EIN" direction="in"/>
<pin name="FIN" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="AOUT" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="EOUT" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="OSCOUT" direction="out"/>
</symbol>
<symbol name="MC14503BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="DIS_A" direction="in"/>
<pin name="DIS_B" direction="in"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT_6" direction="out"/>
</symbol>
<symbol name="MC14503BDG">
<pin name="VDD" direction="pwr"/>
<pin name="DIS_A" direction="in"/>
<pin name="DIS_B" direction="in"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT_6" direction="out"/>
</symbol>
<symbol name="MC14504BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="MODE" direction="in"/>
<pin name="AIN" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="EIN" direction="in"/>
<pin name="FIN" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="AOUT" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="EOUT" direction="out"/>
<pin name="FOUT" direction="out"/>
</symbol>
<symbol name="MC14504BDG">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AIN" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="EIN" direction="in"/>
<pin name="FIN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="AOUT" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="EOUT" direction="out"/>
<pin name="FOUT" direction="out"/>
</symbol>
<symbol name="MC14504BDR2G">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AIN" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="EIN" direction="in"/>
<pin name="FIN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="AOUT" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="EOUT" direction="out"/>
<pin name="FOUT" direction="out"/>
</symbol>
<symbol name="MC14511BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="~LT" direction="in"/>
<pin name="~BI" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="A_2" direction="in"/>
<pin name="B_2" direction="in"/>
<pin name="C_2" direction="in"/>
<pin name="D_2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="A" direction="out"/>
<pin name="B" direction="out"/>
<pin name="C" direction="out"/>
<pin name="D" direction="out"/>
<pin name="E" direction="out"/>
<pin name="F" direction="out"/>
<pin name="G" direction="out"/>
</symbol>
<symbol name="MC14512BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="INH" direction="in"/>
<pin name="DIS" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="X0" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="X3" direction="in"/>
<pin name="X4" direction="in"/>
<pin name="X5" direction="in"/>
<pin name="X6" direction="in"/>
<pin name="X7" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="Z" direction="out"/>
</symbol>
<symbol name="MC14512BDG">
<pin name="VDD" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="X0" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="X3" direction="in"/>
<pin name="X4" direction="in"/>
<pin name="X5" direction="in"/>
<pin name="X6" direction="in"/>
<pin name="X7" direction="in"/>
<pin name="DIS" direction="in"/>
<pin name="INH" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="Z" direction="out"/>
</symbol>
<symbol name="MC14513BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="~LT" direction="in"/>
<pin name="RBI" direction="in"/>
<pin name="RBO" direction="pas"/>
<pin name="~BI" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="A_2" direction="in"/>
<pin name="B_2" direction="in"/>
<pin name="C_2" direction="in"/>
<pin name="D_2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="A" direction="out"/>
<pin name="B" direction="out"/>
<pin name="C" direction="out"/>
<pin name="D" direction="out"/>
<pin name="E" direction="out"/>
<pin name="F" direction="out"/>
<pin name="G" direction="out"/>
</symbol>
<symbol name="MC14516BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="U/D" direction="in"/>
<pin name="~CARRY_IN" direction="in"/>
<pin name="R" direction="in"/>
<pin name="C" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~CARRY_OUT" direction="out"/>
</symbol>
<symbol name="MC14518BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="CA" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="EA" direction="in"/>
<pin name="EB" direction="in"/>
<pin name="RA" direction="in"/>
<pin name="RB" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q0A" direction="out"/>
<pin name="Q0B" direction="out"/>
<pin name="Q1A" direction="out"/>
<pin name="Q1B" direction="out"/>
<pin name="Q2A" direction="out"/>
<pin name="Q2B" direction="out"/>
<pin name="Q3A" direction="out"/>
<pin name="Q3B" direction="out"/>
</symbol>
<symbol name="MC14520BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="RA" direction="in"/>
<pin name="RB" direction="in"/>
<pin name="CA" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="EA" direction="in"/>
<pin name="EB" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q0A" direction="out"/>
<pin name="Q0B" direction="out"/>
<pin name="Q1A" direction="out"/>
<pin name="Q1B" direction="out"/>
<pin name="Q2A" direction="out"/>
<pin name="Q2B" direction="out"/>
<pin name="Q3A" direction="out"/>
<pin name="Q3B" direction="out"/>
</symbol>
<symbol name="MC14521BCPG">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="Q18" direction="out"/>
<pin name="Q19" direction="out"/>
<pin name="Q20" direction="out"/>
<pin name="Q21" direction="out"/>
<pin name="Q22" direction="out"/>
<pin name="Q23" direction="out"/>
<pin name="Q24" direction="out"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC14521BDG">
<pin name="VDD" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="VSS_2" direction="pas"/>
<pin name="RESET" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="Q18" direction="out"/>
<pin name="Q19" direction="out"/>
<pin name="Q20" direction="out"/>
<pin name="Q21" direction="out"/>
<pin name="Q22" direction="out"/>
<pin name="Q23" direction="out"/>
<pin name="Q24" direction="out"/>
</symbol>
<symbol name="MC14528BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="~RESET_1" direction="in"/>
<pin name="~RESET_2" direction="in"/>
<pin name="CX1/RX1" direction="pas"/>
<pin name="CX2/RX2" direction="pas"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q2" direction="out"/>
</symbol>
<symbol name="MC14528BDG">
<pin name="VDD" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="CX1/RX1" direction="in"/>
<pin name="CX2/RX2" direction="in"/>
<pin name="~RESET_1" direction="in"/>
<pin name="~RESET_2" direction="in"/>
<pin name="VSS_2" direction="pas"/>
<pin name="VSS_3" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
</symbol>
<symbol name="MC14532BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="EIN" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="GS" direction="out"/>
<pin name="EOUT" direction="out"/>
</symbol>
<symbol name="MC14536BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="CLOCK_INH" direction="in"/>
<pin name="SET" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="8-BYPASS" direction="in"/>
<pin name="IN_1" direction="in"/>
<pin name="OSC_INH" direction="in"/>
<pin name="MONO-IN" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="DECODE" direction="out"/>
</symbol>
<symbol name="MC14536BDWG">
<pin name="VDD" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="SET" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CLC_INH" direction="in"/>
<pin name="OSC_INH" direction="in"/>
<pin name="IN_1" direction="in"/>
<pin name="MONO-IN" direction="in"/>
<pin name="8-BYPASS" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="DECODE" direction="out"/>
</symbol>
<symbol name="MC14538BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="~RESET_A" direction="in"/>
<pin name="~RESET_B" direction="in"/>
<pin name="CX/RXA" direction="pas"/>
<pin name="CX/RXB" direction="pas"/>
<pin name="AA" direction="in"/>
<pin name="AB" direction="in"/>
<pin name="~BA" direction="in"/>
<pin name="~BB" direction="in"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="QA" direction="out"/>
<pin name="~QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="~QB" direction="out"/>
</symbol>
<symbol name="MC14538BDG">
<pin name="VDD" direction="pwr"/>
<pin name="AA" direction="in"/>
<pin name="AB" direction="in"/>
<pin name="~BA" direction="in"/>
<pin name="~BB" direction="in"/>
<pin name="~RESET_A" direction="in"/>
<pin name="~RESET_B" direction="in"/>
<pin name="CX/RXA" direction="in"/>
<pin name="CX/RXB" direction="in"/>
<pin name="VSS_2" direction="pas"/>
<pin name="VSS_3" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="QA" direction="out"/>
<pin name="~QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="~QB" direction="out"/>
</symbol>
<symbol name="MC14538BDWG">
<pin name="VDD" direction="pwr"/>
<pin name="CX/RXB" direction="in"/>
<pin name="CX/RXA" direction="in"/>
<pin name="~RESET_A" direction="in"/>
<pin name="~RESET_B" direction="in"/>
<pin name="AB" direction="in"/>
<pin name="AA" direction="in"/>
<pin name="~BA" direction="in"/>
<pin name="~BB" direction="in"/>
<pin name="VSS_2" direction="pas"/>
<pin name="VSS_3" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="QA" direction="out"/>
<pin name="~QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="~QB" direction="out"/>
</symbol>
<symbol name="MC14541BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="MODE" direction="in"/>
<pin name="RTC" direction="in"/>
<pin name="CTC" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="AR" direction="in"/>
<pin name="MR" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Q/~Q_SEL" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC14541BDG">
<pin name="VDD" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="RTC" direction="in"/>
<pin name="CTC" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="AR" direction="in"/>
<pin name="MR" direction="in"/>
<pin name="Q/~Q_SEL" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC14541BDR2G">
<pin name="VDD" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="RTC" direction="in"/>
<pin name="CTC" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="AR" direction="in"/>
<pin name="MR" direction="in"/>
<pin name="Q/~Q_SEL" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC14543BDG">
<pin name="VDD" direction="pwr"/>
<pin name="LD" direction="in"/>
<pin name="PH" direction="in"/>
<pin name="BI" direction="in"/>
<pin name="A_2" direction="in"/>
<pin name="B_2" direction="in"/>
<pin name="C_2" direction="in"/>
<pin name="D_2" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="A" direction="out"/>
<pin name="B" direction="out"/>
<pin name="C" direction="out"/>
<pin name="D" direction="out"/>
<pin name="E" direction="out"/>
<pin name="F" direction="out"/>
<pin name="G" direction="out"/>
</symbol>
<symbol name="MC14551BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="CONTROL" direction="pas"/>
<pin name="W0"/>
<pin name="W1"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Z0"/>
<pin name="Z1"/>
<pin name="VEE" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="W"/>
<pin name="X"/>
<pin name="Y"/>
<pin name="Z"/>
</symbol>
<symbol name="MC14551BDG">
<pin name="VDD" direction="pwr"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="W0"/>
<pin name="W1"/>
<pin name="Z0"/>
<pin name="Z1"/>
<pin name="CONTROL" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="W"/>
<pin name="X"/>
<pin name="Y"/>
<pin name="Z"/>
</symbol>
<symbol name="MC14553BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="MR" direction="in"/>
<pin name="CIA" direction="in"/>
<pin name="CIB" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="DIS" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~DS1" direction="pas"/>
<pin name="~DS2" direction="pas"/>
<pin name="~DS3" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="O.F" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
</symbol>
<symbol name="MC14555BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="~EA" direction="in"/>
<pin name="~EB" direction="in"/>
<pin name="AA" direction="in"/>
<pin name="AB" direction="in"/>
<pin name="BA" direction="in"/>
<pin name="BB" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="Q0A" direction="out"/>
<pin name="Q1A" direction="out"/>
<pin name="Q2A" direction="out"/>
<pin name="Q3A" direction="out"/>
<pin name="Q0B" direction="out"/>
<pin name="Q1B" direction="out"/>
<pin name="Q2B" direction="out"/>
<pin name="Q3B" direction="out"/>
</symbol>
<symbol name="MC14557BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="~CE" direction="in"/>
<pin name="A/B_SEL" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="L1" direction="in"/>
<pin name="L2" direction="in"/>
<pin name="L4" direction="in"/>
<pin name="L8" direction="in"/>
<pin name="L16" direction="in"/>
<pin name="L32" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="~Q" direction="out"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC1455BP1G">
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="TRIGGER" direction="in"/>
<pin name="CONTROL_VOLTAGE" direction="in"/>
<pin name="THRESHOLD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DISCHARGE" direction="out"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="MC1455P1G">
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="TRIGGER" direction="in"/>
<pin name="CONTROL_VOLTAGE" direction="in"/>
<pin name="THRESHOLD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DISCHARGE" direction="out"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="MC14569BCPG">
<pin name="VDD" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="CTL1" direction="in"/>
<pin name="CTL2" direction="in"/>
<pin name="ZERO_DETECT" direction="in"/>
<pin name="CASCADE_FEEDBACK" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="MC14584BCPG">
<pin name="VSS" direction="pwr"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
</symbol>
<symbol name="MC14584BDG">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT_6" direction="out"/>
</symbol>
<symbol name="MC14584BDR2G">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT_6" direction="out"/>
</symbol>
<symbol name="MC14585BDG">
<pin name="VDD" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="(A_&gt;_B)IN" direction="in"/>
<pin name="(A_=_B)IN" direction="in"/>
<pin name="(A_&lt;_B)IN" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="(A_&gt;_B)OUT" direction="out"/>
<pin name="(A_&lt;_B)OUT" direction="out"/>
<pin name="(A_=_B)OUT" direction="out"/>
</symbol>
<symbol name="MC1488DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B1" direction="in"/>
<pin name="IN_B2" direction="in"/>
<pin name="IN_C1" direction="in"/>
<pin name="IN_C2" direction="in"/>
<pin name="IN_D1" direction="in"/>
<pin name="IN_D2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="MC1488PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B1" direction="in"/>
<pin name="IN_B2" direction="in"/>
<pin name="IN_C1" direction="in"/>
<pin name="IN_C2" direction="in"/>
<pin name="IN_D1" direction="in"/>
<pin name="IN_D2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="MC1489ADG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_C" direction="in"/>
<pin name="IN_D" direction="in"/>
<pin name="RESPONSE_CONTROL_A" direction="in"/>
<pin name="RESPONSE_CONTROL_B" direction="in"/>
<pin name="RESPONSE_CONTROL_C" direction="in"/>
<pin name="RESPONSE_CONTROL_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="MC1489DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_C" direction="in"/>
<pin name="IN_D" direction="in"/>
<pin name="RESPONSE_CONTROL_A" direction="in"/>
<pin name="RESPONSE_CONTROL_B" direction="in"/>
<pin name="RESPONSE_CONTROL_C" direction="in"/>
<pin name="RESPONSE_CONTROL_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="MC1489PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_C" direction="in"/>
<pin name="IN_D" direction="in"/>
<pin name="RESPONSE_COTROL_A" direction="in"/>
<pin name="RESPONSE_COTROL_B" direction="in"/>
<pin name="RESPONSE_COTROL_C" direction="in"/>
<pin name="RESPONSE_COTROL_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="MC1496BPG">
<pin name="VEE" direction="pwr"/>
<pin name="GAIN_ADJUST" direction="in"/>
<pin name="GAIN_ADJUST_2" direction="in"/>
<pin name="SIGNAL_IN" direction="in"/>
<pin name="SIGNAL_IN_2" direction="in"/>
<pin name="IN_CARRIER" direction="in"/>
<pin name="CARRIER_IN" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="in"/>
<pin name="N/C_4" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="BIAS" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC1496DR2G">
<pin name="IN_CARRIER" direction="pwr"/>
<pin name="CARRIER_IN" direction="pwr"/>
<pin name="SIG_IN" direction="in"/>
<pin name="SIG_IN_2" direction="in"/>
<pin name="GAIN_ADJ" direction="in"/>
<pin name="GAIN_ADJ_2" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C_4" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC3302PG">
<pin name="VCC" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC33033DWR2G">
<pin name="VCC" direction="pwr"/>
<pin name="SA" direction="in"/>
<pin name="SB" direction="in"/>
<pin name="SC" direction="in"/>
<pin name="OSCILLATOR" direction="in"/>
<pin name="FWD/REV" direction="out"/>
<pin name="ERROR_AMP_POS" direction="in"/>
<pin name="60_DEG/120DEG__SELECT" direction="in"/>
<pin name="ERROR_AMP_OUT/PWM_INPUT" direction="in"/>
<pin name="CURRENT_SENSE_POS" direction="in"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="ERROR_AMP_NEG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="AB" direction="out"/>
<pin name="BB" direction="out"/>
<pin name="CB" direction="out"/>
<pin name="AT" direction="out"/>
<pin name="BT" direction="out"/>
<pin name="CT" direction="out"/>
<pin name="REFERENCE_OUTPUT" direction="out"/>
</symbol>
<symbol name="MC33035DWG">
<pin name="VCC" direction="pwr"/>
<pin name="SA" direction="in"/>
<pin name="SB" direction="in"/>
<pin name="SC" direction="in"/>
<pin name="FWD/REV" direction="in"/>
<pin name="BRAKE" direction="in"/>
<pin name="OSCILLATOR" direction="in"/>
<pin name="CURRENT_SENSE_NONINVERTING_INPUT" direction="in"/>
<pin name="ERROR_AMP_NONINVERTING_INPUT" direction="in"/>
<pin name="ERROR_AMP_INVERTING_INPUT" direction="in"/>
<pin name="ERROR_AMP_OUT_PWM_INPUT" direction="in"/>
<pin name="CURRENT_SENSE_INVERTING_INPUT" direction="in"/>
<pin name="60°/~120°_SELECT" direction="in"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VC" direction="out"/>
<pin name="AT" direction="out"/>
<pin name="BT" direction="out"/>
<pin name="CT" direction="out"/>
<pin name="AB" direction="out"/>
<pin name="BB" direction="out"/>
<pin name="CB" direction="out"/>
<pin name="~FAULT_OUTPUT" direction="out"/>
<pin name="REFERENCE_OUTPUT" direction="out"/>
</symbol>
<symbol name="MC33039DG">
<pin name="VCC" direction="pwr"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="RT/CT" direction="in"/>
<pin name="A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~A" direction="out"/>
<pin name="FOUT" direction="out"/>
</symbol>
<symbol name="MC3303PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC33060ADG">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="E" direction="in"/>
<pin name="COMPEN/PWM_COMP_INPUT" direction="in"/>
<pin name="DEAD-TIME_CONTROL" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="POS_IN" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="NEG_IN" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="C" direction="out"/>
</symbol>
<symbol name="MC33063ADG">
<pin name="VCC" direction="pwr"/>
<pin name="COMPTR_NEG" direction="in"/>
<pin name="IPK_SENSE" direction="pas"/>
<pin name="DRVR_C" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW_E" direction="out"/>
<pin name="SW_C" direction="out"/>
<pin name="CT" direction="out"/>
</symbol>
<symbol name="MC33063ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="COMPTR_NEG" direction="in"/>
<pin name="IPK_SENSE" direction="pas"/>
<pin name="DRVR_C" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW_E" direction="out"/>
<pin name="SW_C" direction="out"/>
<pin name="CT" direction="out"/>
</symbol>
<symbol name="MC33063AP1G">
<pin name="VCC" direction="pwr"/>
<pin name="IPK_SEN" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="COMP_NEG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DRVR_C" direction="pas"/>
<pin name="SW_E" direction="pas"/>
<pin name="SW_C" direction="pas"/>
</symbol>
<symbol name="MC33064D-5G">
<pin name="INPUT" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="MC33064D-5R2G">
<pin name="INPUT" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="MC33071ADG">
<pin name="VCC" direction="pwr"/>
<pin name="OFFSET_NULL" direction="in"/>
<pin name="NEG_IN" direction="in"/>
<pin name="POS_IN" direction="in"/>
<pin name="OFFSET_NULL_2" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC33071APG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_2" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="OFS_2" direction="pas"/>
<pin name="OFS" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC33072APG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33072DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33072DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33072PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33074ADG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC33074ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC33074ADTBG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC33074APG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC33074DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC33074DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC33074PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC33077DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33078DG">
<pin name="VCC" direction="pwr"/>
<pin name="+IN_1" direction="in"/>
<pin name="-IN_1" direction="in"/>
<pin name="+IN_2" direction="in"/>
<pin name="-IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33079DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC33079PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC33151PG">
<pin name="VCC" direction="pwr"/>
<pin name="I_A" direction="in"/>
<pin name="I_B" direction="in"/>
<pin name="N.C_2" direction="nc"/>
<pin name="N.C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DRIVE_OUTPUT_A" direction="out"/>
<pin name="DRIVE_OUTPUT_B" direction="out"/>
</symbol>
<symbol name="MC33152DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DRVR_OUTA" direction="out"/>
<pin name="DRVR_OUTB" direction="out"/>
</symbol>
<symbol name="MC33152PG">
<pin name="GND" direction="pas"/>
<pin name="I_A" direction="in"/>
<pin name="I_B" direction="in"/>
<pin name="N.C_2" direction="nc"/>
<pin name="N.C" direction="nc"/>
<pin name="VCC" direction="pwr"/>
<pin name="DRIVE_OUTPUT_A" direction="out"/>
<pin name="DRIVE_OUTPUT_B" direction="out"/>
</symbol>
<symbol name="MC33153DG">
<pin name="VCC" direction="pwr"/>
<pin name="~INPUT" direction="in"/>
<pin name="FAULT_BLANKING/DESATURATION_IN" direction="in"/>
<pin name="CURRENT_SEN_IN" direction="in"/>
<pin name="KELVIN_GND" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="FAULT_OUT" direction="out"/>
<pin name="DRIVE_OUT" direction="out"/>
</symbol>
<symbol name="MC33153DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="~INPUT" direction="in"/>
<pin name="FAULT_BLANKING/DESATURATION_IN" direction="in"/>
<pin name="CURRENT_SENSE_IN" direction="in"/>
<pin name="KELVIN_GND" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="FAULT_OUT" direction="out"/>
<pin name="DRIVE_OUT" direction="out"/>
</symbol>
<symbol name="MC33153PG">
<pin name="VCC" direction="pwr"/>
<pin name="~INPUT" direction="in"/>
<pin name="ISEN_IN" direction="in"/>
<pin name="FAULT_BLANKING/DESATURATION_INPUT" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="KELVIN_GND" direction="pas"/>
<pin name="FLT_OUT" direction="out"/>
<pin name="DR_OUT" direction="out"/>
</symbol>
<symbol name="MC33161DG">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="pas"/>
<pin name="MODE" direction="in"/>
<pin name="IN_1" direction="pwr"/>
<pin name="IN_2" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33161PG">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="pas"/>
<pin name="MODE_SELECT" direction="in"/>
<pin name="INPUT_1" direction="in"/>
<pin name="INPUT_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT_2" direction="out"/>
<pin name="OUTPUT_1" direction="out"/>
</symbol>
<symbol name="MC33164D-3G">
<pin name="INPUT" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="MC33171DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="OFS_2" direction="pas"/>
<pin name="OFS" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC33171PG">
<pin name="VCC" direction="pwr"/>
<pin name="INV._IN" direction="in"/>
<pin name="NONINV._IN" direction="in"/>
<pin name="OFS_2" direction="pas"/>
<pin name="OFS" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC33172DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33172DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33172PG">
<pin name="VCC" direction="pas"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33174PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC33178DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33178PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33179DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC33179DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC33179PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC33201DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN" direction="in"/>
<pin name="POS_IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC33202DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33202PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33202VDG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33204DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC33204DTBG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC33262DG">
<pin name="VCC" direction="pwr"/>
<pin name="ISEN_IN" direction="in"/>
<pin name="VOLTAGE_FEEDBACK_INPUT" direction="in"/>
<pin name="ZERO_CURRENT_DETECT_INPUT" direction="in"/>
<pin name="MULTIPLIER_INPUT" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DRIVE_OUTPUT" direction="out"/>
</symbol>
<symbol name="MC33262PG">
<pin name="VCC" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="MULTIPLIER_INPUT" direction="in"/>
<pin name="ZERO_CURRENT_DETECT_INPUT" direction="in"/>
<pin name="VOLTAGE_FEEDBACK_INPUT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DRIVE_OUTPUT" direction="out"/>
</symbol>
<symbol name="MC33269D-3.3G">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND/ADJ" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT_3" direction="out"/>
<pin name="VOUT_4" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC33269DG">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND/ADJ" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT_3" direction="out"/>
<pin name="VOUT_4" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC33272ADG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33272ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33274APG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC33363ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="COMPENSATION" direction="in"/>
<pin name="POWER_SWITCH_DRAIN" direction="pwr"/>
<pin name="STARTUP_INPUT" direction="in"/>
<pin name="VOLTAGE_FEEDBACK_INPUT" direction="in"/>
<pin name="OVERVOLTAGE_PROTECTION_INPUT" direction="in"/>
<pin name="RT" direction="pas"/>
<pin name="CT" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="REGULATOR_OUTPUT" direction="out"/>
</symbol>
<symbol name="MC33363BDWG">
<pin name="VCC" direction="pwr"/>
<pin name="VOLTAGE_FEEDBACK_INPUT" direction="in"/>
<pin name="COMPENSATION" direction="in"/>
<pin name="OVERVOLTAGE_PROTECTION_INPUT" direction="in"/>
<pin name="STARTUP_INPUT" direction="in"/>
<pin name="POWER_SWITCH_DRAIN" direction="pwr"/>
<pin name="RT" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="REGULATOR_OUTPUT" direction="out"/>
</symbol>
<symbol name="MC33364DG">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="ZERO_CURRENT" direction="in"/>
<pin name="CURRENT_SENSE" direction="in"/>
<pin name="VOLTAGE_FB" direction="pwr"/>
<pin name="FREQ_CLAMP" direction="in"/>
<pin name="LINE" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C_4" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="A_GND" direction="pas"/>
<pin name="P_GND" direction="pas"/>
<pin name="GATE_DRIVE" direction="out"/>
</symbol>
<symbol name="MC33368DG">
<pin name="VCC" direction="pwr"/>
<pin name="CURRENT_SENSE" direction="in"/>
<pin name="5.0_VREF" direction="pwr"/>
<pin name="VOLTAGE_FB" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="ZERO_CURRENT" direction="in"/>
<pin name="MULT" direction="in"/>
<pin name="LINE" direction="in"/>
<pin name="FREQUENCY_CLAMP" direction="in"/>
<pin name="RESTART_DELAY" direction="in"/>
<pin name="LEB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="MC33502DG">
<pin name="VCC" direction="pwr"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33502DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33502PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC33503SNT1G">
<pin name="VCC" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC33761SNT1-050G">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC34023PG">
<pin name="VCC" direction="pwr"/>
<pin name="VC" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="ERROR_AMP_NEG" direction="in"/>
<pin name="ERROR_AMP_POS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="CURRENT_LIMIT_REFERENCE" direction="in"/>
<pin name="CURRENT_LIMIT/SHUTDOWN" direction="in"/>
<pin name="SOFT-START" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="POWER_GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="ERROR_AMP_OUT" direction="out"/>
</symbol>
<symbol name="MC34025PG">
<pin name="VCC" direction="pwr"/>
<pin name="VC" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="ERROR_AMP_NEG" direction="in"/>
<pin name="ERROR_AMP_POS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="CURRENT_LIMIT/SHUTDOWN" direction="in"/>
<pin name="SOFT-START" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="POWER_GND" direction="pas"/>
<pin name="ERROR_AMP_OUT" direction="out"/>
<pin name="OUTPUT_A" direction="out"/>
<pin name="OUTPUT_B" direction="out"/>
</symbol>
<symbol name="MC3403PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE/GND" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC34060APG">
<pin name="VCC" direction="pwr"/>
<pin name="NONINV_IN" direction="in"/>
<pin name="NONINV_IN_2" direction="in"/>
<pin name="INV_IN" direction="in"/>
<pin name="INV_IN_2" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="VREF"/>
<pin name="COMPEN/PWM_COMP_INPUT" direction="in"/>
<pin name="DEAD-TIME_CONTROL" direction="in"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="MC34063ADG">
<pin name="VCC" direction="pwr"/>
<pin name="DRVR_C" direction="in"/>
<pin name="IPK_SENSE" direction="in"/>
<pin name="COMPARATOR_NEG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="TIMING_CAP" direction="out"/>
<pin name="SWITCH_E" direction="out"/>
<pin name="SWITCH_C" direction="out"/>
</symbol>
<symbol name="MC34063AP1G">
<pin name="VCC" direction="pwr"/>
<pin name="IPK_SEN" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="COMP_NEG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DRVR_C" direction="pas"/>
<pin name="SW_E" direction="pas"/>
<pin name="SW_C" direction="pas"/>
</symbol>
<symbol name="MC34064D-5R2G">
<pin name="INPUT" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="MC34067PG">
<pin name="VCC" direction="pwr"/>
<pin name="ENABLE/UVLO_ADJUST" direction="in"/>
<pin name="OSC_CONTROL_CURRENT" direction="in"/>
<pin name="ONE-SHOT_RC" direction="in"/>
<pin name="OSC_CHARGE" direction="in"/>
<pin name="OSC_RC" direction="in"/>
<pin name="FAULT_INPUT" direction="in"/>
<pin name="CSOFT-START" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="POWER_GND" direction="pas"/>
<pin name="VREF" direction="pas"/>
<pin name="ERROR_AMP_OUT" direction="out"/>
<pin name="DRIVE_OUTPUT_A" direction="out"/>
<pin name="DRIVE_OUTPUT_B" direction="out"/>
</symbol>
<symbol name="MC34071DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN" direction="in"/>
<pin name="POS_IN" direction="in"/>
<pin name="OFS_NULL" direction="in"/>
<pin name="OFS_NULL_2" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC34072ADG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC34072APG">
<pin name="VCC" direction="pas"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC34072DG">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC34072DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="NEG_IN_1" direction="in"/>
<pin name="POS_IN_1" direction="in"/>
<pin name="NEG_IN_2" direction="in"/>
<pin name="POS_IN_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC34072PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC34074ADG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC34074APG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC34074DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN1_2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2_2" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3_2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4_2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="MC34074PG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC34074VPG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_1_2" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_2_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_3_2" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_4_2" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="MC34151PG">
<pin name="VCC" direction="pwr"/>
<pin name="I_A" direction="in"/>
<pin name="I_B" direction="in"/>
<pin name="N.C_2" direction="nc"/>
<pin name="N.C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DRIVE_OUTPUT_A" direction="out"/>
<pin name="DRIVE_OUTPUT_B" direction="out"/>
</symbol>
<symbol name="MC34161DG">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="pas"/>
<pin name="MODE" direction="pas"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC34161PG">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="pwr"/>
<pin name="MODE" direction="in"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="MC34163DWG">
<pin name="VCC" direction="pwr"/>
<pin name="BOOTSTRAP_IN" direction="in"/>
<pin name="IPK_SENSE" direction="in"/>
<pin name="SWITCH_COLLECTOR" direction="in"/>
<pin name="SWITCH_COLLECTOR_2" direction="in"/>
<pin name="SWITCH_EMITTER" direction="in"/>
<pin name="SWITCH_EMITTER_2" direction="in"/>
<pin name="DRIVER_COLLECTOR" direction="in"/>
<pin name="TIMING_CAPACITOR" direction="in"/>
<pin name="V_FB_1" direction="in"/>
<pin name="V_FB_2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LVI_OUT" direction="out"/>
</symbol>
<symbol name="MC34163PG">
<pin name="VCC" direction="pwr"/>
<pin name="IPK_SENSE" direction="in"/>
<pin name="TIMING_CAPACITOR" direction="in"/>
<pin name="SWITCH_EMITTER" direction="in"/>
<pin name="SWITCH_EMITTER_2" direction="in"/>
<pin name="VOLTAGE_FEEDBACK_1" direction="in"/>
<pin name="VOLTAGE_FEEDBACK_2" direction="in"/>
<pin name="BOOTSTRAP_INPUT" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH_COLLECTOR" direction="out"/>
<pin name="DRIVER_COLLECTOR" direction="out"/>
<pin name="SWITCH_COLLECTOR_2" direction="out"/>
<pin name="LVI_OUTPUT" direction="out"/>
</symbol>
<symbol name="MC34164D-5G">
<pin name="INPUT" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C._3" direction="nc"/>
<pin name="N.C._4" direction="nc"/>
<pin name="N.C._5" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="MC34262DG">
<pin name="VCC" direction="pwr"/>
<pin name="ISEN_IN" direction="in"/>
<pin name="VOLTAGE_FEEDBACK_INPUT" direction="in"/>
<pin name="ZERO_CURRENT_DETECT_INPUT" direction="in"/>
<pin name="MULTIPLIER_INPUT" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DRIVE_OUTPUT" direction="out"/>
</symbol>
<symbol name="MC34262PG">
<pin name="VCC" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="MULTIPLIER_INPUT" direction="in"/>
<pin name="ZERO_CURRENT_DETECT_INPUT" direction="in"/>
<pin name="VOLTAGE_FEEDBACK_INPUT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DRIVE_OUTPUT" direction="out"/>
</symbol>
<symbol name="MC74AC00DG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74AC02DG">
<pin name="VCC" direction="pwr"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74AC04DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT_6" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC74AC08DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN_7" direction="in"/>
<pin name="IN_8" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC74AC132DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN_7" direction="in"/>
<pin name="IN_8" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC74AC138DG">
<pin name="VCC" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="~E1" direction="in"/>
<pin name="~E2" direction="in"/>
<pin name="E3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~O0" direction="out"/>
<pin name="~O1" direction="out"/>
<pin name="~O2" direction="out"/>
<pin name="~O3" direction="out"/>
<pin name="~O4" direction="out"/>
<pin name="~O5" direction="out"/>
<pin name="~O6" direction="out"/>
<pin name="~O7" direction="out"/>
</symbol>
<symbol name="MC74AC32DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN_7" direction="in"/>
<pin name="IN_8" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC74AC4040DG">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q11" direction="out"/>
<pin name="Q12" direction="out"/>
</symbol>
<symbol name="MC74AC4040NG">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q11" direction="out"/>
<pin name="Q12" direction="out"/>
</symbol>
<symbol name="MC74AC573DWG">
<pin name="VCC" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="O0" direction="out"/>
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
<pin name="O4" direction="out"/>
<pin name="O5" direction="out"/>
<pin name="O6" direction="out"/>
<pin name="O7" direction="out"/>
</symbol>
<symbol name="MC74AC574DWR2G">
<pin name="VCC" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="CP" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="O0" direction="out"/>
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
<pin name="O4" direction="out"/>
<pin name="O5" direction="out"/>
<pin name="O6" direction="out"/>
<pin name="O7" direction="out"/>
</symbol>
<symbol name="MC74AC74DG">
<pin name="VCC" direction="pwr"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="CP1" direction="in"/>
<pin name="CP2" direction="in"/>
<pin name="~SD1" direction="in"/>
<pin name="~SD2" direction="in"/>
<pin name="~CD1" direction="in"/>
<pin name="~CD2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="~Q2" direction="out"/>
</symbol>
<symbol name="MC74AC74NG">
<pin name="VCC" direction="pwr"/>
<pin name="~CD1" direction="in"/>
<pin name="~CD2" direction="in"/>
<pin name="~SD1" direction="in"/>
<pin name="~SD2" direction="in"/>
<pin name="CP1" direction="in"/>
<pin name="CP2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
</symbol>
<symbol name="MC74ACT00DG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74ACT02DG">
<pin name="VCC" direction="pwr"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74ACT05DG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74ACT125DG">
<pin name="VCC" direction="pwr"/>
<pin name="~A1" direction="in"/>
<pin name="~A0" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="~A3" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="~A2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="O0" direction="out"/>
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
</symbol>
<symbol name="MC74ACT132DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN_7" direction="in"/>
<pin name="IN_8" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC74ACT14DG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT_6" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MC74ACT74DG">
<pin name="VCC" direction="pwr"/>
<pin name="CP1" direction="in"/>
<pin name="CP2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="~CD1" direction="in"/>
<pin name="~CD2" direction="in"/>
<pin name="~SD1" direction="in"/>
<pin name="~SD2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="~Q2" direction="out"/>
</symbol>
<symbol name="MC74HC00ADG">
<pin name="VCC" direction="pwr"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC00ANG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC02ADG">
<pin name="VCC" direction="pwr"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC02ANG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC03ADG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC04ADG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HC04ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HC04ADTR2G">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HC08ADG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC08ADTR2G">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC125ADG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2" direction="in"/>
<pin name="OE3" direction="in"/>
<pin name="OE4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC125ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2" direction="in"/>
<pin name="OE3" direction="in"/>
<pin name="OE4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC132ADG">
<pin name="VCC" direction="pwr"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC132ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC132ADTG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC132ANG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC138ADG">
<pin name="VCC" direction="pwr"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="CS3" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y0" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
</symbol>
<symbol name="MC74HC138ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="CS3" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y0" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
</symbol>
<symbol name="MC74HC138ANG">
<pin name="VCC" direction="pwr"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="CS3" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y0" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
</symbol>
<symbol name="MC74HC139ADG">
<pin name="VCC" direction="pwr"/>
<pin name="A0A" direction="in"/>
<pin name="A1A" direction="in"/>
<pin name="A0B" direction="in"/>
<pin name="A1B" direction="in"/>
<pin name="SELECTA" direction="in"/>
<pin name="SELECTB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y0A" direction="out"/>
<pin name="Y1A" direction="out"/>
<pin name="Y2A" direction="out"/>
<pin name="Y3A" direction="out"/>
<pin name="Y0B" direction="out"/>
<pin name="Y1B" direction="out"/>
<pin name="Y2B" direction="out"/>
<pin name="Y3B" direction="out"/>
</symbol>
<symbol name="MC74HC14ADG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HC14ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HC14ADTG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HC14ANG">
<pin name="GND" direction="pas"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HC164ADG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QH" direction="out"/>
</symbol>
<symbol name="MC74HC165ADG">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="CLK_INHIBIT" direction="in"/>
<pin name="SERIAL_SHIFT/~PARALLEL_LOAD" direction="in"/>
<pin name="SA" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="QH" direction="out"/>
<pin name="~QH" direction="out"/>
</symbol>
<symbol name="MC74HC1G04DTT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y" direction="out"/>
</symbol>
<symbol name="MC74HC1G14DTT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74HC240ANG">
<pin name="VCC" direction="pwr"/>
<pin name="EN_A" direction="in"/>
<pin name="EN_B" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="YA1" direction="out"/>
<pin name="YA2" direction="out"/>
<pin name="YA3" direction="out"/>
<pin name="YA4" direction="out"/>
<pin name="YB1" direction="out"/>
<pin name="YB2" direction="out"/>
<pin name="YB3" direction="out"/>
<pin name="YB4" direction="out"/>
</symbol>
<symbol name="MC74HC244ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="ENABLE_A" direction="in"/>
<pin name="ENABLE_B" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="YA1" direction="out"/>
<pin name="YA2" direction="out"/>
<pin name="YA3" direction="out"/>
<pin name="YA4" direction="out"/>
<pin name="YB1" direction="out"/>
<pin name="YB2" direction="out"/>
<pin name="YB3" direction="out"/>
<pin name="YB4" direction="out"/>
</symbol>
<symbol name="MC74HC244ADWR2G">
<pin name="VCC" direction="pwr"/>
<pin name="ENABLE_A" direction="in"/>
<pin name="ENABLE_B" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="YA1" direction="out"/>
<pin name="YA2" direction="out"/>
<pin name="YA3" direction="out"/>
<pin name="YA4" direction="out"/>
<pin name="YB1" direction="out"/>
<pin name="YB2" direction="out"/>
<pin name="YB3" direction="out"/>
<pin name="YB4" direction="out"/>
</symbol>
<symbol name="MC74HC244ANG">
<pin name="VCC" direction="pwr"/>
<pin name="EN_A" direction="in"/>
<pin name="EN_B" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="YA1" direction="out"/>
<pin name="YA2" direction="out"/>
<pin name="YA3" direction="out"/>
<pin name="YA4" direction="out"/>
<pin name="YB1" direction="out"/>
<pin name="YB2" direction="out"/>
<pin name="YB3" direction="out"/>
<pin name="YB4" direction="out"/>
</symbol>
<symbol name="MC74HC245ADTG">
<pin name="VCC" direction="pwr"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="DIRECTION" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_EN"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
</symbol>
<symbol name="MC74HC245ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="DIRECTION" direction="in"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="GND" direction="pas"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
</symbol>
<symbol name="MC74HC245ANG">
<pin name="VCC" direction="pwr"/>
<pin name="DIR" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="GND" direction="pas"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
</symbol>
<symbol name="MC74HC273ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC74HC273ANG">
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC74HC32ADG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HC373ANG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="LATCH_ENABLE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC74HC374ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC74HC374ANG">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC74HC390ADG">
<pin name="VCC" direction="in"/>
<pin name="RSTA" direction="out"/>
<pin name="RST_B" direction="in"/>
<pin name="CLK_AB" direction="in"/>
<pin name="CLK_BA" direction="in"/>
<pin name="CLK_BB" direction="in"/>
<pin name="GND" direction="out"/>
<pin name="CLK_AA" direction="in"/>
<pin name="QAA" direction="in"/>
<pin name="QBA" direction="pas"/>
<pin name="QCA" direction="out"/>
<pin name="QDA" direction="out"/>
<pin name="QAB" direction="out"/>
<pin name="QBB" direction="out"/>
<pin name="QCB" direction="out"/>
<pin name="QDB" direction="out"/>
</symbol>
<symbol name="MC74HC4040ADG">
<pin name="VCC" direction="out"/>
<pin name="RST" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="GND" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q11" direction="out"/>
<pin name="Q12" direction="out"/>
</symbol>
<symbol name="MC74HC4046ADG">
<pin name="VCC" direction="pwr"/>
<pin name="VCOIN" direction="in"/>
<pin name="R1" direction="pas"/>
<pin name="R2" direction="pas"/>
<pin name="C1A" direction="pas"/>
<pin name="C1B" direction="pas"/>
<pin name="INH" direction="in"/>
<pin name="COMPIN" direction="in"/>
<pin name="SIGIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="PCPOUT" direction="out"/>
<pin name="PC1OUT" direction="out"/>
<pin name="PC2OUT" direction="out"/>
<pin name="PC3OUT" direction="out"/>
<pin name="DEMOUT" direction="out"/>
<pin name="VCOOUT" direction="out"/>
</symbol>
<symbol name="MC74HC4046ANG">
<pin name="VCC" direction="pwr"/>
<pin name="INH" direction="in"/>
<pin name="C1A" direction="pas"/>
<pin name="C1B" direction="pas"/>
<pin name="SIGIN" direction="in"/>
<pin name="COMPIN" direction="in"/>
<pin name="VCOIN" direction="in"/>
<pin name="R1" direction="pas"/>
<pin name="R2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VCOOUT" direction="out"/>
<pin name="DEMOUT" direction="out"/>
<pin name="PC1OUT" direction="out"/>
<pin name="PCPOUT" direction="out"/>
<pin name="PC2OUT" direction="out"/>
<pin name="PC3OUT" direction="out"/>
</symbol>
<symbol name="MC74HC4051ADR2G">
<pin name="VCC" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="X0" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="X3" direction="in"/>
<pin name="X4" direction="in"/>
<pin name="X5" direction="in"/>
<pin name="X6" direction="in"/>
<pin name="X7" direction="in"/>
<pin name="VEE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="X" direction="out"/>
</symbol>
<symbol name="MC74HC4051ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="ENABLE" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="X3"/>
<pin name="X4"/>
<pin name="X5"/>
<pin name="X6"/>
<pin name="X7"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="X"/>
</symbol>
<symbol name="MC74HC4052ADTG">
<pin name="VDD" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="X3"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="Y3"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="X"/>
<pin name="Y"/>
</symbol>
<symbol name="MC74HC4052ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="ENABLE" direction="in"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="X3"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="Y3"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="X"/>
<pin name="Y"/>
</symbol>
<symbol name="MC74HC4052ANG">
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="X3"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="Y3"/>
<pin name="GND" direction="pas"/>
<pin name="X"/>
<pin name="Y"/>
</symbol>
<symbol name="MC74HC4053ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="ENABLE" direction="in"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Z0"/>
<pin name="Z1"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="X"/>
<pin name="Y"/>
<pin name="Z"/>
</symbol>
<symbol name="MC74HC4053ANG">
<pin name="VCC" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Z0"/>
<pin name="Z1"/>
<pin name="X"/>
<pin name="Y"/>
<pin name="Z"/>
</symbol>
<symbol name="MC74HC4060ADG">
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="OSC_IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q12" direction="out"/>
<pin name="Q13" direction="out"/>
<pin name="Q14" direction="out"/>
<pin name="OSC_OUT_2" direction="out"/>
<pin name="OSC_OUT_1" direction="out"/>
</symbol>
<symbol name="MC74HC4060ANG">
<pin name="VCC" direction="pwr"/>
<pin name="OSC_IN" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OSC_OUT_1" direction="out"/>
<pin name="OSC_OUT_2" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q12" direction="out"/>
<pin name="Q13" direction="out"/>
<pin name="Q14" direction="out"/>
</symbol>
<symbol name="MC74HC4066ADG">
<pin name="VCC" direction="pwr"/>
<pin name="XA" direction="in"/>
<pin name="XC" direction="in"/>
<pin name="XB" direction="in"/>
<pin name="XD" direction="in"/>
<pin name="A_ON/OFF_CONTROL" direction="in"/>
<pin name="B_ON/OFF_CONTROL" direction="in"/>
<pin name="C_ON/OFF_CONTROL" direction="in"/>
<pin name="D_ON/OFF_CONTROL" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="YA" direction="out"/>
<pin name="YB" direction="out"/>
<pin name="YC" direction="out"/>
<pin name="YD" direction="out"/>
</symbol>
<symbol name="MC74HC4066ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="XA" direction="in"/>
<pin name="XC" direction="in"/>
<pin name="XB" direction="in"/>
<pin name="XD" direction="in"/>
<pin name="A_ON/OFF_CONTROL" direction="in"/>
<pin name="B_ON/OFF_CONTROL" direction="in"/>
<pin name="C_ON/OFF_CONTROL" direction="in"/>
<pin name="D_ON/OFF_CONTROL" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="YA" direction="out"/>
<pin name="YB" direction="out"/>
<pin name="YC" direction="out"/>
<pin name="YD" direction="out"/>
</symbol>
<symbol name="MC74HC4538ADG">
<pin name="VCC" direction="pwr"/>
<pin name="CX2/RX2" direction="pas"/>
<pin name="CX1/RX1" direction="pas"/>
<pin name="RESET_1" direction="in"/>
<pin name="RESET_2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
</symbol>
<symbol name="MC74HC4538ANG">
<pin name="VCC" direction="pwr"/>
<pin name="CX1/RX1" direction="pas"/>
<pin name="CX2/RX2" direction="pas"/>
<pin name="RESET_1" direction="in"/>
<pin name="RESET_2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
</symbol>
<symbol name="MC74HC540ANG">
<pin name="VCC" direction="pwr"/>
<pin name="OE1" direction="in"/>
<pin name="OE2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="Y8" direction="out"/>
</symbol>
<symbol name="MC74HC541ADTG">
<pin name="VCC" direction="pwr"/>
<pin name="OE1" direction="in"/>
<pin name="OE2" direction="out"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="Y8" direction="out"/>
</symbol>
<symbol name="MC74HC541ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="OE1" direction="in"/>
<pin name="OE2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="Y8" direction="out"/>
</symbol>
<symbol name="MC74HC541ADWR2G">
<pin name="VCC" direction="pwr"/>
<pin name="OE1" direction="in"/>
<pin name="OE2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="Y8" direction="out"/>
</symbol>
<symbol name="MC74HC541ANG">
<pin name="VCC" direction="pwr"/>
<pin name="OE1" direction="in"/>
<pin name="OE2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="Y8" direction="out"/>
</symbol>
<symbol name="MC74HC573ADTG">
<pin name="VCC" direction="pwr"/>
<pin name="LATCH_ENABLE" direction="in"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC74HC573ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="LATCH_ENABLE" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC74HC573ANG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="LATCH_ENABLE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC74HC574ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC74HC589ANG">
<pin name="VCC" direction="pwr"/>
<pin name="LATCH_CLK" direction="in"/>
<pin name="SHIFT_CLK" direction="in"/>
<pin name="SER_SHIFT/PAR_LOAD" direction="in"/>
<pin name="OUT_EN" direction="in"/>
<pin name="SA" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="QH" direction="out"/>
</symbol>
<symbol name="MC74HC595ADG">
<pin name="VCC" direction="pwr"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="SHIFT_CLOCK" direction="in"/>
<pin name="LATCH_CLOCK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="SQH" direction="in"/>
<pin name="A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QH" direction="out"/>
</symbol>
<symbol name="MC74HC595ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="OE" direction="in"/>
<pin name="LATCH_CLK" direction="in"/>
<pin name="SHIFT_CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="QA" direction="in"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QH" direction="out"/>
<pin name="SQH" direction="out"/>
</symbol>
<symbol name="MC74HC595ADTR2G">
<pin name="VCC" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="LATCH_CLOCK" direction="in"/>
<pin name="SHIFT_CLOCK" direction="in"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QH" direction="out"/>
<pin name="SQH"/>
</symbol>
<symbol name="MC74HC595ANG">
<pin name="VCC" direction="pwr"/>
<pin name="LATCH_CLK" direction="in"/>
<pin name="SHIFT_CLK" direction="in"/>
<pin name="OUT_EN" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QH" direction="out"/>
<pin name="SQH" direction="out"/>
</symbol>
<symbol name="MC74HC74ADG">
<pin name="VCC" direction="pwr"/>
<pin name="DATA_1" direction="in"/>
<pin name="DATA_2" direction="in"/>
<pin name="CLK_1" direction="in"/>
<pin name="CLK_2" direction="in"/>
<pin name="SET_1" direction="in"/>
<pin name="SET_2" direction="in"/>
<pin name="RESET_1" direction="in"/>
<pin name="RESET_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
</symbol>
<symbol name="MC74HC74ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="DATA_1" direction="in"/>
<pin name="DATA_2" direction="in"/>
<pin name="CLK_1" direction="in"/>
<pin name="CLK_2" direction="in"/>
<pin name="SET_1" direction="in"/>
<pin name="SET_2" direction="in"/>
<pin name="RESET_1" direction="in"/>
<pin name="RESET_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
</symbol>
<symbol name="MC74HC74ANG">
<pin name="VCC" direction="pwr"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="SET1" direction="in"/>
<pin name="SET2" direction="in"/>
<pin name="RESET1" direction="in"/>
<pin name="RESET2" direction="in"/>
<pin name="DATA1" direction="in"/>
<pin name="DATA2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
</symbol>
<symbol name="MC74HC86ADG">
<pin name="VCC" direction="pwr"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC74HCT04ADG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HCT04ANG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HCT14ADG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HCT14ANG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HCT244ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="ENABLE_A" direction="in"/>
<pin name="ENABLE_B" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="YA1" direction="out"/>
<pin name="YA2" direction="out"/>
<pin name="YA3" direction="out"/>
<pin name="YA4" direction="out"/>
<pin name="YB1" direction="out"/>
<pin name="YB2" direction="out"/>
<pin name="YB3" direction="out"/>
<pin name="YB4" direction="out"/>
</symbol>
<symbol name="MC74HCT374ANG">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
</symbol>
<symbol name="MC74HCT541ADWG">
<pin name="VCC" direction="pwr"/>
<pin name="OE1" direction="in"/>
<pin name="OE2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="Y8" direction="out"/>
</symbol>
<symbol name="MC74HCT541ANG">
<pin name="VCC" direction="pwr"/>
<pin name="OE1" direction="in"/>
<pin name="OE2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="Y8" direction="out"/>
</symbol>
<symbol name="MC74HCT74ANG">
<pin name="VCC" direction="pwr"/>
<pin name="CLK_1" direction="in"/>
<pin name="CLK_2" direction="in"/>
<pin name="SET_1" direction="in"/>
<pin name="SET_2" direction="in"/>
<pin name="DATA_1" direction="in"/>
<pin name="DATA_2" direction="in"/>
<pin name="RESET_1" direction="in"/>
<pin name="RESET_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q2" direction="out"/>
</symbol>
<symbol name="MC74HCU04ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74HCU04ANG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
</symbol>
<symbol name="MC74LCX04DG">
<pin name="VCC" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~O0" direction="out"/>
<pin name="~O1" direction="out"/>
<pin name="~O2" direction="out"/>
<pin name="~O4" direction="out"/>
<pin name="~O3" direction="out"/>
<pin name="~O5" direction="out"/>
</symbol>
<symbol name="MC74LCX04DTG">
<pin name="VCC" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~O0" direction="out"/>
<pin name="~O1" direction="out"/>
<pin name="~O2" direction="out"/>
<pin name="~O3" direction="out"/>
<pin name="~O4" direction="out"/>
<pin name="~O5" direction="out"/>
</symbol>
<symbol name="MC74LCX08DG">
<pin name="VCC" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="O0" direction="out"/>
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
</symbol>
<symbol name="MC74LCX08DTG">
<pin name="VCC" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="O0" direction="out"/>
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
</symbol>
<symbol name="MC74LCX14DG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~Y1" direction="out"/>
<pin name="~Y2" direction="out"/>
<pin name="~Y3" direction="out"/>
<pin name="~Y4" direction="out"/>
<pin name="~Y5" direction="out"/>
<pin name="~Y6" direction="out"/>
</symbol>
<symbol name="MC74LCX16245DTG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~OE1" direction="in"/>
<pin name="~OE2" direction="in"/>
<pin name="T/~R1" direction="in"/>
<pin name="T/~R2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="B0" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="B9" direction="out"/>
<pin name="B10" direction="out"/>
<pin name="B11" direction="out"/>
<pin name="B12" direction="out"/>
<pin name="B13" direction="out"/>
<pin name="B14" direction="out"/>
<pin name="B15" direction="out"/>
</symbol>
<symbol name="MC74LCX16245DTR2">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~OE1" direction="in"/>
<pin name="~OE2" direction="in"/>
<pin name="T/~R1" direction="in"/>
<pin name="T/~R2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="B0" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="B9" direction="out"/>
<pin name="B10" direction="out"/>
<pin name="B11" direction="out"/>
<pin name="B12" direction="out"/>
<pin name="B13" direction="out"/>
<pin name="B14" direction="out"/>
<pin name="B15" direction="out"/>
</symbol>
<symbol name="MC74LCX16373DTG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D11" direction="in"/>
<pin name="D12" direction="in"/>
<pin name="D13" direction="in"/>
<pin name="D14" direction="out"/>
<pin name="D15" direction="out"/>
<pin name="OE1" direction="in"/>
<pin name="OE2" direction="in"/>
<pin name="LE1" direction="in"/>
<pin name="LE2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GN_2" direction="pas"/>
<pin name="GN_3" direction="pas"/>
<pin name="GN_4" direction="pas"/>
<pin name="GN" direction="pas"/>
<pin name="O0" direction="out"/>
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
<pin name="O4" direction="out"/>
<pin name="O5" direction="out"/>
<pin name="O6" direction="out"/>
<pin name="O7" direction="out"/>
<pin name="O8" direction="out"/>
<pin name="O9" direction="out"/>
<pin name="O10" direction="out"/>
<pin name="O11" direction="out"/>
<pin name="O12" direction="out"/>
<pin name="O13" direction="out"/>
<pin name="O14" direction="out"/>
<pin name="O15" direction="out"/>
</symbol>
<symbol name="MC74LCX244DWG">
<pin name="VCC" direction="pwr"/>
<pin name="~1OE" direction="in"/>
<pin name="~2OE" direction="in"/>
<pin name="1D0" direction="in"/>
<pin name="1D1" direction="in"/>
<pin name="1D2" direction="in"/>
<pin name="1D3" direction="in"/>
<pin name="2D0" direction="in"/>
<pin name="2D1" direction="in"/>
<pin name="2D2" direction="in"/>
<pin name="2D3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="1O0" direction="out"/>
<pin name="1O1" direction="out"/>
<pin name="1O2" direction="out"/>
<pin name="1O3" direction="out"/>
<pin name="2O0" direction="out"/>
<pin name="2O1" direction="out"/>
<pin name="2O2" direction="out"/>
<pin name="2O3" direction="out"/>
</symbol>
<symbol name="MC74LCX245DWG">
<pin name="VCC" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="T/R" direction="in"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="GND" direction="pas"/>
<pin name="B0"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B7"/>
<pin name="B6"/>
</symbol>
<symbol name="MC74LVX04DTR2G">
<pin name="VCC" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~O0" direction="out"/>
<pin name="~O1" direction="out"/>
<pin name="~O2" direction="out"/>
<pin name="~O3" direction="out"/>
<pin name="~O4" direction="out"/>
<pin name="~O5" direction="out"/>
</symbol>
<symbol name="MC74LVX08DTG">
<pin name="VCC" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="O0" direction="out"/>
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
</symbol>
<symbol name="MC74LVX08DTR2G">
<pin name="VCC" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="O0" direction="out"/>
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
</symbol>
<symbol name="MC74LVX4245DTG">
<pin name="VCCA" direction="pwr"/>
<pin name="VCCB_2" direction="nc"/>
<pin name="VCCB" direction="pwr"/>
<pin name="T/~R" direction="in"/>
<pin name="~OE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B0" direction="out"/>
</symbol>
<symbol name="MC74LVXC3245DTG">
<pin name="VCCA" direction="pwr"/>
<pin name="VCCB" direction="pwr"/>
<pin name="T/~R" direction="in"/>
<pin name="~OE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="B0" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
</symbol>
<symbol name="MC74VHC138DG">
<pin name="VCC" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="~E1" direction="in"/>
<pin name="~E2" direction="in"/>
<pin name="E3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~Y0" direction="out"/>
<pin name="~Y1" direction="out"/>
<pin name="~Y2" direction="out"/>
<pin name="~Y3" direction="out"/>
<pin name="~Y4" direction="out"/>
<pin name="~Y5" direction="out"/>
<pin name="~Y7" direction="out"/>
<pin name="~Y6" direction="out"/>
</symbol>
<symbol name="MC74VHC14DTG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~Y1" direction="out"/>
<pin name="~Y2" direction="out"/>
<pin name="~Y3" direction="out"/>
<pin name="~Y6" direction="out"/>
<pin name="~Y5" direction="out"/>
<pin name="~Y4" direction="out"/>
</symbol>
<symbol name="MC74VHC1G00DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1G00DFT2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1G03DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1G04DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1G05DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1G08DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1G09DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1G125DFT1">
<pin name="VCC" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1G126DFT1">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1G14DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1G32DTT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1G86DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_B" direction="out"/>
<pin name="IN_A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1GT125DF1">
<pin name="VCC" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1GT125DF2">
<pin name="VCC" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1GT125DT1">
<pin name="VCC" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1GT126DF1">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1GT126DF1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1GT32DFT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHC1GT50DTT1">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="MC74VHCT125ADR2G">
<pin name="VCC" direction="pwr"/>
<pin name="~OE1" direction="in"/>
<pin name="~OE2" direction="in"/>
<pin name="~OE3" direction="in"/>
<pin name="~OE4" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MC75174BDWG">
<pin name="VCC" direction="pwr"/>
<pin name="EN12" direction="in"/>
<pin name="EN34" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="1Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="4Y" direction="out"/>
<pin name="1Z" direction="out"/>
<pin name="2Z" direction="out"/>
<pin name="3Z" direction="out"/>
<pin name="4Z" direction="out"/>
</symbol>
<symbol name="MC75174BPG">
<pin name="VCC" direction="pwr"/>
<pin name="EN_12" direction="in"/>
<pin name="EN_34" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="1Z" direction="out"/>
<pin name="2Z" direction="out"/>
<pin name="3Z" direction="out"/>
<pin name="4Z" direction="out"/>
<pin name="1Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="4Y" direction="out"/>
</symbol>
<symbol name="MC78L05ABDG">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78L05ABDR2G">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78L05ACDG">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78L05ACDR2G">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78L08ABDG">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78L08ACDG">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78L09ACDG">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78L12ACDG">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78L12ACDR2G">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78L15ABDG">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78L15ACDG">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78L15ACDR2G">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78LC33NTRG">
<pin name="VIN" direction="pwr"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78LC50NTRG">
<pin name="VIN" direction="pwr"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78PC18NTRG">
<pin name="VIN" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78PC33NTRG">
<pin name="VIN" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC78PC50NTRG">
<pin name="VIN" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC79L05ABDG">
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN_4" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC79L12ACDG">
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN_4" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MC79L15ACDG">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN_3" direction="pwr"/>
<pin name="VIN_4" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MCH12140DG">
<pin name="VCC" direction="pwr"/>
<pin name="R" direction="in"/>
<pin name="V" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="D" direction="out"/>
<pin name="~D" direction="out"/>
<pin name="U" direction="out"/>
<pin name="~U" direction="out"/>
</symbol>
<symbol name="MDC3105DMT1G">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MDC3105LT1G">
<pin name="VIN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="MMBZ5243BLT1G">
<pin name="ANODE" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="N25S830HAS22I">
<pin name="VCC" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="~HOLD" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="SO" direction="out"/>
</symbol>
<symbol name="NB100ELT23LDTG">
<pin name="VCC" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="~D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="~D1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
</symbol>
<symbol name="NB3L553DG">
<pin name="VDD" direction="pwr"/>
<pin name="OE" direction="in"/>
<pin name="ICLK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
</symbol>
<symbol name="NB3N2304NZDTG">
<pin name="VDD" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
</symbol>
<symbol name="NB3N551DG">
<pin name="VDD" direction="pwr"/>
<pin name="OE" direction="in"/>
<pin name="ICLK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
</symbol>
<symbol name="NB6L11DTG">
<pin name="VCC" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="~D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="NB6L14MNG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
<pin name="VREF_AC" direction="out"/>
<pin name="VT" direction="out"/>
</symbol>
<symbol name="NB6L239MNG">
<pin name="VCC" direction="pwr"/>
<pin name="SELA0" direction="in"/>
<pin name="SELA1" direction="in"/>
<pin name="SELB0" direction="in"/>
<pin name="SELB1" direction="in"/>
<pin name="~CLK" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="~MR" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VBBAC" direction="pas"/>
<pin name="VT" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="EP" direction="pwr"/>
<pin name="QA" direction="out"/>
<pin name="~QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="~QB" direction="out"/>
</symbol>
<symbol name="NB6N14SMNG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="~Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="~Q3" direction="out"/>
<pin name="VREF_AC" direction="out"/>
<pin name="VT" direction="out"/>
</symbol>
<symbol name="NBSG11MNG">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~CLK" direction="in"/>
<pin name="~VTCLK" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VTCLK" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="EP" direction="pwr"/>
<pin name="Q0" direction="out"/>
<pin name="~Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="~Q1" direction="out"/>
</symbol>
<symbol name="NCP100SNT1G">
<pin name="REFERENCE" direction="pwr"/>
<pin name="ANODE_2" direction="pas"/>
<pin name="ANODE" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="NCP1055P100G">
<pin name="VCC" direction="pwr"/>
<pin name="CONTROL_INPUT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="POWER_SWITCH_DRAIN" direction="pas"/>
</symbol>
<symbol name="NCP1055P136G">
<pin name="VCC" direction="pwr"/>
<pin name="CONTROL_INPUT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="POWER_SWITCH_DRAIN" direction="pas"/>
</symbol>
<symbol name="NCP1090DG">
<pin name="VPORTP" direction="in"/>
<pin name="RTN" direction="pas"/>
<pin name="VPORTN" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="DET" direction="out"/>
<pin name="CLASS" direction="out"/>
<pin name="PGOOD" direction="out"/>
<pin name="INRUSH" direction="out"/>
</symbol>
<symbol name="NCP1092DG">
<pin name="VPORTP" direction="in"/>
<pin name="RTN" direction="pas"/>
<pin name="VPORTN" direction="pas"/>
<pin name="AUX" direction="in"/>
<pin name="DET" direction="out"/>
<pin name="CLASS" direction="out"/>
<pin name="PGOOD" direction="out"/>
<pin name="INRUSH" direction="out"/>
</symbol>
<symbol name="NCP1200D100R2G">
<pin name="VCC" direction="pwr"/>
<pin name="HV" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DRV" direction="out"/>
</symbol>
<symbol name="NCP1200P100G">
<pin name="VCC" direction="pwr"/>
<pin name="ADJ" direction="pas"/>
<pin name="CS" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="HV" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DRV" direction="out"/>
</symbol>
<symbol name="NCP1200P40G">
<pin name="VCC" direction="pwr"/>
<pin name="ADJ" direction="pas"/>
<pin name="CS" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="HV" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DRV" direction="out"/>
</symbol>
<symbol name="NCP1200P60G">
<pin name="VCC" direction="pwr"/>
<pin name="ADJ" direction="pas"/>
<pin name="CS" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="HV" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DRV" direction="out"/>
</symbol>
<symbol name="NCP1203D100R2G">
<pin name="VCC" direction="pwr"/>
<pin name="HV" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DRV" direction="out"/>
</symbol>
<symbol name="NCP1203D60R2G">
<pin name="VCC" direction="pwr"/>
<pin name="HV" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DRV" direction="out"/>
</symbol>
<symbol name="NCP1230D100R2G">
<pin name="VCC" direction="pwr"/>
<pin name="PFC_VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="HV" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="in"/>
<pin name="DRV" direction="out"/>
</symbol>
<symbol name="NCP1400ASN33T1G">
<pin name="LX" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="NCP1402SN33T1G">
<pin name="LX" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="NCP1402SN50T1G">
<pin name="CE" direction="in"/>
<pin name="LX" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="NCP1450ASN19T1G">
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EXT" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="NCP1450ASN27T1G">
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EXT" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="NCP1450ASN33T1G">
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EXT" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="NCP1521BSNT1G">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="NCP1529ASNT1G">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="NCP1529MUTBG">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="NCP1729SN35T1G">
<pin name="VIN" direction="pwr"/>
<pin name="~SHDN" direction="in"/>
<pin name="C+" direction="pas"/>
<pin name="C-" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP2811BFCCT1G">
<pin name="VP" direction="pwr"/>
<pin name="INR" direction="in"/>
<pin name="INL" direction="in"/>
<pin name="CPM" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="SPVM" direction="pwr"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="PVM" direction="out"/>
<pin name="CPP"/>
</symbol>
<symbol name="NCP2824FCT2G">
<pin name="VDD" direction="pwr"/>
<pin name="INP" direction="in"/>
<pin name="INM" direction="in"/>
<pin name="CNTL" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="OUTP" direction="out"/>
<pin name="OUTM" direction="out"/>
</symbol>
<symbol name="NCP301LSN09T1G">
<pin name="IN" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="RESET_OUT" direction="out"/>
</symbol>
<symbol name="NCP301LSN20T1G">
<pin name="IN" direction="in"/>
<pin name="N.C_2" direction="nc"/>
<pin name="N.C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="RESET_OUT" direction="out"/>
</symbol>
<symbol name="NCP301LSN45T1G">
<pin name="IN" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="RESET_OUT" direction="out"/>
</symbol>
<symbol name="NCP301LSN47T1G">
<pin name="IN" direction="pwr"/>
<pin name="N.C._2" direction="nc"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="RESET_OUT" direction="out"/>
</symbol>
<symbol name="NCP302LSN30T1G">
<pin name="IN" direction="pwr"/>
<pin name="CD" direction="in"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="RESET_OUT" direction="out"/>
</symbol>
<symbol name="NCP302LSN45T1G">
<pin name="IN" direction="pwr"/>
<pin name="CD" direction="in"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="RESET_OUT" direction="out"/>
</symbol>
<symbol name="NCP303LSN09T1G">
<pin name="IN" direction="pwr"/>
<pin name="CD" direction="in"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="RESET_OUT" direction="out"/>
</symbol>
<symbol name="NCP303LSN20T1G">
<pin name="IN" direction="pwr"/>
<pin name="CD" direction="in"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="RESET_OUT" direction="out"/>
</symbol>
<symbol name="NCP3063BDR2G">
<pin name="VCC" direction="pwr"/>
<pin name="COMPARATOR_INVERTING_INPUT" direction="in"/>
<pin name="IPK_SENSE" direction="in"/>
<pin name="SWITCH_EMITTER" direction="in"/>
<pin name="TIMING_CAPACITOR" direction="pas"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH_COLLECTOR" direction="out"/>
</symbol>
<symbol name="NCP3065DR2G">
<pin name="VCC" direction="pwr"/>
<pin name="COMPTR_NEG" direction="in"/>
<pin name="IPK_SENSE" direction="in"/>
<pin name="N.C." direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="SW_E" direction="out"/>
<pin name="SW_C" direction="out"/>
<pin name="CT" direction="out"/>
</symbol>
<symbol name="NCP3065PG">
<pin name="VCC" direction="pwr"/>
<pin name="ISEN" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="COMP_NEG" direction="in"/>
<pin name="N.C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="SW_C" direction="pas"/>
<pin name="SW_E" direction="pas"/>
</symbol>
<symbol name="NCP3163BMNR2G">
<pin name="VCC" direction="pwr"/>
<pin name="IPK_SENSE" direction="in"/>
<pin name="BOOTSTRAP_INPUT" direction="in"/>
<pin name="TC" direction="pas"/>
<pin name="DRIVER_COLLECTOR" direction="pas"/>
<pin name="SWITCH_COLLECTOR" direction="pas"/>
<pin name="SWITCH_COLLECTOR_2" direction="pas"/>
<pin name="SWITCH_COLLECTOR_3" direction="pas"/>
<pin name="SWITCH_COLLECTOR_4" direction="pas"/>
<pin name="SWITCH_EMITTER" direction="pas"/>
<pin name="SWITCH_EMITTER_2" direction="pas"/>
<pin name="SWITCH_EMITTER_3" direction="pas"/>
<pin name="SWITCH_EMITTER_4" direction="pas"/>
<pin name="VOLTAGE_FEEDBACK_2" direction="in"/>
<pin name="VOLTAGE_FEEDBACK1" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LVI_OUTPUT" direction="out"/>
</symbol>
<symbol name="NCP361SNT1G">
<pin name="IN" direction="pwr"/>
<pin name="~EN" direction="in"/>
<pin name="~FLAG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="NCP4587DMX12TCG">
<pin name="VIN" direction="pwr"/>
<pin name="AE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4587DMX18TCG">
<pin name="VIN" direction="pwr"/>
<pin name="AE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4587DMX28TCG">
<pin name="VIN" direction="pwr"/>
<pin name="AE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4587DMX30TCG">
<pin name="VIN" direction="pwr"/>
<pin name="AE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4587DMX33TCG">
<pin name="VIN" direction="pwr"/>
<pin name="AE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4588DSQ10T1G">
<pin name="VIN" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4588DSQ15T1G">
<pin name="VIN" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4588DSQ25T1G">
<pin name="VIN" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4589DMX12TCG">
<pin name="VIN" direction="pwr"/>
<pin name="AE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4589DMX18TCG">
<pin name="VIN" direction="pwr"/>
<pin name="AE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4589DMX28TCG">
<pin name="VIN" direction="pwr"/>
<pin name="AE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4589DMX30TCG">
<pin name="VIN" direction="pwr"/>
<pin name="AE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4589DMX33TCG">
<pin name="VIN" direction="pwr"/>
<pin name="AE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4589DSQ12T1G">
<pin name="VIN" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="AE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4589DSQ18T1G">
<pin name="VIN" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="AE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4589DSQ25T1G">
<pin name="VIN" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="AE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4589DSQ30T1G">
<pin name="VIN" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="AE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP4589DSQ33T1G">
<pin name="VIN" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="AE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP565MNADJT2G">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="EPAD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="ADJ" direction="pas"/>
</symbol>
<symbol name="NCP5810DMUTXG">
<pin name="VS" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="SWP" direction="in"/>
<pin name="SWN" direction="in"/>
<pin name="FBN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="LXP" direction="pas"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUTP" direction="out"/>
</symbol>
<symbol name="NCP699SN18T1G">
<pin name="VIN" direction="pwr"/>
<pin name="ENABLE" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP699SN33T1G">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCP803SN263T1G">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="NCS2001SN1T1G">
<pin name="VCC" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NCV1124DG">
<pin name="VCC" direction="pwr"/>
<pin name="INADJ" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="DIAG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
</symbol>
<symbol name="NCV85082BPD33R2G">
<pin name="VIN" direction="pwr"/>
<pin name="DELAY" direction="pwr"/>
<pin name="WDI" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SENSE" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="~RESET" direction="pas"/>
<pin name="WAKEUP" direction="pas"/>
</symbol>
<symbol name="NCV8537MN180R2G">
<pin name="IN_2" direction="pwr"/>
<pin name="IN" direction="pwr"/>
<pin name="NR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="PWRG" direction="out"/>
<pin name="SENSE" direction="out"/>
</symbol>
<symbol name="NCV8537MN250R2G">
<pin name="IN_2" direction="pwr"/>
<pin name="IN" direction="pwr"/>
<pin name="NR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="PWRG" direction="out"/>
<pin name="SENSE" direction="out"/>
</symbol>
<symbol name="NCV8537MN330R2G">
<pin name="IN_2" direction="pwr"/>
<pin name="IN" direction="pwr"/>
<pin name="NR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="PWRG" direction="out"/>
<pin name="SENSE" direction="out"/>
</symbol>
<symbol name="NCV8537MN500R2G">
<pin name="IN_2" direction="pwr"/>
<pin name="IN" direction="pwr"/>
<pin name="NR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="PWRG" direction="out"/>
<pin name="SENSE" direction="out"/>
</symbol>
<symbol name="NCV8537MNADJR2G">
<pin name="IN_2" direction="pwr"/>
<pin name="IN" direction="pwr"/>
<pin name="NR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="PWRG" direction="out"/>
<pin name="SENSE" direction="out"/>
</symbol>
<symbol name="NE5532AD8G">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="NE5532ANG">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="NE5532DG">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="NE5532NG">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="NE5534ANG">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="OFS" direction="pas"/>
<pin name="OFS/COMP" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="NE5534NG">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="OFS" direction="pas"/>
<pin name="OFS/COMP" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="NE592D14G">
<pin name="V+" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="G1B_GAIN_SELECT" direction="in"/>
<pin name="G2B_GAIN_SELECT" direction="in"/>
<pin name="G1A_GAIN_SELECT" direction="in"/>
<pin name="G2A_GAIN_SELECT" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="NE592D8G">
<pin name="V+" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="G1A_GAIN_SELECT" direction="in"/>
<pin name="G1B_GAIN_SELECT" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="NL17SZ07DFT2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="NL17SZ125DFT2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="~OE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y" direction="out"/>
</symbol>
<symbol name="NL17SZ14DFT2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y" direction="out"/>
</symbol>
<symbol name="NL17SZ17DFT2G">
<pin name="VCC" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="NL17SZ74USG">
<pin name="VCC" direction="pwr"/>
<pin name="CP" direction="in"/>
<pin name="~CLR" direction="in"/>
<pin name="~PR" direction="in"/>
<pin name="D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="~Q" direction="out"/>
</symbol>
<symbol name="NL17SZU04DFT2G">
<pin name="VCC" direction="pwr"/>
<pin name="~A" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="NL27WZ04DTT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A1" direction="in"/>
<pin name="IN_A2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y1" direction="out"/>
<pin name="OUT_~Y2" direction="out"/>
</symbol>
<symbol name="NL27WZ08USG">
<pin name="VCC" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
</symbol>
<symbol name="NL27WZ126USG">
<pin name="VCC" direction="pwr"/>
<pin name="OE1" direction="in"/>
<pin name="OE2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
</symbol>
<symbol name="NL27WZ14DTT1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A1" direction="in"/>
<pin name="IN_A2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y1" direction="out"/>
<pin name="OUT_~Y2" direction="out"/>
</symbol>
<symbol name="NL27WZ16DFT2G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A1" direction="in"/>
<pin name="IN_A2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_Y1" direction="out"/>
<pin name="OUT_Y2" direction="out"/>
</symbol>
<symbol name="NL37WZ14USG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A1" direction="in"/>
<pin name="IN_A2" direction="in"/>
<pin name="IN_A3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Y1" direction="out"/>
<pin name="OUT_~Y2" direction="out"/>
<pin name="OUT_~Y3" direction="out"/>
</symbol>
<symbol name="NL37WZ17USG">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A1" direction="in"/>
<pin name="IN_A2" direction="in"/>
<pin name="IN_A3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT__Y1" direction="out"/>
<pin name="OUT__Y2" direction="out"/>
<pin name="OUT__Y3" direction="out"/>
</symbol>
<symbol name="NLAS4599DTT1G">
<pin name="V+" direction="in"/>
<pin name="SELECT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="NO" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="NLAST4599DTT1G">
<pin name="V+" direction="pwr"/>
<pin name="SELECT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="COM"/>
<pin name="NC"/>
<pin name="NO"/>
</symbol>
<symbol name="NUD3105DMT1G">
<pin name="GATE1" direction="in"/>
<pin name="GATE2" direction="in"/>
<pin name="SOURCE1" direction="in"/>
<pin name="SOURCE2" direction="in"/>
<pin name="DRAIN1" direction="out"/>
<pin name="DRAIN2" direction="out"/>
</symbol>
<symbol name="NUD3105LT1G">
<pin name="VIN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="NUD3112DMT1G">
<pin name="GATE1" direction="in"/>
<pin name="GATE2" direction="in"/>
<pin name="SOURCE1" direction="in"/>
<pin name="SOURCE2" direction="in"/>
<pin name="DRAIN1" direction="out"/>
<pin name="DRAIN2" direction="out"/>
</symbol>
<symbol name="NUD3112LT1G">
<pin name="GATE" direction="in"/>
<pin name="SOURCE" direction="pas"/>
<pin name="DRAIN" direction="out"/>
</symbol>
<symbol name="NUD3124LT1G">
<pin name="GATE" direction="in"/>
<pin name="SOURCE" direction="pas"/>
<pin name="DRAIN" direction="pas"/>
</symbol>
<symbol name="NUD3160DMT1G">
<pin name="GATE1" direction="in"/>
<pin name="GATE2" direction="in"/>
<pin name="SOURCE1" direction="in"/>
<pin name="SOURCE2" direction="in"/>
<pin name="DRAIN1" direction="out"/>
<pin name="DRAIN2" direction="out"/>
</symbol>
<symbol name="NUD3160LT1G">
<pin name="GATE" direction="in"/>
<pin name="SOURCE" direction="pas"/>
<pin name="DRAIN" direction="pas"/>
</symbol>
<symbol name="NUD4001DR2G">
<pin name="VIN" direction="pwr"/>
<pin name="BOOST" direction="in"/>
<pin name="REXT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="IOUT_2" direction="out"/>
<pin name="IOUT_3" direction="out"/>
<pin name="IOUT_4" direction="out"/>
<pin name="IOUT" direction="out"/>
</symbol>
<symbol name="NUD4011DR2G">
<pin name="VIN" direction="pwr"/>
<pin name="BOOST" direction="in"/>
<pin name="REXT" direction="in"/>
<pin name="PWM" direction="in"/>
<pin name="IOUT_2" direction="out"/>
<pin name="IOUT_3" direction="out"/>
<pin name="IOUT_4" direction="out"/>
<pin name="IOUT" direction="out"/>
</symbol>
<symbol name="P2782AF-08SR">
<pin name="VDD" direction="pwr"/>
<pin name="XIN/CLKIN" direction="in"/>
<pin name="FS1" direction="in"/>
<pin name="LF" direction="in"/>
<pin name="FS0" direction="in"/>
<pin name="VSS" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="MODOUT" direction="out"/>
</symbol>
<symbol name="P2784AF-08SR">
<pin name="VDD" direction="pwr"/>
<pin name="XIN/CLKIN" direction="in"/>
<pin name="FS1" direction="in"/>
<pin name="LF" direction="in"/>
<pin name="FS0" direction="in"/>
<pin name="VSS" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="MODOUT" direction="out"/>
</symbol>
<symbol name="PCS3P25811AG08SR">
<pin name="VDD" direction="pwr"/>
<pin name="XIN_/_CLKIN" direction="in"/>
<pin name="FSEL" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="MODOUT" direction="out"/>
<pin name="XOUT" direction="out"/>
</symbol>
<symbol name="SA571DG">
<pin name="VCC" direction="pwr"/>
<pin name="RECT_CAP_1" direction="in"/>
<pin name="RECT_CAP_2" direction="in"/>
<pin name="RECT_IN_1" direction="in"/>
<pin name="RECT_IN_2" direction="in"/>
<pin name="THD_TRIM_1" direction="in"/>
<pin name="THD_TRIM_2" direction="in"/>
<pin name="RES._R3_1" direction="in"/>
<pin name="RES._R3_2" direction="in"/>
<pin name="G_CELL_IN_1" direction="in"/>
<pin name="G_CELL_IN_2" direction="in"/>
<pin name="INV._IN_1" direction="in"/>
<pin name="INV._IN_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
</symbol>
<symbol name="SA571NG">
<pin name="VCC" direction="pwr"/>
<pin name="RES._R3_1" direction="pas"/>
<pin name="RES._R3_2" direction="pas"/>
<pin name="RECT_CAP_1" direction="pas"/>
<pin name="RECT_CAP_2" direction="pas"/>
<pin name="THD_TRIM_1" direction="pas"/>
<pin name="THD_TRIM_2" direction="pas"/>
<pin name="RECT_IN_1" direction="in"/>
<pin name="RECT_IN_2" direction="in"/>
<pin name="INV._IN_1" direction="in"/>
<pin name="INV._IN_2" direction="in"/>
<pin name="G_CELL_IN_1" direction="in"/>
<pin name="G_CELL_IN_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT_1" direction="out"/>
<pin name="OUTPUT_2" direction="out"/>
</symbol>
<symbol name="SA572NG">
<pin name="VCC" direction="pwr"/>
<pin name="TRACK_TRIM_A" direction="pas"/>
<pin name="TRACK_TRIM_B" direction="pas"/>
<pin name="RECOV._CAP_A" direction="pas"/>
<pin name="RECOV._CAP_B" direction="pas"/>
<pin name="THD_TRIM_A" direction="pas"/>
<pin name="THD_TRIM_B" direction="pas"/>
<pin name="ATTACK_CAP_A" direction="pas"/>
<pin name="ATTACK_CAP_B" direction="pas"/>
<pin name="RECT._IN_A" direction="in"/>
<pin name="RECT._IN_B" direction="in"/>
<pin name="G_IN_A" direction="in"/>
<pin name="G_INB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="G_OUT_A" direction="out"/>
<pin name="G_OUT_B" direction="out"/>
</symbol>
<symbol name="SA575DTBG">
<pin name="VCC" direction="pwr"/>
<pin name="+VIN1" direction="in"/>
<pin name="-VIN1" direction="in"/>
<pin name="-VIN2" direction="in"/>
<pin name="+VIN2" direction="in"/>
<pin name="RECT._IN1" direction="in"/>
<pin name="RECT.IN2" direction="in"/>
<pin name="COMP._IN1" direction="in"/>
<pin name="COMP.IN2" direction="in"/>
<pin name="GAIN_CELL_IN1" direction="in"/>
<pin name="GAIN_CELL_IN2" direction="in"/>
<pin name="SUM_NODE_2" direction="in"/>
<pin name="CRECT1" direction="in"/>
<pin name="CRECT2" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
<pin name="SUM_OUT_1" direction="out"/>
<pin name="SUM_OUT2" direction="out"/>
</symbol>
<symbol name="TCA0372DP1G">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_A_2" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_B_2" direction="in"/>
<pin name="VEE/GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="TCA0372DWG">
<pin name="VCC" direction="pwr"/>
<pin name="INPUTS_A" direction="in"/>
<pin name="INPUTS_A_2" direction="in"/>
<pin name="INPUTS_B" direction="in"/>
<pin name="INPUTS_B_2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE/GND_2" direction="pas"/>
<pin name="VEE/GND_3" direction="pas"/>
<pin name="VEE/GND_4" direction="pas"/>
<pin name="VEE/GND" direction="pas"/>
<pin name="OUTPUT_B" direction="out"/>
<pin name="OUTPUT_A" direction="out"/>
</symbol>
<symbol name="TCA0372DWR2G">
<pin name="VCC"/>
<pin name="INPUTS_A" direction="in"/>
<pin name="INPUTS_A_2" direction="in"/>
<pin name="INPUTS_B" direction="in"/>
<pin name="INPUTS_B_2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE/GND_2" direction="pwr"/>
<pin name="VEE/GND_3" direction="pwr"/>
<pin name="VEE/GND_4" direction="pwr"/>
<pin name="VEE/GND" direction="pwr"/>
<pin name="OUTPUT_A" direction="out"/>
<pin name="OUTPUT_B" direction="out"/>
</symbol>
<symbol name="TDA1085CG">
<pin name="+VCC" direction="pwr"/>
<pin name="RAMP_CURRENT_GEN._CONTROL" direction="in"/>
<pin name="SAWTOOTH_SET_CURRENT" direction="in"/>
<pin name="MOTOR_CURRENT_LIMIT" direction="in"/>
<pin name="CLOSED_LOOP_STABILITY" direction="in"/>
<pin name="RAMP_GEN._TIMING" direction="in"/>
<pin name="ACTUAL_SPEED" direction="in"/>
<pin name="SET_SPEED" direction="in"/>
<pin name="DIGITAL_SPEED_SENSE" direction="in"/>
<pin name="CURRENT_SYNCHRONIZATION" direction="in"/>
<pin name="VOLTAGE_SYNCHRONIZATION" direction="in"/>
<pin name="F/VC_PUMP_CAPACITOR" direction="pas"/>
<pin name="SAWTOOTH_CAPACITOR" direction="in"/>
<pin name="SHUNT_REGULATOR_BALLAST_RESISTOR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="TRIGGER_PULSE_OUTPUT" direction="out"/>
</symbol>
<symbol name="TL431ACDG">
<pin name="REF" direction="in"/>
<pin name="ANODE_2" direction="in"/>
<pin name="ANODE_3" direction="in"/>
<pin name="ANODE_4" direction="in"/>
<pin name="ANODE" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="CATHODE" direction="out"/>
</symbol>
<symbol name="TL431AIDG">
<pin name="REF" direction="in"/>
<pin name="ANODE_2" direction="in"/>
<pin name="ANODE_3" direction="in"/>
<pin name="ANODE_4" direction="in"/>
<pin name="ANODE" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="CATHODE" direction="out"/>
</symbol>
<symbol name="TL431AIDR2G">
<pin name="REF" direction="in"/>
<pin name="ANODE_2" direction="in"/>
<pin name="ANODE_3" direction="in"/>
<pin name="ANODE_4" direction="in"/>
<pin name="ANODE" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="CATHODE" direction="out"/>
</symbol>
<symbol name="TL431BIDG">
<pin name="REF" direction="in"/>
<pin name="ANODE_2" direction="in"/>
<pin name="ANODE_3" direction="in"/>
<pin name="ANODE_4" direction="in"/>
<pin name="ANODE" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="CATHODE" direction="out"/>
</symbol>
<symbol name="TL431CDG">
<pin name="REF" direction="in"/>
<pin name="ANODE_2" direction="in"/>
<pin name="ANODE_3" direction="in"/>
<pin name="ANODE_4" direction="in"/>
<pin name="ANODE" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="CATHODE" direction="out"/>
</symbol>
<symbol name="TL431CDR2G">
<pin name="REF" direction="in"/>
<pin name="ANODE_2" direction="in"/>
<pin name="ANODE_3" direction="in"/>
<pin name="ANODE_4" direction="in"/>
<pin name="ANODE" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="CATHODE" direction="out"/>
</symbol>
<symbol name="UAA2016PG">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="HYS._ADJ." direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="TEMP._REDUC." direction="in"/>
<pin name="SENSOR" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="UC2842BD1R2G">
<pin name="VCC" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="VOLTAGE_FB" direction="in"/>
<pin name="CURRENT_SENSE" direction="in"/>
<pin name="RT/CT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="UC2842BDG">
<pin name="VCC" direction="pwr"/>
<pin name="VC" direction="in"/>
<pin name="VOLTAGE_FB" direction="in"/>
<pin name="CURRENT_SENSE" direction="in"/>
<pin name="RT/CT" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="POWER_GND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="UC2843BD1G">
<pin name="VCC" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="VOLTAGE_FB" direction="in"/>
<pin name="CURRENT_SENSE" direction="in"/>
<pin name="RT/CT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="UC2843BNG">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="pas"/>
<pin name="COMPENSATION"/>
<pin name="VOLTAGE_FEEDBACK" direction="in"/>
<pin name="CURRENT_SENSE" direction="in"/>
<pin name="RT/CT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="UC3842BNG">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="pas"/>
<pin name="COMPENSATION"/>
<pin name="VOLTAGE_FEEDBACK" direction="in"/>
<pin name="CURRENT_SENSE" direction="in"/>
<pin name="RT/CT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="UC3843BD1G">
<pin name="VCC" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="VOLTAGE_FB" direction="in"/>
<pin name="CURRENT_SENSE" direction="in"/>
<pin name="RT/CT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="UC3843BVD1G">
<pin name="VCC" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="VOLTAGE_FB" direction="in"/>
<pin name="CURRENT_SENSE" direction="in"/>
<pin name="RT/CT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="UC3844BNG">
<pin name="VCC" direction="pwr"/>
<pin name="COMP"/>
<pin name="VOLTAGE_FEEDBACK" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="RT/CT" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="UC3845BDG">
<pin name="VCC" direction="pwr"/>
<pin name="VC" direction="in"/>
<pin name="VOLTAGE_FB" direction="in"/>
<pin name="CURRENT_SENSE" direction="in"/>
<pin name="RT/CT" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="POWER_GND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="UC3845BVD1G">
<pin name="VCC" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="VOLTAGE_FB" direction="in"/>
<pin name="CURRENT_SENSE" direction="in"/>
<pin name="RT/CT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VREF" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="74HC595DG" prefix="U">
<description>8-Bit Serial-Input/Serial or Parallel-Output Shift Register with Latched 3-State Outputs</description>
<gates>
<gate name="A" symbol="74HC595DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="LATCH_CLOCK" pad="12"/>
<connect gate="A" pin="OUT_EN" pad="13"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="RESET" pad="10"/>
<connect gate="A" pin="SHIFT_CLOCK" pad="11"/>
<connect gate="A" pin="SQH" pad="9"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="74HC595DG"/>
<attribute name="OC_FARNELL" value="1640047"/>
<attribute name="OC_NEWARK" value="75M5727"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A5191HRTLG-XTD" prefix="U">
<description>HART Modem</description>
<gates>
<gate name="A" symbol="A5191HRTLG-XTD"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="AREF" pad="8"/>
<connect gate="A" pin="CBIAS" pad="10"/>
<connect gate="A" pin="CD" pad="26"/>
<connect gate="A" pin="CDREF" pad="9"/>
<connect gate="A" pin="RST" pad="22"/>
<connect gate="A" pin="RXA" pad="14"/>
<connect gate="A" pin="RXAF" pad="15"/>
<connect gate="A" pin="RXAFI" pad="16"/>
<connect gate="A" pin="RXD" pad="25"/>
<connect gate="A" pin="TEST1" pad="28"/>
<connect gate="A" pin="TEST10" pad="11"/>
<connect gate="A" pin="TEST11" pad="24"/>
<connect gate="A" pin="TEST12" pad="27"/>
<connect gate="A" pin="TEST2" pad="29"/>
<connect gate="A" pin="TEST3" pad="30"/>
<connect gate="A" pin="TEST4" pad="32"/>
<connect gate="A" pin="TEST5" pad="1"/>
<connect gate="A" pin="TEST7" pad="3"/>
<connect gate="A" pin="TEST8" pad="4"/>
<connect gate="A" pin="TEST9" pad="5"/>
<connect gate="A" pin="TXA" pad="7"/>
<connect gate="A" pin="TXD" pad="23"/>
<connect gate="A" pin="VDD" pad="31"/>
<connect gate="A" pin="VDDA" pad="13"/>
<connect gate="A" pin="VDD_2" pad="21"/>
<connect gate="A" pin="VSS" pad="20"/>
<connect gate="A" pin="VSSA" pad="12"/>
<connect gate="A" pin="VSSA_2" pad="19"/>
<connect gate="A" pin="VSS_2" pad="6"/>
<connect gate="A" pin="XIN" pad="18"/>
<connect gate="A" pin="XOUT" pad="17"/>
<connect gate="A" pin="~RESET" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="A5191HRTLG-XTD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="03P1166"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADM1024ARUZ" prefix="U">
<description>IC MONITOR SYS TEMP/VOLT</description>
<gates>
<gate name="A" symbol="ADM1024ARUZ"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-24N">
<connects>
<connect gate="A" pin="+12VIN" pad="15"/>
<connect gate="A" pin="+2.5VIN/D2+" pad="18"/>
<connect gate="A" pin="+5.0VIN" pad="16"/>
<connect gate="A" pin="+VCCP1" pad="19"/>
<connect gate="A" pin="CI" pad="7"/>
<connect gate="A" pin="D1+" pad="14"/>
<connect gate="A" pin="D1-" pad="13"/>
<connect gate="A" pin="FAN1/AIN1" pad="5"/>
<connect gate="A" pin="FAN2/AIN2" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="NTEST_IN/AOUT" pad="11"/>
<connect gate="A" pin="NTEST_OUT/ADD" pad="1"/>
<connect gate="A" pin="SCL" pad="4"/>
<connect gate="A" pin="SDA" pad="3"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VCCP2/D2-" pad="17"/>
<connect gate="A" pin="VID0/IRQ0" pad="24"/>
<connect gate="A" pin="VID1/IRQ1" pad="23"/>
<connect gate="A" pin="VID2/IRQ2" pad="22"/>
<connect gate="A" pin="VID3/IRQ3" pad="21"/>
<connect gate="A" pin="VID4/IRQ4" pad="20"/>
<connect gate="A" pin="~INT" pad="10"/>
<connect gate="A" pin="~RESET" pad="12"/>
<connect gate="A" pin="~THERM" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADM1024ARUZ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="19M8680"/>
<attribute name="PACKAGE" value="TSSOP-24"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADM1032ARMZ" prefix="U">
<description>+- 1C Remote and Local System Temperature Monitor</description>
<gates>
<gate name="A" symbol="ADM1032ARMZ"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D+" pad="2"/>
<connect gate="A" pin="D-" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SCLK" pad="8"/>
<connect gate="A" pin="SDATA" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="~ALERT" pad="6"/>
<connect gate="A" pin="~THERM" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADM1032ARMZ"/>
<attribute name="OC_FARNELL" value="1424368"/>
<attribute name="OC_NEWARK" value="82H2751"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADM1032ARZ" prefix="U">
<description>+- 1C Remote and Local System Temperature Monitor</description>
<gates>
<gate name="A" symbol="ADM1032ARZ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D+" pad="2"/>
<connect gate="A" pin="D-" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SCLK" pad="8"/>
<connect gate="A" pin="SDATA" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="~ALERT" pad="6"/>
<connect gate="A" pin="~THERM" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADM1032ARMZ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="59K1789"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADT7461ARMZ" prefix="U">
<description>Temperature Monitor</description>
<gates>
<gate name="A" symbol="ADT7461ARMZ"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D+" pad="2"/>
<connect gate="A" pin="D-" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SCLK" pad="8"/>
<connect gate="A" pin="SDATA" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="~ALERT/~THERM2" pad="6"/>
<connect gate="A" pin="~THERM" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADT7461ARMZ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="19M8743"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADT7462ACPZ-5RL7" prefix="U">
<description>Flexible Temperature Voltage Monitor, and  System Fan Controller</description>
<gates>
<gate name="A" symbol="ADT7462ACPZ-5RL7"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X100-32N">
<connects>
<connect gate="A" pin="ADD" pad="11"/>
<connect gate="A" pin="D1+/+2.5V/+1.8V_15" pad="15"/>
<connect gate="A" pin="D1-/SCSI_TERM1" pad="16"/>
<connect gate="A" pin="D2+" pad="17"/>
<connect gate="A" pin="D2-" pad="18"/>
<connect gate="A" pin="D3+/+1.25V/+0.9V" pad="19"/>
<connect gate="A" pin="D3-/SCSI_TERM2" pad="20"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="PWM3" pad="30"/>
<connect gate="A" pin="PWM4/+3.3V" pad="13"/>
<connect gate="A" pin="SCL" pad="9"/>
<connect gate="A" pin="SDA" pad="10"/>
<connect gate="A" pin="TACH5/+12V1" pad="7"/>
<connect gate="A" pin="TACH6/+12V2" pad="8"/>
<connect gate="A" pin="TACH7/+5V" pad="21"/>
<connect gate="A" pin="TACH8/+12V3" pad="22"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VCCP1/+1.5V/+1.8V/+2.5V" pad="23"/>
<connect gate="A" pin="VCCP2/+1.5V/+1.8V/+2.5V" pad="24"/>
<connect gate="A" pin="VID0/GPIO1/TACH1" pad="1"/>
<connect gate="A" pin="VID1/GPIO2/TACH2" pad="2"/>
<connect gate="A" pin="VID2/GPIO3/TACH3" pad="3"/>
<connect gate="A" pin="VID3/GPIO4/TACH4" pad="4"/>
<connect gate="A" pin="VID4/GPIO5/PWM1" pad="31"/>
<connect gate="A" pin="VID5/GPIO6/PWM2" pad="32"/>
<connect gate="A" pin="VR_HOT1/+1.2V1/+3.3V" pad="25"/>
<connect gate="A" pin="VR_HOT2/+1.2V2/V_BATT" pad="26"/>
<connect gate="A" pin="~ALERT" pad="12"/>
<connect gate="A" pin="~FAN2MAX/CI" pad="27"/>
<connect gate="A" pin="~RESET" pad="14"/>
<connect gate="A" pin="~THERM1/+1.5V1/GPIO7/VID6" pad="28"/>
<connect gate="A" pin="~THERM2/+1.5V2/GPIO8" pad="29"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADT7462ACPZ-5RL7"/>
<attribute name="OC_FARNELL" value="1736459"/>
<attribute name="OC_NEWARK" value="05R5110"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADT7463ARQZ" prefix="U">
<description>Remote Thermal Controller</description>
<gates>
<gate name="A" symbol="ADT7463ARQZ"/>
</gates>
<devices>
<device name="" package="SOP63P600X175-24N">
<connects>
<connect gate="A" pin="+12VIN/VID5" pad="21"/>
<connect gate="A" pin="+2.5VIN/~SMBALERT" pad="22"/>
<connect gate="A" pin="+5VIN/~THERM" pad="20"/>
<connect gate="A" pin="D1+" pad="18"/>
<connect gate="A" pin="D1-" pad="17"/>
<connect gate="A" pin="D2+" pad="16"/>
<connect gate="A" pin="D2-" pad="15"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="PWM1/XTO" pad="24"/>
<connect gate="A" pin="PWM2/~SMBALERT" pad="10"/>
<connect gate="A" pin="PWM3/~ADDRESS_ENABLE" pad="13"/>
<connect gate="A" pin="SCL" pad="2"/>
<connect gate="A" pin="SDA" pad="1"/>
<connect gate="A" pin="TACH1" pad="11"/>
<connect gate="A" pin="TACH2" pad="12"/>
<connect gate="A" pin="TACH3" pad="9"/>
<connect gate="A" pin="TACH4/ADDRESS_SELECT/~THERM" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VCCP" pad="23"/>
<connect gate="A" pin="VID0" pad="5"/>
<connect gate="A" pin="VID1" pad="6"/>
<connect gate="A" pin="VID2" pad="7"/>
<connect gate="A" pin="VID3" pad="8"/>
<connect gate="A" pin="VID4" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADT7463ARQZ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="87H9685"/>
<attribute name="PACKAGE" value="QSOP-24"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADT7467ARQZ" prefix="U">
<description>dBCool Remote Thermal Monitor and Fan Controller</description>
<gates>
<gate name="A" symbol="ADT7467ARQZ"/>
</gates>
<devices>
<device name="" package="SOP63P600X175-16N">
<connects>
<connect gate="A" pin="D1+" pad="13"/>
<connect gate="A" pin="D1-" pad="12"/>
<connect gate="A" pin="D2+" pad="11"/>
<connect gate="A" pin="D2-" pad="10"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="PWM1/XTO" pad="15"/>
<connect gate="A" pin="PWM2/~SMBALERT" pad="5"/>
<connect gate="A" pin="PWM3" pad="8"/>
<connect gate="A" pin="SCL" pad="1"/>
<connect gate="A" pin="SDA" pad="16"/>
<connect gate="A" pin="TACH1" pad="6"/>
<connect gate="A" pin="TACH2" pad="7"/>
<connect gate="A" pin="TACH3" pad="4"/>
<connect gate="A" pin="TACH4/GPIO/~THERM/~SMBALERT" pad="9"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VCCP" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADT7467ARQZ"/>
<attribute name="OC_FARNELL" value="1536247"/>
<attribute name="OC_NEWARK" value="19M8744"/>
<attribute name="PACKAGE" value="QSOP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMIS30624C6244RG" prefix="U">
<description>I2C Micro-stepping Motor Driver</description>
<gates>
<gate name="A" symbol="AMIS30624C6244RG"/>
</gates>
<devices>
<device name="" package="SOIC127P1021X265-20N">
<connects>
<connect gate="A" pin="CPN" pad="9"/>
<connect gate="A" pin="CPP" pad="10"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="14"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="7"/>
<connect gate="A" pin="HW" pad="8"/>
<connect gate="A" pin="MOTXN" pad="16"/>
<connect gate="A" pin="MOTXP" pad="18"/>
<connect gate="A" pin="MOTYN" pad="13"/>
<connect gate="A" pin="MOTYP" pad="15"/>
<connect gate="A" pin="SCK" pad="2"/>
<connect gate="A" pin="SDA" pad="1"/>
<connect gate="A" pin="SWI" pad="20"/>
<connect gate="A" pin="TST1" pad="5"/>
<connect gate="A" pin="TST2" pad="6"/>
<connect gate="A" pin="VBB" pad="19"/>
<connect gate="A" pin="VBB_2" pad="12"/>
<connect gate="A" pin="VCP" pad="11"/>
<connect gate="A" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AMIS30624C6244RG"/>
<attribute name="OC_FARNELL" value="1641410"/>
<attribute name="OC_NEWARK" value="03P0834"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMIS30660CANH2G" prefix="U">
<description>High Speed CAN Transceiver</description>
<gates>
<gate name="A" symbol="AMIS30660CANH2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CANH" pad="7"/>
<connect gate="A" pin="CANL" pad="6"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="RXD" pad="4"/>
<connect gate="A" pin="S" pad="8"/>
<connect gate="A" pin="TXD" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AMIS30660CANH2G"/>
<attribute name="OC_FARNELL" value="1641429"/>
<attribute name="OC_NEWARK" value="03P1154"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMIS30663CANG2G" prefix="U">
<description>High Speed CAN Transceiver</description>
<gates>
<gate name="A" symbol="AMIS30663CANG2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CANH" pad="7"/>
<connect gate="A" pin="CANL" pad="6"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="RXD" pad="4"/>
<connect gate="A" pin="TXD" pad="1"/>
<connect gate="A" pin="V33" pad="8"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AMIS30663CANG2G"/>
<attribute name="OC_FARNELL" value="1641431"/>
<attribute name="OC_NEWARK" value="03P1156"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMIS42770ICAW1RG" prefix="U">
<description>Dual High Speed CAN Transceiver</description>
<gates>
<gate name="A" symbol="AMIS42770ICAW1RG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="CANH1" pad="13"/>
<connect gate="A" pin="CANH2" pad="19"/>
<connect gate="A" pin="CANL1" pad="14"/>
<connect gate="A" pin="CANL2" pad="18"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="6"/>
<connect gate="A" pin="GND_4" pad="15"/>
<connect gate="A" pin="GND_5" pad="16"/>
<connect gate="A" pin="NC" pad="20"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="RINT" pad="9"/>
<connect gate="A" pin="RX0" pad="7"/>
<connect gate="A" pin="TEXT" pad="3"/>
<connect gate="A" pin="TX0" pad="4"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VREF1" pad="8"/>
<connect gate="A" pin="~EN1" pad="10"/>
<connect gate="A" pin="~EN2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AMIS42770ICAW1RG"/>
<attribute name="OC_FARNELL" value="1641442"/>
<attribute name="OC_NEWARK" value="03P1165"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAT24C04LI-G" prefix="U">
<description>CMOS Serial EEPROM</description>
<gates>
<gate name="A" symbol="CAT24C04LI-G"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="SCL" pad="6"/>
<connect gate="A" pin="SDA" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VSS" pad="4"/>
<connect gate="A" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CAT24C04LI-G"/>
<attribute name="OC_FARNELL" value="1718374"/>
<attribute name="OC_NEWARK" value="73P4460"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAT24C16LI-G" prefix="U">
<description>CMOS Serial EEPROM</description>
<gates>
<gate name="A" symbol="CAT24C16LI-G"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="SCL" pad="6"/>
<connect gate="A" pin="SDA" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VSS" pad="4"/>
<connect gate="A" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CAT24C16LI-G"/>
<attribute name="OC_FARNELL" value="1718037"/>
<attribute name="OC_NEWARK" value="06R0533"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAT24C44LI" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="CAT24C44LI"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="DI" pad="3"/>
<connect gate="A" pin="DO" pad="4"/>
<connect gate="A" pin="SK" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VSS" pad="5"/>
<connect gate="A" pin="~RECALL" pad="6"/>
<connect gate="A" pin="~STORE" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CAT24C44LI"/>
<attribute name="OC_FARNELL" value="1718282"/>
<attribute name="OC_NEWARK" value="06R0564"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAT25020LI-G" prefix="U">
<description>Serial CMOS EEPROM</description>
<gates>
<gate name="A" symbol="CAT25020LI-G"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="SCK" pad="6"/>
<connect gate="A" pin="SI" pad="5"/>
<connect gate="A" pin="SO" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VSS" pad="4"/>
<connect gate="A" pin="~CS" pad="1"/>
<connect gate="A" pin="~HOLD" pad="7"/>
<connect gate="A" pin="~WP" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CAT25020LI-G"/>
<attribute name="OC_FARNELL" value="1718043"/>
<attribute name="OC_NEWARK" value="06R0582"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAT25256LI-G" prefix="U">
<description>SPI Serial CMOS EEPROM</description>
<gates>
<gate name="A" symbol="CAT25256LI-G"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="CS" pad="2"/>
<connect gate="A" pin="SCK" pad="6"/>
<connect gate="A" pin="SI" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VSS" pad="4"/>
<connect gate="A" pin="~HOLD" pad="7"/>
<connect gate="A" pin="~SO" pad="1"/>
<connect gate="A" pin="~WP" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CAT25256LI-G"/>
<attribute name="OC_FARNELL" value="1718050"/>
<attribute name="OC_NEWARK" value="06R0614"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAT93C56LI-G" prefix="U">
<description>CMOS EEPROM</description>
<gates>
<gate name="A" symbol="CAT93C56LI-G"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="DI" pad="3"/>
<connect gate="A" pin="DO" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="ORG" pad="7"/>
<connect gate="A" pin="SK" pad="2"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CAT93C56LI-G"/>
<attribute name="OC_FARNELL" value="1718065"/>
<attribute name="OC_NEWARK" value="06R1453"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAT9532WI" prefix="U">
<description>16-bit Programmable LED Dimmer with I2C Interface</description>
<gates>
<gate name="A" symbol="CAT9532WI"/>
</gates>
<devices>
<device name="" package="SOIC127P1031X265-24N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="LED0" pad="4"/>
<connect gate="A" pin="LED1" pad="5"/>
<connect gate="A" pin="LED10" pad="15"/>
<connect gate="A" pin="LED11" pad="16"/>
<connect gate="A" pin="LED12" pad="17"/>
<connect gate="A" pin="LED13" pad="18"/>
<connect gate="A" pin="LED14" pad="19"/>
<connect gate="A" pin="LED15" pad="20"/>
<connect gate="A" pin="LED2" pad="6"/>
<connect gate="A" pin="LED3" pad="7"/>
<connect gate="A" pin="LED4" pad="8"/>
<connect gate="A" pin="LED5" pad="9"/>
<connect gate="A" pin="LED6" pad="10"/>
<connect gate="A" pin="LED7" pad="11"/>
<connect gate="A" pin="LED8" pad="13"/>
<connect gate="A" pin="LED9" pad="14"/>
<connect gate="A" pin="SCL" pad="22"/>
<connect gate="A" pin="SDA" pad="23"/>
<connect gate="A" pin="VCC" pad="24"/>
<connect gate="A" pin="VSS" pad="12"/>
<connect gate="A" pin="~RESET" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CAT9532WI."/>
<attribute name="OC_FARNELL" value="1656134"/>
<attribute name="OC_NEWARK" value="11P0275"/>
<attribute name="PACKAGE" value="SOIC-24"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CS5171ED8G" prefix="U">
<description>1.5 A 280 kHz/560 kHz Boost Regulators</description>
<gates>
<gate name="A" symbol="CS5171ED8G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="PGND" pad="7"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="TEST" pad="3"/>
<connect gate="A" pin="VC" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CS5171ED8G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26K3578"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CS8182YDFR8G" prefix="U">
<description>Micropower 200 mA Low Dropout Tracking Regulator/Line Driver</description>
<gates>
<gate name="A" symbol="CS8182YDFR8G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ADJ" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="3"/>
<connect gate="A" pin="GND_4" pad="6"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VREF/ENABLE" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CS8182YDFR8G"/>
<attribute name="OC_FARNELL" value="1155540"/>
<attribute name="OC_NEWARK" value="71J3571"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CS8190EDWFR20G" prefix="U">
<description>Precision Air-Core Tach/Speedo Driver with Return to Zero</description>
<gates>
<gate name="A" symbol="CS8190EDWFR20G"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="BIAS" pad="11"/>
<connect gate="A" pin="COS+" pad="8"/>
<connect gate="A" pin="COS-" pad="9"/>
<connect gate="A" pin="CP+" pad="1"/>
<connect gate="A" pin="CP-" pad="20"/>
<connect gate="A" pin="F/VOUT" pad="19"/>
<connect gate="A" pin="FREQIN" pad="3"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="14"/>
<connect gate="A" pin="GND_3" pad="15"/>
<connect gate="A" pin="GND_4" pad="16"/>
<connect gate="A" pin="GND_5" pad="17"/>
<connect gate="A" pin="GND_6" pad="4"/>
<connect gate="A" pin="GND_7" pad="5"/>
<connect gate="A" pin="GND_8" pad="6"/>
<connect gate="A" pin="SIN+" pad="13"/>
<connect gate="A" pin="SIN-" pad="12"/>
<connect gate="A" pin="SQOUT" pad="2"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="VREG" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CS8190EDWFR20G"/>
<attribute name="OC_FARNELL" value="1568820"/>
<attribute name="OC_NEWARK" value="26K3580"/>
<attribute name="PACKAGE" value="20SOIC"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CS8190ENF16G" prefix="U">
<description>Precision Air-Core Tach/Speedo Driver</description>
<gates>
<gate name="A" symbol="CS8190ENF16G"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="BIAS" pad="9"/>
<connect gate="A" pin="COS+" pad="6"/>
<connect gate="A" pin="COS-" pad="7"/>
<connect gate="A" pin="CP+" pad="1"/>
<connect gate="A" pin="CP-" pad="16"/>
<connect gate="A" pin="F/VOUT" pad="15"/>
<connect gate="A" pin="FREQIN" pad="3"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="SINE+" pad="11"/>
<connect gate="A" pin="SINE-" pad="10"/>
<connect gate="A" pin="SQOUT" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VREG" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CS8190ENF16G"/>
<attribute name="OC_FARNELL" value="1568827"/>
<attribute name="OC_NEWARK" value="27M2306"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FS6370-01G-XTD" prefix="U">
<description>EEPROM Programmable 3-PLL Clock Generator IC</description>
<gates>
<gate name="A" symbol="FS6370-01G-XTD"/>
</gates>
<devices>
<device name="" package="SOIC127P600X173-16N">
<connects>
<connect gate="A" pin="CLK_A" pad="15"/>
<connect gate="A" pin="CLK_B" pad="13"/>
<connect gate="A" pin="CLK_C" pad="12"/>
<connect gate="A" pin="CLK_D" pad="10"/>
<connect gate="A" pin="MODE" pad="9"/>
<connect gate="A" pin="OE/SDA" pad="7"/>
<connect gate="A" pin="PD/SCL" pad="3"/>
<connect gate="A" pin="SEL_CD" pad="2"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VDD_2" pad="8"/>
<connect gate="A" pin="VDD_3" pad="14"/>
<connect gate="A" pin="VSS" pad="11"/>
<connect gate="A" pin="VSS_2" pad="1"/>
<connect gate="A" pin="VSS_3" pad="4"/>
<connect gate="A" pin="XIN" pad="5"/>
<connect gate="A" pin="XOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="FS6370-01G-XTD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="03P0841"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FS6377-01G-XTD" prefix="U">
<description>Programmable 3-PLL Clock Generator IC</description>
<gates>
<gate name="A" symbol="FS6377-01G-XTD"/>
</gates>
<devices>
<device name="" package="SOIC127P600X173-16N">
<connects>
<connect gate="A" pin="ADDR" pad="9"/>
<connect gate="A" pin="CLK_A" pad="15"/>
<connect gate="A" pin="CLK_B" pad="13"/>
<connect gate="A" pin="CLK_C" pad="12"/>
<connect gate="A" pin="CLK_D" pad="10"/>
<connect gate="A" pin="OE" pad="7"/>
<connect gate="A" pin="PD" pad="3"/>
<connect gate="A" pin="SCL" pad="16"/>
<connect gate="A" pin="SDA" pad="1"/>
<connect gate="A" pin="SEL_CD" pad="2"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VDD_2" pad="8"/>
<connect gate="A" pin="VSS" pad="11"/>
<connect gate="A" pin="VSS_2" pad="4"/>
<connect gate="A" pin="XIN" pad="5"/>
<connect gate="A" pin="XOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="FS6377-01G-XTD"/>
<attribute name="OC_FARNELL" value="1641418"/>
<attribute name="OC_NEWARK" value="03P0842"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FS7140-01G-XTD" prefix="U">
<description>Programmable Phase-Locked Loop Clock Generator</description>
<gates>
<gate name="A" symbol="FS7140-01G-XTD"/>
</gates>
<devices>
<device name="" package="SOIC127P600X173-16N">
<connects>
<connect gate="A" pin="ADDR0" pad="3"/>
<connect gate="A" pin="ADDR1" pad="7"/>
<connect gate="A" pin="CLKN" pad="16"/>
<connect gate="A" pin="CLKP" pad="15"/>
<connect gate="A" pin="IPRG" pad="9"/>
<connect gate="A" pin="N/C" pad="10"/>
<connect gate="A" pin="N/C_2" pad="13"/>
<connect gate="A" pin="REF" pad="12"/>
<connect gate="A" pin="SCL" pad="1"/>
<connect gate="A" pin="SDA" pad="2"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VDD_2" pad="8"/>
<connect gate="A" pin="VSS" pad="11"/>
<connect gate="A" pin="VSS_2" pad="4"/>
<connect gate="A" pin="XIN" pad="5"/>
<connect gate="A" pin="XOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="FS7140-01G-XTD"/>
<attribute name="OC_FARNELL" value="1641420"/>
<attribute name="OC_NEWARK" value="03P0844"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM201ANG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM201ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="COMP" pad="8"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="IN_2" pad="2"/>
<connect gate="A" pin="OFS" pad="1"/>
<connect gate="A" pin="OFS_2" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM201ANG"/>
<attribute name="OC_FARNELL" value="1468701"/>
<attribute name="OC_NEWARK" value="26K3595"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM211DG" prefix="U">
<description>Single Comparators</description>
<gates>
<gate name="A" symbol="LM211DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE/STROBE" pad="6"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="NEG_IN_1" pad="3"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM211DG"/>
<attribute name="OC_FARNELL" value="1468702"/>
<attribute name="OC_NEWARK" value="41K9834"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM224DG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM224DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE,_GND" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM224DG"/>
<attribute name="OC_FARNELL" value="1211091"/>
<attribute name="OC_NEWARK" value="71J4990"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM224DR2G" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM224DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE,_GND" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM224DR2G"/>
<attribute name="OC_FARNELL" value="1426352"/>
<attribute name="OC_NEWARK" value="98H0552"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM224NG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM224NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="IN_3" pad="10"/>
<connect gate="A" pin="IN_3_2" pad="9"/>
<connect gate="A" pin="IN_4" pad="13"/>
<connect gate="A" pin="IN_4_2" pad="12"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM224NG"/>
<attribute name="OC_FARNELL" value="1211137"/>
<attribute name="OC_NEWARK" value="45J0710"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM239DG" prefix="U">
<description>Single Supply Quad Comparators</description>
<gates>
<gate name="A" symbol="LM239DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM239DG"/>
<attribute name="OC_FARNELL" value="1211093"/>
<attribute name="OC_NEWARK" value="45J0711"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM239NG" prefix="U">
<description>Comparators</description>
<gates>
<gate name="A" symbol="LM239NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="+IN_1" pad="5"/>
<connect gate="A" pin="+IN_2" pad="7"/>
<connect gate="A" pin="+IN_3" pad="9"/>
<connect gate="A" pin="+IN_4" pad="11"/>
<connect gate="A" pin="-IN_1" pad="4"/>
<connect gate="A" pin="-IN_2" pad="6"/>
<connect gate="A" pin="-IN_3" pad="8"/>
<connect gate="A" pin="-IN_4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT_1" pad="2"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="OUT_3" pad="14"/>
<connect gate="A" pin="OUT_4" pad="13"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM239NG"/>
<attribute name="OC_FARNELL" value="9665420"/>
<attribute name="OC_NEWARK" value="45J0712"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2574N-5G" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2574N-5G"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="OUTPUT" pad="7"/>
<connect gate="A" pin="PWR_GND" pad="4"/>
<connect gate="A" pin="SIG_GND" pad="2"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~ON/OFF" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2574N-5G"/>
<attribute name="OC_FARNELL" value="1460659"/>
<attribute name="OC_NEWARK" value="70K2987"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM258DG" prefix="U">
<description>Single Supply Dual Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM258DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_A" pad="2"/>
<connect gate="A" pin="NEG_IN_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_IN_A" pad="3"/>
<connect gate="A" pin="POS_IN_B" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE/GND" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM258DG"/>
<attribute name="OC_FARNELL" value="1211094"/>
<attribute name="OC_NEWARK" value="71J4994"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2901DTBR2G" prefix="U">
<description>Quad Comparators</description>
<gates>
<gate name="A" symbol="LM2901DTBR2G"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2901DTBR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7812"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2901NG" prefix="U">
<description>Comparators</description>
<gates>
<gate name="A" symbol="LM2901NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="+IN_1" pad="5"/>
<connect gate="A" pin="+IN_2" pad="7"/>
<connect gate="A" pin="+IN_3" pad="9"/>
<connect gate="A" pin="+IN_4" pad="11"/>
<connect gate="A" pin="-IN_1" pad="4"/>
<connect gate="A" pin="-IN_2" pad="6"/>
<connect gate="A" pin="-IN_3" pad="8"/>
<connect gate="A" pin="-IN_4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT_1" pad="2"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="OUT_3" pad="14"/>
<connect gate="A" pin="OUT_4" pad="13"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2901NG"/>
<attribute name="OC_FARNELL" value="1126406"/>
<attribute name="OC_NEWARK" value="45J0721"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2901VDTBR2G" prefix="U">
<description>Quad Comparators</description>
<gates>
<gate name="A" symbol="LM2901VDTBR2G"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2901VDTBR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7813"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2902DG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM2902DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE,_GND" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2902DG"/>
<attribute name="OC_FARNELL" value="1191816"/>
<attribute name="OC_NEWARK" value="45J0722"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2902NG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM2902NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="3"/>
<connect gate="A" pin="IN_1_2" pad="2"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="IN_3" pad="9"/>
<connect gate="A" pin="IN_3_2" pad="10"/>
<connect gate="A" pin="IN_4" pad="13"/>
<connect gate="A" pin="IN_4_2" pad="12"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2902NG"/>
<attribute name="OC_FARNELL" value="1126407"/>
<attribute name="OC_NEWARK" value="45J0723"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2903VDG" prefix="U">
<description>Low Offset Voltage Dual Comparators</description>
<gates>
<gate name="A" symbol="LM2903VDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NEG_IN_A" pad="2"/>
<connect gate="A" pin="NEG_IN_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_IN_A" pad="3"/>
<connect gate="A" pin="POS_IN_B" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2903VDG"/>
<attribute name="OC_FARNELL" value="1703247"/>
<attribute name="OC_NEWARK" value="98H0564"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2903VDR2G" prefix="U">
<description>Low Offset Voltage Dual Comparators</description>
<gates>
<gate name="A" symbol="LM2903VDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NEG_IN_A" pad="2"/>
<connect gate="A" pin="NEG_IN_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_IN_A" pad="3"/>
<connect gate="A" pin="POS_IN_B" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2903VDR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7815"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2904NG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM2904NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_A_2" pad="3"/>
<connect gate="A" pin="IN_B" pad="6"/>
<connect gate="A" pin="IN_B_2" pad="5"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE/GND" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2904NG"/>
<attribute name="OC_FARNELL" value="1211131"/>
<attribute name="OC_NEWARK" value="45J0729"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931ACDG" prefix="U">
<description>Low Dropout Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2931ACDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ADJUST" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="3"/>
<connect gate="A" pin="GND_4" pad="6"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="OUT_INHIBIT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2931ACDG"/>
<attribute name="OC_FARNELL" value="1703350"/>
<attribute name="OC_NEWARK" value="41K9871"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931AD-5.0G" prefix="U">
<description>Low Dropout Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2931AD-5.0G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ADJUST" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="3"/>
<connect gate="A" pin="GND_4" pad="6"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="OUT_INHIBIT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2931AD-5.0G"/>
<attribute name="OC_FARNELL" value="1211098"/>
<attribute name="OC_NEWARK" value="71J5000"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931CDG" prefix="U">
<description>Low Dropout Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2931CDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ADJUST" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="3"/>
<connect gate="A" pin="GND_4" pad="6"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="OUT_INHIBIT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2931CDG"/>
<attribute name="OC_FARNELL" value="1211100"/>
<attribute name="OC_NEWARK" value="71J5006"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931CDR2G" prefix="U">
<description>Low Dropout Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2931CDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ADJUST" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="3"/>
<connect gate="A" pin="GND_4" pad="6"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="OUT_INHIBIT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2931CDR2G"/>
<attribute name="OC_FARNELL" value="1260088"/>
<attribute name="OC_NEWARK" value="88H4655"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931D-5.0G" prefix="U">
<description>Low Dropout Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2931D-5.0G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="3"/>
<connect gate="A" pin="GND_4" pad="6"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="N.C." pad="4"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2931D-5.0G"/>
<attribute name="OC_FARNELL" value="1214458"/>
<attribute name="OC_NEWARK" value="71J5007"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM301ADG" prefix="U">
<description>Non Compensated Single Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM301ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE_2" pad="1"/>
<connect gate="A" pin="COMP" pad="8"/>
<connect gate="A" pin="NEG_IN" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS_IN" pad="3"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM301ADG"/>
<attribute name="OC_FARNELL" value="1426351"/>
<attribute name="OC_NEWARK" value="45J0731"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM301ANG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM301ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="COMP" pad="8"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="IN_2" pad="2"/>
<connect gate="A" pin="OFS" pad="1"/>
<connect gate="A" pin="OFS_2" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM301ANG"/>
<attribute name="OC_FARNELL" value="1125957"/>
<attribute name="OC_NEWARK" value="26K3624"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM311DG" prefix="U">
<description>Single Comparators</description>
<gates>
<gate name="A" symbol="LM311DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE/STROBE" pad="6"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="NEG_IN" pad="3"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="POS_IN" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM311DG"/>
<attribute name="OC_FARNELL" value="1468705"/>
<attribute name="OC_NEWARK" value="98H0570"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM311NG" prefix="U">
<description>Single Comparators</description>
<gates>
<gate name="A" symbol="LM311NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="IN_2" pad="2"/>
<connect gate="A" pin="OFS" pad="5"/>
<connect gate="A" pin="OFS/STRB" pad="6"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM311NG"/>
<attribute name="OC_FARNELL" value="1214465"/>
<attribute name="OC_NEWARK" value="45J0734"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM317LBDG" prefix="U">
<description>Adjustable Output, Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM317LBDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ADJUST" pad="4"/>
<connect gate="A" pin="N.C." pad="8"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="7"/>
<connect gate="A" pin="VOUT_2" pad="2"/>
<connect gate="A" pin="VOUT_3" pad="3"/>
<connect gate="A" pin="VOUT_4" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM317LBDG"/>
<attribute name="OC_FARNELL" value="1652326"/>
<attribute name="OC_NEWARK" value="88H4658"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM317LDG" prefix="U">
<description>Adjustable Output, Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM317LDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ADJUST" pad="4"/>
<connect gate="A" pin="N.C." pad="8"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="7"/>
<connect gate="A" pin="VOUT_2" pad="2"/>
<connect gate="A" pin="VOUT_3" pad="3"/>
<connect gate="A" pin="VOUT_4" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM317LDG"/>
<attribute name="OC_FARNELL" value="1211101"/>
<attribute name="OC_NEWARK" value="45J0739"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM317LDR2G" prefix="U">
<description>Adjustable Output, Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM317LDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ADJUST" pad="4"/>
<connect gate="A" pin="N.C." pad="8"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="7"/>
<connect gate="A" pin="VOUT_2" pad="2"/>
<connect gate="A" pin="VOUT_3" pad="3"/>
<connect gate="A" pin="VOUT_4" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM317LDR2G"/>
<attribute name="OC_FARNELL" value="1278481"/>
<attribute name="OC_NEWARK" value="84K8732"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM324ANG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM324ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="3"/>
<connect gate="A" pin="IN_1_2" pad="2"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="IN_3" pad="9"/>
<connect gate="A" pin="IN_3_2" pad="10"/>
<connect gate="A" pin="IN_4" pad="13"/>
<connect gate="A" pin="IN_4_2" pad="12"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE,GND" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM324ANG"/>
<attribute name="OC_FARNELL" value="1214466"/>
<attribute name="OC_NEWARK" value="98H0574"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM324DG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM324DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE,_GND" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM324DG"/>
<attribute name="OC_FARNELL" value="1211103"/>
<attribute name="OC_NEWARK" value="45J0744"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM324DR2G" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM324DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE,_GND" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM324DR2G"/>
<attribute name="OC_FARNELL" value="1266199"/>
<attribute name="OC_NEWARK" value="84K8734"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM339DR2G" prefix="U">
<description>Single Supply Quad Comparators</description>
<gates>
<gate name="A" symbol="LM339DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM339DR2G"/>
<attribute name="OC_FARNELL" value="1651910"/>
<attribute name="OC_NEWARK" value="17H1559"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM339NG" prefix="U">
<description>Single Supply Quad Comparators</description>
<gates>
<gate name="A" symbol="LM339NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="+IN_1" pad="5"/>
<connect gate="A" pin="+IN_2" pad="7"/>
<connect gate="A" pin="+IN_3" pad="9"/>
<connect gate="A" pin="+IN_4" pad="11"/>
<connect gate="A" pin="-IN_1" pad="4"/>
<connect gate="A" pin="-IN_2" pad="6"/>
<connect gate="A" pin="-IN_3" pad="8"/>
<connect gate="A" pin="-IN_4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT_1" pad="2"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="OUT_3" pad="14"/>
<connect gate="A" pin="OUT_4" pad="13"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM339NG"/>
<attribute name="OC_FARNELL" value="9664491"/>
<attribute name="OC_NEWARK" value="98H0576"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358DG" prefix="U">
<description>Single Supply Dual Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM358DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_A" pad="2"/>
<connect gate="A" pin="NEG_IN_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_IN_A" pad="3"/>
<connect gate="A" pin="POS_IN_B" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE/GND" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM358DG"/>
<attribute name="OC_FARNELL" value="1211106"/>
<attribute name="OC_NEWARK" value="45J0748"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358DR2G" prefix="U">
<description>Single Supply Dual Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM358DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_A" pad="2"/>
<connect gate="A" pin="NEG_IN_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_IN_A" pad="3"/>
<connect gate="A" pin="POS_IN_B" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE/GND" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM358DR2G"/>
<attribute name="OC_FARNELL" value="1262834"/>
<attribute name="OC_NEWARK" value="83H7264"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358NG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM358NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_A_2" pad="3"/>
<connect gate="A" pin="IN_B" pad="6"/>
<connect gate="A" pin="IN_B_2" pad="5"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE/GND" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM358NG"/>
<attribute name="OC_FARNELL" value="1211132"/>
<attribute name="OC_NEWARK" value="67H6684"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM385BD-1.2G" prefix="U">
<description>Micropower Voltage Reference Diodes</description>
<gates>
<gate name="A" symbol="LM385BD-1.2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ANODE" pad="4"/>
<connect gate="A" pin="CATHODE" pad="8"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="N.C._2" pad="3"/>
<connect gate="A" pin="N.C._3" pad="2"/>
<connect gate="A" pin="N.C._4" pad="6"/>
<connect gate="A" pin="N.C._5" pad="1"/>
<connect gate="A" pin="N.C._6" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM385BD-1.2G"/>
<attribute name="OC_FARNELL" value="1705938"/>
<attribute name="OC_NEWARK" value="45J0749"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM393DG." prefix="U">
<description>Dual Comparators</description>
<gates>
<gate name="A" symbol="LM393DG."/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_A_2" pad="3"/>
<connect gate="A" pin="IN_B" pad="5"/>
<connect gate="A" pin="IN_B_2" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM393DG"/>
<attribute name="OC_FARNELL" value="1211108"/>
<attribute name="OC_NEWARK" value="88H4661"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM393DG" prefix="U">
<description>Low Offset Voltage Dual Comparators</description>
<gates>
<gate name="A" symbol="LM393DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN_A" pad="3"/>
<connect gate="A" pin="+IN_B" pad="5"/>
<connect gate="A" pin="-IN_A" pad="2"/>
<connect gate="A" pin="-IN_B" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM393DG"/>
<attribute name="OC_FARNELL" value="1343575"/>
<attribute name="OC_NEWARK" value="88H4661"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM393DR2G" prefix="U">
<description>Low Offset Voltage Dual Comparators</description>
<gates>
<gate name="A" symbol="LM393DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN_A" pad="3"/>
<connect gate="A" pin="IN_A_2" pad="2"/>
<connect gate="A" pin="IN_B" pad="5"/>
<connect gate="A" pin="IN_B_2" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM393DR2G"/>
<attribute name="OC_FARNELL" value="1258876"/>
<attribute name="OC_NEWARK" value="88H4662"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM393NG" prefix="U">
<description>Dual Comparators</description>
<gates>
<gate name="A" symbol="LM393NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_A_2" pad="3"/>
<connect gate="A" pin="IN_B" pad="5"/>
<connect gate="A" pin="IN_B_2" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM393NG"/>
<attribute name="OC_FARNELL" value="1211133"/>
<attribute name="OC_NEWARK" value="67H6685"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM833NG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM833NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM833NG"/>
<attribute name="OC_FARNELL" value="1214467"/>
<attribute name="OC_NEWARK" value="26K3636"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951ACDG" prefix="U">
<description>Low Power Low Dropout Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2951ACDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SENSE" pad="2"/>
<connect gate="A" pin="SHDN" pad="3"/>
<connect gate="A" pin="VO_TAP" pad="6"/>
<connect gate="A" pin="~ERROR_OUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2951ACDG"/>
<attribute name="OC_FARNELL" value="1652328"/>
<attribute name="OC_NEWARK" value="26K3642"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951ACDR2G" prefix="U">
<description>Low Power Low Dropout Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2951ACDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SENSE" pad="2"/>
<connect gate="A" pin="SHDN" pad="3"/>
<connect gate="A" pin="VO_TAP" pad="6"/>
<connect gate="A" pin="~ERROR_OUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2951ACDR2G"/>
<attribute name="OC_FARNELL" value="1260732"/>
<attribute name="OC_NEWARK" value="41J1709"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951ACNG" prefix="U">
<description>Dropout Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2951ACNG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="FEEDBACK" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INPUT" pad="8"/>
<connect gate="A" pin="OUTPUT" pad="1"/>
<connect gate="A" pin="SENSE" pad="2"/>
<connect gate="A" pin="SHUTDOWN" pad="3"/>
<connect gate="A" pin="VO_TAP" pad="6"/>
<connect gate="A" pin="~ERROR_OUTPUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2951ACNG"/>
<attribute name="OC_FARNELL" value="1213692"/>
<attribute name="OC_NEWARK" value="70K3006"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951CD-3.3R2G" prefix="U">
<description>Low Power Low Dropout Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2951CD-3.3R2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SENSE" pad="2"/>
<connect gate="A" pin="SHDN" pad="3"/>
<connect gate="A" pin="VO_TAP" pad="6"/>
<connect gate="A" pin="~ERROR_OUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2951CD-3.3R2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7822"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951CDG" prefix="U">
<description>Low Power Low Dropout Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2951CDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SENSE" pad="2"/>
<connect gate="A" pin="SHDN" pad="3"/>
<connect gate="A" pin="VO_TAP" pad="6"/>
<connect gate="A" pin="~ERROR_OUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2951CDG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J0757"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1G125DFT1G" prefix="U">
<description>Noninverting 3-State Buffer</description>
<gates>
<gate name="A" symbol="M74VHC1G125DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~OE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1G125DFT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="61K1055"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1G132DFT1G" prefix="U">
<description>2-Input NAND Schmitt-Trigger</description>
<gates>
<gate name="A" symbol="M74VHC1G132DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_~Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1G132DFT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="61K1061"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1GT00DFT1G" prefix="U">
<description>Single 2-Input NAND Gate/ CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="M74VHC1GT00DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1GT00DFT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="61K1023"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1GT04DFT1G" prefix="U">
<description>Inverting Buffer / CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="M74VHC1GT04DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_~Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1GT04DFT1G"/>
<attribute name="OC_FARNELL" value="1567264"/>
<attribute name="OC_NEWARK" value="61K1029"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1GT08DFT1G" prefix="U">
<description>2-Input AND Gate/CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="M74VHC1GT08DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1GT08DFT1G"/>
<attribute name="OC_FARNELL" value="1654343"/>
<attribute name="OC_NEWARK" value="61K1032"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1GT125DF1G" prefix="U">
<description>Noninverting Buffer / CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="M74VHC1GT125DF1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~OE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1GT125DF1G"/>
<attribute name="OC_FARNELL" value="1567363"/>
<attribute name="OC_NEWARK" value="83H7591"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1GT126DF1G" prefix="U">
<description>Noninverting Buffer / CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="M74VHC1GT126DF1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1GT126DF1G"/>
<attribute name="OC_FARNELL" value="1567365"/>
<attribute name="OC_NEWARK" value="83H7593"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1GT126DT1G" prefix="U">
<description>Noninverting Buffer / CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="M74VHC1GT126DT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1GT126DT1G"/>
<attribute name="OC_FARNELL" value="1468708"/>
<attribute name="OC_NEWARK" value="61K1036"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1GT14DFT1G" prefix="U">
<description>Schmitt-Trigger Inverter / CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="M74VHC1GT14DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_~Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1GT14DFT1G"/>
<attribute name="OC_FARNELL" value="1654345"/>
<attribute name="OC_NEWARK" value="61K1037"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1GT32DFT1G" prefix="U">
<description>2-Input OR Gate/CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="M74VHC1GT32DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1GT32DFT1G"/>
<attribute name="OC_FARNELL" value="1567270"/>
<attribute name="OC_NEWARK" value="61K1040"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1GT50DFT1G" prefix="U">
<description>Noninverting Buffer / CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="M74VHC1GT50DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1GT50DFT1G"/>
<attribute name="OC_FARNELL" value="1703292"/>
<attribute name="OC_NEWARK" value="61K1043"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1GT50DTT1G" prefix="U">
<description>Noninverting Buffer / CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="M74VHC1GT50DTT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1GT50DTT1G"/>
<attribute name="OC_FARNELL" value="1654338"/>
<attribute name="OC_NEWARK" value="61K1045"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74VHC1GT86DFT1G" prefix="U">
<description>2-Input Exclusive OR Gate / CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="M74VHC1GT86DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="M74VHC1GT86DFT1G"/>
<attribute name="OC_FARNELL" value="1654346"/>
<attribute name="OC_NEWARK" value="61K1049"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX809JTRG" prefix="U">
<description>Very Low Supply Current 3-Pin Microprocessor  Reset Monitors</description>
<gates>
<gate name="A" symbol="MAX809JTRG"/>
</gates>
<devices>
<device name="" package="SOT95P240X110-3N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="~RESET" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MAX809JTRG"/>
<attribute name="OC_FARNELL" value="1705445"/>
<attribute name="OC_NEWARK" value="04R7823"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX809STRG" prefix="U">
<description>3-Pin Microprocessor</description>
<gates>
<gate name="A" symbol="MAX809STRG"/>
</gates>
<devices>
<device name="" package="SOT95P240X111-3N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="~RESET" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MAX809STRG"/>
<attribute name="OC_FARNELL" value="1652404"/>
<attribute name="OC_NEWARK" value="98H0579"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX809TTRG" prefix="U">
<description>3-Pin Microprocessor</description>
<gates>
<gate name="A" symbol="MAX809TTRG"/>
</gates>
<devices>
<device name="" package="SOT95P240X111-3N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="~RESET" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MAX809TTRG"/>
<attribute name="OC_FARNELL" value="1652405"/>
<attribute name="OC_NEWARK" value="45J0769"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX810MTRG" prefix="U">
<description>3-Pin Microprocessor</description>
<gates>
<gate name="A" symbol="MAX810MTRG"/>
</gates>
<devices>
<device name="" package="SOT95P240X111-3N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="RESET" pad="2"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MAX810MTRG"/>
<attribute name="OC_FARNELL" value="1360058"/>
<attribute name="OC_NEWARK" value="71J5243"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX810RTRG" prefix="U">
<description>3-Pin Microprocessor</description>
<gates>
<gate name="A" symbol="MAX810RTRG"/>
</gates>
<devices>
<device name="" package="SOT95P240X111-3N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="RESET" pad="2"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MAX810RTRG"/>
<attribute name="OC_FARNELL" value="1703427"/>
<attribute name="OC_NEWARK" value="41K9966"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100E016FNG" prefix="U">
<description>Synchronous Binary Up Counter</description>
<gates>
<gate name="A" symbol="MC100E016FNG"/>
</gates>
<devices>
<device name="" package="PLCC127P1257X1257X457-28N">
<connects>
<connect gate="A" pin="CLK" pad="27"/>
<connect gate="A" pin="MR" pad="26"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="P0" pad="3"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="5"/>
<connect gate="A" pin="P3" pad="6"/>
<connect gate="A" pin="P4" pad="7"/>
<connect gate="A" pin="P5" pad="21"/>
<connect gate="A" pin="P6" pad="22"/>
<connect gate="A" pin="P7" pad="23"/>
<connect gate="A" pin="Q0" pad="9"/>
<connect gate="A" pin="Q1" pad="10"/>
<connect gate="A" pin="Q2" pad="11"/>
<connect gate="A" pin="Q3" pad="12"/>
<connect gate="A" pin="Q4" pad="13"/>
<connect gate="A" pin="Q5" pad="15"/>
<connect gate="A" pin="Q6" pad="17"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="A" pin="TCLD" pad="28"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VCCO" pad="20"/>
<connect gate="A" pin="VCCO_2" pad="8"/>
<connect gate="A" pin="VCCO_3" pad="14"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~CE" pad="24"/>
<connect gate="A" pin="~PE" pad="25"/>
<connect gate="A" pin="~TC" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100E016FNG"/>
<attribute name="OC_FARNELL" value="1147616"/>
<attribute name="OC_NEWARK" value="26K3871"/>
<attribute name="PACKAGE" value="PLCC-28"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100E111FNG" prefix="U">
<description>ECL 1:9 Differential Clock Driver</description>
<gates>
<gate name="A" symbol="MC100E111FNG"/>
</gates>
<devices>
<device name="" package="PLCC127P1244X1244X457-28N">
<connects>
<connect gate="A" pin="IN" pad="28"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="Q0" pad="25"/>
<connect gate="A" pin="Q1" pad="23"/>
<connect gate="A" pin="Q2" pad="20"/>
<connect gate="A" pin="Q3" pad="18"/>
<connect gate="A" pin="Q4" pad="16"/>
<connect gate="A" pin="Q5" pad="13"/>
<connect gate="A" pin="Q6" pad="11"/>
<connect gate="A" pin="Q7" pad="9"/>
<connect gate="A" pin="Q8" pad="6"/>
<connect gate="A" pin="VBB" pad="3"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VCCO" pad="22"/>
<connect gate="A" pin="VCCO_2" pad="8"/>
<connect gate="A" pin="VCCO_3" pad="15"/>
<connect gate="A" pin="VEE" pad="26"/>
<connect gate="A" pin="~EN" pad="27"/>
<connect gate="A" pin="~IN" pad="2"/>
<connect gate="A" pin="~Q0" pad="24"/>
<connect gate="A" pin="~Q1" pad="21"/>
<connect gate="A" pin="~Q2" pad="19"/>
<connect gate="A" pin="~Q3" pad="17"/>
<connect gate="A" pin="~Q4" pad="14"/>
<connect gate="A" pin="~Q5" pad="12"/>
<connect gate="A" pin="~Q6" pad="10"/>
<connect gate="A" pin="~Q7" pad="7"/>
<connect gate="A" pin="~Q8" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100E111FNG"/>
<attribute name="OC_FARNELL" value="1192060"/>
<attribute name="OC_NEWARK" value="45J0952"/>
<attribute name="PACKAGE" value="PLCC-28"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EL11DG" prefix="U">
<description>5.0 V ECL 1:2 Differential Fanout Buffer</description>
<gates>
<gate name="A" symbol="MC100EL11DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="6"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EL11DG"/>
<attribute name="OC_FARNELL" value="1607915"/>
<attribute name="OC_NEWARK" value="88H4701"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EL14DWG" prefix="U">
<description>ECL 1:5 Clock Distribution Chip</description>
<gates>
<gate name="A" symbol="MC100EL14DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="NC" pad="17"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="SEL" pad="12"/>
<connect gate="A" pin="VBB" pad="13"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="18"/>
<connect gate="A" pin="VEE" pad="11"/>
<connect gate="A" pin="~CLK" pad="14"/>
<connect gate="A" pin="~EN" pad="19"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
<connect gate="A" pin="~Q2" pad="6"/>
<connect gate="A" pin="~Q3" pad="8"/>
<connect gate="A" pin="~Q4" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EL14DWG"/>
<attribute name="OC_FARNELL" value="1607916"/>
<attribute name="OC_NEWARK" value="88H4704"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EL15DG" prefix="U">
<description>5V ECL 1:4 Clock Distribution Chip</description>
<gates>
<gate name="A" symbol="MC100EL15DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="SCLK" pad="14"/>
<connect gate="A" pin="SEL" pad="10"/>
<connect gate="A" pin="VBB" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VEE" pad="9"/>
<connect gate="A" pin="~CLK" pad="12"/>
<connect gate="A" pin="~EN" pad="15"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
<connect gate="A" pin="~Q2" pad="6"/>
<connect gate="A" pin="~Q3" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EL15DG"/>
<attribute name="OC_FARNELL" value="1258372"/>
<attribute name="OC_NEWARK" value="42K0357"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EL1648DG" prefix="U">
<description>Voltage Controlled Oscillator Amplifier</description>
<gates>
<gate name="A" symbol="MC100EL1648DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="AGC" pad="5"/>
<connect gate="A" pin="BIAS" pad="8"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="TANK" pad="1"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="VCC_2" pad="3"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VEE_2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EL1648DG"/>
<attribute name="OC_FARNELL" value="1192063"/>
<attribute name="OC_NEWARK" value="26K3816"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EL16DG" prefix="U">
<description>5.0V ECL Differential Receiver</description>
<gates>
<gate name="A" symbol="MC100EL16DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EL16DG"/>
<attribute name="OC_FARNELL" value="1192064"/>
<attribute name="OC_NEWARK" value="88H4705"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EL31DG" prefix="U">
<description>Single Supply 3.0 V to 44 V Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC100EL31DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="R" pad="4"/>
<connect gate="A" pin="S" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33071ADG"/>
<attribute name="OC_FARNELL" value="1607707"/>
<attribute name="OC_NEWARK" value="98H0669"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EL32DG" prefix="U">
<description>5V ECL ÷2 Divider</description>
<gates>
<gate name="A" symbol="MC100EL32DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~CLK" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EL32DG"/>
<attribute name="OC_FARNELL" value="1311157"/>
<attribute name="OC_NEWARK" value="26K3825"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EL57DG" prefix="U">
<description>5V ECL 1:4 Differential Multiplexer</description>
<gates>
<gate name="A" symbol="MC100EL57DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="5"/>
<connect gate="A" pin="D3" pad="7"/>
<connect gate="A" pin="Q" pad="13"/>
<connect gate="A" pin="SEL0" pad="15"/>
<connect gate="A" pin="SEL1" pad="14"/>
<connect gate="A" pin="VBB1" pad="11"/>
<connect gate="A" pin="VBB2" pad="10"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VEE" pad="9"/>
<connect gate="A" pin="~D0" pad="2"/>
<connect gate="A" pin="~D1" pad="4"/>
<connect gate="A" pin="~D2" pad="6"/>
<connect gate="A" pin="~D3" pad="8"/>
<connect gate="A" pin="~Q" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EL57DG"/>
<attribute name="OC_FARNELL" value="1150407"/>
<attribute name="OC_NEWARK" value="45J0919"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EL91DWG" prefix="U">
<description>5 V Triple PECL Input to -5 V ECL Output Translator</description>
<gates>
<gate name="A" symbol="MC100EL91DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="5"/>
<connect gate="A" pin="D2" pad="8"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="14"/>
<connect gate="A" pin="PECLVBB" pad="7"/>
<connect gate="A" pin="PECLVBB_2" pad="4"/>
<connect gate="A" pin="Q0" pad="19"/>
<connect gate="A" pin="Q1" pad="16"/>
<connect gate="A" pin="Q2" pad="13"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="11"/>
<connect gate="A" pin="VCC_3" pad="1"/>
<connect gate="A" pin="VEE" pad="10"/>
<connect gate="A" pin="~D0" pad="3"/>
<connect gate="A" pin="~D1" pad="6"/>
<connect gate="A" pin="~D2" pad="9"/>
<connect gate="A" pin="~Q0" pad="18"/>
<connect gate="A" pin="~Q1" pad="15"/>
<connect gate="A" pin="~Q2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EL91DWG"/>
<attribute name="OC_FARNELL" value="1147093"/>
<attribute name="OC_NEWARK" value="26K3834"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100ELT20DG" prefix="U">
<description>5V TTL to Differential PECL Translator</description>
<gates>
<gate name="A" symbol="MC100ELT20DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="6"/>
<connect gate="A" pin="Q" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~Q" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100ELT20DG"/>
<attribute name="OC_FARNELL" value="1607862"/>
<attribute name="OC_NEWARK" value="26K3803"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100ELT20DTG" prefix="U">
<description>5V TTL to Differential PECL  Translator</description>
<gates>
<gate name="A" symbol="MC100ELT20DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="4"/>
<connect gate="A" pin="Q" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~Q" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100ELT20DTG"/>
<attribute name="OC_FARNELL" value="1192068"/>
<attribute name="OC_NEWARK" value="26K3804"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100ELT21DG" prefix="U">
<description>5 V Differential PECL to TTL Translator</description>
<gates>
<gate name="A" symbol="MC100ELT21DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="Q0" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~D0" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100ELT21DG"/>
<attribute name="OC_FARNELL" value="1192069"/>
<attribute name="OC_NEWARK" value="71J5392"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100ELT21DTG" prefix="U">
<description>5V TTL to Differential PECL TTL Translator</description>
<gates>
<gate name="A" symbol="MC100ELT21DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="Q0" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100ELT21DTG"/>
<attribute name="OC_FARNELL" value="1199231"/>
<attribute name="OC_NEWARK" value="26K3805"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100ELT24DG" prefix="U">
<description>5V TTL to Differential ECL Translator</description>
<gates>
<gate name="A" symbol="MC100ELT24DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100ELT24DG"/>
<attribute name="OC_FARNELL" value="1192072"/>
<attribute name="OC_NEWARK" value="26K3810"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100ELT24DTG" prefix="U">
<description>5V TTL to Differential ECL Translator</description>
<gates>
<gate name="A" symbol="MC100ELT24DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100ELT24DTG"/>
<attribute name="OC_FARNELL" value="1224744"/>
<attribute name="OC_NEWARK" value="26K3811"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100ELT25DTG" prefix="U">
<description>-5 V Differential ECL to TTL Translator</description>
<gates>
<gate name="A" symbol="MC100ELT25DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~D" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100ELT25DTG"/>
<attribute name="OC_FARNELL" value="1607863"/>
<attribute name="OC_NEWARK" value="26K3813"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP01DG" prefix="U">
<description>3.3V / 5V ECL 4-Input OR/NOR</description>
<gates>
<gate name="A" symbol="MC100EP01DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="D3" pad="4"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP01DG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="42K0380"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP01DTG" prefix="U">
<description>3.3V / 5V ECL 4-Input  OR/NOR</description>
<gates>
<gate name="A" symbol="MC100EP01DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="D3" pad="4"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP01DTG"/>
<attribute name="OC_FARNELL" value="1607760"/>
<attribute name="OC_NEWARK" value="26K3839"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP05DG" prefix="U">
<description>3.3V / 5V ECL 2-Input Differential AND/NAND</description>
<gates>
<gate name="A" symbol="MC100EP05DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D0" pad="2"/>
<connect gate="A" pin="~D1" pad="4"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP05DG"/>
<attribute name="OC_FARNELL" value="1607761"/>
<attribute name="OC_NEWARK" value="71J5404"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP05DTG" prefix="U">
<description>3.3V / 5V ECL 2-Input Differential AND/NAND</description>
<gates>
<gate name="A" symbol="MC100EP05DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D0" pad="2"/>
<connect gate="A" pin="~D1" pad="4"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP05DTG"/>
<attribute name="OC_FARNELL" value="1155549"/>
<attribute name="OC_NEWARK" value="71J5405"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP08DTG" prefix="U">
<description>3.3V / 5V ECL 2-Input  Differential XOR/XNOR</description>
<gates>
<gate name="A" symbol="MC100EP08DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D0" pad="2"/>
<connect gate="A" pin="~D1" pad="4"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP08DTG"/>
<attribute name="OC_FARNELL" value="1167617"/>
<attribute name="OC_NEWARK" value="61K0831"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP11DG" prefix="U">
<description>3.3V / 5V ECL 1:2 Differential Fanout Buffer</description>
<gates>
<gate name="A" symbol="MC100EP11DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="6"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP11DG"/>
<attribute name="OC_FARNELL" value="1468709"/>
<attribute name="OC_NEWARK" value="45J0937"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="On Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP11DTG" prefix="U">
<description>3.3V / 5V ECL 1:2 Differential Fanout Buffer</description>
<gates>
<gate name="A" symbol="MC100EP11DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="6"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP11DTG"/>
<attribute name="OC_FARNELL" value="1607917"/>
<attribute name="OC_NEWARK" value="45J0938"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP131FAG" prefix="U">
<description>3.3V / 5V ECL Quad D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC100EP131FAG"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="C0" pad="12"/>
<connect gate="A" pin="C1" pad="7"/>
<connect gate="A" pin="C2" pad="3"/>
<connect gate="A" pin="C3" pad="27"/>
<connect gate="A" pin="CC" pad="4"/>
<connect gate="A" pin="D0" pad="14"/>
<connect gate="A" pin="D1" pad="8"/>
<connect gate="A" pin="D2" pad="32"/>
<connect gate="A" pin="D3" pad="29"/>
<connect gate="A" pin="Q0" pad="17"/>
<connect gate="A" pin="Q1" pad="19"/>
<connect gate="A" pin="Q2" pad="21"/>
<connect gate="A" pin="Q3" pad="23"/>
<connect gate="A" pin="R0" pad="15"/>
<connect gate="A" pin="R1" pad="10"/>
<connect gate="A" pin="R2" pad="1"/>
<connect gate="A" pin="R3" pad="30"/>
<connect gate="A" pin="SET" pad="31"/>
<connect gate="A" pin="VCC" pad="25"/>
<connect gate="A" pin="VCC_2" pad="13"/>
<connect gate="A" pin="VCC_3" pad="16"/>
<connect gate="A" pin="VEE" pad="28"/>
<connect gate="A" pin="VEE_2" pad="9"/>
<connect gate="A" pin="~C0" pad="11"/>
<connect gate="A" pin="~C1" pad="6"/>
<connect gate="A" pin="~C2" pad="2"/>
<connect gate="A" pin="~C3" pad="26"/>
<connect gate="A" pin="~CC" pad="5"/>
<connect gate="A" pin="~Q0" pad="18"/>
<connect gate="A" pin="~Q1" pad="20"/>
<connect gate="A" pin="~Q2" pad="22"/>
<connect gate="A" pin="~Q3" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP131FAG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26K3843"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP139DTG" prefix="U">
<description>Clock Generation Chip</description>
<gates>
<gate name="A" symbol="MC100EP139DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-20N">
<connects>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="DIVSELA" pad="10"/>
<connect gate="A" pin="DIVSELB0" pad="3"/>
<connect gate="A" pin="DIVSELB1" pad="9"/>
<connect gate="A" pin="MR" pad="7"/>
<connect gate="A" pin="Q0" pad="19"/>
<connect gate="A" pin="Q1" pad="17"/>
<connect gate="A" pin="Q2" pad="15"/>
<connect gate="A" pin="Q3" pad="13"/>
<connect gate="A" pin="VBB" pad="6"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="1"/>
<connect gate="A" pin="VCC_3" pad="8"/>
<connect gate="A" pin="VEE" pad="11"/>
<connect gate="A" pin="~CLK" pad="5"/>
<connect gate="A" pin="~EN" pad="2"/>
<connect gate="A" pin="~Q0" pad="18"/>
<connect gate="A" pin="~Q1" pad="16"/>
<connect gate="A" pin="~Q2" pad="14"/>
<connect gate="A" pin="~Q3" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP139DTG"/>
<attribute name="OC_FARNELL" value="1126230"/>
<attribute name="OC_NEWARK" value="42K0393"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP140DG" prefix="U">
<description>ECL Phase-Frequency Detector</description>
<gates>
<gate name="A" symbol="MC100EP140DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="4"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="R" pad="7"/>
<connect gate="A" pin="U" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~U" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP140DG"/>
<attribute name="OC_FARNELL" value="1181714"/>
<attribute name="OC_NEWARK" value="71J5409"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP142FAG" prefix="U">
<description>3.3 V / 5 V ECL 9-Bit Shift Register</description>
<gates>
<gate name="A" symbol="MC100EP142FAG"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="CLK0" pad="4"/>
<connect gate="A" pin="CLK1" pad="6"/>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="31"/>
<connect gate="A" pin="D2" pad="30"/>
<connect gate="A" pin="D3" pad="29"/>
<connect gate="A" pin="D4" pad="27"/>
<connect gate="A" pin="D5" pad="26"/>
<connect gate="A" pin="D6" pad="25"/>
<connect gate="A" pin="D7" pad="24"/>
<connect gate="A" pin="D8" pad="23"/>
<connect gate="A" pin="MR" pad="9"/>
<connect gate="A" pin="Q0" pad="10"/>
<connect gate="A" pin="Q1" pad="11"/>
<connect gate="A" pin="Q2" pad="12"/>
<connect gate="A" pin="Q3" pad="14"/>
<connect gate="A" pin="Q4" pad="15"/>
<connect gate="A" pin="Q5" pad="18"/>
<connect gate="A" pin="Q6" pad="19"/>
<connect gate="A" pin="Q7" pad="20"/>
<connect gate="A" pin="Q8" pad="22"/>
<connect gate="A" pin="S-IN" pad="2"/>
<connect gate="A" pin="SEL" pad="8"/>
<connect gate="A" pin="VCC" pad="32"/>
<connect gate="A" pin="VCC_2" pad="13"/>
<connect gate="A" pin="VCC_3" pad="17"/>
<connect gate="A" pin="VEE" pad="28"/>
<connect gate="A" pin="VEE_2" pad="16"/>
<connect gate="A" pin="~CLK0" pad="5"/>
<connect gate="A" pin="~CLK1" pad="7"/>
<connect gate="A" pin="~Q7" pad="21"/>
<connect gate="A" pin="~S-IN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP142FAG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26K3846"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP14DTG" prefix="U">
<description>Differential ECL/PECL/HSTL Clock Driver</description>
<gates>
<gate name="A" symbol="MC100EP14DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-20N">
<connects>
<connect gate="A" pin="CLK0" pad="13"/>
<connect gate="A" pin="CLK1" pad="16"/>
<connect gate="A" pin="CLK_SEL" pad="12"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="VBB" pad="15"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="18"/>
<connect gate="A" pin="VEE" pad="11"/>
<connect gate="A" pin="~CLK0" pad="14"/>
<connect gate="A" pin="~CLK1" pad="17"/>
<connect gate="A" pin="~EN" pad="19"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
<connect gate="A" pin="~Q2" pad="6"/>
<connect gate="A" pin="~Q3" pad="8"/>
<connect gate="A" pin="~Q4" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP14DTG"/>
<attribute name="OC_FARNELL" value="1607918"/>
<attribute name="OC_NEWARK" value="71J5407"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP16DG" prefix="U">
<description>ECL Differential Receiver/Driver</description>
<gates>
<gate name="A" symbol="MC100EP16DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP16DG"/>
<attribute name="OC_FARNELL" value="1192075"/>
<attribute name="OC_NEWARK" value="26K3847"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP16DTG" prefix="U">
<description>ECL Differential Receiver/Driver</description>
<gates>
<gate name="A" symbol="MC100EP16DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP16DTG"/>
<attribute name="OC_FARNELL" value="1607763"/>
<attribute name="OC_NEWARK" value="71J5410"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP16DTR2G" prefix="U">
<description>Differential Receiver/Driver</description>
<gates>
<gate name="A" symbol="MC100EP16DTR2G"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP16DTR2G"/>
<attribute name="OC_FARNELL" value="1364610"/>
<attribute name="OC_NEWARK" value="45J0940"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP195BFAG" prefix="U">
<description>3.3V ECL Programmable Delay Chip</description>
<gates>
<gate name="A" symbol="MC100EP195BFAG"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="CASCADE" pad="15"/>
<connect gate="A" pin="D0" pad="23"/>
<connect gate="A" pin="D1" pad="25"/>
<connect gate="A" pin="D10" pad="3"/>
<connect gate="A" pin="D2" pad="26"/>
<connect gate="A" pin="D3" pad="27"/>
<connect gate="A" pin="D4" pad="29"/>
<connect gate="A" pin="D5" pad="30"/>
<connect gate="A" pin="D6" pad="31"/>
<connect gate="A" pin="D7" pad="32"/>
<connect gate="A" pin="D8" pad="1"/>
<connect gate="A" pin="D9" pad="2"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="LEN" pad="10"/>
<connect gate="A" pin="NC" pad="17"/>
<connect gate="A" pin="Q" pad="21"/>
<connect gate="A" pin="SETMAX" pad="12"/>
<connect gate="A" pin="SETMIN" pad="11"/>
<connect gate="A" pin="VBB" pad="6"/>
<connect gate="A" pin="VCC" pad="18"/>
<connect gate="A" pin="VCC_2" pad="13"/>
<connect gate="A" pin="VCC_3" pad="19"/>
<connect gate="A" pin="VCC_4" pad="22"/>
<connect gate="A" pin="VCF" pad="8"/>
<connect gate="A" pin="VEE" pad="28"/>
<connect gate="A" pin="VEE_2" pad="24"/>
<connect gate="A" pin="VEE_3" pad="9"/>
<connect gate="A" pin="VEF" pad="7"/>
<connect gate="A" pin="~CASCADE" pad="14"/>
<connect gate="A" pin="~EN" pad="16"/>
<connect gate="A" pin="~IN" pad="5"/>
<connect gate="A" pin="~Q" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP195BFAG"/>
<attribute name="OC_FARNELL" value="1517633"/>
<attribute name="OC_NEWARK" value="57M9762"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP195FAG" prefix="U">
<description>3.3V ECL Programmable Delay Chip</description>
<gates>
<gate name="A" symbol="MC100EP195FAG"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="CASCADE" pad="15"/>
<connect gate="A" pin="D0" pad="23"/>
<connect gate="A" pin="D1" pad="25"/>
<connect gate="A" pin="D10" pad="3"/>
<connect gate="A" pin="D2" pad="26"/>
<connect gate="A" pin="D3" pad="27"/>
<connect gate="A" pin="D4" pad="29"/>
<connect gate="A" pin="D5" pad="30"/>
<connect gate="A" pin="D6" pad="31"/>
<connect gate="A" pin="D7" pad="32"/>
<connect gate="A" pin="D8" pad="1"/>
<connect gate="A" pin="D9" pad="2"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="LEN" pad="10"/>
<connect gate="A" pin="NC" pad="17"/>
<connect gate="A" pin="Q" pad="21"/>
<connect gate="A" pin="SETMAX" pad="12"/>
<connect gate="A" pin="SETMIN" pad="11"/>
<connect gate="A" pin="VBB" pad="6"/>
<connect gate="A" pin="VCC" pad="18"/>
<connect gate="A" pin="VCC_2" pad="22"/>
<connect gate="A" pin="VCC_3" pad="19"/>
<connect gate="A" pin="VCC_4" pad="13"/>
<connect gate="A" pin="VCF" pad="8"/>
<connect gate="A" pin="VEE" pad="24"/>
<connect gate="A" pin="VEE_2" pad="9"/>
<connect gate="A" pin="VEE_3" pad="28"/>
<connect gate="A" pin="VEF" pad="7"/>
<connect gate="A" pin="~CASCADE" pad="14"/>
<connect gate="A" pin="~EN" pad="16"/>
<connect gate="A" pin="~IN" pad="5"/>
<connect gate="A" pin="~Q" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP195FAG"/>
<attribute name="OC_FARNELL" value="1607607"/>
<attribute name="OC_NEWARK" value="26K3858"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP196FAG" prefix="U">
<description>3.3V ECL Programmable Delay Chip</description>
<gates>
<gate name="A" symbol="MC100EP196FAG"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="CASCADE" pad="15"/>
<connect gate="A" pin="D0" pad="23"/>
<connect gate="A" pin="D1" pad="25"/>
<connect gate="A" pin="D10" pad="3"/>
<connect gate="A" pin="D2" pad="26"/>
<connect gate="A" pin="D3" pad="27"/>
<connect gate="A" pin="D4" pad="29"/>
<connect gate="A" pin="D5" pad="30"/>
<connect gate="A" pin="D6" pad="31"/>
<connect gate="A" pin="D7" pad="32"/>
<connect gate="A" pin="D8" pad="1"/>
<connect gate="A" pin="D9" pad="2"/>
<connect gate="A" pin="FTUNE" pad="17"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="LEN" pad="10"/>
<connect gate="A" pin="Q" pad="21"/>
<connect gate="A" pin="SETMAX" pad="12"/>
<connect gate="A" pin="SETMIN" pad="11"/>
<connect gate="A" pin="VBB" pad="6"/>
<connect gate="A" pin="VCC" pad="18"/>
<connect gate="A" pin="VCC_2" pad="13"/>
<connect gate="A" pin="VCC_3" pad="19"/>
<connect gate="A" pin="VCC_4" pad="22"/>
<connect gate="A" pin="VCF" pad="8"/>
<connect gate="A" pin="VEE" pad="28"/>
<connect gate="A" pin="VEE_2" pad="24"/>
<connect gate="A" pin="VEE_3" pad="9"/>
<connect gate="A" pin="VEF" pad="7"/>
<connect gate="A" pin="~CASCADE" pad="14"/>
<connect gate="A" pin="~EN" pad="16"/>
<connect gate="A" pin="~IN" pad="5"/>
<connect gate="A" pin="~Q" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP196FAG"/>
<attribute name="OC_FARNELL" value="1703312"/>
<attribute name="OC_NEWARK" value="88H4711"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP210SFAG" prefix="U">
<description>2.5V 1:5 Dual Differential LVDS Compatible Clock Driver</description>
<gates>
<gate name="A" symbol="MC100EP210SFAG"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="CLKA" pad="3"/>
<connect gate="A" pin="CLKB" pad="6"/>
<connect gate="A" pin="QA0" pad="31"/>
<connect gate="A" pin="QA1" pad="29"/>
<connect gate="A" pin="QA2" pad="27"/>
<connect gate="A" pin="QA3" pad="24"/>
<connect gate="A" pin="QA4" pad="22"/>
<connect gate="A" pin="QB0" pad="20"/>
<connect gate="A" pin="QB1" pad="18"/>
<connect gate="A" pin="QB2" pad="15"/>
<connect gate="A" pin="QB3" pad="13"/>
<connect gate="A" pin="QB4" pad="11"/>
<connect gate="A" pin="VCC" pad="25"/>
<connect gate="A" pin="VCC_2" pad="9"/>
<connect gate="A" pin="VCC_3" pad="16"/>
<connect gate="A" pin="VCC_4" pad="32"/>
<connect gate="A" pin="VEE" pad="8"/>
<connect gate="A" pin="VEE_2" pad="1"/>
<connect gate="A" pin="VTA" pad="2"/>
<connect gate="A" pin="VTB" pad="5"/>
<connect gate="A" pin="~CLKA" pad="4"/>
<connect gate="A" pin="~CLKB" pad="7"/>
<connect gate="A" pin="~QA0" pad="30"/>
<connect gate="A" pin="~QA1" pad="28"/>
<connect gate="A" pin="~QA2" pad="26"/>
<connect gate="A" pin="~QA3" pad="23"/>
<connect gate="A" pin="~QA4" pad="21"/>
<connect gate="A" pin="~QB0" pad="19"/>
<connect gate="A" pin="~QB1" pad="17"/>
<connect gate="A" pin="~QB2" pad="14"/>
<connect gate="A" pin="~QB3" pad="12"/>
<connect gate="A" pin="~QB4" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP210SFAG"/>
<attribute name="OC_FARNELL" value="1260024"/>
<attribute name="OC_NEWARK" value="26K3859"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP29DTG" prefix="U">
<description>D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC100EP29DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-20N">
<connects>
<connect gate="A" pin="CLK0" pad="4"/>
<connect gate="A" pin="CLK1" pad="6"/>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="8"/>
<connect gate="A" pin="Q0" pad="17"/>
<connect gate="A" pin="Q1" pad="15"/>
<connect gate="A" pin="R0" pad="19"/>
<connect gate="A" pin="R1" pad="12"/>
<connect gate="A" pin="S0" pad="18"/>
<connect gate="A" pin="S1" pad="13"/>
<connect gate="A" pin="VBB" pad="3"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="10"/>
<connect gate="A" pin="VEE" pad="11"/>
<connect gate="A" pin="~CLK0" pad="5"/>
<connect gate="A" pin="~CLK1" pad="7"/>
<connect gate="A" pin="~D1" pad="9"/>
<connect gate="A" pin="~DO" pad="2"/>
<connect gate="A" pin="~Q0" pad="16"/>
<connect gate="A" pin="~Q1" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP29DTG"/>
<attribute name="OC_FARNELL" value="1126231"/>
<attribute name="OC_NEWARK" value="42K0420"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP31DG" prefix="U">
<description>3.3V / 5V ECL D Flip-Flop with Set and Reset</description>
<gates>
<gate name="A" symbol="MC100EP31DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="RESET" pad="4"/>
<connect gate="A" pin="SET" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP31DG"/>
<attribute name="OC_FARNELL" value="1607711"/>
<attribute name="OC_NEWARK" value="26K3860"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP31DTG" prefix="U">
<description>D Flip-Flop with Set and Reset</description>
<gates>
<gate name="A" symbol="MC100EP31DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="RESET" pad="4"/>
<connect gate="A" pin="SET" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP31DTG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26K3861"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP32DG" prefix="U">
<description>3.3V / 5V ECL /2 Divider</description>
<gates>
<gate name="A" symbol="MC100EP32DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~CLK" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP32DG"/>
<attribute name="OC_FARNELL" value="1607663"/>
<attribute name="OC_NEWARK" value="42K0424"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP32DTG" prefix="U">
<description>3.3V / 5V ECL 2 Divider</description>
<gates>
<gate name="A" symbol="MC100EP32DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~CLK" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP32DTG"/>
<attribute name="OC_FARNELL" value="1607664"/>
<attribute name="OC_NEWARK" value="45J0943"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP33DTG" prefix="U">
<description>3.3V / 5V ECL 4 Divider</description>
<gates>
<gate name="A" symbol="MC100EP33DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~CLK" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP33DTG"/>
<attribute name="OC_FARNELL" value="1607919"/>
<attribute name="OC_NEWARK" value="45J0945"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP40DTG" prefix="U">
<description>Differential Phase-Frequency Detector</description>
<gates>
<gate name="A" symbol="MC100EP40DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-20N">
<connects>
<connect gate="A" pin="D" pad="17"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="NC" pad="12"/>
<connect gate="A" pin="PLD" pad="19"/>
<connect gate="A" pin="R" pad="6"/>
<connect gate="A" pin="U" pad="15"/>
<connect gate="A" pin="VBB" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="13"/>
<connect gate="A" pin="VCC_3" pad="18"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="VEE_2" pad="11"/>
<connect gate="A" pin="VTFB" pad="2"/>
<connect gate="A" pin="VTR" pad="8"/>
<connect gate="A" pin="~D" pad="16"/>
<connect gate="A" pin="~FB" pad="5"/>
<connect gate="A" pin="~R" pad="7"/>
<connect gate="A" pin="~U" pad="14"/>
<connect gate="A" pin="~VTFB" pad="3"/>
<connect gate="A" pin="~VTR" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP40DTG"/>
<attribute name="OC_FARNELL" value="1611370"/>
<attribute name="OC_NEWARK" value="42K0429"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP445FAG" prefix="U">
<description>ECL 8-Bit Serial/Parallel Converter</description>
<gates>
<gate name="A" symbol="MC100EP445FAG"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="CKSEL" pad="7"/>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="PCLK" pad="22"/>
<connect gate="A" pin="Q0" pad="21"/>
<connect gate="A" pin="Q1" pad="19"/>
<connect gate="A" pin="Q2" pad="18"/>
<connect gate="A" pin="Q3" pad="15"/>
<connect gate="A" pin="Q4" pad="14"/>
<connect gate="A" pin="Q5" pad="11"/>
<connect gate="A" pin="Q6" pad="10"/>
<connect gate="A" pin="Q7" pad="9"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="SINA" pad="31"/>
<connect gate="A" pin="SINB" pad="26"/>
<connect gate="A" pin="SINSEL" pad="25"/>
<connect gate="A" pin="SYNC" pad="2"/>
<connect gate="A" pin="VBB0" pad="29"/>
<connect gate="A" pin="VBB1" pad="6"/>
<connect gate="A" pin="VCC" pad="17"/>
<connect gate="A" pin="VCC_2" pad="8"/>
<connect gate="A" pin="VCC_3" pad="12"/>
<connect gate="A" pin="VCC_4" pad="20"/>
<connect gate="A" pin="VCC_5" pad="32"/>
<connect gate="A" pin="VCC_6" pad="13"/>
<connect gate="A" pin="VCC_7" pad="24"/>
<connect gate="A" pin="VEE" pad="16"/>
<connect gate="A" pin="VEE_2" pad="28"/>
<connect gate="A" pin="~CKEN" pad="3"/>
<connect gate="A" pin="~CLK" pad="5"/>
<connect gate="A" pin="~PCLK" pad="23"/>
<connect gate="A" pin="~SINA" pad="30"/>
<connect gate="A" pin="~SINB" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP445FAG"/>
<attribute name="OC_FARNELL" value="1260025"/>
<attribute name="OC_NEWARK" value="26K3865"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP446FAG" prefix="U">
<description>IC CONV 8BIT SER/PAR ECL</description>
<gates>
<gate name="A" symbol="MC100EP446FAG"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="CKEN" pad="7"/>
<connect gate="A" pin="CKSEL" pad="2"/>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="D0" pad="24"/>
<connect gate="A" pin="D1" pad="23"/>
<connect gate="A" pin="D2" pad="22"/>
<connect gate="A" pin="D3" pad="21"/>
<connect gate="A" pin="D4" pad="20"/>
<connect gate="A" pin="D5" pad="19"/>
<connect gate="A" pin="D6" pad="18"/>
<connect gate="A" pin="D7" pad="17"/>
<connect gate="A" pin="PCLK" pad="15"/>
<connect gate="A" pin="SOUT" pad="12"/>
<connect gate="A" pin="SYNC" pad="29"/>
<connect gate="A" pin="VBB1" pad="5"/>
<connect gate="A" pin="VBB2" pad="31"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="VCC_2" pad="32"/>
<connect gate="A" pin="VCC_3" pad="13"/>
<connect gate="A" pin="VCC_4" pad="9"/>
<connect gate="A" pin="VCC_5" pad="25"/>
<connect gate="A" pin="VCC_6" pad="1"/>
<connect gate="A" pin="VCF" pad="26"/>
<connect gate="A" pin="VEE" pad="16"/>
<connect gate="A" pin="VEE_2" pad="8"/>
<connect gate="A" pin="VEE_3" pad="28"/>
<connect gate="A" pin="VEF" pad="27"/>
<connect gate="A" pin="~CKEN" pad="6"/>
<connect gate="A" pin="~CLK" pad="4"/>
<connect gate="A" pin="~PCLK" pad="14"/>
<connect gate="A" pin="~SOUT" pad="11"/>
<connect gate="A" pin="~SYNC" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP446FAG"/>
<attribute name="OC_FARNELL" value="1703314"/>
<attribute name="OC_NEWARK" value="26K3867"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP451FAG" prefix="U">
<description>3.3V / 5V ECL 6-Bit Differential Register</description>
<gates>
<gate name="A" symbol="MC100EP451FAG"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="32"/>
<connect gate="A" pin="D2" pad="30"/>
<connect gate="A" pin="D3" pad="26"/>
<connect gate="A" pin="D4" pad="24"/>
<connect gate="A" pin="D5" pad="22"/>
<connect gate="A" pin="MR" pad="29"/>
<connect gate="A" pin="Q0" pad="7"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q2" pad="11"/>
<connect gate="A" pin="Q3" pad="14"/>
<connect gate="A" pin="Q4" pad="17"/>
<connect gate="A" pin="Q5" pad="20"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VCC_2" pad="16"/>
<connect gate="A" pin="VCC_3" pad="13"/>
<connect gate="A" pin="VEE" pad="28"/>
<connect gate="A" pin="VEE_2" pad="19"/>
<connect gate="A" pin="~CLK" pad="5"/>
<connect gate="A" pin="~D0" pad="3"/>
<connect gate="A" pin="~D1" pad="1"/>
<connect gate="A" pin="~D2" pad="31"/>
<connect gate="A" pin="~D3" pad="27"/>
<connect gate="A" pin="~D4" pad="25"/>
<connect gate="A" pin="~D5" pad="23"/>
<connect gate="A" pin="~Q0" pad="8"/>
<connect gate="A" pin="~Q1" pad="10"/>
<connect gate="A" pin="~Q2" pad="12"/>
<connect gate="A" pin="~Q3" pad="15"/>
<connect gate="A" pin="~Q4" pad="18"/>
<connect gate="A" pin="~Q5" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP451FAG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J0946"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP51DG" prefix="U">
<description>3.3V / 5V ECL D Flip-Flop with Reset and Differential Clock</description>
<gates>
<gate name="A" symbol="MC100EP51DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~CLK" pad="4"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP51DG"/>
<attribute name="OC_FARNELL" value="1607712"/>
<attribute name="OC_NEWARK" value="42K0433"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP51DTG" prefix="U">
<description>3.3V / 5V ECL D Flip-Flop with Reset and Differential  Clock</description>
<gates>
<gate name="A" symbol="MC100EP51DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~CLK" pad="4"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP51DTG"/>
<attribute name="OC_FARNELL" value="1354361"/>
<attribute name="OC_NEWARK" value="71J5411"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP56DTG" prefix="U">
<description>2:1 Multiplexer</description>
<gates>
<gate name="A" symbol="MC100EP56DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-20N">
<connects>
<connect gate="A" pin="COM_SEL" pad="16"/>
<connect gate="A" pin="D0A" pad="1"/>
<connect gate="A" pin="D0B" pad="4"/>
<connect gate="A" pin="D1A" pad="6"/>
<connect gate="A" pin="D1B" pad="9"/>
<connect gate="A" pin="Q0" pad="19"/>
<connect gate="A" pin="Q1" pad="13"/>
<connect gate="A" pin="SEL0" pad="17"/>
<connect gate="A" pin="SEL1" pad="15"/>
<connect gate="A" pin="VBB0" pad="3"/>
<connect gate="A" pin="VBB1" pad="8"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="14"/>
<connect gate="A" pin="VEE" pad="11"/>
<connect gate="A" pin="~D0A" pad="2"/>
<connect gate="A" pin="~D0B" pad="5"/>
<connect gate="A" pin="~D1A" pad="7"/>
<connect gate="A" pin="~D1B" pad="10"/>
<connect gate="A" pin="~Q0" pad="18"/>
<connect gate="A" pin="~Q1" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP56DTG"/>
<attribute name="OC_FARNELL" value="1607687"/>
<attribute name="OC_NEWARK" value="42K0438"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP56DWG" prefix="U">
<description>3.3V / 5V ECL Dual Differential 2:1 Multiplexer</description>
<gates>
<gate name="A" symbol="MC100EP56DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="COM_SEL" pad="16"/>
<connect gate="A" pin="D0A" pad="1"/>
<connect gate="A" pin="D0B" pad="4"/>
<connect gate="A" pin="D1A" pad="6"/>
<connect gate="A" pin="D1B" pad="9"/>
<connect gate="A" pin="Q0" pad="19"/>
<connect gate="A" pin="Q1" pad="13"/>
<connect gate="A" pin="SEL0" pad="17"/>
<connect gate="A" pin="SEL1" pad="15"/>
<connect gate="A" pin="VBB1" pad="8"/>
<connect gate="A" pin="VBBO" pad="3"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VCC_2" pad="20"/>
<connect gate="A" pin="VEE" pad="11"/>
<connect gate="A" pin="~D0A" pad="2"/>
<connect gate="A" pin="~D0B" pad="5"/>
<connect gate="A" pin="~D1A" pad="7"/>
<connect gate="A" pin="~D1B" pad="10"/>
<connect gate="A" pin="~Q0" pad="18"/>
<connect gate="A" pin="~Q1" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP56DWG"/>
<attribute name="OC_FARNELL" value="1607688"/>
<attribute name="OC_NEWARK" value="26K3870"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP57DTG" prefix="U">
<description>ECL 4:1 Differential Multiplexer</description>
<gates>
<gate name="A" symbol="MC100EP57DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-20N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="Q" pad="16"/>
<connect gate="A" pin="SEL0" pad="18"/>
<connect gate="A" pin="SEL1" pad="19"/>
<connect gate="A" pin="VBB1" pad="13"/>
<connect gate="A" pin="VBB2" pad="12"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="1"/>
<connect gate="A" pin="VCC_3" pad="14"/>
<connect gate="A" pin="VCC_4" pad="17"/>
<connect gate="A" pin="VEE" pad="11"/>
<connect gate="A" pin="VEE_2" pad="10"/>
<connect gate="A" pin="~D0" pad="3"/>
<connect gate="A" pin="~D1" pad="5"/>
<connect gate="A" pin="~D2" pad="7"/>
<connect gate="A" pin="~D3" pad="9"/>
<connect gate="A" pin="~Q" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP57DTG"/>
<attribute name="OC_FARNELL" value="1468710"/>
<attribute name="OC_NEWARK" value="71J5412"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP58DG" prefix="U">
<description>3.3V / 5V ECL 2:1 Multiplexer</description>
<gates>
<gate name="A" symbol="MC100EP58DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DA" pad="2"/>
<connect gate="A" pin="DB" pad="3"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="SEL" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP58DG"/>
<attribute name="OC_FARNELL" value="1150414"/>
<attribute name="OC_NEWARK" value="45J0947"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EP58DTG" prefix="U">
<description>3.3V / 5V ECL 2:1 Multiplexer</description>
<gates>
<gate name="A" symbol="MC100EP58DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="DA" pad="2"/>
<connect gate="A" pin="DB" pad="3"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="SEL" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EP58DTG"/>
<attribute name="OC_FARNELL" value="1150415"/>
<attribute name="OC_NEWARK" value="45J0949"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EPT20DG" prefix="U">
<description>3.3V LVTTL/LVCMOS to Differential LVPECL Translator</description>
<gates>
<gate name="A" symbol="MC100EPT20DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="6"/>
<connect gate="A" pin="Q" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~Q" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EPT20DG"/>
<attribute name="OC_FARNELL" value="1607865"/>
<attribute name="OC_NEWARK" value="45J0921"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EPT20DTG" prefix="U">
<description>TTL-CMOS-Differential-ECL-Translator</description>
<gates>
<gate name="A" symbol="MC100EPT20DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="4"/>
<connect gate="A" pin="Q" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~Q" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value=""/>
<attribute name="PACKAGE" value=""/>
<attribute name="SUPPLIER" value=""/>
</technology>
<technology name="TTL-CMOS-DIFFERENTIAL-ECL-TRANSLATOR">
<attribute name="MPN" value="MC100EPT20DTG"/>
<attribute name="OC_FARNELL" value="1192076"/>
<attribute name="OC_NEWARK" value="45J0922"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EPT22DG" prefix="U">
<description>3.3V Dual LVTTL/LVCMOS to Differential LVPECL Translator</description>
<gates>
<gate name="A" symbol="MC100EPT22DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D0" pad="7"/>
<connect gate="A" pin="D1" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EPT22DG"/>
<attribute name="OC_FARNELL" value="1607867"/>
<attribute name="OC_NEWARK" value="45J0924"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EPT22DTG" prefix="U">
<description>LVTTL/LVCMOS to Differential LVPECL Translator</description>
<gates>
<gate name="A" symbol="MC100EPT22DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D0" pad="7"/>
<connect gate="A" pin="D1" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EPT22DTG"/>
<attribute name="OC_FARNELL" value="1192078"/>
<attribute name="OC_NEWARK" value="45J0926"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EPT24DG" prefix="U">
<description>3.3V LVTTL/LVCMOS to Differential LVECL Translator</description>
<gates>
<gate name="A" symbol="MC100EPT24DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EPT24DG"/>
<attribute name="OC_FARNELL" value="1607871"/>
<attribute name="OC_NEWARK" value="45J0731"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EPT24DTG" prefix="U">
<description>LVTTL/LVCMOS to Differential LVECL Translator</description>
<gates>
<gate name="A" symbol="MC100EPT24DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EPT24DTG"/>
<attribute name="OC_FARNELL" value="1607872"/>
<attribute name="OC_NEWARK" value="45J0932"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EPT25DG" prefix="U">
<description>-3.3V / -5V Differential ECL to +3.3V LVTTL Translator</description>
<gates>
<gate name="A" symbol="MC100EPT25DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~D" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EPT25DG"/>
<attribute name="OC_FARNELL" value="1607873"/>
<attribute name="OC_NEWARK" value="45J0933"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EPT25DTG" prefix="U">
<description>Differential ECL to +3.3V LVTTL Translator</description>
<gates>
<gate name="A" symbol="MC100EPT25DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~D" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EPT25DTG"/>
<attribute name="OC_FARNELL" value="1192079"/>
<attribute name="OC_NEWARK" value="45J0934"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EPT26DG" prefix="U">
<description>3.3V 1:2 Fanout Differentia LVPECL/LVDS to LVTTL Translator</description>
<gates>
<gate name="A" symbol="MC100EPT26DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q0" pad="7"/>
<connect gate="A" pin="Q1" pad="6"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~D" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EPT26DG"/>
<attribute name="OC_FARNELL" value="1607874"/>
<attribute name="OC_NEWARK" value="42K0377"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100EPT26DTG" prefix="U">
<description>3.3V 1:2 Fanout Differential LVPECL/LVDS to LVTTL  Translator</description>
<gates>
<gate name="A" symbol="MC100EPT26DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q0" pad="7"/>
<connect gate="A" pin="Q1" pad="6"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~D" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100EPT26DTG"/>
<attribute name="OC_FARNELL" value="1209363"/>
<attribute name="OC_NEWARK" value="26K3838"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEL11DG" prefix="U">
<description>2.5V / 3.3V ECL 1:2 Differential Fanout Buffer</description>
<gates>
<gate name="A" symbol="MC100LVEL11DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="6"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEL11DG"/>
<attribute name="OC_FARNELL" value="1142207"/>
<attribute name="OC_NEWARK" value="71J5430"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEL11DR2G" prefix="U">
<description>1:2 Differential Fanout Buffer</description>
<gates>
<gate name="A" symbol="MC100LVEL11DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="6"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEL11DR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J0990"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEL11DTG" prefix="U">
<description>Differential Fanout Buffer</description>
<gates>
<gate name="A" symbol="MC100LVEL11DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="6"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEL11DTG"/>
<attribute name="OC_FARNELL" value="1364053"/>
<attribute name="OC_NEWARK" value="26K3898"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEL14DWG" prefix="U">
<description>3.3V ECL 1:5 Clock Distribution Chip</description>
<gates>
<gate name="A" symbol="MC100LVEL14DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="NC" pad="17"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="SEL" pad="12"/>
<connect gate="A" pin="VBB" pad="13"/>
<connect gate="A" pin="VCC" pad="18"/>
<connect gate="A" pin="VCC_2" pad="20"/>
<connect gate="A" pin="VEE" pad="11"/>
<connect gate="A" pin="~CLK" pad="14"/>
<connect gate="A" pin="~EN" pad="19"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
<connect gate="A" pin="~Q2" pad="6"/>
<connect gate="A" pin="~Q3" pad="8"/>
<connect gate="A" pin="~Q4" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEL14DWG"/>
<attribute name="OC_FARNELL" value="1192080"/>
<attribute name="OC_NEWARK" value="98H0640"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEL16DG" prefix="U">
<description>3.3V ECL Differential Receiver</description>
<gates>
<gate name="A" symbol="MC100LVEL16DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEL16DG"/>
<attribute name="OC_FARNELL" value="1192081"/>
<attribute name="OC_NEWARK" value="98H0642"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEL16DTG" prefix="U">
<description>ECL Differential Receiver</description>
<gates>
<gate name="A" symbol="MC100LVEL16DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEL16DTG"/>
<attribute name="OC_FARNELL" value="1607608"/>
<attribute name="OC_NEWARK" value="26K3900"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEL29DWG" prefix="U">
<description>D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC100LVEL29DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="CLK0" pad="3"/>
<connect gate="A" pin="CLK1" pad="8"/>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="6"/>
<connect gate="A" pin="Q0" pad="18"/>
<connect gate="A" pin="Q1" pad="13"/>
<connect gate="A" pin="R0" pad="20"/>
<connect gate="A" pin="R1" pad="10"/>
<connect gate="A" pin="S0" pad="16"/>
<connect gate="A" pin="S1" pad="15"/>
<connect gate="A" pin="VBB" pad="5"/>
<connect gate="A" pin="VCC" pad="19"/>
<connect gate="A" pin="VCC_2" pad="14"/>
<connect gate="A" pin="VEE" pad="11"/>
<connect gate="A" pin="~CLK0" pad="4"/>
<connect gate="A" pin="~CLK1" pad="9"/>
<connect gate="A" pin="~D0" pad="2"/>
<connect gate="A" pin="~D1" pad="7"/>
<connect gate="A" pin="~Q0" pad="17"/>
<connect gate="A" pin="~Q1" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEL29DWG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="98H0645"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEL51DG" prefix="U">
<description>3.3V ECL Differential Clock D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC100LVEL51DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="R" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~CLK" pad="4"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEL51DG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26K3911"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEL90DWG" prefix="U">
<description>Output Translator</description>
<gates>
<gate name="A" symbol="MC100LVEL90DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="5"/>
<connect gate="A" pin="D2" pad="8"/>
<connect gate="A" pin="ECLVBB" pad="7"/>
<connect gate="A" pin="ECLVBB_2" pad="4"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="14"/>
<connect gate="A" pin="Q0" pad="19"/>
<connect gate="A" pin="Q0_2" pad="18"/>
<connect gate="A" pin="Q1" pad="15"/>
<connect gate="A" pin="Q1_2" pad="16"/>
<connect gate="A" pin="Q2" pad="12"/>
<connect gate="A" pin="Q2_2" pad="13"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="1"/>
<connect gate="A" pin="VCC_3" pad="11"/>
<connect gate="A" pin="VEE" pad="10"/>
<connect gate="A" pin="~D0" pad="3"/>
<connect gate="A" pin="~D1" pad="6"/>
<connect gate="A" pin="~D2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEL90DWG"/>
<attribute name="OC_FARNELL" value="1607875"/>
<attribute name="OC_NEWARK" value="26K3916"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEL91DWG" prefix="U">
<description>Output Translator</description>
<gates>
<gate name="A" symbol="MC100LVEL91DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="5"/>
<connect gate="A" pin="D2" pad="8"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="14"/>
<connect gate="A" pin="PECLVBB" pad="4"/>
<connect gate="A" pin="PECLVBB_2" pad="7"/>
<connect gate="A" pin="Q0" pad="19"/>
<connect gate="A" pin="Q1" pad="16"/>
<connect gate="A" pin="Q2" pad="13"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="1"/>
<connect gate="A" pin="VCC_3" pad="11"/>
<connect gate="A" pin="VEE" pad="10"/>
<connect gate="A" pin="~D0" pad="3"/>
<connect gate="A" pin="~D1" pad="6"/>
<connect gate="A" pin="~D2" pad="9"/>
<connect gate="A" pin="~Q0" pad="18"/>
<connect gate="A" pin="~Q1" pad="15"/>
<connect gate="A" pin="~Q2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEL91DWG"/>
<attribute name="OC_FARNELL" value="1468712"/>
<attribute name="OC_NEWARK" value="26K3918"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEL92DWG" prefix="U">
<description>5V Triple PECL Input to LVPECL Output Translator</description>
<gates>
<gate name="A" symbol="MC100LVEL92DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="5"/>
<connect gate="A" pin="D2" pad="8"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="LVCC" pad="14"/>
<connect gate="A" pin="LVCC_2" pad="17"/>
<connect gate="A" pin="Q0" pad="19"/>
<connect gate="A" pin="Q1" pad="16"/>
<connect gate="A" pin="Q2" pad="13"/>
<connect gate="A" pin="VBB_PECL" pad="4"/>
<connect gate="A" pin="VBB_PECL_2" pad="7"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="1"/>
<connect gate="A" pin="VCC_3" pad="11"/>
<connect gate="A" pin="~D0" pad="3"/>
<connect gate="A" pin="~D1" pad="6"/>
<connect gate="A" pin="~D2" pad="9"/>
<connect gate="A" pin="~Q0" pad="18"/>
<connect gate="A" pin="~Q1" pad="15"/>
<connect gate="A" pin="~Q2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEL92DWG"/>
<attribute name="OC_FARNELL" value="1155551"/>
<attribute name="OC_NEWARK" value="71J5440"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVELT22DG" prefix="U">
<description>3.3V Dual LVTTL/LVCMOS to Differential LVPECL Translator</description>
<gates>
<gate name="A" symbol="MC100LVELT22DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D0" pad="7"/>
<connect gate="A" pin="D1" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVELT22DG"/>
<attribute name="OC_FARNELL" value="1468713"/>
<attribute name="OC_NEWARK" value="45J0984"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVELT22DTG" prefix="U">
<description>Dual Differential LVPECL/LVDS to LVTTL Translator</description>
<gates>
<gate name="A" symbol="MC100LVELT22DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D0" pad="7"/>
<connect gate="A" pin="D1" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVELT22DTG"/>
<attribute name="OC_FARNELL" value="1150428"/>
<attribute name="OC_NEWARK" value="45J0986"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVELT23DTG" prefix="U">
<description>Dual Differential LVPECL/LVDS to LVTTL Translator</description>
<gates>
<gate name="A" symbol="MC100LVELT23DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="Q0" pad="7"/>
<connect gate="A" pin="Q1" pad="6"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~D0" pad="2"/>
<connect gate="A" pin="~D1" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVELT23DTG"/>
<attribute name="OC_FARNELL" value="1258374"/>
<attribute name="OC_NEWARK" value="42K0472"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEP111FAG" prefix="U">
<description>Differential ECL/PECL/HSTL Clock Driver</description>
<gates>
<gate name="A" symbol="MC100LVEP111FAG"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="CLK0" pad="3"/>
<connect gate="A" pin="CLK1" pad="6"/>
<connect gate="A" pin="CLK_SEL" pad="2"/>
<connect gate="A" pin="Q0" pad="31"/>
<connect gate="A" pin="Q1" pad="29"/>
<connect gate="A" pin="Q2" pad="27"/>
<connect gate="A" pin="Q3" pad="24"/>
<connect gate="A" pin="Q4" pad="22"/>
<connect gate="A" pin="Q5" pad="20"/>
<connect gate="A" pin="Q6" pad="18"/>
<connect gate="A" pin="Q7" pad="15"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="Q9" pad="11"/>
<connect gate="A" pin="VBB" pad="5"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VCC_2" pad="32"/>
<connect gate="A" pin="VCC_3" pad="1"/>
<connect gate="A" pin="VCC_4" pad="25"/>
<connect gate="A" pin="VCC_5" pad="16"/>
<connect gate="A" pin="VEE" pad="8"/>
<connect gate="A" pin="~CLK0" pad="4"/>
<connect gate="A" pin="~CLK1" pad="7"/>
<connect gate="A" pin="~Q0" pad="30"/>
<connect gate="A" pin="~Q1" pad="28"/>
<connect gate="A" pin="~Q2" pad="26"/>
<connect gate="A" pin="~Q3" pad="23"/>
<connect gate="A" pin="~Q4" pad="21"/>
<connect gate="A" pin="~Q5" pad="19"/>
<connect gate="A" pin="~Q6" pad="17"/>
<connect gate="A" pin="~Q7" pad="14"/>
<connect gate="A" pin="~Q8" pad="12"/>
<connect gate="A" pin="~Q9" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEP111FAG"/>
<attribute name="OC_FARNELL" value="1607921"/>
<attribute name="OC_NEWARK" value="98H0648"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEP11DG" prefix="U">
<description>2.5V / 3.3V ECL 1:2 Differential Fanout Buffer</description>
<gates>
<gate name="A" symbol="MC100LVEP11DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="6"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEP11DG"/>
<attribute name="OC_FARNELL" value="1199235"/>
<attribute name="OC_NEWARK" value="26K3919"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEP11DTG" prefix="U">
<description>Buffer</description>
<gates>
<gate name="A" symbol="MC100LVEP11DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="6"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEP11DTG"/>
<attribute name="OC_FARNELL" value="1155552"/>
<attribute name="OC_NEWARK" value="71J5441"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEP14DTG" prefix="U">
<description>Differential ECL/PECL/HSTL Clock Driver</description>
<gates>
<gate name="A" symbol="MC100LVEP14DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-20N">
<connects>
<connect gate="A" pin="CLK0" pad="13"/>
<connect gate="A" pin="CLK1" pad="16"/>
<connect gate="A" pin="CLK_SEL" pad="12"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="VBB" pad="15"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCC_2" pad="18"/>
<connect gate="A" pin="VEE" pad="11"/>
<connect gate="A" pin="~CLK0" pad="14"/>
<connect gate="A" pin="~CLK1" pad="17"/>
<connect gate="A" pin="~EN" pad="19"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
<connect gate="A" pin="~Q2" pad="6"/>
<connect gate="A" pin="~Q3" pad="8"/>
<connect gate="A" pin="~Q4" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEP14DTG"/>
<attribute name="OC_FARNELL" value="1468715"/>
<attribute name="OC_NEWARK" value="42K0489"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC100LVEP16DTG" prefix="U">
<description>ECL Differential Receiver/Driver</description>
<gates>
<gate name="A" symbol="MC100LVEP16DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC100LVEP16DTG"/>
<attribute name="OC_FARNELL" value="1607609"/>
<attribute name="OC_NEWARK" value="71J5443"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10E016FNG" prefix="U">
<description>Synchronous Binary Up Counter</description>
<gates>
<gate name="A" symbol="MC10E016FNG"/>
</gates>
<devices>
<device name="" package="PLCC127P1257X1257X457-28N">
<connects>
<connect gate="A" pin="CLK" pad="27"/>
<connect gate="A" pin="MR" pad="26"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="P0" pad="3"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="5"/>
<connect gate="A" pin="P3" pad="6"/>
<connect gate="A" pin="P4" pad="7"/>
<connect gate="A" pin="P5" pad="21"/>
<connect gate="A" pin="P6" pad="22"/>
<connect gate="A" pin="P7" pad="23"/>
<connect gate="A" pin="Q0" pad="9"/>
<connect gate="A" pin="Q1" pad="10"/>
<connect gate="A" pin="Q2" pad="11"/>
<connect gate="A" pin="Q3" pad="12"/>
<connect gate="A" pin="Q4" pad="13"/>
<connect gate="A" pin="Q5" pad="15"/>
<connect gate="A" pin="Q6" pad="17"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="A" pin="TCLD" pad="28"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VCCO" pad="20"/>
<connect gate="A" pin="VCCO_2" pad="8"/>
<connect gate="A" pin="VCCO_3" pad="14"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~CE" pad="24"/>
<connect gate="A" pin="~PE" pad="25"/>
<connect gate="A" pin="~TC" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10E016FNG"/>
<attribute name="OC_FARNELL" value="1468717"/>
<attribute name="OC_NEWARK" value="26K3738"/>
<attribute name="PACKAGE" value="PLCC-28"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EL01DG" prefix="U">
<description>5V ECL 4-Input OR/NOR</description>
<gates>
<gate name="A" symbol="MC10EL01DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="D3" pad="4"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EL01DG"/>
<attribute name="OC_FARNELL" value="1468718"/>
<attribute name="OC_NEWARK" value="45J0833"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EL04DG" prefix="U">
<description>5V ECL 2-Input AND/NAND</description>
<gates>
<gate name="A" symbol="MC10EL04DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EL04DG"/>
<attribute name="OC_FARNELL" value="1468719"/>
<attribute name="OC_NEWARK" value="98H0612"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EL16DG" prefix="U">
<description>5.0 V ECL Differential Receiver</description>
<gates>
<gate name="A" symbol="MC10EL16DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EL16DG"/>
<attribute name="OC_FARNELL" value="1607876"/>
<attribute name="OC_NEWARK" value="71J5370"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EL16DR2G" prefix="U">
<description>5.0 V ECL Differential Receiver</description>
<gates>
<gate name="A" symbol="MC10EL16DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EL16DR2G"/>
<attribute name="OC_FARNELL" value="1607877"/>
<attribute name="OC_NEWARK" value="83H7289"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EL31DG" prefix="U">
<description>5 V ECL D Flip-Flop With Set and Reset</description>
<gates>
<gate name="A" symbol="MC10EL31DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="R" pad="4"/>
<connect gate="A" pin="S" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EL31DG"/>
<attribute name="OC_FARNELL" value="1607713"/>
<attribute name="OC_NEWARK" value="98H0615"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EL89DG" prefix="U">
<description>5V ECL Coaxial Cable Driver</description>
<gates>
<gate name="A" symbol="MC10EL89DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="6"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EL89DG"/>
<attribute name="OC_FARNELL" value="1192083"/>
<attribute name="OC_NEWARK" value="45J0841"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10ELT20DG" prefix="U">
<description>5V TTL to Differential PECL Translator</description>
<gates>
<gate name="A" symbol="MC10ELT20DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="NC_3" pad="4"/>
<connect gate="A" pin="Q" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~Q" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10ELT20DG"/>
<attribute name="OC_FARNELL" value="1607878"/>
<attribute name="OC_NEWARK" value="88H4693"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10ELT21DG" prefix="U">
<description>5 V Differential PECL to TTL Translator</description>
<gates>
<gate name="A" symbol="MC10ELT21DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="Q0" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~D0" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10ELT21DG"/>
<attribute name="OC_FARNELL" value="1607879"/>
<attribute name="OC_NEWARK" value="98H0610"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10ELT22DG" prefix="U">
<description>5.0 V Dual TTL to Differential PECL Translator</description>
<gates>
<gate name="A" symbol="MC10ELT22DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D0" pad="7"/>
<connect gate="A" pin="D1" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10ELT22DG"/>
<attribute name="OC_FARNELL" value="1155782"/>
<attribute name="OC_NEWARK" value="98H0611"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10ELT24DG" prefix="U">
<description>5V TTL to Differential ECL Translator</description>
<gates>
<gate name="A" symbol="MC10ELT24DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10ELT24DG"/>
<attribute name="OC_FARNELL" value="1607880"/>
<attribute name="OC_NEWARK" value="88H4695"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10ELT25DG" prefix="U">
<description>-5 V Differential ECL to TTL Translator</description>
<gates>
<gate name="A" symbol="MC10ELT25DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~D" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10ELT25DG"/>
<attribute name="OC_FARNELL" value="1607882"/>
<attribute name="OC_NEWARK" value="88H4696"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10ELT25DTG" prefix="U">
<description>ECL to TTL Translator</description>
<gates>
<gate name="A" symbol="MC10ELT25DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="1"/>
<connect gate="A" pin="~D" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10ELT25DTG"/>
<attribute name="OC_FARNELL" value="1147688"/>
<attribute name="OC_NEWARK" value="42K0043"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10ELT28DG" prefix="U">
<description>5 V TTL to Differential PECL and Differential PECL to TTL Translator</description>
<gates>
<gate name="A" symbol="MC10ELT28DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DECL" pad="1"/>
<connect gate="A" pin="DTTL" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="QECL" pad="3"/>
<connect gate="A" pin="QTTL" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DECL" pad="2"/>
<connect gate="A" pin="~QECL" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10ELT28DG"/>
<attribute name="OC_FARNELL" value="1263934"/>
<attribute name="OC_NEWARK" value="26K3714"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EP05DG" prefix="U">
<description>3.3V / 5V ECL 2-Input Differential AND/NAND</description>
<gates>
<gate name="A" symbol="MC10EP05DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D0" pad="2"/>
<connect gate="A" pin="~D1" pad="4"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EP05DG"/>
<attribute name="OC_FARNELL" value="1607764"/>
<attribute name="OC_NEWARK" value="45J0843"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EP16DG" prefix="U">
<description>ECL Differential Receiver/Driver</description>
<gates>
<gate name="A" symbol="MC10EP16DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EP16DG"/>
<attribute name="OC_FARNELL" value="1607766"/>
<attribute name="OC_NEWARK" value="45J0847"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EP16DTG" prefix="U">
<description>Differential Receiver/Driver</description>
<gates>
<gate name="A" symbol="MC10EP16DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EP16DTG"/>
<attribute name="OC_FARNELL" value="1611398"/>
<attribute name="OC_NEWARK" value="26K3728"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EP195FAG" prefix="U">
<description>3.3V ECL Programmable Delay Chip</description>
<gates>
<gate name="A" symbol="MC10EP195FAG"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="CASCADE" pad="15"/>
<connect gate="A" pin="D0" pad="23"/>
<connect gate="A" pin="D1" pad="25"/>
<connect gate="A" pin="D10" pad="3"/>
<connect gate="A" pin="D2" pad="26"/>
<connect gate="A" pin="D3" pad="27"/>
<connect gate="A" pin="D4" pad="29"/>
<connect gate="A" pin="D5" pad="30"/>
<connect gate="A" pin="D6" pad="31"/>
<connect gate="A" pin="D7" pad="32"/>
<connect gate="A" pin="D8" pad="1"/>
<connect gate="A" pin="D9" pad="2"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="LEN" pad="10"/>
<connect gate="A" pin="NC" pad="17"/>
<connect gate="A" pin="Q" pad="21"/>
<connect gate="A" pin="SETMAX" pad="12"/>
<connect gate="A" pin="SETMIN" pad="11"/>
<connect gate="A" pin="VBB" pad="6"/>
<connect gate="A" pin="VCC" pad="18"/>
<connect gate="A" pin="VCC_2" pad="22"/>
<connect gate="A" pin="VCC_3" pad="19"/>
<connect gate="A" pin="VCC_4" pad="13"/>
<connect gate="A" pin="VCF" pad="8"/>
<connect gate="A" pin="VEE" pad="28"/>
<connect gate="A" pin="VEE_2" pad="9"/>
<connect gate="A" pin="VEE_3" pad="24"/>
<connect gate="A" pin="VEF" pad="7"/>
<connect gate="A" pin="~CASCADE" pad="14"/>
<connect gate="A" pin="~EN" pad="16"/>
<connect gate="A" pin="~IN" pad="5"/>
<connect gate="A" pin="~Q" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EP195FAG"/>
<attribute name="OC_FARNELL" value="1258225"/>
<attribute name="OC_NEWARK" value="26K3730"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EP31DG" prefix="U">
<description>3.3V / 5V ECL D Flip-Flop with Set and Reset</description>
<gates>
<gate name="A" symbol="MC10EP31DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="RESET" pad="4"/>
<connect gate="A" pin="SET" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EP31DG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J0849"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10EP32DTG" prefix="U">
<description>ECL by 2 Divider</description>
<gates>
<gate name="A" symbol="MC10EP32DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~CLK" pad="3"/>
<connect gate="A" pin="~Q" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10EP32DTG"/>
<attribute name="OC_FARNELL" value="1258226"/>
<attribute name="OC_NEWARK" value="26K3732"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10H101PG" prefix="U">
<description>Quad OR/NOR Gate</description>
<gates>
<gate name="A" symbol="MC10H101PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="AIN" pad="4"/>
<connect gate="A" pin="AOUT" pad="5"/>
<connect gate="A" pin="BIN" pad="7"/>
<connect gate="A" pin="BOUT" pad="6"/>
<connect gate="A" pin="CIN" pad="10"/>
<connect gate="A" pin="COM_IN" pad="12"/>
<connect gate="A" pin="COUT" pad="11"/>
<connect gate="A" pin="DIN" pad="13"/>
<connect gate="A" pin="DOUT" pad="9"/>
<connect gate="A" pin="VCC1" pad="1"/>
<connect gate="A" pin="VCC2" pad="16"/>
<connect gate="A" pin="VEE" pad="8"/>
<connect gate="A" pin="~AOUT" pad="2"/>
<connect gate="A" pin="~BOUT" pad="3"/>
<connect gate="A" pin="~COUT" pad="14"/>
<connect gate="A" pin="~DOUT" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10H101PG"/>
<attribute name="OC_FARNELL" value="1354350"/>
<attribute name="OC_NEWARK" value="45J0861"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10H102PG" prefix="U">
<description>Quad 2-Input NOR Gate</description>
<gates>
<gate name="A" symbol="MC10H102PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="AIN" pad="4"/>
<connect gate="A" pin="AIN_2" pad="5"/>
<connect gate="A" pin="BIN" pad="7"/>
<connect gate="A" pin="BIN_2" pad="6"/>
<connect gate="A" pin="CIN" pad="10"/>
<connect gate="A" pin="CIN_2" pad="11"/>
<connect gate="A" pin="DIN" pad="12"/>
<connect gate="A" pin="DIN_2" pad="13"/>
<connect gate="A" pin="DOUT" pad="9"/>
<connect gate="A" pin="VCC1" pad="1"/>
<connect gate="A" pin="VCC2" pad="16"/>
<connect gate="A" pin="VEE" pad="8"/>
<connect gate="A" pin="~AOUT" pad="2"/>
<connect gate="A" pin="~BOUT" pad="3"/>
<connect gate="A" pin="~COUT" pad="14"/>
<connect gate="A" pin="~DOUT" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10H102PG"/>
<attribute name="OC_FARNELL" value="1354351"/>
<attribute name="OC_NEWARK" value="45J0862"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10H105PG" prefix="U">
<description>Triple 2-3-2-Input OR/NOR Gate</description>
<gates>
<gate name="A" symbol="MC10H105PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="AIN" pad="4"/>
<connect gate="A" pin="AIN_2" pad="5"/>
<connect gate="A" pin="AOUT" pad="2"/>
<connect gate="A" pin="BIN" pad="10"/>
<connect gate="A" pin="BIN_2" pad="9"/>
<connect gate="A" pin="BIN_3" pad="11"/>
<connect gate="A" pin="BOUT" pad="7"/>
<connect gate="A" pin="BOUT_2" pad="6"/>
<connect gate="A" pin="CIN" pad="12"/>
<connect gate="A" pin="CIN_2" pad="13"/>
<connect gate="A" pin="COUT" pad="15"/>
<connect gate="A" pin="VCC1" pad="1"/>
<connect gate="A" pin="VCC2" pad="16"/>
<connect gate="A" pin="VEE" pad="8"/>
<connect gate="A" pin="~AOUT" pad="3"/>
<connect gate="A" pin="~COUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10H105PG"/>
<attribute name="OC_FARNELL" value="1147790"/>
<attribute name="OC_NEWARK" value="45J0866"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10H116DG" prefix="U">
<description>Triple Line Receiver</description>
<gates>
<gate name="A" symbol="MC10H116DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="AIN" pad="5"/>
<connect gate="A" pin="AOUT" pad="3"/>
<connect gate="A" pin="BIN" pad="10"/>
<connect gate="A" pin="BOUT" pad="7"/>
<connect gate="A" pin="CIN" pad="13"/>
<connect gate="A" pin="COUT" pad="15"/>
<connect gate="A" pin="VBB" pad="11"/>
<connect gate="A" pin="VCC1" pad="1"/>
<connect gate="A" pin="VCC2" pad="16"/>
<connect gate="A" pin="VEE" pad="8"/>
<connect gate="A" pin="~AIN" pad="4"/>
<connect gate="A" pin="~AOUT" pad="2"/>
<connect gate="A" pin="~BIN" pad="9"/>
<connect gate="A" pin="~BOUT" pad="6"/>
<connect gate="A" pin="~CIN" pad="12"/>
<connect gate="A" pin="~COUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10H116DG"/>
<attribute name="OC_FARNELL" value="1607610"/>
<attribute name="OC_NEWARK" value="26K3776"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10H124PG" prefix="U">
<description>Quad TTL-to-MECL Translator With TTL Strobe Input</description>
<gates>
<gate name="A" symbol="MC10H124PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="AIN" pad="5"/>
<connect gate="A" pin="AOUT" pad="2"/>
<connect gate="A" pin="BIN" pad="7"/>
<connect gate="A" pin="BOUT" pad="1"/>
<connect gate="A" pin="CIN" pad="10"/>
<connect gate="A" pin="COMMON_STROBE" pad="6"/>
<connect gate="A" pin="COUT" pad="15"/>
<connect gate="A" pin="DIN" pad="11"/>
<connect gate="A" pin="DOUT" pad="14"/>
<connect gate="A" pin="GND" pad="16"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VEE" pad="8"/>
<connect gate="A" pin="~AOUT" pad="4"/>
<connect gate="A" pin="~BOUT" pad="3"/>
<connect gate="A" pin="~COUT" pad="12"/>
<connect gate="A" pin="~DOUT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10H124PG"/>
<attribute name="OC_FARNELL" value="1607885"/>
<attribute name="OC_NEWARK" value="98H0625"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10H125PG" prefix="U">
<description>Quad MECL-to-TTL Translator</description>
<gates>
<gate name="A" symbol="MC10H125PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="AIN" pad="3"/>
<connect gate="A" pin="AOUT" pad="4"/>
<connect gate="A" pin="BIN" pad="7"/>
<connect gate="A" pin="BOUT" pad="5"/>
<connect gate="A" pin="CIN" pad="11"/>
<connect gate="A" pin="COUT" pad="12"/>
<connect gate="A" pin="DIN" pad="15"/>
<connect gate="A" pin="DOUT" pad="13"/>
<connect gate="A" pin="GND" pad="16"/>
<connect gate="A" pin="VBB" pad="1"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VEE" pad="8"/>
<connect gate="A" pin="~AIN" pad="2"/>
<connect gate="A" pin="~BIN" pad="6"/>
<connect gate="A" pin="~CIN" pad="10"/>
<connect gate="A" pin="~DIN" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10H125PG"/>
<attribute name="OC_FARNELL" value="1607887"/>
<attribute name="OC_NEWARK" value="45J0876"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10H131PG" prefix="U">
<description>Dual D Type Master-Slave Flip-Flop</description>
<gates>
<gate name="A" symbol="MC10H131PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CC" pad="9"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D2" pad="10"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="15"/>
<connect gate="A" pin="R1" pad="4"/>
<connect gate="A" pin="R2" pad="13"/>
<connect gate="A" pin="S1" pad="5"/>
<connect gate="A" pin="S2" pad="12"/>
<connect gate="A" pin="VCC1" pad="1"/>
<connect gate="A" pin="VCC2" pad="16"/>
<connect gate="A" pin="VEE" pad="8"/>
<connect gate="A" pin="~CE1" pad="6"/>
<connect gate="A" pin="~CE2" pad="11"/>
<connect gate="A" pin="~Q1" pad="3"/>
<connect gate="A" pin="~Q2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10H131PG"/>
<attribute name="OC_FARNELL" value="1468724"/>
<attribute name="OC_NEWARK" value="45J0879"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC10H136PG" prefix="U">
<description>Universal Hexadecimal Counter</description>
<gates>
<gate name="A" symbol="MC10H136PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CLOCK" pad="13"/>
<connect gate="A" pin="D0" pad="12"/>
<connect gate="A" pin="D1" pad="11"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="Q0" pad="14"/>
<connect gate="A" pin="Q1" pad="15"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="3"/>
<connect gate="A" pin="S1" pad="9"/>
<connect gate="A" pin="S2" pad="7"/>
<connect gate="A" pin="VCC1" pad="1"/>
<connect gate="A" pin="VCC2" pad="16"/>
<connect gate="A" pin="VEE" pad="8"/>
<connect gate="A" pin="~CIN" pad="10"/>
<connect gate="A" pin="~COUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC10H136PG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J0882"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC12026ADG" prefix="U">
<description>1.1 GHz Dual Modulus Prescaler</description>
<gates>
<gate name="A" symbol="MC12026ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="MC" pad="6"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="~IN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC12026ADG"/>
<attribute name="OC_FARNELL" value="1468725"/>
<attribute name="OC_NEWARK" value="45J1002"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC12080DG" prefix="U">
<description>1.1 GHz Prescaler</description>
<gates>
<gate name="A" symbol="MC12080DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="SW1" pad="3"/>
<connect gate="A" pin="SW2" pad="6"/>
<connect gate="A" pin="SW3" pad="7"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="~IN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC12080DG"/>
<attribute name="OC_FARNELL" value="1607924"/>
<attribute name="OC_NEWARK" value="45J1004"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC12093DG" prefix="U">
<description>÷2, ÷4, ÷8 1.1 GHz Low Power Prescaler with Stand-By Mode</description>
<gates>
<gate name="A" symbol="MC12093DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="SB" pad="7"/>
<connect gate="A" pin="SW1" pad="6"/>
<connect gate="A" pin="SW2" pad="3"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="~IN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC12093DG"/>
<attribute name="OC_FARNELL" value="1607925"/>
<attribute name="OC_NEWARK" value="45J1005"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC12095DG" prefix="U">
<description>2.5 GHz Low Power Prescaler With Stand-By Mode</description>
<gates>
<gate name="A" symbol="MC12095DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="SB" pad="7"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="~IN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC12095DG"/>
<attribute name="OC_FARNELL" value="1607926"/>
<attribute name="OC_NEWARK" value="45J1006"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14001BCPG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14001BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="4"/>
<connect gate="A" pin="OUT_C" pad="10"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14001BCPG"/>
<attribute name="OC_FARNELL" value="9665455"/>
<attribute name="OC_NEWARK" value="45J1007"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14001BDG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14001BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14001BDG"/>
<attribute name="OC_FARNELL" value="9666303"/>
<attribute name="OC_NEWARK" value="26K3924"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14001UBCPG" prefix="U">
<description>CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14001UBCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUT_C" pad="10"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14001UBCPG"/>
<attribute name="OC_FARNELL" value="1211173"/>
<attribute name="OC_NEWARK" value="45J1009"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14001UBDG" prefix="U">
<description>UB-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14001UBDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14001UBDG"/>
<attribute name="OC_FARNELL" value="1191820"/>
<attribute name="OC_NEWARK" value="97K4601"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14007UBDG" prefix="U">
<description>Dual Complementary Pair Plus Inverter</description>
<gates>
<gate name="A" symbol="MC14007UBDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="D-NA" pad="8"/>
<connect gate="A" pin="D-NB" pad="5"/>
<connect gate="A" pin="D-PA" pad="13"/>
<connect gate="A" pin="D-PB" pad="1"/>
<connect gate="A" pin="GATEA" pad="6"/>
<connect gate="A" pin="GATEB" pad="3"/>
<connect gate="A" pin="GATEC" pad="10"/>
<connect gate="A" pin="OUTC" pad="12"/>
<connect gate="A" pin="S-NB" pad="4"/>
<connect gate="A" pin="S-NC" pad="9"/>
<connect gate="A" pin="S-PB" pad="2"/>
<connect gate="A" pin="S-PC" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14007UBDG"/>
<attribute name="OC_FARNELL" value="9665110"/>
<attribute name="OC_NEWARK" value="26K3925"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14008BCPG" prefix="U">
<description>4-Bit Full Adder</description>
<gates>
<gate name="A" symbol="MC14008BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A1" pad="7"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="3"/>
<connect gate="A" pin="A4" pad="1"/>
<connect gate="A" pin="B1" pad="6"/>
<connect gate="A" pin="B2" pad="4"/>
<connect gate="A" pin="B3" pad="2"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="CIN" pad="9"/>
<connect gate="A" pin="COUT" pad="14"/>
<connect gate="A" pin="S1" pad="10"/>
<connect gate="A" pin="S2" pad="11"/>
<connect gate="A" pin="S3" pad="12"/>
<connect gate="A" pin="S4" pad="13"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14008BCPG"/>
<attribute name="OC_FARNELL" value="9665757"/>
<attribute name="OC_NEWARK" value="45J1013"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14011BCPG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14011BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14011BCPG"/>
<attribute name="OC_FARNELL" value="9665463"/>
<attribute name="OC_NEWARK" value="45J1014"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14011BDG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14011BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14011BDG"/>
<attribute name="OC_FARNELL" value="9666311"/>
<attribute name="OC_NEWARK" value="26K3926"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14011BDR2G" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14011BDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14011BDR2G"/>
<attribute name="OC_FARNELL" value="1273009"/>
<attribute name="OC_NEWARK" value="45J1015"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14011UBCPG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14011UBCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14011UBCPG"/>
<attribute name="OC_FARNELL" value="1468726"/>
<attribute name="OC_NEWARK" value="45J1016"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14011UBDG" prefix="U">
<description>UB-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14011UBDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14011UBDG"/>
<attribute name="OC_FARNELL" value="1353832"/>
<attribute name="OC_NEWARK" value="42K0501"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14012BCPG" prefix="U">
<description>Dual 4-Input NAND Gates</description>
<gates>
<gate name="A" symbol="MC14012BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN1A" pad="2"/>
<connect gate="A" pin="IN1B" pad="9"/>
<connect gate="A" pin="IN2A" pad="3"/>
<connect gate="A" pin="IN2B" pad="10"/>
<connect gate="A" pin="IN3A" pad="4"/>
<connect gate="A" pin="IN3B" pad="11"/>
<connect gate="A" pin="IN4A" pad="5"/>
<connect gate="A" pin="IN4B" pad="12"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="13"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14012BCPG"/>
<attribute name="OC_FARNELL" value="9664572"/>
<attribute name="OC_NEWARK" value="45J1017"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14012BDG" prefix="U">
<description>Dual 4-Input NAND Gates</description>
<gates>
<gate name="A" symbol="MC14012BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="2"/>
<connect gate="A" pin="IN_1B" pad="9"/>
<connect gate="A" pin="IN_2A" pad="3"/>
<connect gate="A" pin="IN_2B" pad="10"/>
<connect gate="A" pin="IN_3A" pad="4"/>
<connect gate="A" pin="IN_3B" pad="11"/>
<connect gate="A" pin="IN_4A" pad="5"/>
<connect gate="A" pin="IN_4B" pad="12"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="13"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14012BDG"/>
<attribute name="OC_FARNELL" value="9664840"/>
<attribute name="OC_NEWARK" value="71J5454"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14013BCPG" prefix="U">
<description>Dual Type D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC14013BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="CA" pad="3"/>
<connect gate="A" pin="CB" pad="11"/>
<connect gate="A" pin="DA" pad="5"/>
<connect gate="A" pin="DB" pad="9"/>
<connect gate="A" pin="QA" pad="1"/>
<connect gate="A" pin="QB" pad="13"/>
<connect gate="A" pin="RA" pad="4"/>
<connect gate="A" pin="RB" pad="10"/>
<connect gate="A" pin="SA" pad="6"/>
<connect gate="A" pin="SB" pad="8"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
<connect gate="A" pin="~QA" pad="2"/>
<connect gate="A" pin="~QB" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14013BCPG"/>
<attribute name="OC_FARNELL" value="9665471"/>
<attribute name="OC_NEWARK" value="88H4713"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14013BDG" prefix="U">
<description>Dual Type D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC14013BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="CA" pad="3"/>
<connect gate="A" pin="CB" pad="11"/>
<connect gate="A" pin="DA" pad="5"/>
<connect gate="A" pin="DB" pad="9"/>
<connect gate="A" pin="QA" pad="1"/>
<connect gate="A" pin="QB" pad="13"/>
<connect gate="A" pin="RA" pad="4"/>
<connect gate="A" pin="RB" pad="10"/>
<connect gate="A" pin="SA" pad="6"/>
<connect gate="A" pin="SB" pad="8"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
<connect gate="A" pin="~QA" pad="2"/>
<connect gate="A" pin="~QB" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14013BDG"/>
<attribute name="OC_FARNELL" value="9666320"/>
<attribute name="OC_NEWARK" value="45J1018"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14014BCPG" prefix="U">
<description>8-Bit Static Shift Register</description>
<gates>
<gate name="A" symbol="MC14014BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="DS" pad="11"/>
<connect gate="A" pin="P/S" pad="9"/>
<connect gate="A" pin="P1" pad="7"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="5"/>
<connect gate="A" pin="P4" pad="4"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="14"/>
<connect gate="A" pin="P7" pad="15"/>
<connect gate="A" pin="P8" pad="1"/>
<connect gate="A" pin="Q6" pad="2"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="Q8" pad="3"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14014BCPG"/>
<attribute name="OC_FARNELL" value="9664580"/>
<attribute name="OC_NEWARK" value="45J1020"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14016BCPG" prefix="U">
<description>Quad Multiplexer</description>
<gates>
<gate name="A" symbol="MC14016BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="CONTROL_1" pad="13"/>
<connect gate="A" pin="CONTROL_2" pad="5"/>
<connect gate="A" pin="CONTROL_3" pad="6"/>
<connect gate="A" pin="CONTROL_4" pad="12"/>
<connect gate="A" pin="IN_1" pad="1"/>
<connect gate="A" pin="IN_2" pad="4"/>
<connect gate="A" pin="IN_3" pad="8"/>
<connect gate="A" pin="IN_4" pad="11"/>
<connect gate="A" pin="OUT_1" pad="2"/>
<connect gate="A" pin="OUT_2" pad="3"/>
<connect gate="A" pin="OUT_3" pad="9"/>
<connect gate="A" pin="OUT_4" pad="10"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14016BCPG"/>
<attribute name="OC_FARNELL" value="9665706"/>
<attribute name="OC_NEWARK" value="45J1024"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14016BDG" prefix="U">
<description>Quad Analog Switch/Quad Multiplexer</description>
<gates>
<gate name="A" symbol="MC14016BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="CONTROL1" pad="13"/>
<connect gate="A" pin="CONTROL2" pad="5"/>
<connect gate="A" pin="CONTROL3" pad="6"/>
<connect gate="A" pin="CONTROL4" pad="12"/>
<connect gate="A" pin="IN1" pad="1"/>
<connect gate="A" pin="IN2" pad="4"/>
<connect gate="A" pin="IN3" pad="8"/>
<connect gate="A" pin="IN4" pad="11"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="3"/>
<connect gate="A" pin="OUT3" pad="9"/>
<connect gate="A" pin="OUT4" pad="10"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14016BDG"/>
<attribute name="OC_FARNELL" value="9666338"/>
<attribute name="OC_NEWARK" value="71J5456"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14017BCPG" prefix="U">
<description>Decade Counter</description>
<gates>
<gate name="A" symbol="MC14017BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="COUT" pad="12"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="4"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="10"/>
<connect gate="A" pin="Q5" pad="1"/>
<connect gate="A" pin="Q6" pad="5"/>
<connect gate="A" pin="Q7" pad="6"/>
<connect gate="A" pin="Q8" pad="9"/>
<connect gate="A" pin="Q9" pad="11"/>
<connect gate="A" pin="RESET" pad="15"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~CE" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14017BCPG"/>
<attribute name="OC_FARNELL" value="9666621"/>
<attribute name="OC_NEWARK" value="45J1025"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14017BDG" prefix="U">
<description>Decade Counter</description>
<gates>
<gate name="A" symbol="MC14017BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="COUT" pad="12"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="4"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="10"/>
<connect gate="A" pin="Q5" pad="1"/>
<connect gate="A" pin="Q6" pad="5"/>
<connect gate="A" pin="Q7" pad="6"/>
<connect gate="A" pin="Q8" pad="9"/>
<connect gate="A" pin="Q9" pad="11"/>
<connect gate="A" pin="RESET" pad="15"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~CE" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14017BDG"/>
<attribute name="OC_FARNELL" value="1104712"/>
<attribute name="OC_NEWARK" value="42K0508"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14020BCPG" prefix="U">
<description>14-Bit Binary Counter</description>
<gates>
<gate name="A" symbol="MC14020BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q10" pad="14"/>
<connect gate="A" pin="Q11" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q13" pad="2"/>
<connect gate="A" pin="Q14" pad="3"/>
<connect gate="A" pin="Q4" pad="7"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="4"/>
<connect gate="A" pin="Q7" pad="6"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="Q9" pad="12"/>
<connect gate="A" pin="R" pad="11"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14020BCPG"/>
<attribute name="OC_FARNELL" value="9665480"/>
<attribute name="OC_NEWARK" value="45J1027"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14020BDG" prefix="U">
<description>14-Bit Binary Counter</description>
<gates>
<gate name="A" symbol="MC14020BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q10" pad="14"/>
<connect gate="A" pin="Q11" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q13" pad="2"/>
<connect gate="A" pin="Q14" pad="3"/>
<connect gate="A" pin="Q4" pad="7"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="4"/>
<connect gate="A" pin="Q7" pad="6"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="Q9" pad="12"/>
<connect gate="A" pin="R" pad="11"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14020BDG"/>
<attribute name="OC_FARNELL" value="1191821"/>
<attribute name="OC_NEWARK" value="26K3930"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14022BCPG" prefix="U">
<description>Octal Counter</description>
<gates>
<gate name="A" symbol="MC14022BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="COUT" pad="12"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="11"/>
<connect gate="A" pin="Q5" pad="4"/>
<connect gate="A" pin="Q6" pad="5"/>
<connect gate="A" pin="Q7" pad="10"/>
<connect gate="A" pin="R" pad="15"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~CE" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14022BCPG"/>
<attribute name="OC_FARNELL" value="1607666"/>
<attribute name="OC_NEWARK" value="45J1032"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14022BDG" prefix="U">
<description>Octal Counter</description>
<gates>
<gate name="A" symbol="MC14022BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="COUT" pad="12"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="11"/>
<connect gate="A" pin="Q5" pad="4"/>
<connect gate="A" pin="Q6" pad="5"/>
<connect gate="A" pin="Q7" pad="10"/>
<connect gate="A" pin="R" pad="15"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~CE" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14022BDG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26K3931"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14023BCPG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14023BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="3"/>
<connect gate="A" pin="IN_1C" pad="11"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="4"/>
<connect gate="A" pin="IN_2C" pad="12"/>
<connect gate="A" pin="IN_3A" pad="8"/>
<connect gate="A" pin="IN_3B" pad="5"/>
<connect gate="A" pin="IN_3C" pad="13"/>
<connect gate="A" pin="OUT_A" pad="9"/>
<connect gate="A" pin="OUT_B" pad="6"/>
<connect gate="A" pin="OUT_C" pad="10"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14023BCPG"/>
<attribute name="OC_FARNELL" value="9665501"/>
<attribute name="OC_NEWARK" value="73K0840"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14023BDG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14023BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="3"/>
<connect gate="A" pin="IN_1C" pad="11"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="4"/>
<connect gate="A" pin="IN_2C" pad="12"/>
<connect gate="A" pin="IN_3A" pad="8"/>
<connect gate="A" pin="IN_3B" pad="5"/>
<connect gate="A" pin="IN_3C" pad="13"/>
<connect gate="A" pin="OUTA" pad="9"/>
<connect gate="A" pin="OUTB" pad="6"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14023BDG"/>
<attribute name="OC_FARNELL" value="1191823"/>
<attribute name="OC_NEWARK" value="26K3932"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14024BCPG" prefix="U">
<description>7-Stage Ripple Counter</description>
<gates>
<gate name="A" symbol="MC14024BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="Q1" pad="12"/>
<connect gate="A" pin="Q2" pad="11"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="6"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="4"/>
<connect gate="A" pin="Q7" pad="3"/>
<connect gate="A" pin="RESET" pad="2"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14024BCPG"/>
<attribute name="OC_FARNELL" value="9664610"/>
<attribute name="OC_NEWARK" value="45J1036"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14025BCPG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14025BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="3"/>
<connect gate="A" pin="IN_1C" pad="11"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="4"/>
<connect gate="A" pin="IN_2C" pad="12"/>
<connect gate="A" pin="IN_3A" pad="8"/>
<connect gate="A" pin="IN_3B" pad="5"/>
<connect gate="A" pin="IN_3C" pad="13"/>
<connect gate="A" pin="OUT_A" pad="9"/>
<connect gate="A" pin="OUT_B" pad="6"/>
<connect gate="A" pin="OUT_C" pad="10"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14025BCPG"/>
<attribute name="OC_FARNELL" value="9665285"/>
<attribute name="OC_NEWARK" value="45J1037"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14025BDG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14025BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="3"/>
<connect gate="A" pin="IN_1C" pad="11"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="4"/>
<connect gate="A" pin="IN_2C" pad="12"/>
<connect gate="A" pin="IN_3A" pad="8"/>
<connect gate="A" pin="IN_3B" pad="5"/>
<connect gate="A" pin="IN_3C" pad="13"/>
<connect gate="A" pin="OUTA" pad="9"/>
<connect gate="A" pin="OUTB" pad="6"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14025BDG"/>
<attribute name="OC_FARNELL" value="1191824"/>
<attribute name="OC_NEWARK" value="26K3933"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14027BCPG" prefix="U">
<description>Dual J-K Flip-Flop</description>
<gates>
<gate name="A" symbol="MC14027BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CA" pad="3"/>
<connect gate="A" pin="CB" pad="13"/>
<connect gate="A" pin="JA" pad="6"/>
<connect gate="A" pin="JB" pad="10"/>
<connect gate="A" pin="KA" pad="5"/>
<connect gate="A" pin="KB" pad="11"/>
<connect gate="A" pin="QA" pad="1"/>
<connect gate="A" pin="QB" pad="15"/>
<connect gate="A" pin="RA" pad="4"/>
<connect gate="A" pin="RB" pad="12"/>
<connect gate="A" pin="SA" pad="7"/>
<connect gate="A" pin="SB" pad="9"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~QA" pad="2"/>
<connect gate="A" pin="~QB" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14027BCPG"/>
<attribute name="OC_FARNELL" value="9665510"/>
<attribute name="OC_NEWARK" value="45J1039"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14027BDG" prefix="U">
<description>Dual J-K Flip-Flop</description>
<gates>
<gate name="A" symbol="MC14027BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="CA" pad="3"/>
<connect gate="A" pin="CB" pad="13"/>
<connect gate="A" pin="JA" pad="6"/>
<connect gate="A" pin="JB" pad="10"/>
<connect gate="A" pin="KA" pad="5"/>
<connect gate="A" pin="KB" pad="11"/>
<connect gate="A" pin="QA" pad="1"/>
<connect gate="A" pin="QB" pad="15"/>
<connect gate="A" pin="RA" pad="4"/>
<connect gate="A" pin="RB" pad="12"/>
<connect gate="A" pin="SA" pad="7"/>
<connect gate="A" pin="SB" pad="9"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~QA" pad="2"/>
<connect gate="A" pin="~QB" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14027BDG"/>
<attribute name="OC_FARNELL" value="9666354"/>
<attribute name="OC_NEWARK" value="71J5463"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14028BDG" prefix="U">
<description>BCD-To-Decimal Decoder Binary-To-Octal Decoder</description>
<gates>
<gate name="A" symbol="MC14028BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="13"/>
<connect gate="A" pin="C" pad="12"/>
<connect gate="A" pin="D" pad="11"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="14"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="15"/>
<connect gate="A" pin="Q4" pad="1"/>
<connect gate="A" pin="Q5" pad="6"/>
<connect gate="A" pin="Q6" pad="7"/>
<connect gate="A" pin="Q7" pad="4"/>
<connect gate="A" pin="Q8" pad="9"/>
<connect gate="A" pin="Q9" pad="5"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14028BDG"/>
<attribute name="OC_FARNELL" value="9666362"/>
<attribute name="OC_NEWARK" value="71J5465"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14029BCPG" prefix="U">
<description>Binary/Decade Up/Down Counter</description>
<gates>
<gate name="A" symbol="MC14029BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="B/D" pad="9"/>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="P0" pad="4"/>
<connect gate="A" pin="P1" pad="12"/>
<connect gate="A" pin="P2" pad="13"/>
<connect gate="A" pin="P3" pad="3"/>
<connect gate="A" pin="PE" pad="1"/>
<connect gate="A" pin="Q0" pad="6"/>
<connect gate="A" pin="Q1" pad="11"/>
<connect gate="A" pin="Q2" pad="14"/>
<connect gate="A" pin="Q3" pad="2"/>
<connect gate="A" pin="U/D" pad="10"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~CIN" pad="5"/>
<connect gate="A" pin="~COUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14029BCPG"/>
<attribute name="OC_FARNELL" value="9664629"/>
<attribute name="OC_NEWARK" value="45J1041"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14029BDR2G" prefix="U">
<description>Binary/Decade Up/Down Counter</description>
<gates>
<gate name="A" symbol="MC14029BDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="B/D" pad="9"/>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="P0" pad="4"/>
<connect gate="A" pin="P1" pad="12"/>
<connect gate="A" pin="P2" pad="13"/>
<connect gate="A" pin="P3" pad="3"/>
<connect gate="A" pin="PE" pad="1"/>
<connect gate="A" pin="Q0" pad="6"/>
<connect gate="A" pin="Q1" pad="11"/>
<connect gate="A" pin="Q2" pad="14"/>
<connect gate="A" pin="Q3" pad="2"/>
<connect gate="A" pin="U/D" pad="10"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~CIN" pad="5"/>
<connect gate="A" pin="~COUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14029BDR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7793"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14040BCPG" prefix="U">
<description>12-Bit Binary Counter</description>
<gates>
<gate name="A" symbol="MC14040BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q10" pad="14"/>
<connect gate="A" pin="Q11" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="A" pin="Q5" pad="3"/>
<connect gate="A" pin="Q6" pad="2"/>
<connect gate="A" pin="Q7" pad="4"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="Q9" pad="12"/>
<connect gate="A" pin="R" pad="11"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14040BCPG"/>
<attribute name="OC_FARNELL" value="9665544"/>
<attribute name="OC_NEWARK" value="45J1045"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14040BDG" prefix="U">
<description>12-Bit Binary Counter</description>
<gates>
<gate name="A" symbol="MC14040BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q10" pad="14"/>
<connect gate="A" pin="Q11" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="A" pin="Q5" pad="3"/>
<connect gate="A" pin="Q6" pad="2"/>
<connect gate="A" pin="Q7" pad="4"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="Q9" pad="12"/>
<connect gate="A" pin="R" pad="11"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14040BDG"/>
<attribute name="OC_FARNELL" value="9666370"/>
<attribute name="OC_NEWARK" value="45J1046"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14040BDR2G" prefix="U">
<description>12-Bit Binary Counter</description>
<gates>
<gate name="A" symbol="MC14040BDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q10" pad="14"/>
<connect gate="A" pin="Q11" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="A" pin="Q5" pad="3"/>
<connect gate="A" pin="Q6" pad="2"/>
<connect gate="A" pin="Q7" pad="4"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="Q9" pad="12"/>
<connect gate="A" pin="R" pad="11"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14040BDR2G"/>
<attribute name="OC_FARNELL" value="1364057"/>
<attribute name="OC_NEWARK" value="26K3935"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14042BDG" prefix="U">
<description>Quad Transparent Latch</description>
<gates>
<gate name="A" symbol="MC14042BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="CLK" pad="5"/>
<connect gate="A" pin="D0" pad="4"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D2" pad="13"/>
<connect gate="A" pin="D3" pad="14"/>
<connect gate="A" pin="POLARITY" pad="6"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="10"/>
<connect gate="A" pin="Q2" pad="11"/>
<connect gate="A" pin="Q3" pad="1"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~Q0" pad="3"/>
<connect gate="A" pin="~Q1" pad="9"/>
<connect gate="A" pin="~Q2" pad="12"/>
<connect gate="A" pin="~Q3" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14042BDG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="71J5467"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14043BCPG" prefix="U">
<description>CMOS MSI</description>
<gates>
<gate name="A" symbol="MC14043BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="E" pad="5"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q2" pad="10"/>
<connect gate="A" pin="Q3" pad="1"/>
<connect gate="A" pin="R0" pad="3"/>
<connect gate="A" pin="R1" pad="7"/>
<connect gate="A" pin="R2" pad="11"/>
<connect gate="A" pin="R3" pad="15"/>
<connect gate="A" pin="S0" pad="4"/>
<connect gate="A" pin="S1" pad="6"/>
<connect gate="A" pin="S2" pad="12"/>
<connect gate="A" pin="S3" pad="14"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14043BCPG"/>
<attribute name="OC_FARNELL" value="9664645"/>
<attribute name="OC_NEWARK" value="45J1048"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14043BDG" prefix="U">
<description>CMOS MSI</description>
<gates>
<gate name="A" symbol="MC14043BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="E" pad="5"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q2" pad="10"/>
<connect gate="A" pin="Q3" pad="1"/>
<connect gate="A" pin="R0" pad="3"/>
<connect gate="A" pin="R1" pad="7"/>
<connect gate="A" pin="R2" pad="11"/>
<connect gate="A" pin="R3" pad="15"/>
<connect gate="A" pin="S0" pad="4"/>
<connect gate="A" pin="S1" pad="6"/>
<connect gate="A" pin="S2" pad="12"/>
<connect gate="A" pin="S3" pad="14"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14043BDG"/>
<attribute name="OC_FARNELL" value="9665145"/>
<attribute name="OC_NEWARK" value="26K3936"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14044BCPG" prefix="U">
<description>CMOS MSI</description>
<gates>
<gate name="A" symbol="MC14044BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="E" pad="5"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="Q0" pad="13"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q2" pad="10"/>
<connect gate="A" pin="Q3" pad="1"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~R0" pad="4"/>
<connect gate="A" pin="~R1" pad="6"/>
<connect gate="A" pin="~R2" pad="12"/>
<connect gate="A" pin="~R3" pad="14"/>
<connect gate="A" pin="~S0" pad="3"/>
<connect gate="A" pin="~S1" pad="7"/>
<connect gate="A" pin="~S2" pad="11"/>
<connect gate="A" pin="~S3" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14044BCPG"/>
<attribute name="OC_FARNELL" value="9664653"/>
<attribute name="OC_NEWARK" value="45J1050"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14046BCPG" prefix="U">
<description>Phase Locked Loop</description>
<gates>
<gate name="A" symbol="MC14046BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="C1A" pad="6"/>
<connect gate="A" pin="C1B" pad="7"/>
<connect gate="A" pin="INH" pad="5"/>
<connect gate="A" pin="LD" pad="1"/>
<connect gate="A" pin="PC1OUT" pad="2"/>
<connect gate="A" pin="PC2OUT" pad="13"/>
<connect gate="A" pin="PCAIN" pad="14"/>
<connect gate="A" pin="PCBIN" pad="3"/>
<connect gate="A" pin="R1" pad="11"/>
<connect gate="A" pin="R2" pad="12"/>
<connect gate="A" pin="SFOUT" pad="10"/>
<connect gate="A" pin="VCOIN" pad="9"/>
<connect gate="A" pin="VCOOUT" pad="4"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="ZENER" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14046BCPG"/>
<attribute name="OC_FARNELL" value="9664661"/>
<attribute name="OC_NEWARK" value="45J1053"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14049BCPG" prefix="U">
<description>Hex Buffer</description>
<gates>
<gate name="A" symbol="MC14049BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="INA" pad="3"/>
<connect gate="A" pin="INB" pad="5"/>
<connect gate="A" pin="INC" pad="7"/>
<connect gate="A" pin="IND" pad="9"/>
<connect gate="A" pin="INE" pad="11"/>
<connect gate="A" pin="INF" pad="14"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="6"/>
<connect gate="A" pin="OUTD" pad="10"/>
<connect gate="A" pin="OUTE" pad="12"/>
<connect gate="A" pin="OUTF" pad="15"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14049BCPG"/>
<attribute name="OC_FARNELL" value="9664670"/>
<attribute name="OC_NEWARK" value="26K3937"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14049BDG" prefix="U">
<description>Hex Buffer</description>
<gates>
<gate name="A" symbol="MC14049BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="INA" pad="3"/>
<connect gate="A" pin="INB" pad="5"/>
<connect gate="A" pin="INC" pad="7"/>
<connect gate="A" pin="IND" pad="9"/>
<connect gate="A" pin="INE" pad="11"/>
<connect gate="A" pin="INF" pad="14"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="6"/>
<connect gate="A" pin="OUTD" pad="10"/>
<connect gate="A" pin="OUTE" pad="12"/>
<connect gate="A" pin="OUTF" pad="15"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14049BDG"/>
<attribute name="OC_FARNELL" value="1468727"/>
<attribute name="OC_NEWARK" value="71J5469"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14049UBCPG" prefix="U">
<description>Hex Buffers</description>
<gates>
<gate name="A" symbol="MC14049UBCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="INA" pad="3"/>
<connect gate="A" pin="INB" pad="5"/>
<connect gate="A" pin="INC" pad="7"/>
<connect gate="A" pin="IND" pad="9"/>
<connect gate="A" pin="INE" pad="11"/>
<connect gate="A" pin="INF" pad="14"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="6"/>
<connect gate="A" pin="OUTD" pad="10"/>
<connect gate="A" pin="OUTE" pad="12"/>
<connect gate="A" pin="OUTF" pad="15"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14049UBCPG"/>
<attribute name="OC_FARNELL" value="9664688"/>
<attribute name="OC_NEWARK" value="45J1056"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14049UBDG" prefix="U">
<description>Hex Buffer</description>
<gates>
<gate name="A" symbol="MC14049UBDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="INA" pad="3"/>
<connect gate="A" pin="INB" pad="5"/>
<connect gate="A" pin="INC" pad="7"/>
<connect gate="A" pin="IND" pad="9"/>
<connect gate="A" pin="INE" pad="11"/>
<connect gate="A" pin="INF" pad="14"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="6"/>
<connect gate="A" pin="OUTD" pad="10"/>
<connect gate="A" pin="OUTE" pad="12"/>
<connect gate="A" pin="OUTF" pad="15"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14049UBDG"/>
<attribute name="OC_FARNELL" value="9665170"/>
<attribute name="OC_NEWARK" value="71J5471"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14049UBDR2G" prefix="U">
<description>Hex Buffer</description>
<gates>
<gate name="A" symbol="MC14049UBDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="INA" pad="3"/>
<connect gate="A" pin="INB" pad="5"/>
<connect gate="A" pin="INC" pad="7"/>
<connect gate="A" pin="IND" pad="9"/>
<connect gate="A" pin="INE" pad="11"/>
<connect gate="A" pin="INF" pad="14"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="6"/>
<connect gate="A" pin="OUTD" pad="10"/>
<connect gate="A" pin="OUTE" pad="12"/>
<connect gate="A" pin="OUTF" pad="15"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14049UBDR2G"/>
<attribute name="OC_FARNELL" value="1365190"/>
<attribute name="OC_NEWARK" value="84K8744"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14050BCPG" prefix="U">
<description>Hex Buffer</description>
<gates>
<gate name="A" symbol="MC14050BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="INA" pad="3"/>
<connect gate="A" pin="INB" pad="5"/>
<connect gate="A" pin="INC" pad="7"/>
<connect gate="A" pin="IND" pad="9"/>
<connect gate="A" pin="INE" pad="11"/>
<connect gate="A" pin="INF" pad="14"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="6"/>
<connect gate="A" pin="OUTD" pad="10"/>
<connect gate="A" pin="OUTE" pad="12"/>
<connect gate="A" pin="OUTF" pad="15"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14050BCPG"/>
<attribute name="OC_FARNELL" value="9665552"/>
<attribute name="OC_NEWARK" value="45J1058"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14050BDG" prefix="U">
<description>Hex Buffer</description>
<gates>
<gate name="A" symbol="MC14050BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="INA" pad="3"/>
<connect gate="A" pin="INB" pad="5"/>
<connect gate="A" pin="INC" pad="7"/>
<connect gate="A" pin="IND" pad="9"/>
<connect gate="A" pin="INE" pad="11"/>
<connect gate="A" pin="INF" pad="14"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="6"/>
<connect gate="A" pin="OUTD" pad="10"/>
<connect gate="A" pin="OUTE" pad="12"/>
<connect gate="A" pin="OUTF" pad="15"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14050BDG"/>
<attribute name="OC_FARNELL" value="9666397"/>
<attribute name="OC_NEWARK" value="26K3938"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14050BDR2G" prefix="U">
<description>Hex Buffer</description>
<gates>
<gate name="A" symbol="MC14050BDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="INA" pad="3"/>
<connect gate="A" pin="INB" pad="5"/>
<connect gate="A" pin="INC" pad="7"/>
<connect gate="A" pin="IND" pad="9"/>
<connect gate="A" pin="INE" pad="11"/>
<connect gate="A" pin="INF" pad="14"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="6"/>
<connect gate="A" pin="OUTD" pad="10"/>
<connect gate="A" pin="OUTE" pad="12"/>
<connect gate="A" pin="OUTF" pad="15"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14050BDR2G"/>
<attribute name="OC_FARNELL" value="1365191"/>
<attribute name="OC_NEWARK" value="84K8745"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14051BCPG" prefix="U">
<description>Multiplexers/Demultiplexers</description>
<gates>
<gate name="A" symbol="MC14051BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="INH" pad="6"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="X" pad="3"/>
<connect gate="A" pin="X0" pad="13"/>
<connect gate="A" pin="X1" pad="14"/>
<connect gate="A" pin="X2" pad="15"/>
<connect gate="A" pin="X3" pad="12"/>
<connect gate="A" pin="X4" pad="1"/>
<connect gate="A" pin="X5" pad="5"/>
<connect gate="A" pin="X6" pad="2"/>
<connect gate="A" pin="X7" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14051BCPG"/>
<attribute name="OC_FARNELL" value="9665684"/>
<attribute name="OC_NEWARK" value="45J1060"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14051BDG" prefix="U">
<description>Analog Multiplexers/Demultiplexers</description>
<gates>
<gate name="A" symbol="MC14051BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="INH" pad="6"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="X" pad="3"/>
<connect gate="A" pin="X0" pad="13"/>
<connect gate="A" pin="X1" pad="14"/>
<connect gate="A" pin="X2" pad="15"/>
<connect gate="A" pin="X3" pad="12"/>
<connect gate="A" pin="X4" pad="1"/>
<connect gate="A" pin="X5" pad="5"/>
<connect gate="A" pin="X6" pad="2"/>
<connect gate="A" pin="X7" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14051BDG"/>
<attribute name="OC_FARNELL" value="9666400"/>
<attribute name="OC_NEWARK" value="45J1061"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14051BDTR2G" prefix="U">
<description>Multiplexers/Demultiplexers</description>
<gates>
<gate name="A" symbol="MC14051BDTR2G"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-16N">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="INH" pad="6"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="X" pad="3"/>
<connect gate="A" pin="X0" pad="13"/>
<connect gate="A" pin="X1" pad="14"/>
<connect gate="A" pin="X2" pad="15"/>
<connect gate="A" pin="X3" pad="12"/>
<connect gate="A" pin="X4" pad="1"/>
<connect gate="A" pin="X5" pad="5"/>
<connect gate="A" pin="X6" pad="2"/>
<connect gate="A" pin="X7" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14051BDTR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="42K0523"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14052BCPG" prefix="U">
<description>Multiplexers/Demultiplexers</description>
<gates>
<gate name="A" symbol="MC14052BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="9"/>
<connect gate="A" pin="INH" pad="6"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="X" pad="13"/>
<connect gate="A" pin="X0" pad="12"/>
<connect gate="A" pin="X1" pad="14"/>
<connect gate="A" pin="X2" pad="15"/>
<connect gate="A" pin="X3" pad="11"/>
<connect gate="A" pin="Y" pad="3"/>
<connect gate="A" pin="Y0" pad="1"/>
<connect gate="A" pin="Y1" pad="5"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14052BCPG"/>
<attribute name="OC_FARNELL" value="9665692"/>
<attribute name="OC_NEWARK" value="98H0653"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14053BCPG" prefix="U">
<description>Multiplexers/Demultiplexers</description>
<gates>
<gate name="A" symbol="MC14053BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="INH" pad="6"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="X" pad="14"/>
<connect gate="A" pin="X0" pad="12"/>
<connect gate="A" pin="X1" pad="13"/>
<connect gate="A" pin="Y" pad="15"/>
<connect gate="A" pin="Y0" pad="2"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Z" pad="4"/>
<connect gate="A" pin="Z0" pad="5"/>
<connect gate="A" pin="Z1" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14053BCPG"/>
<attribute name="OC_FARNELL" value="9664696"/>
<attribute name="OC_NEWARK" value="45J1063"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14053BDG" prefix="U">
<description>Analog Multiplexers/Demultiplexers</description>
<gates>
<gate name="A" symbol="MC14053BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="INH" pad="6"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="X" pad="14"/>
<connect gate="A" pin="X0" pad="12"/>
<connect gate="A" pin="X1" pad="13"/>
<connect gate="A" pin="Y" pad="15"/>
<connect gate="A" pin="Y0" pad="2"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Z" pad="4"/>
<connect gate="A" pin="Z0" pad="5"/>
<connect gate="A" pin="Z1" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14053BDG"/>
<attribute name="OC_FARNELL" value="9666427"/>
<attribute name="OC_NEWARK" value="45J1064"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14053BDTR2G" prefix="U">
<description>Multiplexers/Demultiplexers</description>
<gates>
<gate name="A" symbol="MC14053BDTR2G"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-16N">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="INH" pad="6"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="X" pad="14"/>
<connect gate="A" pin="X0" pad="12"/>
<connect gate="A" pin="X1" pad="13"/>
<connect gate="A" pin="Y" pad="15"/>
<connect gate="A" pin="Y0" pad="2"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Z" pad="4"/>
<connect gate="A" pin="Z0" pad="5"/>
<connect gate="A" pin="Z1" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14053BDTR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7824"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14060BCPG" prefix="U">
<description>14-Bit Binary Counter</description>
<gates>
<gate name="A" symbol="MC14060BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="OUT_1" pad="10"/>
<connect gate="A" pin="OUT_2" pad="9"/>
<connect gate="A" pin="Q10" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q13" pad="2"/>
<connect gate="A" pin="Q14" pad="3"/>
<connect gate="A" pin="Q4" pad="7"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="4"/>
<connect gate="A" pin="Q7" pad="6"/>
<connect gate="A" pin="Q8" pad="14"/>
<connect gate="A" pin="Q9" pad="13"/>
<connect gate="A" pin="RESET" pad="12"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14060BCPG"/>
<attribute name="OC_FARNELL" value="9665560"/>
<attribute name="OC_NEWARK" value="45J1065"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14060BDG" prefix="U">
<description>14-Bit Binary Counter and Oscillator</description>
<gates>
<gate name="A" symbol="MC14060BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="OUT_1" pad="10"/>
<connect gate="A" pin="OUT_2" pad="9"/>
<connect gate="A" pin="Q10" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q13" pad="2"/>
<connect gate="A" pin="Q14" pad="3"/>
<connect gate="A" pin="Q4" pad="7"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="4"/>
<connect gate="A" pin="Q7" pad="6"/>
<connect gate="A" pin="Q8" pad="14"/>
<connect gate="A" pin="Q9" pad="13"/>
<connect gate="A" pin="RESET" pad="12"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14060BDG"/>
<attribute name="OC_FARNELL" value="9666435"/>
<attribute name="OC_NEWARK" value="71J5473"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14066BCPG" prefix="U">
<description>Quad Analog Switch/Quad Multiplexer</description>
<gates>
<gate name="A" symbol="MC14066BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="CONTROL_1" pad="13"/>
<connect gate="A" pin="CONTROL_2" pad="5"/>
<connect gate="A" pin="CONTROL_3" pad="6"/>
<connect gate="A" pin="CONTROL_4" pad="12"/>
<connect gate="A" pin="IN_1" pad="1"/>
<connect gate="A" pin="IN_2" pad="4"/>
<connect gate="A" pin="IN_3" pad="8"/>
<connect gate="A" pin="IN_4" pad="11"/>
<connect gate="A" pin="OUT_1" pad="2"/>
<connect gate="A" pin="OUT_2" pad="3"/>
<connect gate="A" pin="OUT_3" pad="9"/>
<connect gate="A" pin="OUT_4" pad="10"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14066BCPG"/>
<attribute name="OC_FARNELL" value="9664700"/>
<attribute name="OC_NEWARK" value="45J1067"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14066BDG" prefix="U">
<description>Quad Analog Switch/Quad Multiplexer</description>
<gates>
<gate name="A" symbol="MC14066BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="CONTROL_1" pad="13"/>
<connect gate="A" pin="CONTROL_2" pad="5"/>
<connect gate="A" pin="CONTROL_3" pad="6"/>
<connect gate="A" pin="CONTROL_4" pad="12"/>
<connect gate="A" pin="IN_1" pad="1"/>
<connect gate="A" pin="IN_2" pad="4"/>
<connect gate="A" pin="IN_3" pad="8"/>
<connect gate="A" pin="IN_4" pad="11"/>
<connect gate="A" pin="OUT_1" pad="2"/>
<connect gate="A" pin="OUT_2" pad="3"/>
<connect gate="A" pin="OUT_3" pad="9"/>
<connect gate="A" pin="OUT_4" pad="10"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14066BDG"/>
<attribute name="OC_FARNELL" value="9666443"/>
<attribute name="OC_NEWARK" value="45J1068"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14066BDR2G" prefix="U">
<description>Quad Multiplexer</description>
<gates>
<gate name="A" symbol="MC14066BDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="CNTR1" pad="13"/>
<connect gate="A" pin="CNTR2" pad="5"/>
<connect gate="A" pin="CNTR3" pad="6"/>
<connect gate="A" pin="CNTR4" pad="12"/>
<connect gate="A" pin="IN1" pad="1"/>
<connect gate="A" pin="IN2" pad="4"/>
<connect gate="A" pin="IN3" pad="8"/>
<connect gate="A" pin="IN4" pad="11"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="3"/>
<connect gate="A" pin="OUT3" pad="9"/>
<connect gate="A" pin="OUT4" pad="10"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14066BDR2G"/>
<attribute name="OC_FARNELL" value="1887036"/>
<attribute name="OC_NEWARK" value="98H0656"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14066BDTR2G" prefix="U">
<description>Quad Mux</description>
<gates>
<gate name="A" symbol="MC14066BDTR2G"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="CONTROL1" pad="13"/>
<connect gate="A" pin="CONTROL2" pad="5"/>
<connect gate="A" pin="CONTROL3" pad="6"/>
<connect gate="A" pin="CONTROL4" pad="12"/>
<connect gate="A" pin="IN1" pad="1"/>
<connect gate="A" pin="IN2" pad="4"/>
<connect gate="A" pin="IN3" pad="8"/>
<connect gate="A" pin="IN4" pad="11"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="3"/>
<connect gate="A" pin="OUT3" pad="9"/>
<connect gate="A" pin="OUT4" pad="10"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14066BDTR2G"/>
<attribute name="OC_FARNELL" value="1568904"/>
<attribute name="OC_NEWARK" value="42K0527"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14067BDWG" prefix="U">
<description>Analog Multiplexers/Demultiplexers</description>
<gates>
<gate name="A" symbol="MC14067BDWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-24N">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="11"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="INHIBIT" pad="15"/>
<connect gate="A" pin="VDD" pad="24"/>
<connect gate="A" pin="VSS" pad="12"/>
<connect gate="A" pin="X" pad="1"/>
<connect gate="A" pin="X0" pad="9"/>
<connect gate="A" pin="X1" pad="8"/>
<connect gate="A" pin="X10" pad="21"/>
<connect gate="A" pin="X11" pad="20"/>
<connect gate="A" pin="X12" pad="19"/>
<connect gate="A" pin="X13" pad="18"/>
<connect gate="A" pin="X14" pad="17"/>
<connect gate="A" pin="X15" pad="16"/>
<connect gate="A" pin="X2" pad="7"/>
<connect gate="A" pin="X3" pad="6"/>
<connect gate="A" pin="X5" pad="5"/>
<connect gate="A" pin="X5_2" pad="4"/>
<connect gate="A" pin="X6" pad="3"/>
<connect gate="A" pin="X7" pad="2"/>
<connect gate="A" pin="X8" pad="23"/>
<connect gate="A" pin="X9" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14067BDWG"/>
<attribute name="OC_FARNELL" value="9664882"/>
<attribute name="OC_NEWARK" value="45J1070"/>
<attribute name="PACKAGE" value="SOIC-24"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14069UBCPG" prefix="U">
<description>Hex Inverter</description>
<gates>
<gate name="A" symbol="MC14069UBCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="1"/>
<connect gate="A" pin="IN_2" pad="3"/>
<connect gate="A" pin="IN_3" pad="5"/>
<connect gate="A" pin="IN_4" pad="9"/>
<connect gate="A" pin="IN_5" pad="11"/>
<connect gate="A" pin="IN_6" pad="13"/>
<connect gate="A" pin="OUT_1" pad="2"/>
<connect gate="A" pin="OUT_2" pad="4"/>
<connect gate="A" pin="OUT_3" pad="6"/>
<connect gate="A" pin="OUT_4" pad="8"/>
<connect gate="A" pin="OUT_5" pad="10"/>
<connect gate="A" pin="OUT_6" pad="12"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14069UBCPG"/>
<attribute name="OC_FARNELL" value="9665579"/>
<attribute name="OC_NEWARK" value="45J1072"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14069UBDG" prefix="U">
<description>Hex Inverter</description>
<gates>
<gate name="A" symbol="MC14069UBDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1" pad="1"/>
<connect gate="A" pin="IN_2" pad="3"/>
<connect gate="A" pin="IN_3" pad="5"/>
<connect gate="A" pin="IN_4" pad="9"/>
<connect gate="A" pin="IN_5" pad="11"/>
<connect gate="A" pin="IN_6" pad="13"/>
<connect gate="A" pin="OUT_1" pad="2"/>
<connect gate="A" pin="OUT_2" pad="4"/>
<connect gate="A" pin="OUT_3" pad="6"/>
<connect gate="A" pin="OUT_4" pad="8"/>
<connect gate="A" pin="OUT_5" pad="10"/>
<connect gate="A" pin="OUT_6" pad="12"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14069UBDG"/>
<attribute name="OC_FARNELL" value="9666451"/>
<attribute name="OC_NEWARK" value="45J1073"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14070BCPG" prefix="U">
<description>Quad Exclusive ?OR? and ?NOR? Gates</description>
<gates>
<gate name="A" symbol="MC14070BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="4"/>
<connect gate="A" pin="OUT_C" pad="10"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14070BCPG"/>
<attribute name="OC_FARNELL" value="9665714"/>
<attribute name="OC_NEWARK" value="45J1075"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14070BDG" prefix="U">
<description>CMOS SSI</description>
<gates>
<gate name="A" symbol="MC14070BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14070BDG"/>
<attribute name="OC_FARNELL" value="9666460"/>
<attribute name="OC_NEWARK" value="71J5474"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14071BCPG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14071BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="4"/>
<connect gate="A" pin="OUT_C" pad="10"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14071BCPG"/>
<attribute name="OC_FARNELL" value="9665587"/>
<attribute name="OC_NEWARK" value="88H4715"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14071BDG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14071BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14071BDG"/>
<attribute name="OC_FARNELL" value="9666478"/>
<attribute name="OC_NEWARK" value="26K3944"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14073BDG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14073BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="3"/>
<connect gate="A" pin="IN_1C" pad="11"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="4"/>
<connect gate="A" pin="IN_2C" pad="12"/>
<connect gate="A" pin="IN_3A" pad="8"/>
<connect gate="A" pin="IN_3B" pad="5"/>
<connect gate="A" pin="IN_3C" pad="13"/>
<connect gate="A" pin="OUTA" pad="9"/>
<connect gate="A" pin="OUTB" pad="6"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14073BDG"/>
<attribute name="OC_FARNELL" value="1705997"/>
<attribute name="OC_NEWARK" value="71J5475"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14077BDG" prefix="U">
<description>CMOS SSI</description>
<gates>
<gate name="A" symbol="MC14077BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14077BDG"/>
<attribute name="OC_FARNELL" value="9666486"/>
<attribute name="OC_NEWARK" value="26K3945"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14081BCPG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14081BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="4"/>
<connect gate="A" pin="OUT_C" pad="10"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14081BCPG"/>
<attribute name="OC_FARNELL" value="9665595"/>
<attribute name="OC_NEWARK" value="45J1085"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14081BDG" prefix="U">
<description>B-Suffix Series CMOS Gates</description>
<gates>
<gate name="A" symbol="MC14081BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14081BDG"/>
<attribute name="OC_FARNELL" value="9666494"/>
<attribute name="OC_NEWARK" value="45J1086"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14093BCPG" prefix="U">
<description>Quad 2-Input NAND" Schmitt Trigger</description>
<gates>
<gate name="A" symbol="MC14093BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="4"/>
<connect gate="A" pin="OUT_C" pad="10"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14093BCPG"/>
<attribute name="OC_FARNELL" value="9665609"/>
<attribute name="OC_NEWARK" value="45J1089"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14093BDG" prefix="U">
<description>Quad 2-Input "NAND" Schmitt Trigger</description>
<gates>
<gate name="A" symbol="MC14093BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1A" pad="1"/>
<connect gate="A" pin="IN_1B" pad="5"/>
<connect gate="A" pin="IN_1C" pad="8"/>
<connect gate="A" pin="IN_1D" pad="12"/>
<connect gate="A" pin="IN_2A" pad="2"/>
<connect gate="A" pin="IN_2B" pad="6"/>
<connect gate="A" pin="IN_2C" pad="9"/>
<connect gate="A" pin="IN_2D" pad="13"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="4"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14093BDG"/>
<attribute name="OC_FARNELL" value="9666508"/>
<attribute name="OC_NEWARK" value="71J5481"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14094BDG" prefix="U">
<description>8-Stage Shift/Store Register with Three-State Outputs</description>
<gates>
<gate name="A" symbol="MC14094BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="DATA" pad="2"/>
<connect gate="A" pin="OUT_EN" pad="15"/>
<connect gate="A" pin="Q1" pad="4"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="7"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="13"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="Q8" pad="11"/>
<connect gate="A" pin="QS" pad="9"/>
<connect gate="A" pin="QS_2" pad="10"/>
<connect gate="A" pin="STROBE" pad="1"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14094BDG"/>
<attribute name="OC_FARNELL" value="9666516"/>
<attribute name="OC_NEWARK" value="45J1092"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14099BCPG" prefix="U">
<description>8-Bit Addressable Latches</description>
<gates>
<gate name="A" symbol="MC14099BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A0" pad="5"/>
<connect gate="A" pin="A1" pad="6"/>
<connect gate="A" pin="A2" pad="7"/>
<connect gate="A" pin="DATA" pad="3"/>
<connect gate="A" pin="Q0" pad="9"/>
<connect gate="A" pin="Q1" pad="10"/>
<connect gate="A" pin="Q2" pad="11"/>
<connect gate="A" pin="Q3" pad="12"/>
<connect gate="A" pin="Q4" pad="13"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="15"/>
<connect gate="A" pin="Q7" pad="1"/>
<connect gate="A" pin="RESET" pad="2"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="WRITE_DISABLE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14099BCPG"/>
<attribute name="OC_FARNELL" value="9665722"/>
<attribute name="OC_NEWARK" value="45J1093"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14106BDG" prefix="U">
<description>Hex Schmitt Trigger</description>
<gates>
<gate name="A" symbol="MC14106BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN" pad="13"/>
<connect gate="A" pin="IN_2" pad="1"/>
<connect gate="A" pin="IN_3" pad="11"/>
<connect gate="A" pin="IN_4" pad="3"/>
<connect gate="A" pin="IN_5" pad="5"/>
<connect gate="A" pin="IN_6" pad="9"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="OUT_2" pad="8"/>
<connect gate="A" pin="OUT_3" pad="4"/>
<connect gate="A" pin="OUT_4" pad="12"/>
<connect gate="A" pin="OUT_5" pad="10"/>
<connect gate="A" pin="OUT_6" pad="2"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14106BDG"/>
<attribute name="OC_FARNELL" value="9666524"/>
<attribute name="OC_NEWARK" value="71J5483"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14175BCPG" prefix="U">
<description>Quad Type D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC14175BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="D0" pad="4"/>
<connect gate="A" pin="D1" pad="5"/>
<connect gate="A" pin="D2" pad="12"/>
<connect gate="A" pin="D3" pad="13"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="7"/>
<connect gate="A" pin="Q2" pad="10"/>
<connect gate="A" pin="Q3" pad="15"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~Q0" pad="3"/>
<connect gate="A" pin="~Q1" pad="6"/>
<connect gate="A" pin="~Q2" pad="11"/>
<connect gate="A" pin="~Q3" pad="14"/>
<connect gate="A" pin="~R" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14175BCPG"/>
<attribute name="OC_FARNELL" value="1607714"/>
<attribute name="OC_NEWARK" value="45J1098"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14490DWG" prefix="U">
<description>Hex Contact Bounce Eliminator</description>
<gates>
<gate name="A" symbol="MC14490DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="AIN" pad="1"/>
<connect gate="A" pin="AOUT" pad="15"/>
<connect gate="A" pin="BIN" pad="14"/>
<connect gate="A" pin="BOUT" pad="2"/>
<connect gate="A" pin="CIN" pad="3"/>
<connect gate="A" pin="COUT" pad="13"/>
<connect gate="A" pin="DIN" pad="12"/>
<connect gate="A" pin="DOUT" pad="4"/>
<connect gate="A" pin="EIN" pad="5"/>
<connect gate="A" pin="EOUT" pad="11"/>
<connect gate="A" pin="FIN" pad="10"/>
<connect gate="A" pin="FOUT" pad="6"/>
<connect gate="A" pin="OSCIN" pad="7"/>
<connect gate="A" pin="OSCOUT" pad="9"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14490DWG"/>
<attribute name="OC_FARNELL" value="1191828"/>
<attribute name="OC_NEWARK" value="26K3951"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14490PG" prefix="U">
<description>Hex Contact Bounce Eliminator</description>
<gates>
<gate name="A" symbol="MC14490PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="AIN" pad="1"/>
<connect gate="A" pin="AOUT" pad="15"/>
<connect gate="A" pin="BIN" pad="14"/>
<connect gate="A" pin="BOUT" pad="2"/>
<connect gate="A" pin="CIN" pad="3"/>
<connect gate="A" pin="COUT" pad="13"/>
<connect gate="A" pin="DIN" pad="12"/>
<connect gate="A" pin="DOUT" pad="4"/>
<connect gate="A" pin="EIN" pad="5"/>
<connect gate="A" pin="EOUT" pad="11"/>
<connect gate="A" pin="FIN" pad="10"/>
<connect gate="A" pin="FOUT" pad="6"/>
<connect gate="A" pin="OSCIN" pad="7"/>
<connect gate="A" pin="OSCOUT" pad="9"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14490PG"/>
<attribute name="OC_FARNELL" value="9664947"/>
<attribute name="OC_NEWARK" value="45J1099"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14503BCPG" prefix="U">
<description>Hex Non-Inverting 3-State Buffer</description>
<gates>
<gate name="A" symbol="MC14503BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="DIS_A" pad="1"/>
<connect gate="A" pin="DIS_B" pad="15"/>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_2" pad="4"/>
<connect gate="A" pin="IN_3" pad="6"/>
<connect gate="A" pin="IN_4" pad="10"/>
<connect gate="A" pin="IN_5" pad="12"/>
<connect gate="A" pin="IN_6" pad="14"/>
<connect gate="A" pin="OUT_1" pad="3"/>
<connect gate="A" pin="OUT_2" pad="5"/>
<connect gate="A" pin="OUT_3" pad="7"/>
<connect gate="A" pin="OUT_4" pad="9"/>
<connect gate="A" pin="OUT_5" pad="11"/>
<connect gate="A" pin="OUT_6" pad="13"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14503BCPG"/>
<attribute name="OC_FARNELL" value="9664769"/>
<attribute name="OC_NEWARK" value="45J1100"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14503BDG" prefix="U">
<description>Hex Non-Inverting 3-State Buffer</description>
<gates>
<gate name="A" symbol="MC14503BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="DIS_A" pad="1"/>
<connect gate="A" pin="DIS_B" pad="15"/>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_2" pad="4"/>
<connect gate="A" pin="IN_3" pad="6"/>
<connect gate="A" pin="IN_4" pad="10"/>
<connect gate="A" pin="IN_5" pad="12"/>
<connect gate="A" pin="IN_6" pad="14"/>
<connect gate="A" pin="OUT_1" pad="3"/>
<connect gate="A" pin="OUT_2" pad="5"/>
<connect gate="A" pin="OUT_3" pad="7"/>
<connect gate="A" pin="OUT_4" pad="9"/>
<connect gate="A" pin="OUT_5" pad="11"/>
<connect gate="A" pin="OUT_6" pad="13"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14503BDG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="71J5487"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14504BCPG" prefix="U">
<description>Hex Level Shifter</description>
<gates>
<gate name="A" symbol="MC14504BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="AIN" pad="3"/>
<connect gate="A" pin="AOUT" pad="2"/>
<connect gate="A" pin="BIN" pad="5"/>
<connect gate="A" pin="BOUT" pad="4"/>
<connect gate="A" pin="CIN" pad="7"/>
<connect gate="A" pin="COUT" pad="6"/>
<connect gate="A" pin="DIN" pad="9"/>
<connect gate="A" pin="DOUT" pad="10"/>
<connect gate="A" pin="EIN" pad="11"/>
<connect gate="A" pin="EOUT" pad="12"/>
<connect gate="A" pin="FIN" pad="14"/>
<connect gate="A" pin="FOUT" pad="15"/>
<connect gate="A" pin="MODE" pad="13"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14504BCPG"/>
<attribute name="OC_FARNELL" value="9665064"/>
<attribute name="OC_NEWARK" value="45J1101"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14504BDG" prefix="U">
<description>Hex Level Shifter for TTL to CMOS or CMOS to CMOS</description>
<gates>
<gate name="A" symbol="MC14504BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="AIN" pad="3"/>
<connect gate="A" pin="AOUT" pad="2"/>
<connect gate="A" pin="BIN" pad="5"/>
<connect gate="A" pin="BOUT" pad="4"/>
<connect gate="A" pin="CIN" pad="7"/>
<connect gate="A" pin="COUT" pad="6"/>
<connect gate="A" pin="DIN" pad="9"/>
<connect gate="A" pin="DOUT" pad="10"/>
<connect gate="A" pin="EIN" pad="11"/>
<connect gate="A" pin="EOUT" pad="12"/>
<connect gate="A" pin="FIN" pad="14"/>
<connect gate="A" pin="FOUT" pad="15"/>
<connect gate="A" pin="MODE" pad="13"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14504BDG"/>
<attribute name="OC_FARNELL" value="9665218"/>
<attribute name="OC_NEWARK" value="71J5489"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14504BDR2G" prefix="U">
<description>Hex Level Shifter for TTL to CMOS or CMOS to CMOS</description>
<gates>
<gate name="A" symbol="MC14504BDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="AIN" pad="3"/>
<connect gate="A" pin="AOUT" pad="2"/>
<connect gate="A" pin="BIN" pad="5"/>
<connect gate="A" pin="BOUT" pad="4"/>
<connect gate="A" pin="CIN" pad="7"/>
<connect gate="A" pin="COUT" pad="6"/>
<connect gate="A" pin="DIN" pad="9"/>
<connect gate="A" pin="DOUT" pad="10"/>
<connect gate="A" pin="EIN" pad="11"/>
<connect gate="A" pin="EOUT" pad="12"/>
<connect gate="A" pin="FIN" pad="14"/>
<connect gate="A" pin="FOUT" pad="15"/>
<connect gate="A" pin="MODE" pad="13"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14504BDR2G"/>
<attribute name="OC_FARNELL" value="1273197"/>
<attribute name="OC_NEWARK" value="84K8754"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14511BCPG" prefix="U">
<description>BCD-To-Seven Segment</description>
<gates>
<gate name="A" symbol="MC14511BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A" pad="13"/>
<connect gate="A" pin="A_2" pad="7"/>
<connect gate="A" pin="B" pad="12"/>
<connect gate="A" pin="B_2" pad="1"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="C_2" pad="2"/>
<connect gate="A" pin="D" pad="10"/>
<connect gate="A" pin="D_2" pad="6"/>
<connect gate="A" pin="E" pad="9"/>
<connect gate="A" pin="F" pad="15"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="LE" pad="5"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~BI" pad="4"/>
<connect gate="A" pin="~LT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14511BCPG"/>
<attribute name="OC_FARNELL" value="9665617"/>
<attribute name="OC_NEWARK" value="45J1104"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14512BCPG" prefix="U">
<description>8-Channel Data Selector</description>
<gates>
<gate name="A" symbol="MC14512BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="12"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="DIS" pad="15"/>
<connect gate="A" pin="INH" pad="10"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="X0" pad="1"/>
<connect gate="A" pin="X1" pad="2"/>
<connect gate="A" pin="X2" pad="3"/>
<connect gate="A" pin="X3" pad="4"/>
<connect gate="A" pin="X4" pad="5"/>
<connect gate="A" pin="X5" pad="6"/>
<connect gate="A" pin="X6" pad="7"/>
<connect gate="A" pin="X7" pad="9"/>
<connect gate="A" pin="Z" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14512BCPG"/>
<attribute name="OC_FARNELL" value="9665625"/>
<attribute name="OC_NEWARK" value="45J1105"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14512BDG" prefix="U">
<description>8-Channel Data Selector</description>
<gates>
<gate name="A" symbol="MC14512BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="12"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="DIS" pad="15"/>
<connect gate="A" pin="INH" pad="10"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="X0" pad="1"/>
<connect gate="A" pin="X1" pad="2"/>
<connect gate="A" pin="X2" pad="3"/>
<connect gate="A" pin="X3" pad="4"/>
<connect gate="A" pin="X4" pad="5"/>
<connect gate="A" pin="X5" pad="6"/>
<connect gate="A" pin="X6" pad="7"/>
<connect gate="A" pin="X7" pad="9"/>
<connect gate="A" pin="Z" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14512BDG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="71J5491"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14513BCPG" prefix="U">
<description>BCD-To-Seven Segment</description>
<gates>
<gate name="A" symbol="MC14513BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-18">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="A_2" pad="7"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="B_2" pad="1"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="C_2" pad="2"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="A" pin="D_2" pad="6"/>
<connect gate="A" pin="E" pad="11"/>
<connect gate="A" pin="F" pad="17"/>
<connect gate="A" pin="G" pad="16"/>
<connect gate="A" pin="LE" pad="5"/>
<connect gate="A" pin="RBI" pad="8"/>
<connect gate="A" pin="RBO" pad="10"/>
<connect gate="A" pin="VDD" pad="18"/>
<connect gate="A" pin="VSS" pad="9"/>
<connect gate="A" pin="~BI" pad="4"/>
<connect gate="A" pin="~LT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14513BCPG"/>
<attribute name="OC_FARNELL" value="1353501"/>
<attribute name="OC_NEWARK" value="71J5493"/>
<attribute name="PACKAGE" value="PDIP-18"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14516BCPG" prefix="U">
<description>Binary Up/Down Counter</description>
<gates>
<gate name="A" symbol="MC14516BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="C" pad="15"/>
<connect gate="A" pin="P0" pad="4"/>
<connect gate="A" pin="P1" pad="12"/>
<connect gate="A" pin="P2" pad="13"/>
<connect gate="A" pin="P3" pad="3"/>
<connect gate="A" pin="PE" pad="1"/>
<connect gate="A" pin="Q0" pad="6"/>
<connect gate="A" pin="Q1" pad="11"/>
<connect gate="A" pin="Q2" pad="14"/>
<connect gate="A" pin="Q3" pad="2"/>
<connect gate="A" pin="R" pad="9"/>
<connect gate="A" pin="U/D" pad="10"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~CARRY_IN" pad="5"/>
<connect gate="A" pin="~CARRY_OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14516BCPG"/>
<attribute name="OC_FARNELL" value="9665293"/>
<attribute name="OC_NEWARK" value="45J1108"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14518BCPG" prefix="U">
<description>Dual Up Counters</description>
<gates>
<gate name="A" symbol="MC14518BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CA" pad="1"/>
<connect gate="A" pin="CB" pad="9"/>
<connect gate="A" pin="EA" pad="2"/>
<connect gate="A" pin="EB" pad="10"/>
<connect gate="A" pin="Q0A" pad="3"/>
<connect gate="A" pin="Q0B" pad="11"/>
<connect gate="A" pin="Q1A" pad="4"/>
<connect gate="A" pin="Q1B" pad="12"/>
<connect gate="A" pin="Q2A" pad="5"/>
<connect gate="A" pin="Q2B" pad="13"/>
<connect gate="A" pin="Q3A" pad="6"/>
<connect gate="A" pin="Q3B" pad="14"/>
<connect gate="A" pin="RA" pad="7"/>
<connect gate="A" pin="RB" pad="15"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14518BCPG"/>
<attribute name="OC_FARNELL" value="9665633"/>
<attribute name="OC_NEWARK" value="45J1110"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14520BCPG" prefix="U">
<description>Dual Up Counters</description>
<gates>
<gate name="A" symbol="MC14520BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CA" pad="1"/>
<connect gate="A" pin="CB" pad="9"/>
<connect gate="A" pin="EA" pad="2"/>
<connect gate="A" pin="EB" pad="10"/>
<connect gate="A" pin="Q0A" pad="3"/>
<connect gate="A" pin="Q0B" pad="11"/>
<connect gate="A" pin="Q1A" pad="4"/>
<connect gate="A" pin="Q1B" pad="12"/>
<connect gate="A" pin="Q2A" pad="5"/>
<connect gate="A" pin="Q2B" pad="13"/>
<connect gate="A" pin="Q3A" pad="6"/>
<connect gate="A" pin="Q3B" pad="14"/>
<connect gate="A" pin="RA" pad="7"/>
<connect gate="A" pin="RB" pad="15"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14520BCPG"/>
<attribute name="OC_FARNELL" value="9665676"/>
<attribute name="OC_NEWARK" value="45J1111"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14521BCPG" prefix="U">
<description>24-Stage Frequency Divider</description>
<gates>
<gate name="A" symbol="MC14521BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="IN_1" pad="9"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="7"/>
<connect gate="A" pin="OUT_2" pad="4"/>
<connect gate="A" pin="Q18" pad="10"/>
<connect gate="A" pin="Q19" pad="11"/>
<connect gate="A" pin="Q20" pad="12"/>
<connect gate="A" pin="Q21" pad="13"/>
<connect gate="A" pin="Q22" pad="14"/>
<connect gate="A" pin="Q23" pad="15"/>
<connect gate="A" pin="Q24" pad="1"/>
<connect gate="A" pin="RESET" pad="2"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VDD_2" pad="5"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="VSS_2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14521BCPG"/>
<attribute name="OC_FARNELL" value="9664793"/>
<attribute name="OC_NEWARK" value="45J1112"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14521BDG" prefix="U">
<description>24-Stage Frequency Divider</description>
<gates>
<gate name="A" symbol="MC14521BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="IN_1" pad="9"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT_2" pad="4"/>
<connect gate="A" pin="Q18" pad="10"/>
<connect gate="A" pin="Q19" pad="11"/>
<connect gate="A" pin="Q20" pad="12"/>
<connect gate="A" pin="Q21" pad="13"/>
<connect gate="A" pin="Q22" pad="14"/>
<connect gate="A" pin="Q23" pad="15"/>
<connect gate="A" pin="Q24" pad="1"/>
<connect gate="A" pin="RESET" pad="2"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VDD_2" pad="5"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="VSS_2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14521BDG"/>
<attribute name="OC_FARNELL" value="1705943"/>
<attribute name="OC_NEWARK" value="45J1113"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14528BCPG" prefix="U">
<description>Dual Monostable Multivibrator</description>
<gates>
<gate name="A" symbol="MC14528BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="12"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="11"/>
<connect gate="A" pin="CX1/RX1" pad="2"/>
<connect gate="A" pin="CX2/RX2" pad="14"/>
<connect gate="A" pin="Q1" pad="6"/>
<connect gate="A" pin="Q2" pad="10"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="1"/>
<connect gate="A" pin="VSS_2" pad="8"/>
<connect gate="A" pin="VSS_3" pad="15"/>
<connect gate="A" pin="~Q1" pad="7"/>
<connect gate="A" pin="~Q2" pad="9"/>
<connect gate="A" pin="~RESET_1" pad="3"/>
<connect gate="A" pin="~RESET_2" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14528BCPG"/>
<attribute name="OC_FARNELL" value="9665749"/>
<attribute name="OC_NEWARK" value="45J1116"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14528BDG" prefix="U">
<description>Dual Monostable Multivibrator</description>
<gates>
<gate name="A" symbol="MC14528BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="12"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="11"/>
<connect gate="A" pin="CX1/RX1" pad="2"/>
<connect gate="A" pin="CX2/RX2" pad="14"/>
<connect gate="A" pin="Q1" pad="6"/>
<connect gate="A" pin="Q2" pad="10"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="15"/>
<connect gate="A" pin="VSS_2" pad="1"/>
<connect gate="A" pin="VSS_3" pad="8"/>
<connect gate="A" pin="~Q1" pad="7"/>
<connect gate="A" pin="~Q2" pad="9"/>
<connect gate="A" pin="~RESET_1" pad="3"/>
<connect gate="A" pin="~RESET_2" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14528BDG"/>
<attribute name="OC_FARNELL" value="9666567"/>
<attribute name="OC_NEWARK" value="26K3964"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14532BCPG" prefix="U">
<description>8-Bit Priority Encoder</description>
<gates>
<gate name="A" symbol="MC14532BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="D0" pad="10"/>
<connect gate="A" pin="D1" pad="11"/>
<connect gate="A" pin="D2" pad="12"/>
<connect gate="A" pin="D3" pad="13"/>
<connect gate="A" pin="D4" pad="1"/>
<connect gate="A" pin="D5" pad="2"/>
<connect gate="A" pin="D6" pad="3"/>
<connect gate="A" pin="D7" pad="4"/>
<connect gate="A" pin="EIN" pad="5"/>
<connect gate="A" pin="EOUT" pad="15"/>
<connect gate="A" pin="GS" pad="14"/>
<connect gate="A" pin="Q0" pad="9"/>
<connect gate="A" pin="Q1" pad="7"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14532BCPG"/>
<attribute name="OC_FARNELL" value="9665641"/>
<attribute name="OC_NEWARK" value="45J1118"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14536BCPG" prefix="U">
<description>Programmable Timer</description>
<gates>
<gate name="A" symbol="MC14536BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="8-BYPASS" pad="6"/>
<connect gate="A" pin="A" pad="9"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="CLOCK_INH" pad="7"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="A" pin="DECODE" pad="13"/>
<connect gate="A" pin="IN_1" pad="3"/>
<connect gate="A" pin="MONO-IN" pad="15"/>
<connect gate="A" pin="OSC_INH" pad="14"/>
<connect gate="A" pin="OUT_1" pad="4"/>
<connect gate="A" pin="OUT_2" pad="5"/>
<connect gate="A" pin="RESET" pad="2"/>
<connect gate="A" pin="SET" pad="1"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14536BCPG"/>
<attribute name="OC_FARNELL" value="9664807"/>
<attribute name="OC_NEWARK" value="26K3966"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14536BDWG" prefix="U">
<description>Programmable Timer</description>
<gates>
<gate name="A" symbol="MC14536BDWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="8-BYPASS" pad="6"/>
<connect gate="A" pin="A" pad="9"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="CLC_INH" pad="7"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="A" pin="DECODE" pad="13"/>
<connect gate="A" pin="IN_1" pad="3"/>
<connect gate="A" pin="MONO-IN" pad="15"/>
<connect gate="A" pin="OSC_INH" pad="14"/>
<connect gate="A" pin="OUT_1" pad="4"/>
<connect gate="A" pin="OUT_2" pad="5"/>
<connect gate="A" pin="RESET" pad="2"/>
<connect gate="A" pin="SET" pad="1"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14536BDWG"/>
<attribute name="OC_FARNELL" value="9665234"/>
<attribute name="OC_NEWARK" value="26K3967"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14538BCPG" prefix="U">
<description>Monostable Multivibrator</description>
<gates>
<gate name="A" symbol="MC14538BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="AA" pad="4"/>
<connect gate="A" pin="AB" pad="12"/>
<connect gate="A" pin="CX/RXA" pad="2"/>
<connect gate="A" pin="CX/RXB" pad="14"/>
<connect gate="A" pin="QA" pad="6"/>
<connect gate="A" pin="QB" pad="10"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="VSS_2" pad="1"/>
<connect gate="A" pin="VSS_3" pad="15"/>
<connect gate="A" pin="~BA" pad="5"/>
<connect gate="A" pin="~BB" pad="11"/>
<connect gate="A" pin="~QA" pad="7"/>
<connect gate="A" pin="~QB" pad="9"/>
<connect gate="A" pin="~RESET_A" pad="3"/>
<connect gate="A" pin="~RESET_B" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14538BCPG"/>
<attribute name="OC_FARNELL" value="9665650"/>
<attribute name="OC_NEWARK" value="45J1120"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14538BDG" prefix="U">
<description>Dual Precision Retriggerable/Resettable Monostable Multivibrator</description>
<gates>
<gate name="A" symbol="MC14538BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="AA" pad="4"/>
<connect gate="A" pin="AB" pad="12"/>
<connect gate="A" pin="CX/RXA" pad="2"/>
<connect gate="A" pin="CX/RXB" pad="14"/>
<connect gate="A" pin="QA" pad="6"/>
<connect gate="A" pin="QB" pad="10"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="VSS_2" pad="15"/>
<connect gate="A" pin="VSS_3" pad="1"/>
<connect gate="A" pin="~BA" pad="5"/>
<connect gate="A" pin="~BB" pad="11"/>
<connect gate="A" pin="~QA" pad="7"/>
<connect gate="A" pin="~QB" pad="9"/>
<connect gate="A" pin="~RESET_A" pad="3"/>
<connect gate="A" pin="~RESET_B" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14538BDG"/>
<attribute name="OC_FARNELL" value="9666575"/>
<attribute name="OC_NEWARK" value="45J1121"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14538BDWG" prefix="U">
<description>Dual Precision Retriggerable/Resettable Monostable Multivibrator</description>
<gates>
<gate name="A" symbol="MC14538BDWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="AA" pad="4"/>
<connect gate="A" pin="AB" pad="12"/>
<connect gate="A" pin="CX/RXA" pad="2"/>
<connect gate="A" pin="CX/RXB" pad="14"/>
<connect gate="A" pin="QA" pad="6"/>
<connect gate="A" pin="QB" pad="10"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="1"/>
<connect gate="A" pin="VSS_2" pad="15"/>
<connect gate="A" pin="VSS_3" pad="8"/>
<connect gate="A" pin="~BA" pad="5"/>
<connect gate="A" pin="~BB" pad="11"/>
<connect gate="A" pin="~QA" pad="7"/>
<connect gate="A" pin="~QB" pad="9"/>
<connect gate="A" pin="~RESET_A" pad="3"/>
<connect gate="A" pin="~RESET_B" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14538BDWG"/>
<attribute name="OC_FARNELL" value="9664920"/>
<attribute name="OC_NEWARK" value="26K3968"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14541BCPG" prefix="U">
<description>Programmable Timer</description>
<gates>
<gate name="A" symbol="MC14541BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="A" pad="12"/>
<connect gate="A" pin="AR" pad="5"/>
<connect gate="A" pin="B" pad="13"/>
<connect gate="A" pin="CTC" pad="2"/>
<connect gate="A" pin="MODE" pad="10"/>
<connect gate="A" pin="MR" pad="6"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="A" pin="Q/~Q_SEL" pad="9"/>
<connect gate="A" pin="RS" pad="3"/>
<connect gate="A" pin="RTC" pad="1"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14541BCPG"/>
<attribute name="OC_FARNELL" value="9665668"/>
<attribute name="OC_NEWARK" value="45J1124"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14541BDG" prefix="U">
<description>Programmable Timer</description>
<gates>
<gate name="A" symbol="MC14541BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A" pad="12"/>
<connect gate="A" pin="AR" pad="5"/>
<connect gate="A" pin="B" pad="13"/>
<connect gate="A" pin="CTC" pad="2"/>
<connect gate="A" pin="MODE" pad="10"/>
<connect gate="A" pin="MR" pad="6"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="A" pin="Q/~Q_SEL" pad="9"/>
<connect gate="A" pin="RS" pad="3"/>
<connect gate="A" pin="RTC" pad="1"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14541BDG"/>
<attribute name="OC_FARNELL" value="9666583"/>
<attribute name="OC_NEWARK" value="26K3971"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14541BDR2G" prefix="U">
<description>Programmable Timer</description>
<gates>
<gate name="A" symbol="MC14541BDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A" pad="12"/>
<connect gate="A" pin="AR" pad="5"/>
<connect gate="A" pin="B" pad="13"/>
<connect gate="A" pin="CTC" pad="2"/>
<connect gate="A" pin="MODE" pad="10"/>
<connect gate="A" pin="MR" pad="6"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="A" pin="Q/~Q_SEL" pad="9"/>
<connect gate="A" pin="RS" pad="3"/>
<connect gate="A" pin="RTC" pad="1"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14541BDR2G"/>
<attribute name="OC_FARNELL" value="1365197"/>
<attribute name="OC_NEWARK" value="84K8755"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14543BDG" prefix="U">
<description>BCD-to-Seven Segment Latch/Decoder/Driver for Liquid Crystals</description>
<gates>
<gate name="A" symbol="MC14543BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A" pad="9"/>
<connect gate="A" pin="A_2" pad="5"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="BI" pad="7"/>
<connect gate="A" pin="B_2" pad="3"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="C_2" pad="2"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="A" pin="D_2" pad="4"/>
<connect gate="A" pin="E" pad="13"/>
<connect gate="A" pin="F" pad="15"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="LD" pad="1"/>
<connect gate="A" pin="PH" pad="6"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14543BDG"/>
<attribute name="OC_FARNELL" value="9664939"/>
<attribute name="OC_NEWARK" value="71J5499"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14551BCPG" prefix="U">
<description>Multiplexer/Demultiplexer</description>
<gates>
<gate name="A" symbol="MC14551BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CONTROL" pad="9"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="W" pad="14"/>
<connect gate="A" pin="W0" pad="15"/>
<connect gate="A" pin="W1" pad="1"/>
<connect gate="A" pin="X" pad="4"/>
<connect gate="A" pin="X0" pad="2"/>
<connect gate="A" pin="X1" pad="3"/>
<connect gate="A" pin="Y" pad="5"/>
<connect gate="A" pin="Y0" pad="6"/>
<connect gate="A" pin="Y1" pad="10"/>
<connect gate="A" pin="Z" pad="13"/>
<connect gate="A" pin="Z0" pad="11"/>
<connect gate="A" pin="Z1" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14551BCPG"/>
<attribute name="OC_FARNELL" value="9665072"/>
<attribute name="OC_NEWARK" value="45J1130"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14551BDG" prefix="U">
<description>Quad 2-Channel Analog Multiplexer/Demultiplexer</description>
<gates>
<gate name="A" symbol="MC14551BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="CONTROL" pad="9"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="W" pad="14"/>
<connect gate="A" pin="W0" pad="15"/>
<connect gate="A" pin="W1" pad="1"/>
<connect gate="A" pin="X" pad="4"/>
<connect gate="A" pin="X0" pad="2"/>
<connect gate="A" pin="X1" pad="3"/>
<connect gate="A" pin="Y" pad="5"/>
<connect gate="A" pin="Y0" pad="6"/>
<connect gate="A" pin="Y1" pad="10"/>
<connect gate="A" pin="Z" pad="13"/>
<connect gate="A" pin="Z0" pad="11"/>
<connect gate="A" pin="Z1" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14551BDG"/>
<attribute name="OC_FARNELL" value="9665242"/>
<attribute name="OC_NEWARK" value="71J5501"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14553BCPG" prefix="U">
<description>3-Digit BCD Counter</description>
<gates>
<gate name="A" symbol="MC14553BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CIA" pad="4"/>
<connect gate="A" pin="CIB" pad="3"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="DIS" pad="11"/>
<connect gate="A" pin="LE" pad="10"/>
<connect gate="A" pin="MR" pad="13"/>
<connect gate="A" pin="O.F" pad="14"/>
<connect gate="A" pin="Q0" pad="9"/>
<connect gate="A" pin="Q1" pad="7"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="5"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~DS1" pad="2"/>
<connect gate="A" pin="~DS2" pad="1"/>
<connect gate="A" pin="~DS3" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14553BCPG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J1131"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14555BCPG" prefix="U">
<description>Dual Binary to 1-of-4 Decoder/Demultiplexer</description>
<gates>
<gate name="A" symbol="MC14555BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="AA" pad="2"/>
<connect gate="A" pin="AB" pad="14"/>
<connect gate="A" pin="BA" pad="3"/>
<connect gate="A" pin="BB" pad="13"/>
<connect gate="A" pin="Q0A" pad="4"/>
<connect gate="A" pin="Q0B" pad="12"/>
<connect gate="A" pin="Q1A" pad="5"/>
<connect gate="A" pin="Q1B" pad="11"/>
<connect gate="A" pin="Q2A" pad="6"/>
<connect gate="A" pin="Q2B" pad="10"/>
<connect gate="A" pin="Q3A" pad="7"/>
<connect gate="A" pin="Q3B" pad="9"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~EA" pad="1"/>
<connect gate="A" pin="~EB" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14555BCPG"/>
<attribute name="OC_FARNELL" value="9665277"/>
<attribute name="OC_NEWARK" value="45J1132"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14557BCPG" prefix="U">
<description>Shift Register</description>
<gates>
<gate name="A" symbol="MC14557BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A" pad="7"/>
<connect gate="A" pin="A/B_SEL" pad="9"/>
<connect gate="A" pin="B" pad="6"/>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="L1" pad="2"/>
<connect gate="A" pin="L16" pad="13"/>
<connect gate="A" pin="L2" pad="1"/>
<connect gate="A" pin="L32" pad="12"/>
<connect gate="A" pin="L4" pad="15"/>
<connect gate="A" pin="L8" pad="14"/>
<connect gate="A" pin="Q" pad="10"/>
<connect gate="A" pin="RESET" pad="3"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~CE" pad="5"/>
<connect gate="A" pin="~Q" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14557BCPG"/>
<attribute name="OC_FARNELL" value="1191819"/>
<attribute name="OC_NEWARK" value="45J1134"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1455BP1G" prefix="U">
<description>Timers</description>
<gates>
<gate name="A" symbol="MC1455BP1G"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="CONTROL_VOLTAGE" pad="5"/>
<connect gate="A" pin="DISCHARGE" pad="7"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="OUTPUT" pad="3"/>
<connect gate="A" pin="RESET" pad="4"/>
<connect gate="A" pin="THRESHOLD" pad="6"/>
<connect gate="A" pin="TRIGGER" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC1455BP1G"/>
<attribute name="OC_FARNELL" value="1468729"/>
<attribute name="OC_NEWARK" value="98H0658"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1455P1G" prefix="U">
<description>Timers</description>
<gates>
<gate name="A" symbol="MC1455P1G"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="CONTROL_VOLTAGE" pad="5"/>
<connect gate="A" pin="DISCHARGE" pad="7"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="OUTPUT" pad="3"/>
<connect gate="A" pin="RESET" pad="4"/>
<connect gate="A" pin="THRESHOLD" pad="6"/>
<connect gate="A" pin="TRIGGER" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC1455P1G"/>
<attribute name="OC_FARNELL" value="9664394"/>
<attribute name="OC_NEWARK" value="88H4718"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14569BCPG" prefix="U">
<description>Programmable Divide-By-N Dual 4-Bit Binary/BCD Down Counter</description>
<gates>
<gate name="A" symbol="MC14569BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CASCADE_FEEDBACK" pad="7"/>
<connect gate="A" pin="CLOCK" pad="9"/>
<connect gate="A" pin="CTL1" pad="2"/>
<connect gate="A" pin="CTL2" pad="10"/>
<connect gate="A" pin="P0" pad="3"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="5"/>
<connect gate="A" pin="P3" pad="6"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="12"/>
<connect gate="A" pin="P6" pad="13"/>
<connect gate="A" pin="P7" pad="14"/>
<connect gate="A" pin="Q" pad="15"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="ZERO_DETECT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14569BCPG"/>
<attribute name="OC_FARNELL" value="1191831"/>
<attribute name="OC_NEWARK" value="45J1136"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14584BCPG" prefix="U">
<description>Hex Schmitt Trigger</description>
<gates>
<gate name="A" symbol="MC14584BCPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN1" pad="1"/>
<connect gate="A" pin="IN2" pad="3"/>
<connect gate="A" pin="IN3" pad="5"/>
<connect gate="A" pin="IN4" pad="9"/>
<connect gate="A" pin="IN5" pad="11"/>
<connect gate="A" pin="IN6" pad="13"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="4"/>
<connect gate="A" pin="OUT3" pad="6"/>
<connect gate="A" pin="OUT4" pad="8"/>
<connect gate="A" pin="OUT5" pad="10"/>
<connect gate="A" pin="OUT6" pad="12"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14584BCPG"/>
<attribute name="OC_FARNELL" value="9665099"/>
<attribute name="OC_NEWARK" value="45J1139"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14584BDG" prefix="U">
<description>Hex Schmitt Trigger</description>
<gates>
<gate name="A" symbol="MC14584BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1" pad="1"/>
<connect gate="A" pin="IN_2" pad="3"/>
<connect gate="A" pin="IN_3" pad="5"/>
<connect gate="A" pin="IN_4" pad="9"/>
<connect gate="A" pin="IN_5" pad="11"/>
<connect gate="A" pin="IN_6" pad="13"/>
<connect gate="A" pin="OUT_1" pad="2"/>
<connect gate="A" pin="OUT_2" pad="4"/>
<connect gate="A" pin="OUT_3" pad="6"/>
<connect gate="A" pin="OUT_4" pad="8"/>
<connect gate="A" pin="OUT_5" pad="10"/>
<connect gate="A" pin="OUT_6" pad="12"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14584BDG"/>
<attribute name="OC_FARNELL" value="9665102"/>
<attribute name="OC_NEWARK" value="45J1140"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14584BDR2G" prefix="U">
<description>Hex Schmitt Trigger</description>
<gates>
<gate name="A" symbol="MC14584BDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN_1" pad="1"/>
<connect gate="A" pin="IN_2" pad="3"/>
<connect gate="A" pin="IN_3" pad="5"/>
<connect gate="A" pin="IN_4" pad="9"/>
<connect gate="A" pin="IN_5" pad="11"/>
<connect gate="A" pin="IN_6" pad="13"/>
<connect gate="A" pin="OUT_1" pad="2"/>
<connect gate="A" pin="OUT_2" pad="4"/>
<connect gate="A" pin="OUT_3" pad="6"/>
<connect gate="A" pin="OUT_4" pad="8"/>
<connect gate="A" pin="OUT_5" pad="10"/>
<connect gate="A" pin="OUT_6" pad="12"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14584BDR2G"/>
<attribute name="OC_FARNELL" value="1365199"/>
<attribute name="OC_NEWARK" value="84K8756"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14585BDG" prefix="U">
<description>4-Bit Magnitude Comparator</description>
<gates>
<gate name="A" symbol="MC14585BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="(A_&lt;_B)IN" pad="5"/>
<connect gate="A" pin="(A_&lt;_B)OUT" pad="12"/>
<connect gate="A" pin="(A_=_B)IN" pad="6"/>
<connect gate="A" pin="(A_=_B)OUT" pad="3"/>
<connect gate="A" pin="(A_&gt;_B)IN" pad="4"/>
<connect gate="A" pin="(A_&gt;_B)OUT" pad="13"/>
<connect gate="A" pin="A0" pad="10"/>
<connect gate="A" pin="A1" pad="7"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="A3" pad="15"/>
<connect gate="A" pin="B0" pad="11"/>
<connect gate="A" pin="B1" pad="9"/>
<connect gate="A" pin="B2" pad="1"/>
<connect gate="A" pin="B3" pad="14"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC14585BDG"/>
<attribute name="OC_FARNELL" value="1191839"/>
<attribute name="OC_NEWARK" value="71J5507"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1488DG" prefix="U">
<description>Quad Line EIA-232D Driver</description>
<gates>
<gate name="A" symbol="MC1488DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B1" pad="4"/>
<connect gate="A" pin="IN_B2" pad="5"/>
<connect gate="A" pin="IN_C1" pad="10"/>
<connect gate="A" pin="IN_C2" pad="9"/>
<connect gate="A" pin="IN_D1" pad="13"/>
<connect gate="A" pin="IN_D2" pad="12"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="6"/>
<connect gate="A" pin="OUT_C" pad="8"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VEE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC1488DG"/>
<attribute name="OC_FARNELL" value="1147618"/>
<attribute name="OC_NEWARK" value="26K3980"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1488PG" prefix="U">
<description>Quad Line EIA-232D Driver</description>
<gates>
<gate name="A" symbol="MC1488PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B1" pad="4"/>
<connect gate="A" pin="IN_B2" pad="5"/>
<connect gate="A" pin="IN_C1" pad="10"/>
<connect gate="A" pin="IN_C2" pad="9"/>
<connect gate="A" pin="IN_D1" pad="13"/>
<connect gate="A" pin="IN_D2" pad="12"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="6"/>
<connect gate="A" pin="OUT_C" pad="8"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VEE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC1488PG"/>
<attribute name="OC_FARNELL" value="9664530"/>
<attribute name="OC_NEWARK" value="98H0659"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1489ADG" prefix="U">
<description>Quad Line EIA-232D Receivers</description>
<gates>
<gate name="A" symbol="MC1489ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN_A" pad="1"/>
<connect gate="A" pin="IN_B" pad="4"/>
<connect gate="A" pin="IN_C" pad="10"/>
<connect gate="A" pin="IN_D" pad="13"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="6"/>
<connect gate="A" pin="OUT_C" pad="8"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="RESPONSE_CONTROL_A" pad="2"/>
<connect gate="A" pin="RESPONSE_CONTROL_B" pad="5"/>
<connect gate="A" pin="RESPONSE_CONTROL_C" pad="9"/>
<connect gate="A" pin="RESPONSE_CONTROL_D" pad="12"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC1489ADG"/>
<attribute name="OC_FARNELL" value="1350100"/>
<attribute name="OC_NEWARK" value="42K0556"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1489DG" prefix="U">
<description>Quad Line EIA-232D Receivers</description>
<gates>
<gate name="A" symbol="MC1489DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN_A" pad="1"/>
<connect gate="A" pin="IN_B" pad="4"/>
<connect gate="A" pin="IN_C" pad="10"/>
<connect gate="A" pin="IN_D" pad="13"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="6"/>
<connect gate="A" pin="OUT_C" pad="8"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="RESPONSE_CONTROL_A" pad="2"/>
<connect gate="A" pin="RESPONSE_CONTROL_B" pad="5"/>
<connect gate="A" pin="RESPONSE_CONTROL_C" pad="9"/>
<connect gate="A" pin="RESPONSE_CONTROL_D" pad="12"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC1489DG"/>
<attribute name="OC_FARNELL" value="1607611"/>
<attribute name="OC_NEWARK" value="45J1146"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1489PG" prefix="U">
<description>Quad Line EIA-232D Receivers</description>
<gates>
<gate name="A" symbol="MC1489PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN_A" pad="1"/>
<connect gate="A" pin="IN_B" pad="4"/>
<connect gate="A" pin="IN_C" pad="10"/>
<connect gate="A" pin="IN_D" pad="13"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="6"/>
<connect gate="A" pin="OUT_C" pad="8"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="RESPONSE_COTROL_A" pad="2"/>
<connect gate="A" pin="RESPONSE_COTROL_B" pad="5"/>
<connect gate="A" pin="RESPONSE_COTROL_C" pad="9"/>
<connect gate="A" pin="RESPONSE_COTROL_D" pad="12"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC1489PG"/>
<attribute name="OC_FARNELL" value="1211144"/>
<attribute name="OC_NEWARK" value="98H0661"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1496BPG" prefix="U">
<description>Balanced Modulators /Demodulators</description>
<gates>
<gate name="A" symbol="MC1496BPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="CARRIER_IN" pad="10"/>
<connect gate="A" pin="GAIN_ADJUST" pad="2"/>
<connect gate="A" pin="GAIN_ADJUST_2" pad="3"/>
<connect gate="A" pin="IN_CARRIER" pad="8"/>
<connect gate="A" pin="N/C" pad="7"/>
<connect gate="A" pin="N/C_2" pad="11"/>
<connect gate="A" pin="N/C_3" pad="9"/>
<connect gate="A" pin="N/C_4" pad="13"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="OUT_2" pad="12"/>
<connect gate="A" pin="SIGNAL_IN" pad="1"/>
<connect gate="A" pin="SIGNAL_IN_2" pad="4"/>
<connect gate="A" pin="VEE" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC1496BPG"/>
<attribute name="OC_FARNELL" value="1125967"/>
<attribute name="OC_NEWARK" value="26K3981"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1496DR2G" prefix="U">
<description>Balanced Modulators/Demodulators</description>
<gates>
<gate name="A" symbol="MC1496DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="CARRIER_IN" pad="10"/>
<connect gate="A" pin="GAIN_ADJ" pad="2"/>
<connect gate="A" pin="GAIN_ADJ_2" pad="3"/>
<connect gate="A" pin="IN_CARRIER" pad="8"/>
<connect gate="A" pin="N/C" pad="13"/>
<connect gate="A" pin="N/C_2" pad="7"/>
<connect gate="A" pin="N/C_3" pad="9"/>
<connect gate="A" pin="N/C_4" pad="11"/>
<connect gate="A" pin="OUT" pad="12"/>
<connect gate="A" pin="OUT_2" pad="6"/>
<connect gate="A" pin="SIG_IN" pad="4"/>
<connect gate="A" pin="SIG_IN_2" pad="1"/>
<connect gate="A" pin="VEE" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC1496DR2G"/>
<attribute name="OC_FARNELL" value="1651904"/>
<attribute name="OC_NEWARK" value="45J1148"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC3302PG" prefix="U">
<description>Comparators</description>
<gates>
<gate name="A" symbol="MC3302PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC3302PG"/>
<attribute name="OC_FARNELL" value="1468733"/>
<attribute name="OC_NEWARK" value="71J5510"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33033DWR2G" prefix="U">
<description>Brushless DC Motor Controller</description>
<gates>
<gate name="A" symbol="MC33033DWR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="60_DEG/120DEG__SELECT" pad="18"/>
<connect gate="A" pin="AB" pad="17"/>
<connect gate="A" pin="AT" pad="2"/>
<connect gate="A" pin="BB" pad="16"/>
<connect gate="A" pin="BT" pad="1"/>
<connect gate="A" pin="CB" pad="15"/>
<connect gate="A" pin="CT" pad="20"/>
<connect gate="A" pin="CURRENT_SENSE_POS" pad="12"/>
<connect gate="A" pin="ERROR_AMP_NEG" pad="10"/>
<connect gate="A" pin="ERROR_AMP_OUT/PWM_INPUT" pad="11"/>
<connect gate="A" pin="ERROR_AMP_POS" pad="9"/>
<connect gate="A" pin="FWD/REV" pad="3"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="OSCILLATOR" pad="8"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="19"/>
<connect gate="A" pin="REFERENCE_OUTPUT" pad="7"/>
<connect gate="A" pin="SA" pad="4"/>
<connect gate="A" pin="SB" pad="5"/>
<connect gate="A" pin="SC" pad="6"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33033DWR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84K8758"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33035DWG" prefix="U">
<description>Brushless DC Motor Controller</description>
<gates>
<gate name="A" symbol="MC33035DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-24N">
<connects>
<connect gate="A" pin="60°/~120°_SELECT" pad="22"/>
<connect gate="A" pin="AB" pad="21"/>
<connect gate="A" pin="AT" pad="2"/>
<connect gate="A" pin="BB" pad="20"/>
<connect gate="A" pin="BRAKE" pad="23"/>
<connect gate="A" pin="BT" pad="1"/>
<connect gate="A" pin="CB" pad="19"/>
<connect gate="A" pin="CT" pad="24"/>
<connect gate="A" pin="CURRENT_SENSE_INVERTING_INPUT" pad="15"/>
<connect gate="A" pin="CURRENT_SENSE_NONINVERTING_INPUT" pad="9"/>
<connect gate="A" pin="ERROR_AMP_INVERTING_INPUT" pad="12"/>
<connect gate="A" pin="ERROR_AMP_NONINVERTING_INPUT" pad="11"/>
<connect gate="A" pin="ERROR_AMP_OUT_PWM_INPUT" pad="13"/>
<connect gate="A" pin="FWD/REV" pad="3"/>
<connect gate="A" pin="GND" pad="16"/>
<connect gate="A" pin="OSCILLATOR" pad="10"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="7"/>
<connect gate="A" pin="REFERENCE_OUTPUT" pad="8"/>
<connect gate="A" pin="SA" pad="4"/>
<connect gate="A" pin="SB" pad="5"/>
<connect gate="A" pin="SC" pad="6"/>
<connect gate="A" pin="VC" pad="18"/>
<connect gate="A" pin="VCC" pad="17"/>
<connect gate="A" pin="~FAULT_OUTPUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33035DWG"/>
<attribute name="OC_FARNELL" value="1652428"/>
<attribute name="OC_NEWARK" value="26K3990"/>
<attribute name="PACKAGE" value="SOIC-24"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33039DG" prefix="U">
<description>Closed Loop Brushless Motor Adapter</description>
<gates>
<gate name="A" symbol="MC33039DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="A" pin="FOUT" pad="5"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="RT/CT" pad="6"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~A" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33039DG"/>
<attribute name="OC_FARNELL" value="1211112"/>
<attribute name="OC_NEWARK" value="45J1154"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC3303PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC3303PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="IN_3" pad="9"/>
<connect gate="A" pin="IN_3_2" pad="10"/>
<connect gate="A" pin="IN_4" pad="12"/>
<connect gate="A" pin="IN_4_2" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC3303PG"/>
<attribute name="OC_FARNELL" value="1426358"/>
<attribute name="OC_NEWARK" value="26K3986"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33060ADG" prefix="U">
<description>Fixed Frequency, PWM, Voltage Mode Single Ended Controllers</description>
<gates>
<gate name="A" symbol="MC33060ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="COMPEN/PWM_COMP_INPUT" pad="3"/>
<connect gate="A" pin="CT" pad="5"/>
<connect gate="A" pin="DEAD-TIME_CONTROL" pad="4"/>
<connect gate="A" pin="E" pad="8"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="N.C." pad="11"/>
<connect gate="A" pin="NEG_IN" pad="2"/>
<connect gate="A" pin="NEG_IN_2" pad="13"/>
<connect gate="A" pin="POS_IN" pad="14"/>
<connect gate="A" pin="POS_IN_2" pad="1"/>
<connect gate="A" pin="RT" pad="6"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="VREF" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33060ADG"/>
<attribute name="OC_FARNELL" value="1468735"/>
<attribute name="OC_NEWARK" value="71J5511"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33063ADG" prefix="U">
<description>Step-Up/Down/Inverting Switching Regulators</description>
<gates>
<gate name="A" symbol="MC33063ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMPTR_NEG" pad="5"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="DRVR_C" pad="8"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IPK_SENSE" pad="7"/>
<connect gate="A" pin="SW_C" pad="1"/>
<connect gate="A" pin="SW_E" pad="2"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33063ADG"/>
<attribute name="OC_FARNELL" value="9664440"/>
<attribute name="OC_NEWARK" value="88H4720"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33063ADR2G" prefix="U">
<description>Step-Up/Down/Inverting Switching Regulators</description>
<gates>
<gate name="A" symbol="MC33063ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMPTR_NEG" pad="5"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="DRVR_C" pad="8"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IPK_SENSE" pad="7"/>
<connect gate="A" pin="SW_C" pad="1"/>
<connect gate="A" pin="SW_E" pad="2"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33063ADR2G"/>
<attribute name="OC_FARNELL" value="1569173"/>
<attribute name="OC_NEWARK" value="88H4721"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33063AP1G" prefix="U">
<description>Regulators</description>
<gates>
<gate name="A" symbol="MC33063AP1G"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COMP_NEG" pad="5"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="DRVR_C" pad="8"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IPK_SEN" pad="7"/>
<connect gate="A" pin="SW_C" pad="1"/>
<connect gate="A" pin="SW_E" pad="2"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33063AP1G"/>
<attribute name="OC_FARNELL" value="9664432"/>
<attribute name="OC_NEWARK" value="45J1156"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33064D-5G" prefix="U">
<description>Undervoltage Sensing Circuit</description>
<gates>
<gate name="A" symbol="MC33064D-5G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INPUT" pad="2"/>
<connect gate="A" pin="N.C." pad="7"/>
<connect gate="A" pin="N.C._2" pad="3"/>
<connect gate="A" pin="N.C._3" pad="8"/>
<connect gate="A" pin="N.C._4" pad="5"/>
<connect gate="A" pin="N.C._5" pad="6"/>
<connect gate="A" pin="~RESET" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33064D-5G"/>
<attribute name="OC_FARNELL" value="1211114"/>
<attribute name="OC_NEWARK" value="26K3992"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33064D-5R2G" prefix="U">
<description>Undervoltage Sensing Circuit</description>
<gates>
<gate name="A" symbol="MC33064D-5R2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INPUT" pad="2"/>
<connect gate="A" pin="N.C." pad="8"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="N.C._3" pad="3"/>
<connect gate="A" pin="N.C._4" pad="7"/>
<connect gate="A" pin="N.C._5" pad="6"/>
<connect gate="A" pin="~RESET" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33064D-5R2G"/>
<attribute name="OC_FARNELL" value="1155800"/>
<attribute name="OC_NEWARK" value="98H0668"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33071ADG" prefix="U">
<description>Single Supply 3.0 V to 44 V Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33071ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NEG_IN" pad="2"/>
<connect gate="A" pin="OFFSET_NULL" pad="1"/>
<connect gate="A" pin="OFFSET_NULL_2" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS_IN" pad="3"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33071ADG"/>
<attribute name="OC_FARNELL" value="1155801"/>
<attribute name="OC_NEWARK" value="98H0669"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33071APG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33071APG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="IN_2" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OFS" pad="5"/>
<connect gate="A" pin="OFS_2" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33071APG"/>
<attribute name="OC_FARNELL" value="1315259"/>
<attribute name="OC_NEWARK" value="42K0570"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33072APG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33072APG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33072APG"/>
<attribute name="OC_FARNELL" value="1147620"/>
<attribute name="OC_NEWARK" value="26K3998"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33072DG" prefix="U">
<description>Single Supply 3.0 V to 44 V Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33072DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33072DG"/>
<attribute name="OC_FARNELL" value="1651872"/>
<attribute name="OC_NEWARK" value="71J5514"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33072DR2G" prefix="U">
<description>Single Supply 3.0 V to 44 V Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33072DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN_1" pad="3"/>
<connect gate="A" pin="IN_1_2" pad="2"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33072DR2G"/>
<attribute name="OC_FARNELL" value="1261138"/>
<attribute name="OC_NEWARK" value="88H4723"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33072PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33072PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33072PG"/>
<attribute name="OC_FARNELL" value="1191841"/>
<attribute name="OC_NEWARK" value="98H0672"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33074ADG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33074ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33074ADG"/>
<attribute name="OC_FARNELL" value="1136151"/>
<attribute name="OC_NEWARK" value="45J1159"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33074ADR2G" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33074ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33074ADR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="98H0673"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33074ADTBG" prefix="U">
<description>Single Supply 3.0 V to 44 V OPAMPs</description>
<gates>
<gate name="A" symbol="MC33074ADTBG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33074ADTBG"/>
<attribute name="OC_FARNELL" value="1705871"/>
<attribute name="OC_NEWARK" value="42K0572"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33074APG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33074APG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="3"/>
<connect gate="A" pin="IN_1_2" pad="2"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="IN_3" pad="9"/>
<connect gate="A" pin="IN_3_2" pad="10"/>
<connect gate="A" pin="IN_4" pad="13"/>
<connect gate="A" pin="IN_4_2" pad="12"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33074APG"/>
<attribute name="OC_FARNELL" value="1126236"/>
<attribute name="OC_NEWARK" value="42K0574"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33074DG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33074DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33074DG"/>
<attribute name="OC_FARNELL" value="1211115"/>
<attribute name="OC_NEWARK" value="45J1160"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33074DR2G" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33074DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33074DR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="98H0674"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33074PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33074PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="IN_3" pad="10"/>
<connect gate="A" pin="IN_3_2" pad="9"/>
<connect gate="A" pin="IN_4" pad="13"/>
<connect gate="A" pin="IN_4_2" pad="12"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33074PG"/>
<attribute name="OC_FARNELL" value="9666800"/>
<attribute name="OC_NEWARK" value="26K3999"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33077DG" prefix="U">
<description>Low Noise Dual Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33077DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="2"/>
<connect gate="A" pin="NEG_IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="3"/>
<connect gate="A" pin="POS_IN_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33077DG"/>
<attribute name="OC_FARNELL" value="1211116"/>
<attribute name="OC_NEWARK" value="98H0675"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33078DG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33078DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN_1" pad="3"/>
<connect gate="A" pin="+IN_2" pad="5"/>
<connect gate="A" pin="-IN_1" pad="2"/>
<connect gate="A" pin="-IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33078DG"/>
<attribute name="OC_FARNELL" value="9665323"/>
<attribute name="OC_NEWARK" value="71J5515"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33079DG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33079DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="5"/>
<connect gate="A" pin="IN2_2" pad="6"/>
<connect gate="A" pin="IN3" pad="9"/>
<connect gate="A" pin="IN3_2" pad="10"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33079DG"/>
<attribute name="OC_FARNELL" value="9665331"/>
<attribute name="OC_NEWARK" value="98H0677"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33079PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33079PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="IN_3" pad="9"/>
<connect gate="A" pin="IN_3_2" pad="10"/>
<connect gate="A" pin="IN_4" pad="12"/>
<connect gate="A" pin="IN_4_2" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33079PG"/>
<attribute name="OC_FARNELL" value="9665030"/>
<attribute name="OC_NEWARK" value="98H0678"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33151PG" prefix="U">
<description>Dual MOSFET Drivers</description>
<gates>
<gate name="A" symbol="MC33151PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="DRIVE_OUTPUT_A" pad="7"/>
<connect gate="A" pin="DRIVE_OUTPUT_B" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="I_A" pad="2"/>
<connect gate="A" pin="I_B" pad="4"/>
<connect gate="A" pin="N.C" pad="8"/>
<connect gate="A" pin="N.C_2" pad="1"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33151PG"/>
<attribute name="OC_FARNELL" value="9666770"/>
<attribute name="OC_NEWARK" value="45J1165"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33152DG" prefix="U">
<description>High Speed Dual MOSFET Drivers</description>
<gates>
<gate name="A" symbol="MC33152DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DRVR_OUTA" pad="7"/>
<connect gate="A" pin="DRVR_OUTB" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="4"/>
<connect gate="A" pin="N.C." pad="8"/>
<connect gate="A" pin="N.C._2" pad="1"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33152DG"/>
<attribute name="OC_FARNELL" value="1191817"/>
<attribute name="OC_NEWARK" value="26K4001"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33152PG" prefix="U">
<description>Dual MOSFET Drivers</description>
<gates>
<gate name="A" symbol="MC33152PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="DRIVE_OUTPUT_A" pad="7"/>
<connect gate="A" pin="DRIVE_OUTPUT_B" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="I_A" pad="2"/>
<connect gate="A" pin="I_B" pad="4"/>
<connect gate="A" pin="N.C" pad="8"/>
<connect gate="A" pin="N.C_2" pad="1"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33152PG"/>
<attribute name="OC_FARNELL" value="9666788"/>
<attribute name="OC_NEWARK" value="45J1167"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33153DG" prefix="U">
<description>Single IGBT Gate Driver</description>
<gates>
<gate name="A" symbol="MC33153DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CURRENT_SEN_IN" pad="1"/>
<connect gate="A" pin="DRIVE_OUT" pad="5"/>
<connect gate="A" pin="FAULT_BLANKING/DESATURATION_IN" pad="8"/>
<connect gate="A" pin="FAULT_OUT" pad="7"/>
<connect gate="A" pin="KELVIN_GND" pad="2"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="~INPUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33153DG"/>
<attribute name="OC_FARNELL" value="1104702"/>
<attribute name="OC_NEWARK" value="42K0579"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33153DR2G" prefix="U">
<description>Single IGBT Gate Driver</description>
<gates>
<gate name="A" symbol="MC33153DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CURRENT_SENSE_IN" pad="1"/>
<connect gate="A" pin="DRIVE_OUT" pad="5"/>
<connect gate="A" pin="FAULT_BLANKING/DESATURATION_IN" pad="8"/>
<connect gate="A" pin="FAULT_OUT" pad="7"/>
<connect gate="A" pin="KELVIN_GND" pad="2"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="~INPUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33153DR2G"/>
<attribute name="OC_FARNELL" value="1278011"/>
<attribute name="OC_NEWARK" value="42K0580"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33153PG" prefix="U">
<description>Single IGBT Gate Driver</description>
<gates>
<gate name="A" symbol="MC33153PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="DR_OUT" pad="5"/>
<connect gate="A" pin="FAULT_BLANKING/DESATURATION_INPUT" pad="8"/>
<connect gate="A" pin="FLT_OUT" pad="7"/>
<connect gate="A" pin="ISEN_IN" pad="1"/>
<connect gate="A" pin="KELVIN_GND" pad="2"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="~INPUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33153PG"/>
<attribute name="OC_FARNELL" value="1104713"/>
<attribute name="OC_NEWARK" value="42K0581"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33161DG" prefix="U">
<description>Universal Voltage Monitors</description>
<gates>
<gate name="A" symbol="MC33161DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_2" pad="3"/>
<connect gate="A" pin="MODE" pad="7"/>
<connect gate="A" pin="OUT_1" pad="6"/>
<connect gate="A" pin="OUT_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33161DG"/>
<attribute name="OC_FARNELL" value="1192059"/>
<attribute name="OC_NEWARK" value="98H0679"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33161PG" prefix="U">
<description>Universal Voltage Monitors</description>
<gates>
<gate name="A" symbol="MC33161PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INPUT_1" pad="2"/>
<connect gate="A" pin="INPUT_2" pad="3"/>
<connect gate="A" pin="MODE_SELECT" pad="7"/>
<connect gate="A" pin="OUTPUT_1" pad="6"/>
<connect gate="A" pin="OUTPUT_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33161PG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J1168"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33164D-3G" prefix="U">
<description>Micropower Undervoltage Sensing Circuits</description>
<gates>
<gate name="A" symbol="MC33164D-3G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INPUT" pad="2"/>
<connect gate="A" pin="N.C." pad="8"/>
<connect gate="A" pin="N.C._2" pad="5"/>
<connect gate="A" pin="N.C._3" pad="3"/>
<connect gate="A" pin="N.C._4" pad="7"/>
<connect gate="A" pin="N.C._5" pad="6"/>
<connect gate="A" pin="~RESET" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33164D-3G"/>
<attribute name="OC_FARNELL" value="1705998"/>
<attribute name="OC_NEWARK" value="71J5517"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33171DG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33171DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OFS" pad="1"/>
<connect gate="A" pin="OFS_2" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33171DG"/>
<attribute name="OC_FARNELL" value="1104707"/>
<attribute name="OC_NEWARK" value="42K0590"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33171PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33171PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="INV._IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NONINV._IN" pad="3"/>
<connect gate="A" pin="OFS" pad="5"/>
<connect gate="A" pin="OFS_2" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33171PG"/>
<attribute name="OC_FARNELL" value="9664955"/>
<attribute name="OC_NEWARK" value="26K4011"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33172DG" prefix="U">
<description>Single Supply 3.0 V to 44 V, Low Power Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33172DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="2"/>
<connect gate="A" pin="NEG_IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="3"/>
<connect gate="A" pin="POS_IN_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33172DG"/>
<attribute name="OC_FARNELL" value="9665307"/>
<attribute name="OC_NEWARK" value="17H1572"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33172DR2G" prefix="U">
<description>Single Supply 3.0 V to 44 V, Low Power Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33172DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="2"/>
<connect gate="A" pin="NEG_IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="3"/>
<connect gate="A" pin="POS_IN_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33172DR2G"/>
<attribute name="OC_FARNELL" value="1651873"/>
<attribute name="OC_NEWARK" value="84K8759"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33172PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33172PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33172PG"/>
<attribute name="OC_FARNELL" value="9664963"/>
<attribute name="OC_NEWARK" value="45J1173"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33174PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33174PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="IN_3" pad="9"/>
<connect gate="A" pin="IN_3_2" pad="10"/>
<connect gate="A" pin="IN_4" pad="12"/>
<connect gate="A" pin="IN_4_2" pad="13"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33174PG"/>
<attribute name="OC_FARNELL" value="9664971"/>
<attribute name="OC_NEWARK" value="71J5520"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33178DG" prefix="U">
<description>Low Power, Low Noise Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33178DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="2"/>
<connect gate="A" pin="NEG_IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="3"/>
<connect gate="A" pin="POS_IN_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33178DG"/>
<attribute name="OC_FARNELL" value="1468737"/>
<attribute name="OC_NEWARK" value="88H4724"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33178PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33178PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33178PG"/>
<attribute name="OC_FARNELL" value="9666818"/>
<attribute name="OC_NEWARK" value="71J5521"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33179DG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33179DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="5"/>
<connect gate="A" pin="IN2_2" pad="6"/>
<connect gate="A" pin="IN3" pad="9"/>
<connect gate="A" pin="IN3_2" pad="10"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33179DG"/>
<attribute name="OC_FARNELL" value="1651874"/>
<attribute name="OC_NEWARK" value="98H0686"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33179DR2G" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33179DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="2"/>
<connect gate="A" pin="IN1_2" pad="3"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="9"/>
<connect gate="A" pin="IN3_2" pad="10"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33179DR2G"/>
<attribute name="OC_FARNELL" value="1261557"/>
<attribute name="OC_NEWARK" value="98H0687"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33179PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33179PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="IN_3" pad="9"/>
<connect gate="A" pin="IN_3_2" pad="10"/>
<connect gate="A" pin="IN_4" pad="12"/>
<connect gate="A" pin="IN_4_2" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33179PG"/>
<attribute name="OC_FARNELL" value="9666826"/>
<attribute name="OC_NEWARK" value="26K4013"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33201DG" prefix="U">
<description>Low Voltage, Rail-to-Rail Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33201DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NEG_IN" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS_IN" pad="3"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33201DG"/>
<attribute name="OC_FARNELL" value="9666656"/>
<attribute name="OC_NEWARK" value="71J5522"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33202DG" prefix="U">
<description>Low Voltage, Rail-to-Rail Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33202DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="3"/>
<connect gate="A" pin="NEG_IN_2" pad="5"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="2"/>
<connect gate="A" pin="POS_IN_2" pad="6"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33202DG"/>
<attribute name="OC_FARNELL" value="9666672"/>
<attribute name="OC_NEWARK" value="17H1575"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33202PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33202PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33202PG"/>
<attribute name="OC_FARNELL" value="9666680"/>
<attribute name="OC_NEWARK" value="71J5524"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33202VDG" prefix="U">
<description>Low Voltage, Rail-to-Rail Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33202VDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN_1" pad="3"/>
<connect gate="A" pin="IN_1_2" pad="2"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33202VDG"/>
<attribute name="OC_FARNELL" value="1143534"/>
<attribute name="OC_NEWARK" value="26K4016"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33204DG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33204DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="5"/>
<connect gate="A" pin="IN2_2" pad="6"/>
<connect gate="A" pin="IN3" pad="9"/>
<connect gate="A" pin="IN3_2" pad="10"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33204DG"/>
<attribute name="OC_FARNELL" value="9666699"/>
<attribute name="OC_NEWARK" value="45J1178"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33204DTBG" prefix="U">
<description>Low Voltage, Rail-to-Rail OPAMPs</description>
<gates>
<gate name="A" symbol="MC33204DTBG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33204DTBG"/>
<attribute name="OC_FARNELL" value="1703205"/>
<attribute name="OC_NEWARK" value="42K0597"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33262DG" prefix="U">
<description>Power Factor Controllers</description>
<gates>
<gate name="A" symbol="MC33262DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="DRIVE_OUTPUT" pad="7"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ISEN_IN" pad="4"/>
<connect gate="A" pin="MULTIPLIER_INPUT" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK_INPUT" pad="1"/>
<connect gate="A" pin="ZERO_CURRENT_DETECT_INPUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33262DG"/>
<attribute name="OC_FARNELL" value="9664475"/>
<attribute name="OC_NEWARK" value="88H4727"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33262PG" prefix="U">
<description>Power Factor Controllers</description>
<gates>
<gate name="A" symbol="MC33262PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="DRIVE_OUTPUT" pad="7"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ISEN" pad="4"/>
<connect gate="A" pin="MULTIPLIER_INPUT" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK_INPUT" pad="1"/>
<connect gate="A" pin="ZERO_CURRENT_DETECT_INPUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33262PG"/>
<attribute name="OC_FARNELL" value="9666745"/>
<attribute name="OC_NEWARK" value="98H0691"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33269D-3.3G" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC33269D-3.3G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND/ADJ" pad="1"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
<connect gate="A" pin="VOUT_2" pad="2"/>
<connect gate="A" pin="VOUT_3" pad="7"/>
<connect gate="A" pin="VOUT_4" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33269D-3.3G"/>
<attribute name="OC_FARNELL" value="1652329"/>
<attribute name="OC_NEWARK" value="45J1180"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33269DG" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC33269DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND/ADJ" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="7"/>
<connect gate="A" pin="VOUT_2" pad="6"/>
<connect gate="A" pin="VOUT_3" pad="2"/>
<connect gate="A" pin="VOUT_4" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33269DG"/>
<attribute name="OC_FARNELL" value="1260774"/>
<attribute name="OC_NEWARK" value="42K0603"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33272ADG" prefix="U">
<description>Single Supply,High Slew Rate,Low Input Offset Voltage,Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33272ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="2"/>
<connect gate="A" pin="NEG_IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="3"/>
<connect gate="A" pin="POS_IN_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33272ADG"/>
<attribute name="OC_FARNELL" value="1651875"/>
<attribute name="OC_NEWARK" value="45J1186"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33272ADR2G" prefix="U">
<description>Single Supply,High Slew Rate,Low Input Offset Voltage,Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33272ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="3"/>
<connect gate="A" pin="NEG_IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="2"/>
<connect gate="A" pin="POS_IN_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33272ADR2G"/>
<attribute name="OC_FARNELL" value="1258879"/>
<attribute name="OC_NEWARK" value="88H4728"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33274APG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC33274APG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="IN_3" pad="9"/>
<connect gate="A" pin="IN_3_2" pad="10"/>
<connect gate="A" pin="IN_4" pad="12"/>
<connect gate="A" pin="IN_4_2" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33274APG"/>
<attribute name="OC_FARNELL" value="9666842"/>
<attribute name="OC_NEWARK" value="26K4020"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33363ADWG" prefix="U">
<description>High Voltage Switching Regulator</description>
<gates>
<gate name="A" symbol="MC33363ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="COMPENSATION" pad="9"/>
<connect gate="A" pin="CT" pad="7"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="5"/>
<connect gate="A" pin="OVERVOLTAGE_PROTECTION_INPUT" pad="11"/>
<connect gate="A" pin="POWER_SWITCH_DRAIN" pad="16"/>
<connect gate="A" pin="REGULATOR_OUTPUT" pad="8"/>
<connect gate="A" pin="RT" pad="6"/>
<connect gate="A" pin="STARTUP_INPUT" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK_INPUT" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33363ADWG"/>
<attribute name="OC_FARNELL" value="1136116"/>
<attribute name="OC_NEWARK" value="42K0622"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33363BDWG" prefix="U">
<description>High Voltage Switching Regulator</description>
<gates>
<gate name="A" symbol="MC33363BDWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="COMPENSATION" pad="9"/>
<connect gate="A" pin="CT" pad="7"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="5"/>
<connect gate="A" pin="OVERVOLTAGE_PROTECTION_INPUT" pad="11"/>
<connect gate="A" pin="POWER_SWITCH_DRAIN" pad="16"/>
<connect gate="A" pin="REGULATOR_OUTPUT" pad="8"/>
<connect gate="A" pin="RT" pad="6"/>
<connect gate="A" pin="STARTUP_INPUT" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK_INPUT" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33363BDWG"/>
<attribute name="OC_FARNELL" value="1192057"/>
<attribute name="OC_NEWARK" value="42K0623"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33364DG" prefix="U">
<description>Critical Conduction GreenLinet SMPS Controller</description>
<gates>
<gate name="A" symbol="MC33364DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A_GND" pad="9"/>
<connect gate="A" pin="CURRENT_SENSE" pad="3"/>
<connect gate="A" pin="FREQ_CLAMP" pad="8"/>
<connect gate="A" pin="GATE_DRIVE" pad="11"/>
<connect gate="A" pin="LINE" pad="16"/>
<connect gate="A" pin="N/C" pad="2"/>
<connect gate="A" pin="N/C_2" pad="7"/>
<connect gate="A" pin="N/C_3" pad="5"/>
<connect gate="A" pin="N/C_4" pad="13"/>
<connect gate="A" pin="P_GND" pad="10"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VOLTAGE_FB" pad="4"/>
<connect gate="A" pin="VREF" pad="6"/>
<connect gate="A" pin="ZERO_CURRENT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33364DG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="42K0624"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33368DG" prefix="U">
<description>High Voltage GreenLinet Power Factor Controller</description>
<gates>
<gate name="A" symbol="MC33368DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="5.0_VREF" pad="1"/>
<connect gate="A" pin="AGND" pad="8"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="CURRENT_SENSE" pad="6"/>
<connect gate="A" pin="FREQUENCY_CLAMP" pad="13"/>
<connect gate="A" pin="GATE" pad="11"/>
<connect gate="A" pin="LEB" pad="9"/>
<connect gate="A" pin="LINE" pad="16"/>
<connect gate="A" pin="MULT" pad="5"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RESTART_DELAY" pad="2"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VOLTAGE_FB" pad="3"/>
<connect gate="A" pin="ZERO_CURRENT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33368DG"/>
<attribute name="OC_FARNELL" value="1468740"/>
<attribute name="OC_NEWARK" value="42K0627"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33502DG" prefix="U">
<description>1.0 V, Rail-to-Rail, Dual Operational Amplifier</description>
<gates>
<gate name="A" symbol="MC33502DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="2"/>
<connect gate="A" pin="NEG_IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="3"/>
<connect gate="A" pin="POS_IN_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33502DG"/>
<attribute name="OC_FARNELL" value="1468742"/>
<attribute name="OC_NEWARK" value="26K4035"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33502DR2G" prefix="U">
<description>1.0 V, Rail-to-Rail, Dual Operational Amplifier</description>
<gates>
<gate name="A" symbol="MC33502DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="2"/>
<connect gate="A" pin="NEG_IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="3"/>
<connect gate="A" pin="POS_IN_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33502DR2G"/>
<attribute name="OC_FARNELL" value="1703207"/>
<attribute name="OC_NEWARK" value="84K8761"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33502PG" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="MC33502PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="IN_1" pad="3"/>
<connect gate="A" pin="IN_1_2" pad="2"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33502PG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="70K3089"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33503SNT1G" prefix="U">
<description>Micropower Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC33503SNT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VEE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33503SNT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J1202"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33761SNT1-050G" prefix="U">
<description>Dropout Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC33761SNT1-050G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC33761SNT1-050G"/>
<attribute name="OC_FARNELL" value="1232007"/>
<attribute name="OC_NEWARK" value="83H7303"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34023PG" prefix="U">
<description>High Speed Single-Ended PWM Controller</description>
<gates>
<gate name="A" symbol="MC34023PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CLOCK" pad="4"/>
<connect gate="A" pin="CT" pad="6"/>
<connect gate="A" pin="CURRENT_LIMIT/SHUTDOWN" pad="9"/>
<connect gate="A" pin="CURRENT_LIMIT_REFERENCE" pad="11"/>
<connect gate="A" pin="ERROR_AMP_NEG" pad="1"/>
<connect gate="A" pin="ERROR_AMP_OUT" pad="3"/>
<connect gate="A" pin="ERROR_AMP_POS" pad="2"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OUT" pad="14"/>
<connect gate="A" pin="POWER_GND" pad="12"/>
<connect gate="A" pin="RAMP" pad="7"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SOFT-START" pad="8"/>
<connect gate="A" pin="VC" pad="13"/>
<connect gate="A" pin="VCC" pad="15"/>
<connect gate="A" pin="VREF" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34023PG"/>
<attribute name="OC_FARNELL" value="1143553"/>
<attribute name="OC_NEWARK" value="61K0888"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34025PG" prefix="U">
<description>High Speed Double-Ended PWM Controller</description>
<gates>
<gate name="A" symbol="MC34025PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CLOCK" pad="4"/>
<connect gate="A" pin="CT" pad="6"/>
<connect gate="A" pin="CURRENT_LIMIT/SHUTDOWN" pad="9"/>
<connect gate="A" pin="ERROR_AMP_NEG" pad="1"/>
<connect gate="A" pin="ERROR_AMP_OUT" pad="3"/>
<connect gate="A" pin="ERROR_AMP_POS" pad="2"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OUTPUT_A" pad="11"/>
<connect gate="A" pin="OUTPUT_B" pad="14"/>
<connect gate="A" pin="POWER_GND" pad="12"/>
<connect gate="A" pin="RAMP" pad="7"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SOFT-START" pad="8"/>
<connect gate="A" pin="VC" pad="13"/>
<connect gate="A" pin="VCC" pad="15"/>
<connect gate="A" pin="VREF" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34025PG"/>
<attribute name="OC_FARNELL" value="1364615"/>
<attribute name="OC_NEWARK" value="45J1204"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC3403PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC3403PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="3"/>
<connect gate="A" pin="IN_1_2" pad="2"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="IN_3" pad="10"/>
<connect gate="A" pin="IN_3_2" pad="9"/>
<connect gate="A" pin="IN_4" pad="13"/>
<connect gate="A" pin="IN_4_2" pad="12"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE/GND" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC3403PG"/>
<attribute name="OC_FARNELL" value="1126440"/>
<attribute name="OC_NEWARK" value="45J1207"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34060APG" prefix="U">
<description>Fixed Frequency, PWM, Voltage Mode Single Ended Controllers</description>
<gates>
<gate name="A" symbol="MC34060APG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="COMPEN/PWM_COMP_INPUT" pad="3"/>
<connect gate="A" pin="CT" pad="5"/>
<connect gate="A" pin="DEAD-TIME_CONTROL" pad="4"/>
<connect gate="A" pin="E" pad="8"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="INV_IN" pad="2"/>
<connect gate="A" pin="INV_IN_2" pad="13"/>
<connect gate="A" pin="N.C." pad="11"/>
<connect gate="A" pin="NONINV_IN" pad="1"/>
<connect gate="A" pin="NONINV_IN_2" pad="14"/>
<connect gate="A" pin="RT" pad="6"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="VREF" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34060APG"/>
<attribute name="OC_FARNELL" value="1214461"/>
<attribute name="OC_NEWARK" value="26K4038"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34063ADG" prefix="U">
<description>Switching Regulators</description>
<gates>
<gate name="A" symbol="MC34063ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMPARATOR_NEG" pad="5"/>
<connect gate="A" pin="DRVR_C" pad="8"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IPK_SENSE" pad="7"/>
<connect gate="A" pin="SWITCH_C" pad="1"/>
<connect gate="A" pin="SWITCH_E" pad="2"/>
<connect gate="A" pin="TIMING_CAP" pad="3"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34063ADG"/>
<attribute name="OC_FARNELL" value="1211119"/>
<attribute name="OC_NEWARK" value="45J1208"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34063AP1G" prefix="U">
<description>Regulators</description>
<gates>
<gate name="A" symbol="MC34063AP1G"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COMP_NEG" pad="5"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="DRVR_C" pad="8"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IPK_SEN" pad="7"/>
<connect gate="A" pin="SW_C" pad="1"/>
<connect gate="A" pin="SW_E" pad="2"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34063AP1G"/>
<attribute name="OC_FARNELL" value="1191818"/>
<attribute name="OC_NEWARK" value="67H6703"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34064D-5R2G" prefix="U">
<description>Undervoltage Sensing Circuit</description>
<gates>
<gate name="A" symbol="MC34064D-5R2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INPUT" pad="2"/>
<connect gate="A" pin="N.C." pad="7"/>
<connect gate="A" pin="N.C._2" pad="6"/>
<connect gate="A" pin="N.C._3" pad="8"/>
<connect gate="A" pin="N.C._4" pad="3"/>
<connect gate="A" pin="N.C._5" pad="5"/>
<connect gate="A" pin="~RESET" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34064D-5R2G"/>
<attribute name="OC_FARNELL" value="1364616"/>
<attribute name="OC_NEWARK" value="45J1210"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34067PG" prefix="U">
<description>High Performance Resonant Mode Controllers</description>
<gates>
<gate name="A" symbol="MC34067PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CSOFT-START" pad="11"/>
<connect gate="A" pin="DRIVE_OUTPUT_A" pad="14"/>
<connect gate="A" pin="DRIVE_OUTPUT_B" pad="12"/>
<connect gate="A" pin="ENABLE/UVLO_ADJUST" pad="9"/>
<connect gate="A" pin="ERROR_AMP_OUT" pad="6"/>
<connect gate="A" pin="FAULT_INPUT" pad="10"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NEG" pad="7"/>
<connect gate="A" pin="ONE-SHOT_RC" pad="16"/>
<connect gate="A" pin="OSC_CHARGE" pad="1"/>
<connect gate="A" pin="OSC_CONTROL_CURRENT" pad="3"/>
<connect gate="A" pin="OSC_RC" pad="2"/>
<connect gate="A" pin="POS" pad="8"/>
<connect gate="A" pin="POWER_GND" pad="13"/>
<connect gate="A" pin="VCC" pad="15"/>
<connect gate="A" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34067PG"/>
<attribute name="OC_FARNELL" value="1652411"/>
<attribute name="OC_NEWARK" value="88H4731"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34071DG" prefix="U">
<description>Single Supply 3.0 V to 44 V Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC34071DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NEG_IN" pad="2"/>
<connect gate="A" pin="OFS_NULL" pad="5"/>
<connect gate="A" pin="OFS_NULL_2" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS_IN" pad="3"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34071DG"/>
<attribute name="OC_FARNELL" value="1468744"/>
<attribute name="OC_NEWARK" value="45J1214"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34072ADG" prefix="U">
<description>Single Supply 3.0 V to 44 V Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC34072ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="2"/>
<connect gate="A" pin="NEG_IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="3"/>
<connect gate="A" pin="POS_IN_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34072ADG"/>
<attribute name="OC_FARNELL" value="1426371"/>
<attribute name="OC_NEWARK" value="45J1215"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34072APG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC34072APG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34072APG"/>
<attribute name="OC_FARNELL" value="1703202"/>
<attribute name="OC_NEWARK" value="45J1216"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34072DG" prefix="U">
<description>Single Supply 3.0 V to 44 V Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC34072DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="2"/>
<connect gate="A" pin="NEG_IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="3"/>
<connect gate="A" pin="POS_IN_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34072DG"/>
<attribute name="OC_FARNELL" value="9664416"/>
<attribute name="OC_NEWARK" value="88H4732"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34072DR2G" prefix="U">
<description>Single Supply 3.0 V to 44 V Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC34072DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_IN_1" pad="2"/>
<connect gate="A" pin="NEG_IN_2" pad="6"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="POS_IN_1" pad="3"/>
<connect gate="A" pin="POS_IN_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34072DR2G"/>
<attribute name="OC_FARNELL" value="1258880"/>
<attribute name="OC_NEWARK" value="88H4733"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34072PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC34072PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="6"/>
<connect gate="A" pin="IN_2_2" pad="5"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34072PG"/>
<attribute name="OC_FARNELL" value="1468745"/>
<attribute name="OC_NEWARK" value="45J1217"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34074ADG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC34074ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34074ADG"/>
<attribute name="OC_FARNELL" value="1426373"/>
<attribute name="OC_NEWARK" value="45J1218"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34074APG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC34074APG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="IN_3" pad="10"/>
<connect gate="A" pin="IN_3_2" pad="9"/>
<connect gate="A" pin="IN_4" pad="12"/>
<connect gate="A" pin="IN_4_2" pad="13"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34074APG"/>
<attribute name="OC_FARNELL" value="1468746"/>
<attribute name="OC_NEWARK" value="42K0653"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34074DG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC34074DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN1_2" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN2_2" pad="5"/>
<connect gate="A" pin="IN3" pad="10"/>
<connect gate="A" pin="IN3_2" pad="9"/>
<connect gate="A" pin="IN4" pad="13"/>
<connect gate="A" pin="IN4_2" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34074DG"/>
<attribute name="OC_FARNELL" value="1426372"/>
<attribute name="OC_NEWARK" value="42K0654"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34074PG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC34074PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="3"/>
<connect gate="A" pin="IN_1_2" pad="2"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="IN_3" pad="9"/>
<connect gate="A" pin="IN_3_2" pad="10"/>
<connect gate="A" pin="IN_4" pad="12"/>
<connect gate="A" pin="IN_4_2" pad="13"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34074PG"/>
<attribute name="OC_FARNELL" value="1651876"/>
<attribute name="OC_NEWARK" value="45J1220"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34074VPG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="MC34074VPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_1_2" pad="3"/>
<connect gate="A" pin="IN_2" pad="5"/>
<connect gate="A" pin="IN_2_2" pad="6"/>
<connect gate="A" pin="IN_3" pad="10"/>
<connect gate="A" pin="IN_3_2" pad="9"/>
<connect gate="A" pin="IN_4" pad="13"/>
<connect gate="A" pin="IN_4_2" pad="12"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34074VPG"/>
<attribute name="OC_FARNELL" value="1705800"/>
<attribute name="OC_NEWARK" value="26K4046"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34151PG" prefix="U">
<description>Dual MOSFET Drivers</description>
<gates>
<gate name="A" symbol="MC34151PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="DRIVE_OUTPUT_A" pad="7"/>
<connect gate="A" pin="DRIVE_OUTPUT_B" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="I_A" pad="2"/>
<connect gate="A" pin="I_B" pad="4"/>
<connect gate="A" pin="N.C" pad="8"/>
<connect gate="A" pin="N.C_2" pad="1"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34151PG"/>
<attribute name="OC_FARNELL" value="9664459"/>
<attribute name="OC_NEWARK" value="71J5536"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34161DG" prefix="U">
<description>Universal Voltage Monitors</description>
<gates>
<gate name="A" symbol="MC34161DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_2" pad="3"/>
<connect gate="A" pin="MODE" pad="7"/>
<connect gate="A" pin="OUT_1" pad="6"/>
<connect gate="A" pin="OUT_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34161DG"/>
<attribute name="OC_FARNELL" value="1652462"/>
<attribute name="OC_NEWARK" value="98H0701"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34161PG" prefix="U">
<description>Universal Voltage Monitors</description>
<gates>
<gate name="A" symbol="MC34161PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN_1" pad="2"/>
<connect gate="A" pin="IN_2" pad="3"/>
<connect gate="A" pin="MODE" pad="7"/>
<connect gate="A" pin="OUT_1" pad="6"/>
<connect gate="A" pin="OUT_2" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34161PG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="27M2485"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34163DWG" prefix="U">
<description>3.4 A, Step-Up/Down/ Inverting Switching Regulators</description>
<gates>
<gate name="A" symbol="MC34163DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="BOOTSTRAP_IN" pad="16"/>
<connect gate="A" pin="DRIVER_COLLECTOR" pad="9"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="13"/>
<connect gate="A" pin="IPK_SENSE" pad="8"/>
<connect gate="A" pin="LVI_OUT" pad="1"/>
<connect gate="A" pin="SWITCH_COLLECTOR" pad="10"/>
<connect gate="A" pin="SWITCH_COLLECTOR_2" pad="11"/>
<connect gate="A" pin="SWITCH_EMITTER" pad="15"/>
<connect gate="A" pin="SWITCH_EMITTER_2" pad="14"/>
<connect gate="A" pin="TIMING_CAPACITOR" pad="6"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="V_FB_1" pad="3"/>
<connect gate="A" pin="V_FB_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34163DWG"/>
<attribute name="OC_FARNELL" value="1096691"/>
<attribute name="OC_NEWARK" value="26K4047"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34163PG" prefix="U">
<description>3.4 A, Step-Up/Down/ Inverting Switching Regulators</description>
<gates>
<gate name="A" symbol="MC34163PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-16">
<connects>
<connect gate="A" pin="BOOTSTRAP_INPUT" pad="16"/>
<connect gate="A" pin="DRIVER_COLLECTOR" pad="9"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="13"/>
<connect gate="A" pin="IPK_SENSE" pad="8"/>
<connect gate="A" pin="LVI_OUTPUT" pad="1"/>
<connect gate="A" pin="SWITCH_COLLECTOR" pad="11"/>
<connect gate="A" pin="SWITCH_COLLECTOR_2" pad="10"/>
<connect gate="A" pin="SWITCH_EMITTER" pad="14"/>
<connect gate="A" pin="SWITCH_EMITTER_2" pad="15"/>
<connect gate="A" pin="TIMING_CAPACITOR" pad="6"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK_1" pad="3"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34163PG"/>
<attribute name="OC_FARNELL" value="1468747"/>
<attribute name="OC_NEWARK" value="71J5539"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34164D-5G" prefix="U">
<description>Micropower Undervoltage Sensing Circuits</description>
<gates>
<gate name="A" symbol="MC34164D-5G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INPUT" pad="2"/>
<connect gate="A" pin="N.C." pad="8"/>
<connect gate="A" pin="N.C._2" pad="6"/>
<connect gate="A" pin="N.C._3" pad="5"/>
<connect gate="A" pin="N.C._4" pad="7"/>
<connect gate="A" pin="N.C._5" pad="3"/>
<connect gate="A" pin="~RESET" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34164D-5G"/>
<attribute name="OC_FARNELL" value="1703462"/>
<attribute name="OC_NEWARK" value="26K4049"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34262DG" prefix="U">
<description>Power Factor Controllers</description>
<gates>
<gate name="A" symbol="MC34262DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="DRIVE_OUTPUT" pad="7"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ISEN_IN" pad="4"/>
<connect gate="A" pin="MULTIPLIER_INPUT" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK_INPUT" pad="1"/>
<connect gate="A" pin="ZERO_CURRENT_DETECT_INPUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34262DG"/>
<attribute name="OC_FARNELL" value="1468748"/>
<attribute name="OC_NEWARK" value="88H4735"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34262PG" prefix="U">
<description>Power Factor Controllers</description>
<gates>
<gate name="A" symbol="MC34262PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="DRIVE_OUTPUT" pad="7"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ISEN" pad="4"/>
<connect gate="A" pin="MULTIPLIER_INPUT" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK_INPUT" pad="1"/>
<connect gate="A" pin="ZERO_CURRENT_DETECT_INPUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC34262PG"/>
<attribute name="OC_FARNELL" value="1468749"/>
<attribute name="OC_NEWARK" value="42K0668"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC00DG" prefix="U">
<description>Quad 2-Input NAND Gate</description>
<gates>
<gate name="A" symbol="MC74AC00DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC00DG"/>
<attribute name="OC_FARNELL" value="1886881"/>
<attribute name="OC_NEWARK" value="45J1255"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC02DG" prefix="U">
<description>Quad 2-Input NOR Gate</description>
<gates>
<gate name="A" symbol="MC74AC02DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="8"/>
<connect gate="A" pin="A4" pad="11"/>
<connect gate="A" pin="B1" pad="3"/>
<connect gate="A" pin="B2" pad="6"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="B4" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="10"/>
<connect gate="A" pin="Y4" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC02DG"/>
<attribute name="OC_FARNELL" value="1706001"/>
<attribute name="OC_NEWARK" value="71J5560"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC04DG" prefix="U">
<description>Hex Inverter</description>
<gates>
<gate name="A" symbol="MC74AC04DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN" pad="11"/>
<connect gate="A" pin="IN_2" pad="1"/>
<connect gate="A" pin="IN_3" pad="3"/>
<connect gate="A" pin="IN_4" pad="5"/>
<connect gate="A" pin="IN_5" pad="13"/>
<connect gate="A" pin="IN_6" pad="9"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="OUT_2" pad="12"/>
<connect gate="A" pin="OUT_3" pad="4"/>
<connect gate="A" pin="OUT_4" pad="2"/>
<connect gate="A" pin="OUT_5" pad="10"/>
<connect gate="A" pin="OUT_6" pad="6"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC04DG"/>
<attribute name="OC_FARNELL" value="1136093"/>
<attribute name="OC_NEWARK" value="26K4108"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC08DG" prefix="U">
<description>Quad 2-Input AND Gate</description>
<gates>
<gate name="A" symbol="MC74AC08DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN" pad="9"/>
<connect gate="A" pin="IN_2" pad="4"/>
<connect gate="A" pin="IN_3" pad="1"/>
<connect gate="A" pin="IN_4" pad="5"/>
<connect gate="A" pin="IN_5" pad="2"/>
<connect gate="A" pin="IN_6" pad="10"/>
<connect gate="A" pin="IN_7" pad="12"/>
<connect gate="A" pin="IN_8" pad="13"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="OUT_2" pad="6"/>
<connect gate="A" pin="OUT_3" pad="3"/>
<connect gate="A" pin="OUT_4" pad="11"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC08DG"/>
<attribute name="OC_FARNELL" value="1468750"/>
<attribute name="OC_NEWARK" value="26K4111"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC132DG" prefix="U">
<description>Quad 2-Input NAND Schmitt Trigger</description>
<gates>
<gate name="A" symbol="MC74AC132DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN" pad="9"/>
<connect gate="A" pin="IN_2" pad="4"/>
<connect gate="A" pin="IN_3" pad="1"/>
<connect gate="A" pin="IN_4" pad="5"/>
<connect gate="A" pin="IN_5" pad="2"/>
<connect gate="A" pin="IN_6" pad="10"/>
<connect gate="A" pin="IN_7" pad="12"/>
<connect gate="A" pin="IN_8" pad="13"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="OUT_2" pad="3"/>
<connect gate="A" pin="OUT_3" pad="6"/>
<connect gate="A" pin="OUT_4" pad="11"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC132DG"/>
<attribute name="OC_FARNELL" value="1705802"/>
<attribute name="OC_NEWARK" value="26K4116"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC138DG" prefix="U">
<description>1-of-8 Decoder/Demultiplexer</description>
<gates>
<gate name="A" symbol="MC74AC138DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="E3" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~E1" pad="4"/>
<connect gate="A" pin="~E2" pad="5"/>
<connect gate="A" pin="~O0" pad="15"/>
<connect gate="A" pin="~O1" pad="14"/>
<connect gate="A" pin="~O2" pad="13"/>
<connect gate="A" pin="~O3" pad="12"/>
<connect gate="A" pin="~O4" pad="11"/>
<connect gate="A" pin="~O5" pad="10"/>
<connect gate="A" pin="~O6" pad="9"/>
<connect gate="A" pin="~O7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC138DG"/>
<attribute name="OC_FARNELL" value="1468752"/>
<attribute name="OC_NEWARK" value="26K4118"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC32DG" prefix="U">
<description>Quad 2-Input OR Gate</description>
<gates>
<gate name="A" symbol="MC74AC32DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN" pad="5"/>
<connect gate="A" pin="IN_2" pad="2"/>
<connect gate="A" pin="IN_3" pad="10"/>
<connect gate="A" pin="IN_4" pad="4"/>
<connect gate="A" pin="IN_5" pad="12"/>
<connect gate="A" pin="IN_6" pad="13"/>
<connect gate="A" pin="IN_7" pad="1"/>
<connect gate="A" pin="IN_8" pad="9"/>
<connect gate="A" pin="OUT" pad="11"/>
<connect gate="A" pin="OUT_2" pad="8"/>
<connect gate="A" pin="OUT_3" pad="6"/>
<connect gate="A" pin="OUT_4" pad="3"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC32DG"/>
<attribute name="OC_FARNELL" value="1147692"/>
<attribute name="OC_NEWARK" value="42K0801"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC4040DG" prefix="U">
<description>12-Stage Binary Ripple Counter</description>
<gates>
<gate name="A" symbol="MC74AC4040DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q10" pad="14"/>
<connect gate="A" pin="Q11" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="A" pin="Q5" pad="3"/>
<connect gate="A" pin="Q6" pad="2"/>
<connect gate="A" pin="Q7" pad="4"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="Q9" pad="12"/>
<connect gate="A" pin="RESET" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC4040DG"/>
<attribute name="OC_FARNELL" value="1607667"/>
<attribute name="OC_NEWARK" value="26K4154"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC4040NG" prefix="U">
<description>12-Stage Binary Ripple Counter</description>
<gates>
<gate name="A" symbol="MC74AC4040NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q10" pad="14"/>
<connect gate="A" pin="Q11" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="A" pin="Q5" pad="3"/>
<connect gate="A" pin="Q6" pad="2"/>
<connect gate="A" pin="Q7" pad="4"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="Q9" pad="12"/>
<connect gate="A" pin="RESET" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC4040NG"/>
<attribute name="OC_FARNELL" value="1703293"/>
<attribute name="OC_NEWARK" value="42K0810"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC573DWG" prefix="U">
<description>Octal Buffer/Line Driver</description>
<gates>
<gate name="A" symbol="MC74AC573DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="D5" pad="7"/>
<connect gate="A" pin="D6" pad="8"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="LE" pad="11"/>
<connect gate="A" pin="O0" pad="19"/>
<connect gate="A" pin="O1" pad="18"/>
<connect gate="A" pin="O2" pad="17"/>
<connect gate="A" pin="O3" pad="16"/>
<connect gate="A" pin="O4" pad="15"/>
<connect gate="A" pin="O5" pad="14"/>
<connect gate="A" pin="O6" pad="13"/>
<connect gate="A" pin="O7" pad="12"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="~OE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC573DWG"/>
<attribute name="OC_FARNELL" value="1607715"/>
<attribute name="OC_NEWARK" value="42K0814"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC574DWR2G" prefix="U">
<description>Octal D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74AC574DWR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="CP" pad="11"/>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="D5" pad="7"/>
<connect gate="A" pin="D6" pad="8"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="O0" pad="19"/>
<connect gate="A" pin="O1" pad="18"/>
<connect gate="A" pin="O2" pad="17"/>
<connect gate="A" pin="O3" pad="16"/>
<connect gate="A" pin="O4" pad="15"/>
<connect gate="A" pin="O5" pad="14"/>
<connect gate="A" pin="O6" pad="13"/>
<connect gate="A" pin="O7" pad="12"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="~OE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC574DWR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26K4165"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC74DG" prefix="U">
<description>Dual D-Type Positive Edge-Triggered Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74AC74DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="CP1" pad="3"/>
<connect gate="A" pin="CP2" pad="11"/>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="D2" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~CD1" pad="1"/>
<connect gate="A" pin="~CD2" pad="13"/>
<connect gate="A" pin="~Q1" pad="6"/>
<connect gate="A" pin="~Q2" pad="8"/>
<connect gate="A" pin="~SD1" pad="4"/>
<connect gate="A" pin="~SD2" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC74DG"/>
<attribute name="OC_FARNELL" value="1705876"/>
<attribute name="OC_NEWARK" value="42K0818"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74AC74NG" prefix="U">
<description>Dual D-Type Positive Edge-Triggered Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74AC74NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="CP1" pad="3"/>
<connect gate="A" pin="CP2" pad="11"/>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="D2" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~CD1" pad="1"/>
<connect gate="A" pin="~CD2" pad="13"/>
<connect gate="A" pin="~Q1" pad="6"/>
<connect gate="A" pin="~Q2" pad="8"/>
<connect gate="A" pin="~SD1" pad="4"/>
<connect gate="A" pin="~SD2" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74AC74NG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J1265"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74ACT00DG" prefix="U">
<description>Quad 2-Input NAND Gate</description>
<gates>
<gate name="A" symbol="MC74ACT00DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74ACT00DG"/>
<attribute name="OC_FARNELL" value="1652018"/>
<attribute name="OC_NEWARK" value="42K0673"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74ACT02DG" prefix="U">
<description>Quad 2-Input NOR Gate</description>
<gates>
<gate name="A" symbol="MC74ACT02DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="8"/>
<connect gate="A" pin="A4" pad="11"/>
<connect gate="A" pin="B1" pad="3"/>
<connect gate="A" pin="B2" pad="6"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="B4" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="10"/>
<connect gate="A" pin="Y4" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74ACT02DG"/>
<attribute name="OC_FARNELL" value="1607770"/>
<attribute name="OC_NEWARK" value="45J1231"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74ACT05DG" prefix="U">
<description>Hex Inverter with Open-Drain Outputs</description>
<gates>
<gate name="A" symbol="MC74ACT05DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74ACT05DG"/>
<attribute name="OC_FARNELL" value="1353833"/>
<attribute name="OC_NEWARK" value="42K0680"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74ACT125DG" prefix="U">
<description>Quad Buffer with 3-State Outputs</description>
<gates>
<gate name="A" symbol="MC74ACT125DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="B0" pad="2"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="O0" pad="3"/>
<connect gate="A" pin="O1" pad="6"/>
<connect gate="A" pin="O2" pad="11"/>
<connect gate="A" pin="O3" pad="8"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~A0" pad="1"/>
<connect gate="A" pin="~A1" pad="4"/>
<connect gate="A" pin="~A2" pad="13"/>
<connect gate="A" pin="~A3" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74ACT125DG"/>
<attribute name="OC_FARNELL" value="1705944"/>
<attribute name="OC_NEWARK" value="45J1238"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74ACT132DG" prefix="U">
<description>Quad 2-Input NAND Schmitt Trigger</description>
<gates>
<gate name="A" symbol="MC74ACT132DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN" pad="9"/>
<connect gate="A" pin="IN_2" pad="4"/>
<connect gate="A" pin="IN_3" pad="1"/>
<connect gate="A" pin="IN_4" pad="5"/>
<connect gate="A" pin="IN_5" pad="2"/>
<connect gate="A" pin="IN_6" pad="10"/>
<connect gate="A" pin="IN_7" pad="12"/>
<connect gate="A" pin="IN_8" pad="13"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="OUT_2" pad="3"/>
<connect gate="A" pin="OUT_3" pad="6"/>
<connect gate="A" pin="OUT_4" pad="11"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74ACT132DG"/>
<attribute name="OC_FARNELL" value="1607771"/>
<attribute name="OC_NEWARK" value="42K0691"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74ACT14DG" prefix="U">
<description>Hex Inverter Schmitt Trigger</description>
<gates>
<gate name="A" symbol="MC74ACT14DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN" pad="5"/>
<connect gate="A" pin="IN_2" pad="3"/>
<connect gate="A" pin="IN_3" pad="11"/>
<connect gate="A" pin="IN_4" pad="13"/>
<connect gate="A" pin="IN_5" pad="1"/>
<connect gate="A" pin="IN_6" pad="9"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="OUT_2" pad="2"/>
<connect gate="A" pin="OUT_3" pad="6"/>
<connect gate="A" pin="OUT_4" pad="10"/>
<connect gate="A" pin="OUT_5" pad="4"/>
<connect gate="A" pin="OUT_6" pad="12"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74ACT14DG"/>
<attribute name="OC_FARNELL" value="1652019"/>
<attribute name="OC_NEWARK" value="42K0699"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74ACT74DG" prefix="U">
<description>Dual D-Type Positive Edge-Triggered Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74ACT74DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="CP1" pad="3"/>
<connect gate="A" pin="CP2" pad="11"/>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="D2" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~CD1" pad="1"/>
<connect gate="A" pin="~CD2" pad="13"/>
<connect gate="A" pin="~Q1" pad="6"/>
<connect gate="A" pin="~Q2" pad="8"/>
<connect gate="A" pin="~SD1" pad="4"/>
<connect gate="A" pin="~SD2" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74ACT74DG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="42K0750"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC00ADG" prefix="U">
<description>Quad 2-Input NAND Gate</description>
<gates>
<gate name="A" symbol="MC74HC00ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC00ADG"/>
<attribute name="OC_FARNELL" value="9666885"/>
<attribute name="OC_NEWARK" value="71J5589"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC00ANG" prefix="U">
<description>Quad 2-Input NAND Gate</description>
<gates>
<gate name="A" symbol="MC74HC00ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC00ANG"/>
<attribute name="OC_FARNELL" value="9665773"/>
<attribute name="OC_NEWARK" value="45J1279"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC02ADG" prefix="U">
<description>Quad 2-Input NOR Gate</description>
<gates>
<gate name="A" symbol="MC74HC02ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="8"/>
<connect gate="A" pin="A4" pad="11"/>
<connect gate="A" pin="B1" pad="3"/>
<connect gate="A" pin="B2" pad="6"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="B4" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="10"/>
<connect gate="A" pin="Y4" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC02ADG"/>
<attribute name="OC_FARNELL" value="9666893"/>
<attribute name="OC_NEWARK" value="45J1280"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC02ANG" prefix="U">
<description>Quad 2-Input NOR Gate</description>
<gates>
<gate name="A" symbol="MC74HC02ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="8"/>
<connect gate="A" pin="A4" pad="11"/>
<connect gate="A" pin="B1" pad="3"/>
<connect gate="A" pin="B2" pad="6"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="B4" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="10"/>
<connect gate="A" pin="Y4" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC02ANG"/>
<attribute name="OC_FARNELL" value="9665781"/>
<attribute name="OC_NEWARK" value="45J1282"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC03ADG" prefix="U">
<description>Quad 2-Input NAND Gate with Open-Drain Outputs</description>
<gates>
<gate name="A" symbol="MC74HC03ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC03ADG"/>
<attribute name="OC_FARNELL" value="1364064"/>
<attribute name="OC_NEWARK" value="26K4195"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC04ADG" prefix="U">
<description>Hex Inverter</description>
<gates>
<gate name="A" symbol="MC74HC04ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC04ADG"/>
<attribute name="OC_FARNELL" value="1104714"/>
<attribute name="OC_NEWARK" value="42K0843"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC04ADR2G" prefix="U">
<description>Hex Inverter</description>
<gates>
<gate name="A" symbol="MC74HC04ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC04ADR2G"/>
<attribute name="OC_FARNELL" value="1147801"/>
<attribute name="OC_NEWARK" value="45J1284"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC04ADTR2G" prefix="U">
<description>Hex Inverter</description>
<gates>
<gate name="A" symbol="MC74HC04ADTR2G"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC04ADTR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7796"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC08ADG" prefix="U">
<description>Quad 2-Input AND Gate</description>
<gates>
<gate name="A" symbol="MC74HC08ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC08ADG"/>
<attribute name="OC_FARNELL" value="9666907"/>
<attribute name="OC_NEWARK" value="45J1285"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC08ADTR2G" prefix="U">
<description>Quad 2-Input AND Gate</description>
<gates>
<gate name="A" symbol="MC74HC08ADTR2G"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC08ADTR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7797"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC125ADG" prefix="U">
<description>Quad 3-State Noninverting Buffers</description>
<gates>
<gate name="A" symbol="MC74HC125ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="OE2" pad="4"/>
<connect gate="A" pin="OE3" pad="10"/>
<connect gate="A" pin="OE4" pad="13"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC125ADG"/>
<attribute name="OC_FARNELL" value="9666915"/>
<attribute name="OC_NEWARK" value="45J1290"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC125ADR2G" prefix="U">
<description>Quad 3-State Noninverting Buffers</description>
<gates>
<gate name="A" symbol="MC74HC125ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="OE2" pad="4"/>
<connect gate="A" pin="OE3" pad="10"/>
<connect gate="A" pin="OE4" pad="13"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC125ADR2G"/>
<attribute name="OC_FARNELL" value="1262898"/>
<attribute name="OC_NEWARK" value="84K8774"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC132ADG" prefix="U">
<description>Quad 2-Input NAND Gate with Schmitt-Trigger Inputs</description>
<gates>
<gate name="A" symbol="MC74HC132ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC132ADG"/>
<attribute name="OC_FARNELL" value="9666923"/>
<attribute name="OC_NEWARK" value="45J1294"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC132ADR2G" prefix="U">
<description>Quad 2-Input NAND Gate with Schmitt-Trigger Inputs</description>
<gates>
<gate name="A" symbol="MC74HC132ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC132ADR2G"/>
<attribute name="OC_FARNELL" value="1268658"/>
<attribute name="OC_NEWARK" value="84K8775"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC132ADTG" prefix="U">
<description>Quad 2-Input NAND Gate with Schmitt-Trigger Inputs</description>
<gates>
<gate name="A" symbol="MC74HC132ADTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC132ADTG"/>
<attribute name="OC_FARNELL" value="1104719"/>
<attribute name="OC_NEWARK" value="42K0850"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC132ANG" prefix="U">
<description>Quad 2-Input NAND Gate</description>
<gates>
<gate name="A" symbol="MC74HC132ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC132ANG"/>
<attribute name="OC_FARNELL" value="9665820"/>
<attribute name="OC_NEWARK" value="45J1296"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC138ADG" prefix="U">
<description>1-of-8 Decoder/Demultiplexer</description>
<gates>
<gate name="A" symbol="MC74HC138ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="CS1" pad="6"/>
<connect gate="A" pin="CS2" pad="4"/>
<connect gate="A" pin="CS3" pad="5"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="Y0" pad="15"/>
<connect gate="A" pin="Y1" pad="14"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="9"/>
<connect gate="A" pin="Y7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC138ADG"/>
<attribute name="OC_FARNELL" value="1104715"/>
<attribute name="OC_NEWARK" value="42K0852"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC138ADR2G" prefix="U">
<description>1-of-8 Decoder/Demultiplexer</description>
<gates>
<gate name="A" symbol="MC74HC138ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="CS1" pad="6"/>
<connect gate="A" pin="CS2" pad="4"/>
<connect gate="A" pin="CS3" pad="5"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="Y0" pad="15"/>
<connect gate="A" pin="Y1" pad="14"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="9"/>
<connect gate="A" pin="Y7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC138ADR2G"/>
<attribute name="OC_FARNELL" value="1266201"/>
<attribute name="OC_NEWARK" value="84K8776"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC138ANG" prefix="U">
<description>1-of-8 Decoder/Demultiplexer</description>
<gates>
<gate name="A" symbol="MC74HC138ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="CS1" pad="6"/>
<connect gate="A" pin="CS2" pad="4"/>
<connect gate="A" pin="CS3" pad="5"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="Y0" pad="15"/>
<connect gate="A" pin="Y1" pad="14"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="9"/>
<connect gate="A" pin="Y7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC138ANG"/>
<attribute name="OC_FARNELL" value="9665838"/>
<attribute name="OC_NEWARK" value="45J1298"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC139ADG" prefix="U">
<description>Dual 1-of-4 Decoder/Demultiplexer</description>
<gates>
<gate name="A" symbol="MC74HC139ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A0A" pad="2"/>
<connect gate="A" pin="A0B" pad="14"/>
<connect gate="A" pin="A1A" pad="3"/>
<connect gate="A" pin="A1B" pad="13"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="SELECTA" pad="1"/>
<connect gate="A" pin="SELECTB" pad="15"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="Y0A" pad="4"/>
<connect gate="A" pin="Y0B" pad="12"/>
<connect gate="A" pin="Y1A" pad="5"/>
<connect gate="A" pin="Y1B" pad="11"/>
<connect gate="A" pin="Y2A" pad="6"/>
<connect gate="A" pin="Y2B" pad="10"/>
<connect gate="A" pin="Y3A" pad="7"/>
<connect gate="A" pin="Y3B" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC139ADG"/>
<attribute name="OC_FARNELL" value="1104716"/>
<attribute name="OC_NEWARK" value="42K0853"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC14ADG" prefix="U">
<description>Hex Schmitt-Trigger Inverter</description>
<gates>
<gate name="A" symbol="MC74HC14ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC14ADG"/>
<attribute name="OC_FARNELL" value="9666931"/>
<attribute name="OC_NEWARK" value="71J5595"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC14ADR2G" prefix="U">
<description>Hex Schmitt-Trigger Inverter</description>
<gates>
<gate name="A" symbol="MC74HC14ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC14ADR2G"/>
<attribute name="OC_FARNELL" value="1607772"/>
<attribute name="OC_NEWARK" value="45J1301"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC14ADTG" prefix="U">
<description>Hex Schmitt-Trigger Inverter</description>
<gates>
<gate name="A" symbol="MC74HC14ADTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC14ADTG"/>
<attribute name="OC_FARNELL" value="1104717"/>
<attribute name="OC_NEWARK" value="42K0855"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC14ANG" prefix="U">
<description>Hex Schmitt Trigger Inverter</description>
<gates>
<gate name="A" symbol="MC74HC14ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC14ANG"/>
<attribute name="OC_FARNELL" value="9665854"/>
<attribute name="OC_NEWARK" value="45J1302"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC164ADG" prefix="U">
<description>8-Bit Serial-Input/Parallel- Output Shift Register</description>
<gates>
<gate name="A" symbol="MC74HC164ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="CLK" pad="8"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="4"/>
<connect gate="A" pin="QC" pad="5"/>
<connect gate="A" pin="QD" pad="6"/>
<connect gate="A" pin="QE" pad="10"/>
<connect gate="A" pin="QF" pad="11"/>
<connect gate="A" pin="QG" pad="12"/>
<connect gate="A" pin="QH" pad="13"/>
<connect gate="A" pin="RESET" pad="9"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC164ADG"/>
<attribute name="OC_FARNELL" value="1287963"/>
<attribute name="OC_NEWARK" value="71J5599"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC165ADG" prefix="U">
<description>8-Bit Serial or Parallel-Input/Serial-Output Shift Register</description>
<gates>
<gate name="A" symbol="MC74HC165ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="12"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="CLK_INHIBIT" pad="15"/>
<connect gate="A" pin="D" pad="14"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="A" pin="F" pad="4"/>
<connect gate="A" pin="G" pad="5"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="H" pad="6"/>
<connect gate="A" pin="QH" pad="9"/>
<connect gate="A" pin="SA" pad="10"/>
<connect gate="A" pin="SERIAL_SHIFT/~PARALLEL_LOAD" pad="1"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~QH" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC165ADG"/>
<attribute name="OC_FARNELL" value="9664483"/>
<attribute name="OC_NEWARK" value="45J1308"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC1G04DTT1G" prefix="U">
<description>Single Inverter</description>
<gates>
<gate name="A" symbol="MC74HC1G04DTT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_~Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC1G04DTT1G"/>
<attribute name="OC_FARNELL" value="1706041"/>
<attribute name="OC_NEWARK" value="95K5518"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC1G14DTT1G" prefix="U">
<description>Single Inverter with Schmitt-Trigger Input</description>
<gates>
<gate name="A" symbol="MC74HC1G14DTT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC1G14DTT1G"/>
<attribute name="OC_FARNELL" value="1468757"/>
<attribute name="OC_NEWARK" value="71J5593"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC240ANG" prefix="U">
<description>Octal 3-State Inverting Buffer/Line Driver/Line Receiver</description>
<gates>
<gate name="A" symbol="MC74HC240ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="B1" pad="11"/>
<connect gate="A" pin="B2" pad="13"/>
<connect gate="A" pin="B3" pad="15"/>
<connect gate="A" pin="B4" pad="17"/>
<connect gate="A" pin="EN_A" pad="1"/>
<connect gate="A" pin="EN_B" pad="19"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="YA1" pad="18"/>
<connect gate="A" pin="YA2" pad="16"/>
<connect gate="A" pin="YA3" pad="14"/>
<connect gate="A" pin="YA4" pad="12"/>
<connect gate="A" pin="YB1" pad="9"/>
<connect gate="A" pin="YB2" pad="7"/>
<connect gate="A" pin="YB3" pad="5"/>
<connect gate="A" pin="YB4" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC240ANG"/>
<attribute name="OC_FARNELL" value="9665889"/>
<attribute name="OC_NEWARK" value="71J5601"/>
<attribute name="PACKAGE" value="DIP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC244ADWG" prefix="U">
<description>Noninverting Buffer/Line Driver/Line Receiver</description>
<gates>
<gate name="A" symbol="MC74HC244ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="B1" pad="11"/>
<connect gate="A" pin="B2" pad="13"/>
<connect gate="A" pin="B3" pad="15"/>
<connect gate="A" pin="B4" pad="17"/>
<connect gate="A" pin="ENABLE_A" pad="1"/>
<connect gate="A" pin="ENABLE_B" pad="19"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="YA1" pad="18"/>
<connect gate="A" pin="YA2" pad="16"/>
<connect gate="A" pin="YA3" pad="14"/>
<connect gate="A" pin="YA4" pad="12"/>
<connect gate="A" pin="YB1" pad="9"/>
<connect gate="A" pin="YB2" pad="7"/>
<connect gate="A" pin="YB3" pad="5"/>
<connect gate="A" pin="YB4" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC244ADWG"/>
<attribute name="OC_FARNELL" value="1468758"/>
<attribute name="OC_NEWARK" value="42K0866"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC244ADWR2G" prefix="U">
<description>Noninverting Buffer/Line Driver/Line Receiver</description>
<gates>
<gate name="A" symbol="MC74HC244ADWR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="B1" pad="11"/>
<connect gate="A" pin="B2" pad="13"/>
<connect gate="A" pin="B3" pad="15"/>
<connect gate="A" pin="B4" pad="17"/>
<connect gate="A" pin="ENABLE_A" pad="1"/>
<connect gate="A" pin="ENABLE_B" pad="19"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="YA1" pad="18"/>
<connect gate="A" pin="YA2" pad="16"/>
<connect gate="A" pin="YA3" pad="14"/>
<connect gate="A" pin="YA4" pad="12"/>
<connect gate="A" pin="YB1" pad="9"/>
<connect gate="A" pin="YB2" pad="7"/>
<connect gate="A" pin="YB3" pad="5"/>
<connect gate="A" pin="YB4" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC244ADWR2G"/>
<attribute name="OC_FARNELL" value="1150453"/>
<attribute name="OC_NEWARK" value="45J1313"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC244ANG" prefix="U">
<description>Octal 3-State Inverting Buffer/Line Driver/Line Receiver</description>
<gates>
<gate name="A" symbol="MC74HC244ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="B1" pad="11"/>
<connect gate="A" pin="B2" pad="13"/>
<connect gate="A" pin="B3" pad="15"/>
<connect gate="A" pin="B4" pad="17"/>
<connect gate="A" pin="EN_A" pad="1"/>
<connect gate="A" pin="EN_B" pad="19"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="YA1" pad="18"/>
<connect gate="A" pin="YA2" pad="16"/>
<connect gate="A" pin="YA3" pad="14"/>
<connect gate="A" pin="YA4" pad="12"/>
<connect gate="A" pin="YB1" pad="9"/>
<connect gate="A" pin="YB2" pad="7"/>
<connect gate="A" pin="YB3" pad="5"/>
<connect gate="A" pin="YB4" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC244ANG"/>
<attribute name="OC_FARNELL" value="9665897"/>
<attribute name="OC_NEWARK" value="71J5603"/>
<attribute name="PACKAGE" value="DIP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC245ADTG" prefix="U">
<description>Octal 3-State Noninverting Bus Transceiver</description>
<gates>
<gate name="A" symbol="MC74HC245ADTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-20N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIRECTION" pad="1"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OUT_EN" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC245ADTG"/>
<attribute name="OC_FARNELL" value="1104722"/>
<attribute name="OC_NEWARK" value="42K0867"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC245ADWG" prefix="U">
<description>Octal Noninverting Bus Transceiver</description>
<gates>
<gate name="A" symbol="MC74HC245ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIRECTION" pad="1"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC245ADWG"/>
<attribute name="OC_FARNELL" value="1703301"/>
<attribute name="OC_NEWARK" value="45J1314"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC245ANG" prefix="U">
<description>Octal 3-State Noninverting Bus Transceiver</description>
<gates>
<gate name="A" symbol="MC74HC245ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIR" pad="1"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OE" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC245ANG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="71J5606"/>
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC273ADWG" prefix="U">
<description>Octal D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74HC273ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="CLOCK" pad="11"/>
<connect gate="A" pin="D0" pad="3"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="7"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="17"/>
<connect gate="A" pin="D7" pad="18"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="15"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="19"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC273ADWG"/>
<attribute name="OC_FARNELL" value="1607717"/>
<attribute name="OC_NEWARK" value="42K0869"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC273ANG" prefix="U">
<description>Octal D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74HC273ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-20">
<connects>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="D0" pad="3"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="7"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="17"/>
<connect gate="A" pin="D7" pad="18"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="15"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="19"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC273ANG"/>
<attribute name="OC_FARNELL" value="9665927"/>
<attribute name="OC_NEWARK" value="71J5608"/>
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC32ADG" prefix="U">
<description>Quad 2-Input OR Gate</description>
<gates>
<gate name="A" symbol="MC74HC32ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC32ADG"/>
<attribute name="OC_FARNELL" value="9666966"/>
<attribute name="OC_NEWARK" value="26K4221"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC373ANG" prefix="U">
<description>Octal 3-State Non-Inverting Transparent Latch</description>
<gates>
<gate name="A" symbol="MC74HC373ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-20">
<connects>
<connect gate="A" pin="D0" pad="3"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="7"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="17"/>
<connect gate="A" pin="D7" pad="18"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="LATCH_ENABLE" pad="11"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="1"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="15"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC373ANG"/>
<attribute name="OC_FARNELL" value="9665943"/>
<attribute name="OC_NEWARK" value="71J5611"/>
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC374ADWG" prefix="U">
<description>Octal Non-Inverting D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74HC374ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="CLOCK" pad="11"/>
<connect gate="A" pin="D0" pad="3"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="7"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="17"/>
<connect gate="A" pin="D7" pad="18"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="1"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="15"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC374ADWG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26K4225"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC374ANG" prefix="U">
<description>D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74HC374ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-20">
<connects>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="D0" pad="3"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="7"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="17"/>
<connect gate="A" pin="D7" pad="18"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="15"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC374ANG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26K4228"/>
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC390ADG" prefix="U">
<description>High-Performance Silicon-Gate CMOS</description>
<gates>
<gate name="A" symbol="MC74HC390ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="CLK_AA" pad="1"/>
<connect gate="A" pin="CLK_AB" pad="15"/>
<connect gate="A" pin="CLK_BA" pad="4"/>
<connect gate="A" pin="CLK_BB" pad="12"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="QAA" pad="3"/>
<connect gate="A" pin="QAB" pad="13"/>
<connect gate="A" pin="QBA" pad="5"/>
<connect gate="A" pin="QBB" pad="11"/>
<connect gate="A" pin="QCA" pad="6"/>
<connect gate="A" pin="QCB" pad="10"/>
<connect gate="A" pin="QDA" pad="7"/>
<connect gate="A" pin="QDB" pad="9"/>
<connect gate="A" pin="RSTA" pad="2"/>
<connect gate="A" pin="RST_B" pad="14"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC390ADG"/>
<attribute name="OC_FARNELL" value="1147859"/>
<attribute name="OC_NEWARK" value="71J5612"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4040ADG" prefix="U">
<description>12-Stage Binary Ripple Counter</description>
<gates>
<gate name="A" symbol="MC74HC4040ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q10" pad="14"/>
<connect gate="A" pin="Q11" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="A" pin="Q5" pad="3"/>
<connect gate="A" pin="Q6" pad="2"/>
<connect gate="A" pin="Q7" pad="4"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="Q9" pad="12"/>
<connect gate="A" pin="RST" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4040ADG"/>
<attribute name="OC_FARNELL" value="1705807"/>
<attribute name="OC_NEWARK" value="26K4229"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4046ADG" prefix="U">
<description>Phase-Locked Loop</description>
<gates>
<gate name="A" symbol="MC74HC4046ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="C1A" pad="6"/>
<connect gate="A" pin="C1B" pad="7"/>
<connect gate="A" pin="COMPIN" pad="3"/>
<connect gate="A" pin="DEMOUT" pad="10"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="INH" pad="5"/>
<connect gate="A" pin="PC1OUT" pad="2"/>
<connect gate="A" pin="PC2OUT" pad="13"/>
<connect gate="A" pin="PC3OUT" pad="15"/>
<connect gate="A" pin="PCPOUT" pad="1"/>
<connect gate="A" pin="R1" pad="11"/>
<connect gate="A" pin="R2" pad="12"/>
<connect gate="A" pin="SIGIN" pad="14"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VCOIN" pad="9"/>
<connect gate="A" pin="VCOOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4046ADG"/>
<attribute name="OC_FARNELL" value="1354337"/>
<attribute name="OC_NEWARK" value="26K4230"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4046ANG" prefix="U">
<description>Phase-Locked Loop</description>
<gates>
<gate name="A" symbol="MC74HC4046ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="C1A" pad="6"/>
<connect gate="A" pin="C1B" pad="7"/>
<connect gate="A" pin="COMPIN" pad="3"/>
<connect gate="A" pin="DEMOUT" pad="10"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="INH" pad="5"/>
<connect gate="A" pin="PC1OUT" pad="2"/>
<connect gate="A" pin="PC2OUT" pad="13"/>
<connect gate="A" pin="PC3OUT" pad="15"/>
<connect gate="A" pin="PCPOUT" pad="1"/>
<connect gate="A" pin="R1" pad="11"/>
<connect gate="A" pin="R2" pad="12"/>
<connect gate="A" pin="SIGIN" pad="14"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VCOIN" pad="9"/>
<connect gate="A" pin="VCOOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4046ANG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J1324"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4051ADR2G" prefix="U">
<description>High-Performance Silicon-Gate CMOS</description>
<gates>
<gate name="A" symbol="MC74HC4051ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="X" pad="3"/>
<connect gate="A" pin="X0" pad="13"/>
<connect gate="A" pin="X1" pad="14"/>
<connect gate="A" pin="X2" pad="15"/>
<connect gate="A" pin="X3" pad="12"/>
<connect gate="A" pin="X4" pad="1"/>
<connect gate="A" pin="X5" pad="5"/>
<connect gate="A" pin="X6" pad="2"/>
<connect gate="A" pin="X7" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4051ADR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84K8780"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4051ADWG" prefix="U">
<description>Analog Multiplexers/ Demultiplexers</description>
<gates>
<gate name="A" symbol="MC74HC4051ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="ENABLE" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="X" pad="3"/>
<connect gate="A" pin="X0" pad="13"/>
<connect gate="A" pin="X1" pad="14"/>
<connect gate="A" pin="X2" pad="15"/>
<connect gate="A" pin="X3" pad="12"/>
<connect gate="A" pin="X4" pad="1"/>
<connect gate="A" pin="X5" pad="5"/>
<connect gate="A" pin="X6" pad="2"/>
<connect gate="A" pin="X7" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4051ADWG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="42K0888"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4052ADTG" prefix="U">
<description>Multiplexers/Demultiplexers</description>
<gates>
<gate name="A" symbol="MC74HC4052ADTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-16N">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="9"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="X" pad="13"/>
<connect gate="A" pin="X0" pad="12"/>
<connect gate="A" pin="X1" pad="14"/>
<connect gate="A" pin="X2" pad="15"/>
<connect gate="A" pin="X3" pad="11"/>
<connect gate="A" pin="Y" pad="3"/>
<connect gate="A" pin="Y0" pad="1"/>
<connect gate="A" pin="Y1" pad="5"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4052ADTG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="42K0889"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4052ADWG" prefix="U">
<description>Analog Multiplexers/ Demultiplexers</description>
<gates>
<gate name="A" symbol="MC74HC4052ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="9"/>
<connect gate="A" pin="ENABLE" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="X" pad="13"/>
<connect gate="A" pin="X0" pad="12"/>
<connect gate="A" pin="X1" pad="14"/>
<connect gate="A" pin="X2" pad="15"/>
<connect gate="A" pin="X3" pad="11"/>
<connect gate="A" pin="Y" pad="3"/>
<connect gate="A" pin="Y0" pad="1"/>
<connect gate="A" pin="Y1" pad="5"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4052ADWG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26K4233"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4052ANG" prefix="U">
<description>Analog Multiplexers / Demultiplexers</description>
<gates>
<gate name="A" symbol="MC74HC4052ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="9"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="X" pad="13"/>
<connect gate="A" pin="X0" pad="12"/>
<connect gate="A" pin="X1" pad="14"/>
<connect gate="A" pin="X2" pad="15"/>
<connect gate="A" pin="X3" pad="11"/>
<connect gate="A" pin="Y" pad="3"/>
<connect gate="A" pin="Y0" pad="1"/>
<connect gate="A" pin="Y1" pad="5"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4052ANG"/>
<attribute name="OC_FARNELL" value="9664548"/>
<attribute name="OC_NEWARK" value="45J1328"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4053ADWG" prefix="U">
<description>Analog Multiplexers/ Demultiplexers</description>
<gates>
<gate name="A" symbol="MC74HC4053ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="ENABLE" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="X" pad="14"/>
<connect gate="A" pin="X0" pad="12"/>
<connect gate="A" pin="X1" pad="13"/>
<connect gate="A" pin="Y" pad="15"/>
<connect gate="A" pin="Y0" pad="2"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Z" pad="4"/>
<connect gate="A" pin="Z0" pad="5"/>
<connect gate="A" pin="Z1" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4053ADWG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26K4235"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4053ANG" prefix="U">
<description>Analog Multiplexers Demultiplexers</description>
<gates>
<gate name="A" symbol="MC74HC4053ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="X" pad="14"/>
<connect gate="A" pin="X0" pad="12"/>
<connect gate="A" pin="X1" pad="13"/>
<connect gate="A" pin="Y" pad="15"/>
<connect gate="A" pin="Y0" pad="2"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Z" pad="4"/>
<connect gate="A" pin="Z0" pad="5"/>
<connect gate="A" pin="Z1" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4053ANG"/>
<attribute name="OC_FARNELL" value="9665978"/>
<attribute name="OC_NEWARK" value="45J1330"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4060ADG" prefix="U">
<description>14-Stage Binary Ripple Counter With Oscillator</description>
<gates>
<gate name="A" symbol="MC74HC4060ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="OSC_IN" pad="11"/>
<connect gate="A" pin="OSC_OUT_1" pad="10"/>
<connect gate="A" pin="OSC_OUT_2" pad="9"/>
<connect gate="A" pin="Q10" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q13" pad="2"/>
<connect gate="A" pin="Q14" pad="3"/>
<connect gate="A" pin="Q4" pad="7"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="4"/>
<connect gate="A" pin="Q7" pad="6"/>
<connect gate="A" pin="Q8" pad="14"/>
<connect gate="A" pin="Q9" pad="13"/>
<connect gate="A" pin="RESET" pad="12"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4060ADG"/>
<attribute name="OC_FARNELL" value="1705808"/>
<attribute name="OC_NEWARK" value="26K4237"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4060ANG" prefix="U">
<description>14-Stage Binary Ripple Counter With Oscillator</description>
<gates>
<gate name="A" symbol="MC74HC4060ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="OSC_IN" pad="11"/>
<connect gate="A" pin="OSC_OUT_1" pad="10"/>
<connect gate="A" pin="OSC_OUT_2" pad="9"/>
<connect gate="A" pin="Q10" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q13" pad="2"/>
<connect gate="A" pin="Q14" pad="3"/>
<connect gate="A" pin="Q4" pad="7"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="4"/>
<connect gate="A" pin="Q7" pad="6"/>
<connect gate="A" pin="Q8" pad="14"/>
<connect gate="A" pin="Q9" pad="13"/>
<connect gate="A" pin="RESET" pad="12"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4060ANG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="70K3160"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4066ADG" prefix="U">
<description>Quad Analog Switch/Multiplexer/Demultiplexer</description>
<gates>
<gate name="A" symbol="MC74HC4066ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A_ON/OFF_CONTROL" pad="13"/>
<connect gate="A" pin="B_ON/OFF_CONTROL" pad="5"/>
<connect gate="A" pin="C_ON/OFF_CONTROL" pad="6"/>
<connect gate="A" pin="D_ON/OFF_CONTROL" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="XA" pad="1"/>
<connect gate="A" pin="XB" pad="4"/>
<connect gate="A" pin="XC" pad="8"/>
<connect gate="A" pin="XD" pad="11"/>
<connect gate="A" pin="YA" pad="2"/>
<connect gate="A" pin="YB" pad="3"/>
<connect gate="A" pin="YC" pad="9"/>
<connect gate="A" pin="YD" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4066ADG"/>
<attribute name="OC_FARNELL" value="9666990"/>
<attribute name="OC_NEWARK" value="45J1332"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4066ADR2G" prefix="U">
<description>Quad Analog Switch/Multiplexer/Demultiplexer</description>
<gates>
<gate name="A" symbol="MC74HC4066ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A_ON/OFF_CONTROL" pad="13"/>
<connect gate="A" pin="B_ON/OFF_CONTROL" pad="5"/>
<connect gate="A" pin="C_ON/OFF_CONTROL" pad="6"/>
<connect gate="A" pin="D_ON/OFF_CONTROL" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="XA" pad="1"/>
<connect gate="A" pin="XB" pad="4"/>
<connect gate="A" pin="XC" pad="8"/>
<connect gate="A" pin="XD" pad="11"/>
<connect gate="A" pin="YA" pad="2"/>
<connect gate="A" pin="YB" pad="3"/>
<connect gate="A" pin="YC" pad="9"/>
<connect gate="A" pin="YD" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4066ADR2G"/>
<attribute name="OC_FARNELL" value="1273200"/>
<attribute name="OC_NEWARK" value="84K8781"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4538ADG" prefix="U">
<description>Dual Precision Monostable  Multivibrator</description>
<gates>
<gate name="A" symbol="MC74HC4538ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="12"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="11"/>
<connect gate="A" pin="CX1/RX1" pad="2"/>
<connect gate="A" pin="CX2/RX2" pad="14"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="15"/>
<connect gate="A" pin="GND_3" pad="1"/>
<connect gate="A" pin="Q1" pad="6"/>
<connect gate="A" pin="Q2" pad="10"/>
<connect gate="A" pin="RESET_1" pad="3"/>
<connect gate="A" pin="RESET_2" pad="13"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~Q1" pad="7"/>
<connect gate="A" pin="~Q2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4538ADG"/>
<attribute name="OC_FARNELL" value="1607840"/>
<attribute name="OC_NEWARK" value="45J1336"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC4538ANG" prefix="U">
<description>Dual Precision Monostable Multivibrator</description>
<gates>
<gate name="A" symbol="MC74HC4538ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="12"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="11"/>
<connect gate="A" pin="CX1/RX1" pad="2"/>
<connect gate="A" pin="CX2/RX2" pad="14"/>
<connect gate="A" pin="GND" pad="15"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="8"/>
<connect gate="A" pin="Q1" pad="6"/>
<connect gate="A" pin="Q2" pad="10"/>
<connect gate="A" pin="RESET_1" pad="3"/>
<connect gate="A" pin="RESET_2" pad="13"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~Q1" pad="7"/>
<connect gate="A" pin="~Q2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC4538ANG"/>
<attribute name="OC_FARNELL" value="9665986"/>
<attribute name="OC_NEWARK" value="45J1338"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC540ANG" prefix="U">
<description>Octal 3-State Inverting Buffer</description>
<gates>
<gate name="A" symbol="MC74HC540ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="OE2" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC540ANG"/>
<attribute name="OC_FARNELL" value="9665994"/>
<attribute name="OC_NEWARK" value="26K4250"/>
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC541ADTG" prefix="U">
<description>IC BUFFER/DRIVER TRI-STATE 8BIT</description>
<gates>
<gate name="A" symbol="MC74HC541ADTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-20N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="OE2" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC541ADTG"/>
<attribute name="OC_FARNELL" value="1104726"/>
<attribute name="OC_NEWARK" value="42K0902"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC541ADWG" prefix="U">
<description>Noninverting Buffer/Line Driver/Line Receiver</description>
<gates>
<gate name="A" symbol="MC74HC541ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="OE2" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC541ADWG"/>
<attribute name="OC_FARNELL" value="1607612"/>
<attribute name="OC_NEWARK" value="42K0904"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC541ADWR2G" prefix="U">
<description>Noninverting Buffer/Line Driver/Line Receiver</description>
<gates>
<gate name="A" symbol="MC74HC541ADWR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="OE2" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC541ADWR2G"/>
<attribute name="OC_FARNELL" value="1276833"/>
<attribute name="OC_NEWARK" value="84K8782"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC541ANG" prefix="U">
<description>Octal 3-State Inverting Buffer</description>
<gates>
<gate name="A" symbol="MC74HC541ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="OE2" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC541ANG"/>
<attribute name="OC_FARNELL" value="9666001"/>
<attribute name="OC_NEWARK" value="45J1340"/>
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC573ADTG" prefix="U">
<description>Octal Noninverting Latch</description>
<gates>
<gate name="A" symbol="MC74HC573ADTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-20N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="D5" pad="7"/>
<connect gate="A" pin="D6" pad="8"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="LATCH_ENABLE" pad="11"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="1"/>
<connect gate="A" pin="Q0" pad="19"/>
<connect gate="A" pin="Q1" pad="18"/>
<connect gate="A" pin="Q2" pad="17"/>
<connect gate="A" pin="Q3" pad="16"/>
<connect gate="A" pin="Q4" pad="15"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="13"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC573ADTG"/>
<attribute name="OC_FARNELL" value="1104727"/>
<attribute name="OC_NEWARK" value="42K0905"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC573ADWG" prefix="U">
<description>Octal Noninverting Transparent Latch</description>
<gates>
<gate name="A" symbol="MC74HC573ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="D5" pad="7"/>
<connect gate="A" pin="D6" pad="8"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="LATCH_ENABLE" pad="11"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="1"/>
<connect gate="A" pin="Q0" pad="19"/>
<connect gate="A" pin="Q1" pad="18"/>
<connect gate="A" pin="Q2" pad="17"/>
<connect gate="A" pin="Q3" pad="16"/>
<connect gate="A" pin="Q4" pad="15"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="13"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC573ADWG"/>
<attribute name="OC_FARNELL" value="1095313"/>
<attribute name="OC_NEWARK" value="45J1341"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC573ANG" prefix="U">
<description>Octal 3-State Noninverting Transparent Latch</description>
<gates>
<gate name="A" symbol="MC74HC573ANG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="D5" pad="7"/>
<connect gate="A" pin="D6" pad="8"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="LATCH_ENABLE" pad="11"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="1"/>
<connect gate="A" pin="Q0" pad="19"/>
<connect gate="A" pin="Q1" pad="18"/>
<connect gate="A" pin="Q2" pad="17"/>
<connect gate="A" pin="Q3" pad="16"/>
<connect gate="A" pin="Q4" pad="15"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="13"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC573ANG"/>
<attribute name="OC_FARNELL" value="9666010"/>
<attribute name="OC_NEWARK" value="45J1343"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC574ADWG" prefix="U">
<description>Octal Noninverting D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74HC574ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="CLOCK" pad="11"/>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="D5" pad="7"/>
<connect gate="A" pin="D6" pad="8"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="1"/>
<connect gate="A" pin="Q0" pad="19"/>
<connect gate="A" pin="Q1" pad="18"/>
<connect gate="A" pin="Q2" pad="17"/>
<connect gate="A" pin="Q3" pad="16"/>
<connect gate="A" pin="Q4" pad="15"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="13"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC574ADWG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="42K0908"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC589ANG" prefix="U">
<description>8-Bit Serial or Parallel-Input/Serial-Output Shift Register</description>
<gates>
<gate name="A" symbol="MC74HC589ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="2"/>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="E" pad="4"/>
<connect gate="A" pin="F" pad="5"/>
<connect gate="A" pin="G" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="H" pad="7"/>
<connect gate="A" pin="LATCH_CLK" pad="12"/>
<connect gate="A" pin="OUT_EN" pad="10"/>
<connect gate="A" pin="QH" pad="9"/>
<connect gate="A" pin="SA" pad="14"/>
<connect gate="A" pin="SER_SHIFT/PAR_LOAD" pad="13"/>
<connect gate="A" pin="SHIFT_CLK" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC589ANG"/>
<attribute name="OC_FARNELL" value="1703300"/>
<attribute name="OC_NEWARK" value="45J1346"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC595ADG" prefix="U">
<description>8-Bit Serial-Input/Serial or Parallel-Output Shift Register with Latched 3-State Outputs</description>
<gates>
<gate name="A" symbol="MC74HC595ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="LATCH_CLOCK" pad="12"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="13"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="4"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="2"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="RESET" pad="10"/>
<connect gate="A" pin="SHIFT_CLOCK" pad="11"/>
<connect gate="A" pin="SQH" pad="9"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC595ADG"/>
<attribute name="OC_FARNELL" value="9667008"/>
<attribute name="OC_NEWARK" value="45J1347"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC595ADR2G" prefix="U">
<description>8-Bit Serial-Input/Serial Parallel-Output Shift  3-State Outputs</description>
<gates>
<gate name="A" symbol="MC74HC595ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="LATCH_CLK" pad="12"/>
<connect gate="A" pin="OE" pad="13"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="RESET" pad="10"/>
<connect gate="A" pin="SHIFT_CLK" pad="11"/>
<connect gate="A" pin="SQH" pad="9"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC595ADR2G"/>
<attribute name="OC_FARNELL" value="1278491"/>
<attribute name="OC_NEWARK" value="84K8783"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC595ADTR2G" prefix="U">
<description>8-Bit Serial-Input/Serial or Parallel-Output Shift Register with Latched 3-State Outputs</description>
<gates>
<gate name="A" symbol="MC74HC595ADTR2G"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-16N">
<connects>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="LATCH_CLOCK" pad="12"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="13"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="RESET" pad="10"/>
<connect gate="A" pin="SHIFT_CLOCK" pad="11"/>
<connect gate="A" pin="SQH" pad="9"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC595ADTR2G"/>
<attribute name="OC_FARNELL" value="1607848"/>
<attribute name="OC_NEWARK" value="42K0910"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC595ANG" prefix="U">
<description>8-Bit Serial or Parallel-Input/Serial-Output Shift Register</description>
<gates>
<gate name="A" symbol="MC74HC595ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="LATCH_CLK" pad="12"/>
<connect gate="A" pin="OUT_EN" pad="13"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="RESET" pad="10"/>
<connect gate="A" pin="SHIFT_CLK" pad="11"/>
<connect gate="A" pin="SQH" pad="9"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC595ANG"/>
<attribute name="OC_FARNELL" value="9666036"/>
<attribute name="OC_NEWARK" value="45J1349"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="On semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC74ADG" prefix="U">
<description>Dual D Flip-Flop with Set and Reset</description>
<gates>
<gate name="A" symbol="MC74HC74ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="CLK_1" pad="3"/>
<connect gate="A" pin="CLK_2" pad="11"/>
<connect gate="A" pin="DATA_1" pad="2"/>
<connect gate="A" pin="DATA_2" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="RESET_1" pad="1"/>
<connect gate="A" pin="RESET_2" pad="13"/>
<connect gate="A" pin="SET_1" pad="4"/>
<connect gate="A" pin="SET_2" pad="10"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~Q1" pad="6"/>
<connect gate="A" pin="~Q2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC74ADG"/>
<attribute name="OC_FARNELL" value="9667016"/>
<attribute name="OC_NEWARK" value="26K4258"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC74ADR2G" prefix="U">
<description>Dual D Flip-Flop with Set and Reset</description>
<gates>
<gate name="A" symbol="MC74HC74ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="CLK_1" pad="3"/>
<connect gate="A" pin="CLK_2" pad="11"/>
<connect gate="A" pin="DATA_1" pad="2"/>
<connect gate="A" pin="DATA_2" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="RESET_1" pad="1"/>
<connect gate="A" pin="RESET_2" pad="13"/>
<connect gate="A" pin="SET_1" pad="4"/>
<connect gate="A" pin="SET_2" pad="10"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~Q1" pad="6"/>
<connect gate="A" pin="~Q2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC74ADR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84K8784"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC74ANG" prefix="U">
<description>Dual D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74HC74ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="CLK1" pad="3"/>
<connect gate="A" pin="CLK2" pad="11"/>
<connect gate="A" pin="DATA1" pad="2"/>
<connect gate="A" pin="DATA2" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="RESET1" pad="1"/>
<connect gate="A" pin="RESET2" pad="13"/>
<connect gate="A" pin="SET1" pad="4"/>
<connect gate="A" pin="SET2" pad="10"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~Q1" pad="6"/>
<connect gate="A" pin="~Q2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC74ANG"/>
<attribute name="OC_FARNELL" value="9666044"/>
<attribute name="OC_NEWARK" value="98H0712"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HC86ADG" prefix="U">
<description>Quad 2-Input Exclusive OR Gate</description>
<gates>
<gate name="A" symbol="MC74HC86ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="10"/>
<connect gate="A" pin="B4" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HC86ADG"/>
<attribute name="OC_FARNELL" value="1705810"/>
<attribute name="OC_NEWARK" value="26K4260"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HCT04ADG" prefix="U">
<description>Hex Inverter</description>
<gates>
<gate name="A" symbol="MC74HCT04ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HCT04ADG"/>
<attribute name="OC_FARNELL" value="1155561"/>
<attribute name="OC_NEWARK" value="71J5579"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HCT04ANG" prefix="U">
<description>Hex Inverter</description>
<gates>
<gate name="A" symbol="MC74HCT04ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HCT04ANG"/>
<attribute name="OC_FARNELL" value="1150450"/>
<attribute name="OC_NEWARK" value="45J1266"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HCT14ADG" prefix="U">
<description>Hex Schmitt-Trigger Inverter with LSTTL Compatible Inputs</description>
<gates>
<gate name="A" symbol="MC74HCT14ADG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HCT14ADG"/>
<attribute name="OC_FARNELL" value="1607774"/>
<attribute name="OC_NEWARK" value="45J1267"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HCT14ANG" prefix="U">
<description>Hex Schmitt-Trigger Inverter</description>
<gates>
<gate name="A" symbol="MC74HCT14ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HCT14ANG"/>
<attribute name="OC_FARNELL" value="9666079"/>
<attribute name="OC_NEWARK" value="45J1269"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HCT244ADWG" prefix="U">
<description>Octal Noninverting Buffer/Line Driver/Line Receiver</description>
<gates>
<gate name="A" symbol="MC74HCT244ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="B1" pad="11"/>
<connect gate="A" pin="B2" pad="13"/>
<connect gate="A" pin="B3" pad="15"/>
<connect gate="A" pin="B4" pad="17"/>
<connect gate="A" pin="ENABLE_A" pad="1"/>
<connect gate="A" pin="ENABLE_B" pad="19"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="YA1" pad="18"/>
<connect gate="A" pin="YA2" pad="16"/>
<connect gate="A" pin="YA3" pad="14"/>
<connect gate="A" pin="YA4" pad="12"/>
<connect gate="A" pin="YB1" pad="9"/>
<connect gate="A" pin="YB2" pad="7"/>
<connect gate="A" pin="YB3" pad="5"/>
<connect gate="A" pin="YB4" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HCT244ADWG"/>
<attribute name="OC_FARNELL" value="1607614"/>
<attribute name="OC_NEWARK" value="45J1270"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HCT374ANG" prefix="U">
<description>Octal 3-State Noninverting D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74HCT374ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-20">
<connects>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="D0" pad="3"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="7"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="17"/>
<connect gate="A" pin="D7" pad="18"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="15"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HCT374ANG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="42K0833"/>
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HCT541ADWG" prefix="U">
<description>Octal Noninverting Buffer/Line Driver/Line Receiver</description>
<gates>
<gate name="A" symbol="MC74HCT541ADWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="OE2" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HCT541ADWG"/>
<attribute name="OC_FARNELL" value="1260776"/>
<attribute name="OC_NEWARK" value="42K0835"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HCT541ANG" prefix="U">
<description>Octal 3-State Non-Inverting Buffer</description>
<gates>
<gate name="A" symbol="MC74HCT541ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="OE2" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HCT541ANG"/>
<attribute name="OC_FARNELL" value="1149622"/>
<attribute name="OC_NEWARK" value="26K4184"/>
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HCT74ANG" prefix="U">
<description>Dual D Flip-Flop</description>
<gates>
<gate name="A" symbol="MC74HCT74ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="CLK_1" pad="3"/>
<connect gate="A" pin="CLK_2" pad="11"/>
<connect gate="A" pin="DATA_1" pad="2"/>
<connect gate="A" pin="DATA_2" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="RESET_1" pad="1"/>
<connect gate="A" pin="RESET_2" pad="13"/>
<connect gate="A" pin="SET_1" pad="4"/>
<connect gate="A" pin="SET_2" pad="10"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~Q1" pad="6"/>
<connect gate="A" pin="~Q2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HCT74ANG"/>
<attribute name="OC_FARNELL" value="9666087"/>
<attribute name="OC_NEWARK" value="26K4190"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HCU04ADR2G" prefix="U">
<description>Hex Unbuffered Inverter</description>
<gates>
<gate name="A" symbol="MC74HCU04ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HCU04ADR2G"/>
<attribute name="OC_FARNELL" value="1268657"/>
<attribute name="OC_NEWARK" value="84K8771"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74HCU04ANG" prefix="U">
<description>Hex Unbuffered Inverter</description>
<gates>
<gate name="A" symbol="MC74HCU04ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X469-14">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="2"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Y3" pad="6"/>
<connect gate="A" pin="Y4" pad="8"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74HCU04ANG"/>
<attribute name="OC_FARNELL" value="9666052"/>
<attribute name="OC_NEWARK" value="45J1277"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="On Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LCX04DG" prefix="U">
<description>Low-Voltage CMOS Hex Inverter</description>
<gates>
<gate name="A" symbol="MC74LCX04DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="13"/>
<connect gate="A" pin="A4" pad="11"/>
<connect gate="A" pin="A5" pad="9"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~O0" pad="2"/>
<connect gate="A" pin="~O1" pad="4"/>
<connect gate="A" pin="~O2" pad="6"/>
<connect gate="A" pin="~O3" pad="12"/>
<connect gate="A" pin="~O4" pad="10"/>
<connect gate="A" pin="~O5" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LCX04DG"/>
<attribute name="OC_FARNELL" value="1353836"/>
<attribute name="OC_NEWARK" value="42K0924"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LCX04DTG" prefix="U">
<description>CMOS Hex Inverter</description>
<gates>
<gate name="A" symbol="MC74LCX04DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="13"/>
<connect gate="A" pin="A4" pad="11"/>
<connect gate="A" pin="A5" pad="9"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~O0" pad="2"/>
<connect gate="A" pin="~O1" pad="4"/>
<connect gate="A" pin="~O2" pad="6"/>
<connect gate="A" pin="~O3" pad="12"/>
<connect gate="A" pin="~O4" pad="10"/>
<connect gate="A" pin="~O5" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LCX04DTG"/>
<attribute name="OC_FARNELL" value="1705884"/>
<attribute name="OC_NEWARK" value="42K0925"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LCX08DG" prefix="U">
<description>Quad 2-Input AND Gate</description>
<gates>
<gate name="A" symbol="MC74LCX08DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="13"/>
<connect gate="A" pin="A3" pad="10"/>
<connect gate="A" pin="B0" pad="2"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="O0" pad="3"/>
<connect gate="A" pin="O1" pad="6"/>
<connect gate="A" pin="O2" pad="11"/>
<connect gate="A" pin="O3" pad="8"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LCX08DG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="98H0713"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LCX08DTG" prefix="U">
<description>Low-Voltage CMOS Quad 2-Input AND Gate</description>
<gates>
<gate name="A" symbol="MC74LCX08DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="13"/>
<connect gate="A" pin="A3" pad="10"/>
<connect gate="A" pin="B0" pad="2"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="O0" pad="3"/>
<connect gate="A" pin="O1" pad="6"/>
<connect gate="A" pin="O2" pad="11"/>
<connect gate="A" pin="O3" pad="8"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LCX08DTG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="70K3162"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LCX14DG" prefix="U">
<description>Low Voltage CMOS Hex Schmitt Inverter With 5 V-Tolerant Inputs</description>
<gates>
<gate name="A" symbol="MC74LCX14DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~Y1" pad="2"/>
<connect gate="A" pin="~Y2" pad="4"/>
<connect gate="A" pin="~Y3" pad="6"/>
<connect gate="A" pin="~Y4" pad="8"/>
<connect gate="A" pin="~Y5" pad="10"/>
<connect gate="A" pin="~Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LCX14DG"/>
<attribute name="OC_FARNELL" value="1567138"/>
<attribute name="OC_NEWARK" value="27M2486"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LCX16245DTG" prefix="U">
<description>Low-Voltage CMOS 16-Bit Transceiver</description>
<gates>
<gate name="A" symbol="MC74LCX16245DTG"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-48N">
<connects>
<connect gate="A" pin="A0" pad="47"/>
<connect gate="A" pin="A1" pad="46"/>
<connect gate="A" pin="A10" pad="33"/>
<connect gate="A" pin="A11" pad="32"/>
<connect gate="A" pin="A12" pad="30"/>
<connect gate="A" pin="A13" pad="29"/>
<connect gate="A" pin="A14" pad="27"/>
<connect gate="A" pin="A15" pad="26"/>
<connect gate="A" pin="A2" pad="44"/>
<connect gate="A" pin="A3" pad="43"/>
<connect gate="A" pin="A4" pad="41"/>
<connect gate="A" pin="A5" pad="40"/>
<connect gate="A" pin="A6" pad="38"/>
<connect gate="A" pin="A7" pad="37"/>
<connect gate="A" pin="A8" pad="36"/>
<connect gate="A" pin="A9" pad="35"/>
<connect gate="A" pin="B0" pad="2"/>
<connect gate="A" pin="B1" pad="3"/>
<connect gate="A" pin="B10" pad="16"/>
<connect gate="A" pin="B11" pad="17"/>
<connect gate="A" pin="B12" pad="19"/>
<connect gate="A" pin="B13" pad="20"/>
<connect gate="A" pin="B14" pad="22"/>
<connect gate="A" pin="B15" pad="23"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="6"/>
<connect gate="A" pin="B4" pad="8"/>
<connect gate="A" pin="B5" pad="9"/>
<connect gate="A" pin="B6" pad="11"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="13"/>
<connect gate="A" pin="B9" pad="14"/>
<connect gate="A" pin="GND" pad="39"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="21"/>
<connect gate="A" pin="GND_4" pad="10"/>
<connect gate="A" pin="GND_5" pad="15"/>
<connect gate="A" pin="GND_6" pad="28"/>
<connect gate="A" pin="GND_7" pad="45"/>
<connect gate="A" pin="GND_8" pad="34"/>
<connect gate="A" pin="T/~R1" pad="1"/>
<connect gate="A" pin="T/~R2" pad="24"/>
<connect gate="A" pin="VCC" pad="18"/>
<connect gate="A" pin="VCC_2" pad="7"/>
<connect gate="A" pin="VCC_3" pad="42"/>
<connect gate="A" pin="VCC_4" pad="31"/>
<connect gate="A" pin="~OE1" pad="48"/>
<connect gate="A" pin="~OE2" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LCX16245DTG"/>
<attribute name="OC_FARNELL" value="1468759"/>
<attribute name="OC_NEWARK" value="45J1362"/>
<attribute name="PACKAGE" value="48-TSSOP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LCX16245DTR2" prefix="U">
<description>Low-Voltage CMOS 16-Bit Transceiver</description>
<gates>
<gate name="A" symbol="MC74LCX16245DTR2"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-48N">
<connects>
<connect gate="A" pin="A0" pad="47"/>
<connect gate="A" pin="A1" pad="46"/>
<connect gate="A" pin="A10" pad="33"/>
<connect gate="A" pin="A11" pad="32"/>
<connect gate="A" pin="A12" pad="30"/>
<connect gate="A" pin="A13" pad="29"/>
<connect gate="A" pin="A14" pad="27"/>
<connect gate="A" pin="A15" pad="26"/>
<connect gate="A" pin="A2" pad="44"/>
<connect gate="A" pin="A3" pad="43"/>
<connect gate="A" pin="A4" pad="41"/>
<connect gate="A" pin="A5" pad="40"/>
<connect gate="A" pin="A6" pad="38"/>
<connect gate="A" pin="A7" pad="37"/>
<connect gate="A" pin="A8" pad="36"/>
<connect gate="A" pin="A9" pad="35"/>
<connect gate="A" pin="B0" pad="2"/>
<connect gate="A" pin="B1" pad="3"/>
<connect gate="A" pin="B10" pad="16"/>
<connect gate="A" pin="B11" pad="17"/>
<connect gate="A" pin="B12" pad="19"/>
<connect gate="A" pin="B13" pad="20"/>
<connect gate="A" pin="B14" pad="22"/>
<connect gate="A" pin="B15" pad="23"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="6"/>
<connect gate="A" pin="B4" pad="8"/>
<connect gate="A" pin="B5" pad="9"/>
<connect gate="A" pin="B6" pad="11"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="13"/>
<connect gate="A" pin="B9" pad="14"/>
<connect gate="A" pin="GND" pad="39"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="21"/>
<connect gate="A" pin="GND_4" pad="10"/>
<connect gate="A" pin="GND_5" pad="15"/>
<connect gate="A" pin="GND_6" pad="28"/>
<connect gate="A" pin="GND_7" pad="45"/>
<connect gate="A" pin="GND_8" pad="34"/>
<connect gate="A" pin="T/~R1" pad="1"/>
<connect gate="A" pin="T/~R2" pad="24"/>
<connect gate="A" pin="VCC" pad="18"/>
<connect gate="A" pin="VCC_2" pad="7"/>
<connect gate="A" pin="VCC_3" pad="42"/>
<connect gate="A" pin="VCC_4" pad="31"/>
<connect gate="A" pin="~OE1" pad="48"/>
<connect gate="A" pin="~OE2" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LCX16245DTR2"/>
<attribute name="OC_FARNELL" value="7615280"/>
<attribute name="OC_NEWARK" value="75C2896"/>
<attribute name="PACKAGE" value="48-TSSOP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LCX16373DTG" prefix="U">
<description>Low-Voltage CMOS 16-Bit Transparent Latch</description>
<gates>
<gate name="A" symbol="MC74LCX16373DTG"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-48N">
<connects>
<connect gate="A" pin="D0" pad="47"/>
<connect gate="A" pin="D1" pad="46"/>
<connect gate="A" pin="D10" pad="33"/>
<connect gate="A" pin="D11" pad="32"/>
<connect gate="A" pin="D12" pad="30"/>
<connect gate="A" pin="D13" pad="29"/>
<connect gate="A" pin="D14" pad="27"/>
<connect gate="A" pin="D15" pad="26"/>
<connect gate="A" pin="D2" pad="44"/>
<connect gate="A" pin="D3" pad="43"/>
<connect gate="A" pin="D4" pad="41"/>
<connect gate="A" pin="D5" pad="40"/>
<connect gate="A" pin="D6" pad="38"/>
<connect gate="A" pin="D7" pad="37"/>
<connect gate="A" pin="D8" pad="36"/>
<connect gate="A" pin="D9" pad="35"/>
<connect gate="A" pin="GN" pad="39"/>
<connect gate="A" pin="GND" pad="15"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="21"/>
<connect gate="A" pin="GND_4" pad="10"/>
<connect gate="A" pin="GN_2" pad="28"/>
<connect gate="A" pin="GN_3" pad="45"/>
<connect gate="A" pin="GN_4" pad="34"/>
<connect gate="A" pin="LE1" pad="48"/>
<connect gate="A" pin="LE2" pad="25"/>
<connect gate="A" pin="O0" pad="2"/>
<connect gate="A" pin="O1" pad="3"/>
<connect gate="A" pin="O10" pad="16"/>
<connect gate="A" pin="O11" pad="17"/>
<connect gate="A" pin="O12" pad="19"/>
<connect gate="A" pin="O13" pad="20"/>
<connect gate="A" pin="O14" pad="22"/>
<connect gate="A" pin="O15" pad="23"/>
<connect gate="A" pin="O2" pad="5"/>
<connect gate="A" pin="O3" pad="6"/>
<connect gate="A" pin="O4" pad="8"/>
<connect gate="A" pin="O5" pad="9"/>
<connect gate="A" pin="O6" pad="11"/>
<connect gate="A" pin="O7" pad="12"/>
<connect gate="A" pin="O8" pad="13"/>
<connect gate="A" pin="O9" pad="14"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="OE2" pad="24"/>
<connect gate="A" pin="VCC" pad="42"/>
<connect gate="A" pin="VCC_2" pad="7"/>
<connect gate="A" pin="VCC_3" pad="18"/>
<connect gate="A" pin="VCC_4" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LCX16373DTG"/>
<attribute name="OC_FARNELL" value="1706048"/>
<attribute name="OC_NEWARK" value="98H0715"/>
<attribute name="PACKAGE" value="48-TSSOP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LCX244DWG" prefix="U">
<description>CMOS Octal Buffer</description>
<gates>
<gate name="A" symbol="MC74LCX244DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="1D0" pad="2"/>
<connect gate="A" pin="1D1" pad="4"/>
<connect gate="A" pin="1D2" pad="6"/>
<connect gate="A" pin="1D3" pad="8"/>
<connect gate="A" pin="1O0" pad="18"/>
<connect gate="A" pin="1O1" pad="16"/>
<connect gate="A" pin="1O2" pad="14"/>
<connect gate="A" pin="1O3" pad="12"/>
<connect gate="A" pin="2D0" pad="17"/>
<connect gate="A" pin="2D1" pad="15"/>
<connect gate="A" pin="2D2" pad="13"/>
<connect gate="A" pin="2D3" pad="11"/>
<connect gate="A" pin="2O0" pad="3"/>
<connect gate="A" pin="2O1" pad="5"/>
<connect gate="A" pin="2O2" pad="7"/>
<connect gate="A" pin="2O3" pad="9"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="~1OE" pad="1"/>
<connect gate="A" pin="~2OE" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LCX244DWG"/>
<attribute name="OC_FARNELL" value="1468760"/>
<attribute name="OC_NEWARK" value="88H4742"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LCX245DWG" prefix="U">
<description>Low-Voltage CMOS Octal Transceiver</description>
<gates>
<gate name="A" symbol="MC74LCX245DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="A0" pad="2"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="6"/>
<connect gate="A" pin="A5" pad="7"/>
<connect gate="A" pin="A6" pad="8"/>
<connect gate="A" pin="A7" pad="9"/>
<connect gate="A" pin="B0" pad="18"/>
<connect gate="A" pin="B1" pad="17"/>
<connect gate="A" pin="B2" pad="16"/>
<connect gate="A" pin="B3" pad="15"/>
<connect gate="A" pin="B4" pad="14"/>
<connect gate="A" pin="B5" pad="13"/>
<connect gate="A" pin="B6" pad="12"/>
<connect gate="A" pin="B7" pad="11"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="T/R" pad="1"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="~OE" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LCX245DWG"/>
<attribute name="OC_FARNELL" value="1607898"/>
<attribute name="OC_NEWARK" value="71J5643"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LVX04DTR2G" prefix="U">
<description>Hex Inverter</description>
<gates>
<gate name="A" symbol="MC74LVX04DTR2G"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="11"/>
<connect gate="A" pin="A5" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~O0" pad="2"/>
<connect gate="A" pin="~O1" pad="4"/>
<connect gate="A" pin="~O2" pad="6"/>
<connect gate="A" pin="~O3" pad="8"/>
<connect gate="A" pin="~O4" pad="10"/>
<connect gate="A" pin="~O5" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LVX04DTR2G"/>
<attribute name="OC_FARNELL" value="1364067"/>
<attribute name="OC_NEWARK" value="26K4277"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LVX08DTG" prefix="U">
<description>Quad 2-Input AND Gate</description>
<gates>
<gate name="A" symbol="MC74LVX08DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="13"/>
<connect gate="A" pin="A3" pad="10"/>
<connect gate="A" pin="B0" pad="2"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="O0" pad="3"/>
<connect gate="A" pin="O1" pad="6"/>
<connect gate="A" pin="O2" pad="11"/>
<connect gate="A" pin="O3" pad="8"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LVX08DTG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="42K1002"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LVX08DTR2G" prefix="U">
<description>Quad 2-Input AND Gate</description>
<gates>
<gate name="A" symbol="MC74LVX08DTR2G"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="13"/>
<connect gate="A" pin="A3" pad="10"/>
<connect gate="A" pin="B0" pad="2"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="O0" pad="3"/>
<connect gate="A" pin="O1" pad="6"/>
<connect gate="A" pin="O2" pad="11"/>
<connect gate="A" pin="O3" pad="8"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LVX08DTR2G"/>
<attribute name="OC_FARNELL" value="1353762"/>
<attribute name="OC_NEWARK" value="26K4279"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LVX4245DTG" prefix="U">
<description>Dual Supply Octal Translating Transceiver</description>
<gates>
<gate name="A" symbol="MC74LVX4245DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-24N">
<connects>
<connect gate="A" pin="A0" pad="3"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="7"/>
<connect gate="A" pin="A5" pad="8"/>
<connect gate="A" pin="A6" pad="9"/>
<connect gate="A" pin="A7" pad="10"/>
<connect gate="A" pin="B0" pad="21"/>
<connect gate="A" pin="B1" pad="20"/>
<connect gate="A" pin="B2" pad="19"/>
<connect gate="A" pin="B3" pad="18"/>
<connect gate="A" pin="B4" pad="17"/>
<connect gate="A" pin="B5" pad="16"/>
<connect gate="A" pin="B6" pad="15"/>
<connect gate="A" pin="B7" pad="14"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="T/~R" pad="2"/>
<connect gate="A" pin="VCCA" pad="1"/>
<connect gate="A" pin="VCCB" pad="24"/>
<connect gate="A" pin="VCCB_2" pad="23"/>
<connect gate="A" pin="~OE" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LVX4245DTG"/>
<attribute name="OC_FARNELL" value="1607901"/>
<attribute name="OC_NEWARK" value="42K1044"/>
<attribute name="PACKAGE" value="SOP-24"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74LVXC3245DTG" prefix="U">
<description>Configurable Dual Supply Octal Transceiver</description>
<gates>
<gate name="A" symbol="MC74LVXC3245DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-24N">
<connects>
<connect gate="A" pin="A0" pad="3"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="7"/>
<connect gate="A" pin="A5" pad="8"/>
<connect gate="A" pin="A6" pad="9"/>
<connect gate="A" pin="A7" pad="10"/>
<connect gate="A" pin="B0" pad="21"/>
<connect gate="A" pin="B1" pad="20"/>
<connect gate="A" pin="B2" pad="19"/>
<connect gate="A" pin="B3" pad="18"/>
<connect gate="A" pin="B4" pad="17"/>
<connect gate="A" pin="B5" pad="16"/>
<connect gate="A" pin="B6" pad="15"/>
<connect gate="A" pin="B7" pad="14"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="NC" pad="23"/>
<connect gate="A" pin="T/~R" pad="2"/>
<connect gate="A" pin="VCCA" pad="1"/>
<connect gate="A" pin="VCCB" pad="24"/>
<connect gate="A" pin="~OE" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74LVXC3245DTG"/>
<attribute name="OC_FARNELL" value="1126244"/>
<attribute name="OC_NEWARK" value="42K0978"/>
<attribute name="PACKAGE" value="TSSOP-24"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC138DG" prefix="U">
<description>3--to--8 Line Decoder</description>
<gates>
<gate name="A" symbol="MC74VHC138DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="E3" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~E1" pad="4"/>
<connect gate="A" pin="~E2" pad="5"/>
<connect gate="A" pin="~Y0" pad="15"/>
<connect gate="A" pin="~Y1" pad="14"/>
<connect gate="A" pin="~Y2" pad="13"/>
<connect gate="A" pin="~Y3" pad="12"/>
<connect gate="A" pin="~Y4" pad="11"/>
<connect gate="A" pin="~Y5" pad="10"/>
<connect gate="A" pin="~Y6" pad="9"/>
<connect gate="A" pin="~Y7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC138DG"/>
<attribute name="OC_FARNELL" value="1345135"/>
<attribute name="OC_NEWARK" value="42K1128"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC14DTG" prefix="U">
<description>Hex Schmitt Inverter</description>
<gates>
<gate name="A" symbol="MC74VHC14DTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-14N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~Y1" pad="2"/>
<connect gate="A" pin="~Y2" pad="4"/>
<connect gate="A" pin="~Y3" pad="6"/>
<connect gate="A" pin="~Y4" pad="8"/>
<connect gate="A" pin="~Y5" pad="10"/>
<connect gate="A" pin="~Y6" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC14DTG"/>
<attribute name="OC_FARNELL" value="1420212"/>
<attribute name="OC_NEWARK" value="42K1131"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G00DFT1G" prefix="U">
<description>Single 2-Input NAND Gate</description>
<gates>
<gate name="A" symbol="MC74VHC1G00DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_~Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G00DFT1G"/>
<attribute name="OC_FARNELL" value="1607775"/>
<attribute name="OC_NEWARK" value="67H6739"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G00DFT2G" prefix="U">
<description>Single 2-Input NAND Gate</description>
<gates>
<gate name="A" symbol="MC74VHC1G00DFT2G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_~Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G00DFT2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7798"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G03DFT1G" prefix="U">
<description>Single 2-Input NOR Gate with Open Drain Output</description>
<gates>
<gate name="A" symbol="MC74VHC1G03DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_~Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G03DFT1G"/>
<attribute name="OC_FARNELL" value="1311401"/>
<attribute name="OC_NEWARK" value="67H6745"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G04DFT1G" prefix="U">
<description>Single Inverter</description>
<gates>
<gate name="A" symbol="MC74VHC1G04DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_~Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G04DFT1G"/>
<attribute name="OC_FARNELL" value="6389478"/>
<attribute name="OC_NEWARK" value="09H2337"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G05DFT1G" prefix="U">
<description>Single Inverter with Open Drain Output</description>
<gates>
<gate name="A" symbol="MC74VHC1G05DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_~Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G05DFT1G"/>
<attribute name="OC_FARNELL" value="1155487"/>
<attribute name="OC_NEWARK" value="67H6747"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G08DFT1G" prefix="U">
<description>Single 2-Input AND Gate</description>
<gates>
<gate name="A" symbol="MC74VHC1G08DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G08DFT1G"/>
<attribute name="OC_FARNELL" value="1353867"/>
<attribute name="OC_NEWARK" value="67H6751"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G09DFT1G" prefix="U">
<description>2-Input AND Gate with Open Drain Output</description>
<gates>
<gate name="A" symbol="MC74VHC1G09DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G09DFT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="67H6753"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G125DFT1" prefix="U">
<description>Noninverting 3-State Buffer</description>
<gates>
<gate name="A" symbol="MC74VHC1G125DFT1"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~OE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G125DFT1"/>
<attribute name="OC_FARNELL" value="4523088"/>
<attribute name="OC_NEWARK" value="27C8252"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G126DFT1" prefix="U">
<description>Noninverting 3-State Buffer</description>
<gates>
<gate name="A" symbol="MC74VHC1G126DFT1"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G126DFT1"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="27C8257"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G14DFT1G" prefix="U">
<description>Single Schmitt-Trigger Inverter</description>
<gates>
<gate name="A" symbol="MC74VHC1G14DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_~Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G14DFT1G"/>
<attribute name="OC_FARNELL" value="1353868"/>
<attribute name="OC_NEWARK" value="67H6763"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G32DTT1G" prefix="U">
<description>Single 2-Input OR Gate</description>
<gates>
<gate name="A" symbol="MC74VHC1G32DTT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G32DTT1G"/>
<attribute name="OC_FARNELL" value="1607778"/>
<attribute name="OC_NEWARK" value="83H7308"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1G86DFT1G" prefix="U">
<description>Single 2-Input Exclusive OR Gate</description>
<gates>
<gate name="A" symbol="MC74VHC1G86DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1G86DFT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="67H6771"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1GT125DF1" prefix="U">
<description>Noninverting Buffer /CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="MC74VHC1GT125DF1"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~OE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1GT125DF1"/>
<attribute name="OC_FARNELL" value="4542496"/>
<attribute name="OC_NEWARK" value="35C3055"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1GT125DF2" prefix="U">
<description>Noninverting Buffer /CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="MC74VHC1GT125DF2"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~OE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1GT125DF2"/>
<attribute name="OC_FARNELL" value="4782239"/>
<attribute name="OC_NEWARK" value="27C8237"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1GT125DT1" prefix="U">
<description>Noninverting Buffer /CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="MC74VHC1GT125DT1"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~OE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1GT125DT1"/>
<attribute name="OC_FARNELL" value="4523039"/>
<attribute name="OC_NEWARK" value="27C8239"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1GT126DF1" prefix="U">
<description>Noninverting Buffer / CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="MC74VHC1GT126DF1"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1GT126DF1"/>
<attribute name="OC_FARNELL" value="4812918"/>
<attribute name="OC_NEWARK" value="35C3056"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1GT126DF1G" prefix="U">
<description>Noninverting Buffer / CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="MC74VHC1GT126DF1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1GT126DF1G"/>
<attribute name="OC_FARNELL" value="1654341"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1GT32DFT1G" prefix="U">
<description>2-Input OR Gate/CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="MC74VHC1GT32DFT1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1GT32DFT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74R1832"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHC1GT50DTT1" prefix="U">
<description>Noninverting Buffer / CMOS Logic Level Shifter</description>
<gates>
<gate name="A" symbol="MC74VHC1GT50DTT1"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHC1GT50DTT1"/>
<attribute name="OC_FARNELL" value="1652259"/>
<attribute name="OC_NEWARK" value="35C3058"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC74VHCT125ADR2G" prefix="U">
<description>Quad Bus Buffer</description>
<gates>
<gate name="A" symbol="MC74VHCT125ADR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="~OE1" pad="1"/>
<connect gate="A" pin="~OE2" pad="4"/>
<connect gate="A" pin="~OE3" pad="10"/>
<connect gate="A" pin="~OE4" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC74VHCT125ADR2G"/>
<attribute name="OC_FARNELL" value="1468762"/>
<attribute name="OC_NEWARK" value="26K4324"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC75174BDWG" prefix="U">
<description>Quad RS-485 Line Drivers</description>
<gates>
<gate name="A" symbol="MC75174BDWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="1A" pad="1"/>
<connect gate="A" pin="1Y" pad="2"/>
<connect gate="A" pin="1Z" pad="4"/>
<connect gate="A" pin="2A" pad="9"/>
<connect gate="A" pin="2Y" pad="8"/>
<connect gate="A" pin="2Z" pad="6"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3Y" pad="12"/>
<connect gate="A" pin="3Z" pad="14"/>
<connect gate="A" pin="4A" pad="19"/>
<connect gate="A" pin="4Y" pad="18"/>
<connect gate="A" pin="4Z" pad="16"/>
<connect gate="A" pin="EN12" pad="5"/>
<connect gate="A" pin="EN34" pad="15"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="NC" pad="17"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="NC_4" pad="13"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC75174BDWG"/>
<attribute name="OC_FARNELL" value="1258376"/>
<attribute name="OC_NEWARK" value="42K1167"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC75174BPG" prefix="U">
<description>Quad EIA-485 Line Drivers with Three-State Outputs</description>
<gates>
<gate name="A" symbol="MC75174BPG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="1A" pad="1"/>
<connect gate="A" pin="1Y" pad="2"/>
<connect gate="A" pin="1Z" pad="3"/>
<connect gate="A" pin="2A" pad="7"/>
<connect gate="A" pin="2Y" pad="6"/>
<connect gate="A" pin="2Z" pad="5"/>
<connect gate="A" pin="3A" pad="9"/>
<connect gate="A" pin="3Y" pad="10"/>
<connect gate="A" pin="3Z" pad="11"/>
<connect gate="A" pin="4A" pad="15"/>
<connect gate="A" pin="4Y" pad="14"/>
<connect gate="A" pin="4Z" pad="13"/>
<connect gate="A" pin="EN_12" pad="4"/>
<connect gate="A" pin="EN_34" pad="12"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC75174BPG"/>
<attribute name="OC_FARNELL" value="1252475"/>
<attribute name="OC_NEWARK" value="42K1168"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L05ABDG" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L05ABDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L05ABDG"/>
<attribute name="OC_FARNELL" value="1652342"/>
<attribute name="OC_NEWARK" value="71J5712"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L05ABDR2G" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L05ABDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L05ABDR2G"/>
<attribute name="OC_FARNELL" value="1353941"/>
<attribute name="OC_NEWARK" value="88H4745"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L05ACDG" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L05ACDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L05ACDG"/>
<attribute name="OC_FARNELL" value="9666265"/>
<attribute name="OC_NEWARK" value="88H4746"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L05ACDR2G" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L05ACDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L05ACDR2G"/>
<attribute name="OC_FARNELL" value="1278565"/>
<attribute name="OC_NEWARK" value="88H4747"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L08ABDG" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L08ABDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L08ABDG"/>
<attribute name="OC_FARNELL" value="1155721"/>
<attribute name="OC_NEWARK" value="88H4750"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L08ACDG" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L08ACDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L08ACDG"/>
<attribute name="OC_FARNELL" value="1211120"/>
<attribute name="OC_NEWARK" value="45J1406"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L09ACDG" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L09ACDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L09ACDG"/>
<attribute name="OC_FARNELL" value="1147860"/>
<attribute name="OC_NEWARK" value="71J5715"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L12ACDG" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L12ACDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L12ACDG"/>
<attribute name="OC_FARNELL" value="9666273"/>
<attribute name="OC_NEWARK" value="71J5719"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L12ACDR2G" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L12ACDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L12ACDR2G"/>
<attribute name="OC_FARNELL" value="1278494"/>
<attribute name="OC_NEWARK" value="84K8788"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L15ABDG" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L15ABDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L15ABDG"/>
<attribute name="OC_FARNELL" value="1705888"/>
<attribute name="OC_NEWARK" value="42K1177"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L15ACDG" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L15ACDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L15ACDG"/>
<attribute name="OC_FARNELL" value="1211121"/>
<attribute name="OC_NEWARK" value="71J5721"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78L15ACDR2G" prefix="U">
<description>Positive Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78L15ACDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78L15ACDR2G"/>
<attribute name="OC_FARNELL" value="1278495"/>
<attribute name="OC_NEWARK" value="84K8789"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78LC33NTRG" prefix="U">
<description>Micropower Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78LC33NTRG"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="N/C" pad="4"/>
<connect gate="A" pin="N/C_2" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78LC33NTRG"/>
<attribute name="OC_FARNELL" value="1652349"/>
<attribute name="OC_NEWARK" value="71J5709"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78LC50NTRG" prefix="U">
<description>Micropower Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78LC50NTRG"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="N/C" pad="4"/>
<connect gate="A" pin="N/C_2" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78LC50NTRG"/>
<attribute name="OC_FARNELL" value="1652350"/>
<attribute name="OC_NEWARK" value="26K4390"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78PC18NTRG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78PC18NTRG"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="N/C" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78PC18NTRG"/>
<attribute name="OC_FARNELL" value="1130695"/>
<attribute name="OC_NEWARK" value="88H4756"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78PC33NTRG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78PC33NTRG"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="N/C" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78PC33NTRG"/>
<attribute name="OC_FARNELL" value="1652356"/>
<attribute name="OC_NEWARK" value="45J1438"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78PC50NTRG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC78PC50NTRG"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="N/C" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC78PC50NTRG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="42K1216"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC79L05ABDG" prefix="U">
<description>Negative Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC79L05ABDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VIN_2" pad="6"/>
<connect gate="A" pin="VIN_3" pad="2"/>
<connect gate="A" pin="VIN_4" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC79L05ABDG"/>
<attribute name="OC_FARNELL" value="1652359"/>
<attribute name="OC_NEWARK" value="71J5761"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC79L12ACDG" prefix="U">
<description>Negative Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC79L12ACDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VIN_2" pad="6"/>
<connect gate="A" pin="VIN_3" pad="2"/>
<connect gate="A" pin="VIN_4" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC79L12ACDG"/>
<attribute name="OC_FARNELL" value="1652361"/>
<attribute name="OC_NEWARK" value="26K4410"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC79L15ACDG" prefix="U">
<description>Negative Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="MC79L15ACDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VIN_2" pad="6"/>
<connect gate="A" pin="VIN_3" pad="2"/>
<connect gate="A" pin="VIN_4" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MC79L15ACDG"/>
<attribute name="OC_FARNELL" value="1211126"/>
<attribute name="OC_NEWARK" value="26K4415"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCH12140DG" prefix="U">
<description>Phase-Frequency Detector</description>
<gates>
<gate name="A" symbol="MCH12140DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="4"/>
<connect gate="A" pin="R" pad="7"/>
<connect gate="A" pin="U" pad="2"/>
<connect gate="A" pin="V" pad="6"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="~D" pad="3"/>
<connect gate="A" pin="~U" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MCH12140DG"/>
<attribute name="OC_FARNELL" value="1704006"/>
<attribute name="OC_NEWARK" value="45J0812"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MDC3105DMT1G" prefix="U">
<description>Integrated Relay,Inductive Load Driver</description>
<gates>
<gate name="A" symbol="MDC3105DMT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-6N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VIN_2" pad="5"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="VOUT_2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MDC3105DMT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7836"/>
<attribute name="PACKAGE" value="SC-74-6"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MDC3105LT1G" prefix="U">
<description>Integrated Relay,  Inductive Load Driver</description>
<gates>
<gate name="A" symbol="MDC3105LT1G"/>
</gates>
<devices>
<device name="" package="SOT95P240X110-3N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MDC3105LT1G"/>
<attribute name="OC_FARNELL" value="1126459"/>
<attribute name="OC_NEWARK" value="45J1474"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMBZ5243BLT1G" prefix="U">
<description>Zener Voltage Regulators</description>
<gates>
<gate name="A" symbol="MMBZ5243BLT1G"/>
</gates>
<devices>
<device name="" package="SOT95P240X110-3N">
<connects>
<connect gate="A" pin="ANODE" pad="1"/>
<connect gate="A" pin="CATHODE" pad="3"/>
<connect gate="A" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MMBZ5243BLT1G"/>
<attribute name="OC_FARNELL" value="1899437"/>
<attribute name="OC_NEWARK" value="98H0778"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="N25S830HAS22I" prefix="U">
<description>256 Kb Low Power Serial SRAMs</description>
<gates>
<gate name="A" symbol="N25S830HAS22I"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="SCK" pad="6"/>
<connect gate="A" pin="SI" pad="5"/>
<connect gate="A" pin="SO" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VSS" pad="4"/>
<connect gate="A" pin="~CS" pad="1"/>
<connect gate="A" pin="~HOLD" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="N25S830HAS22I"/>
<attribute name="OC_FARNELL" value="1668757"/>
<attribute name="OC_NEWARK" value="03P1180"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NB100ELT23LDTG" prefix="U">
<description>Translator</description>
<gates>
<gate name="A" symbol="NB100ELT23LDTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="Q0" pad="7"/>
<connect gate="A" pin="Q1" pad="6"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~D0" pad="2"/>
<connect gate="A" pin="~D1" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NB100ELT23LDTG"/>
<attribute name="OC_FARNELL" value="1607888"/>
<attribute name="OC_NEWARK" value="45J1769"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NB3L553DG" prefix="U">
<description>2.5 V / 3.3 V / 5.0 V 1:4 Clock Fanout Buffer</description>
<gates>
<gate name="A" symbol="NB3L553DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ICLK" pad="5"/>
<connect gate="A" pin="OE" pad="8"/>
<connect gate="A" pin="Q0" pad="2"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NB3L553DG"/>
<attribute name="OC_FARNELL" value="1705282"/>
<attribute name="OC_NEWARK" value="02M9803"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NB3N2304NZDTG" prefix="U">
<description>Buffer</description>
<gates>
<gate name="A" symbol="NB3N2304NZDTG"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OE" pad="2"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="8"/>
<connect gate="A" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NB3N2304NZDTG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="27M2498"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NB3N551DG" prefix="U">
<description>3.3 V / 5.0 V Ultra-Low Skew 1:4 Clock Fanout Buffer</description>
<gates>
<gate name="A" symbol="NB3N551DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ICLK" pad="1"/>
<connect gate="A" pin="OE" pad="8"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="4"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="A" pin="VDD" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NB3N551DG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="02M9807"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NB6L11DTG" prefix="U">
<description>Translator</description>
<gates>
<gate name="A" symbol="NB6L11DTG"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~D" pad="6"/>
<connect gate="A" pin="~Q0" pad="2"/>
<connect gate="A" pin="~Q1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NB6L11DTG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="61K1178"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NB6L14MNG" prefix="U">
<description>1:4 Fanout Buffer</description>
<gates>
<gate name="A" symbol="NB6L14MNG"/>
</gates>
<devices>
<device name="" package="QFN50P300X300X100-17N">
<connects>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="IN" pad="12"/>
<connect gate="A" pin="Q0" pad="15"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="5"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VCC_2" pad="7"/>
<connect gate="A" pin="VREF_AC" pad="10"/>
<connect gate="A" pin="VT" pad="11"/>
<connect gate="A" pin="~IN" pad="9"/>
<connect gate="A" pin="~Q0" pad="16"/>
<connect gate="A" pin="~Q1" pad="2"/>
<connect gate="A" pin="~Q2" pad="4"/>
<connect gate="A" pin="~Q3" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NB6L14MNG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M7325"/>
<attribute name="PACKAGE" value="QFN-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NB6L239MNG" prefix="U">
<description>Clock Driver</description>
<gates>
<gate name="A" symbol="NB6L239MNG"/>
</gates>
<devices>
<device name="" package="QFN50P300X300X100-17N">
<connects>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="QA" pad="12"/>
<connect gate="A" pin="QB" pad="10"/>
<connect gate="A" pin="SELA0" pad="15"/>
<connect gate="A" pin="SELA1" pad="14"/>
<connect gate="A" pin="SELB0" pad="6"/>
<connect gate="A" pin="SELB1" pad="7"/>
<connect gate="A" pin="VBBAC" pad="4"/>
<connect gate="A" pin="VCC" pad="13"/>
<connect gate="A" pin="VEE" pad="8"/>
<connect gate="A" pin="VT" pad="1"/>
<connect gate="A" pin="~CLK" pad="3"/>
<connect gate="A" pin="~EN" pad="5"/>
<connect gate="A" pin="~MR" pad="16"/>
<connect gate="A" pin="~QA" pad="11"/>
<connect gate="A" pin="~QB" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NB6L239MNG"/>
<attribute name="OC_FARNELL" value="1258239"/>
<attribute name="OC_NEWARK" value="26K4793"/>
<attribute name="PACKAGE" value="QFN-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NB6N14SMNG" prefix="U">
<description>1:4 Fanout Buffer/Translator</description>
<gates>
<gate name="A" symbol="NB6N14SMNG"/>
</gates>
<devices>
<device name="" package="QFN50P300X300X100-17N">
<connects>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="IN" pad="12"/>
<connect gate="A" pin="Q0" pad="15"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="5"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VCC_2" pad="7"/>
<connect gate="A" pin="VREF_AC" pad="10"/>
<connect gate="A" pin="VT" pad="11"/>
<connect gate="A" pin="~IN" pad="9"/>
<connect gate="A" pin="~Q0" pad="16"/>
<connect gate="A" pin="~Q1" pad="2"/>
<connect gate="A" pin="~Q2" pad="4"/>
<connect gate="A" pin="~Q3" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NB6N14SMNG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="02M9811"/>
<attribute name="PACKAGE" value="QFN-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NBSG11MNG" prefix="U">
<description>Clock Driver</description>
<gates>
<gate name="A" symbol="NBSG11MNG"/>
</gates>
<devices>
<device name="" package="QFN50P300X300X100-17N">
<connects>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="NC" pad="15"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="NC_4" pad="14"/>
<connect gate="A" pin="Q0" pad="12"/>
<connect gate="A" pin="Q1" pad="10"/>
<connect gate="A" pin="VCC" pad="13"/>
<connect gate="A" pin="VCC_2" pad="8"/>
<connect gate="A" pin="VEE" pad="16"/>
<connect gate="A" pin="VEE_2" pad="5"/>
<connect gate="A" pin="VTCLK" pad="4"/>
<connect gate="A" pin="~CLK" pad="2"/>
<connect gate="A" pin="~Q0" pad="11"/>
<connect gate="A" pin="~Q1" pad="9"/>
<connect gate="A" pin="~VTCLK" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NBSG11MNG"/>
<attribute name="OC_FARNELL" value="1364630"/>
<attribute name="OC_NEWARK" value="45J1760"/>
<attribute name="PACKAGE" value="QFN-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP100SNT1G" prefix="U">
<description>Sub 1.0 V Precision Adjustable Shunt Regulator</description>
<gates>
<gate name="A" symbol="NCP100SNT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="ANODE" pad="2"/>
<connect gate="A" pin="ANODE_2" pad="5"/>
<connect gate="A" pin="CATHODE" pad="3"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="REFERENCE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP100SNT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J1778"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1055P100G" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="NCP1055P100G"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="CONTROL_INPUT" pad="2"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="GND_3" pad="8"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="POWER_SWITCH_DRAIN" pad="5"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1055P100G"/>
<attribute name="OC_FARNELL" value="1155580"/>
<attribute name="OC_NEWARK" value="71J6558"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1055P136G" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="NCP1055P136G"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="CONTROL_INPUT" pad="2"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="GND_3" pad="8"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="POWER_SWITCH_DRAIN" pad="5"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1055P136G"/>
<attribute name="OC_FARNELL" value="1364573"/>
<attribute name="OC_NEWARK" value="42K1799"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1090DG" prefix="U">
<description>Integrated IEEE 802.3af PoE-PD Interface Controller</description>
<gates>
<gate name="A" symbol="NCP1090DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X172-8N">
<connects>
<connect gate="A" pin="CLASS" pad="2"/>
<connect gate="A" pin="DET" pad="3"/>
<connect gate="A" pin="INRUSH" pad="1"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="PGOOD" pad="6"/>
<connect gate="A" pin="RTN" pad="5"/>
<connect gate="A" pin="VPORTN" pad="4"/>
<connect gate="A" pin="VPORTP" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1090DG"/>
<attribute name="OC_FARNELL" value="1901642"/>
<attribute name="OC_NEWARK" value="55T3598"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1092DG" prefix="U">
<description>Integrated IEEE 802.3af PoE-PD Interface Controller</description>
<gates>
<gate name="A" symbol="NCP1092DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X172-8N">
<connects>
<connect gate="A" pin="AUX" pad="7"/>
<connect gate="A" pin="CLASS" pad="2"/>
<connect gate="A" pin="DET" pad="3"/>
<connect gate="A" pin="INRUSH" pad="1"/>
<connect gate="A" pin="PGOOD" pad="6"/>
<connect gate="A" pin="RTN" pad="5"/>
<connect gate="A" pin="VPORTN" pad="4"/>
<connect gate="A" pin="VPORTP" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1092DG"/>
<attribute name="OC_FARNELL" value="1901647"/>
<attribute name="OC_NEWARK" value="55T3602"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1200D100R2G" prefix="U">
<description>Fixed Frequency Flyback Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="NCP1200D100R2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="CS" pad="3"/>
<connect gate="A" pin="DRV" pad="5"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="HV" pad="8"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1200D100R2G"/>
<attribute name="OC_FARNELL" value="1652430"/>
<attribute name="OC_NEWARK" value="88H4976"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1200P100G" prefix="U">
<description>PWM Current-Mode</description>
<gates>
<gate name="A" symbol="NCP1200P100G"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="CS" pad="3"/>
<connect gate="A" pin="DRV" pad="5"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="HV" pad="8"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1200P100G"/>
<attribute name="OC_FARNELL" value="1652431"/>
<attribute name="OC_NEWARK" value="88H4977"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1200P40G" prefix="U">
<description>PWM Current-Mode</description>
<gates>
<gate name="A" symbol="NCP1200P40G"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="CS" pad="3"/>
<connect gate="A" pin="DRV" pad="5"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="HV" pad="8"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1200P40G"/>
<attribute name="OC_FARNELL" value="1652432"/>
<attribute name="OC_NEWARK" value="88H4978"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1200P60G" prefix="U">
<description>PWM Current-Mode</description>
<gates>
<gate name="A" symbol="NCP1200P60G"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="CS" pad="3"/>
<connect gate="A" pin="DRV" pad="5"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="HV" pad="8"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1200P60G"/>
<attribute name="OC_FARNELL" value="1652433"/>
<attribute name="OC_NEWARK" value="88H4979"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1203D100R2G" prefix="U">
<description>Fixed Frequency Flyback Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="NCP1203D100R2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="CS" pad="3"/>
<connect gate="A" pin="DRV" pad="5"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="HV" pad="8"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1203D100R2G"/>
<attribute name="OC_FARNELL" value="1652434"/>
<attribute name="OC_NEWARK" value="98H0874"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1203D60R2G" prefix="U">
<description>Fixed Frequency Flyback Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="NCP1203D60R2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="CS" pad="3"/>
<connect gate="A" pin="DRV" pad="5"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="HV" pad="8"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1203D60R2G"/>
<attribute name="OC_FARNELL" value="1652435"/>
<attribute name="OC_NEWARK" value="45J1797"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1230D100R2G" prefix="U">
<description>Low-Standby Power High Performance PWM Controller</description>
<gates>
<gate name="A" symbol="NCP1230D100R2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CS" pad="3"/>
<connect gate="A" pin="DRV" pad="5"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="HV" pad="8"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="PFC_VCC" pad="1"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1230D100R2G"/>
<attribute name="OC_FARNELL" value="1736555"/>
<attribute name="OC_NEWARK" value="77M8942"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1400ASN33T1G" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="NCP1400ASN33T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="LX" pad="5"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1400ASN33T1G"/>
<attribute name="OC_FARNELL" value="1652392"/>
<attribute name="OC_NEWARK" value="42K1839"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1402SN33T1G" prefix="U">
<description>Micropower Switching Regulator</description>
<gates>
<gate name="A" symbol="NCP1402SN33T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="LX" pad="5"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1402SN33T1G"/>
<attribute name="OC_FARNELL" value="1703414"/>
<attribute name="OC_NEWARK" value="45J1846"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1402SN50T1G" prefix="U">
<description>200 mA, PFM Step-Up Micropower Switching Regulator</description>
<gates>
<gate name="A" symbol="NCP1402SN50T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="LX" pad="5"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1402SN50T1G"/>
<attribute name="OC_FARNELL" value="1652393"/>
<attribute name="OC_NEWARK" value="98H0882"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1450ASN19T1G" prefix="U">
<description>PWM Step-up DC-DC Controller</description>
<gates>
<gate name="A" symbol="NCP1450ASN19T1G"/>
</gates>
<devices>
<device name="" package="SOT95P280X110-5N">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="EXT" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1450ASN19T1G"/>
<attribute name="OC_FARNELL" value="1924868"/>
<attribute name="OC_NEWARK" value="58T2051"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1450ASN27T1G" prefix="U">
<description>PWM Step-up DC-DC Controller</description>
<gates>
<gate name="A" symbol="NCP1450ASN27T1G"/>
</gates>
<devices>
<device name="" package="SOT95P280X110-5N">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="EXT" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1450ASN27T1G"/>
<attribute name="OC_FARNELL" value="1924869"/>
<attribute name="OC_NEWARK" value="58T2052"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1450ASN33T1G" prefix="U">
<description>PWM Step-up DC-DC Controller</description>
<gates>
<gate name="A" symbol="NCP1450ASN33T1G"/>
</gates>
<devices>
<device name="" package="SOT95P280X110-5N">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="EXT" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1450ASN33T1G"/>
<attribute name="OC_FARNELL" value="1924870"/>
<attribute name="OC_NEWARK" value="58T2053"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1521BSNT1G" prefix="U">
<description>1.5 MHz, 600 mA Step-Down DC-DC Converter</description>
<gates>
<gate name="A" symbol="NCP1521BSNT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="LX" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1521BSNT1G"/>
<attribute name="OC_FARNELL" value="1432258"/>
<attribute name="OC_NEWARK" value="04R7840"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1529ASNT1G" prefix="U">
<description>1.7MHz, 1A, High Efficiency, Low Ripple, Adjustable Output Voltage Step-down Converter</description>
<gates>
<gate name="A" symbol="NCP1529ASNT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="VIN" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1529ASNT1G"/>
<attribute name="OC_FARNELL" value="1642398"/>
<attribute name="OC_NEWARK" value="75M5084"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1529MUTBG" prefix="U">
<description>Voltage Step-down Converter</description>
<gates>
<gate name="A" symbol="NCP1529MUTBG"/>
</gates>
<devices>
<device name="" package="DFN200X200X55-7N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1529MUTBG"/>
<attribute name="OC_FARNELL" value="1642428"/>
<attribute name="OC_NEWARK" value="95M6817"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1729SN35T1G" prefix="U">
<description>Switched Capacitor Voltage Inverter</description>
<gates>
<gate name="A" symbol="NCP1729SN35T1G"/>
</gates>
<devices>
<device name="" package="SOP95P275X110-6N">
<connects>
<connect gate="A" pin="C+" pad="6"/>
<connect gate="A" pin="C-" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="~SHDN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP1729SN35T1G"/>
<attribute name="OC_FARNELL" value="1652414"/>
<attribute name="OC_NEWARK" value="45J1868"/>
<attribute name="PACKAGE" value="TSOP-6"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP2811BFCCT1G" prefix="U">
<description>Stereo Headphone Amplifier</description>
<gates>
<gate name="A" symbol="NCP2811BFCCT1G"/>
</gates>
<devices>
<device name="" package="BGA12C50P4X3_150X200X60">
<connects>
<connect gate="A" pin="AGND" pad="A1"/>
<connect gate="A" pin="CPM" pad="C3"/>
<connect gate="A" pin="CPP" pad="C1"/>
<connect gate="A" pin="INL" pad="B3"/>
<connect gate="A" pin="INR" pad="B2"/>
<connect gate="A" pin="OUTL" pad="A4"/>
<connect gate="A" pin="OUTR" pad="A3"/>
<connect gate="A" pin="PGND" pad="C2"/>
<connect gate="A" pin="PVM" pad="C4"/>
<connect gate="A" pin="SPVM" pad="B4"/>
<connect gate="A" pin="VP" pad="B1"/>
<connect gate="A" pin="~SD" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP2811BFCCT1G"/>
<attribute name="OC_FARNELL" value="1885119"/>
<attribute name="OC_NEWARK" value="41T0724"/>
<attribute name="PACKAGE" value="Flip-Chip -12"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP2824FCT2G" prefix="U">
<description>Class D Amplifier</description>
<gates>
<gate name="A" symbol="NCP2824FCT2G"/>
</gates>
<devices>
<device name="" package="BGA9C50P3X3_145X145X66">
<connects>
<connect gate="A" pin="AGND" pad="B1"/>
<connect gate="A" pin="CNTL" pad="C2"/>
<connect gate="A" pin="INM" pad="C1"/>
<connect gate="A" pin="INP" pad="A1"/>
<connect gate="A" pin="NC" pad="B2"/>
<connect gate="A" pin="OUTM" pad="C3"/>
<connect gate="A" pin="OUTP" pad="A3"/>
<connect gate="A" pin="PGND" pad="B3"/>
<connect gate="A" pin="VDD" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP2824FCT2G"/>
<attribute name="OC_FARNELL" value="1885120"/>
<attribute name="OC_NEWARK" value="41T0725"/>
<attribute name="PACKAGE" value="WCSP-9"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP301LSN09T1G" prefix="U">
<description>Voltage Detector Series</description>
<gates>
<gate name="A" symbol="NCP301LSN09T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="N.C._2" pad="4"/>
<connect gate="A" pin="RESET_OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP301LSN09T1G"/>
<attribute name="OC_FARNELL" value="1705034"/>
<attribute name="OC_NEWARK" value="71J6593"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP301LSN20T1G" prefix="U">
<description>Voltage Detector Series</description>
<gates>
<gate name="A" symbol="NCP301LSN20T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="N.C" pad="4"/>
<connect gate="A" pin="N.C_2" pad="5"/>
<connect gate="A" pin="RESET_OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP301LSN20T1G"/>
<attribute name="OC_FARNELL" value="1311235"/>
<attribute name="OC_NEWARK" value="45J1876"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP301LSN45T1G" prefix="U">
<description>Voltage Detector Series</description>
<gates>
<gate name="A" symbol="NCP301LSN45T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="N.C._2" pad="4"/>
<connect gate="A" pin="RESET_OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP301LSN45T1G"/>
<attribute name="OC_FARNELL" value="1468769"/>
<attribute name="OC_NEWARK" value="98H0891"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP301LSN47T1G" prefix="U">
<description>Voltage Detector Series</description>
<gates>
<gate name="A" symbol="NCP301LSN47T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="N.C._2" pad="4"/>
<connect gate="A" pin="RESET_OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP301LSN47T1G"/>
<attribute name="OC_FARNELL" value="1364633"/>
<attribute name="OC_NEWARK" value="45J1877"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP302LSN30T1G" prefix="U">
<description>Voltage Detector Series with Programmable Delay</description>
<gates>
<gate name="A" symbol="NCP302LSN30T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="CD" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="N.C." pad="4"/>
<connect gate="A" pin="RESET_OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP302LSN30T1G"/>
<attribute name="OC_FARNELL" value="1136366"/>
<attribute name="OC_NEWARK" value="88H4986"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP302LSN45T1G" prefix="U">
<description>Voltage Detector Series with Programmable Delay</description>
<gates>
<gate name="A" symbol="NCP302LSN45T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="CD" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="N.C." pad="4"/>
<connect gate="A" pin="RESET_OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP302LSN45T1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="45J1882"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP303LSN09T1G" prefix="U">
<description>Voltage Detector Series with Programmable Delay</description>
<gates>
<gate name="A" symbol="NCP303LSN09T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="CD" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="N.C." pad="4"/>
<connect gate="A" pin="RESET_OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP303LSN09T1G"/>
<attribute name="OC_FARNELL" value="1364634"/>
<attribute name="OC_NEWARK" value="45J1883"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP303LSN20T1G" prefix="U">
<description>Voltage Detector Series with Programmable Delay</description>
<gates>
<gate name="A" symbol="NCP303LSN20T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="CD" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="N.C." pad="4"/>
<connect gate="A" pin="RESET_OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP303LSN20T1G"/>
<attribute name="OC_FARNELL" value="1652299"/>
<attribute name="OC_NEWARK" value="83H7654"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP3063BDR2G" prefix="U">
<description>Inverting Switching Regulators</description>
<gates>
<gate name="A" symbol="NCP3063BDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMPARATOR_INVERTING_INPUT" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IPK_SENSE" pad="7"/>
<connect gate="A" pin="N.C." pad="8"/>
<connect gate="A" pin="SWITCH_COLLECTOR" pad="1"/>
<connect gate="A" pin="SWITCH_EMITTER" pad="2"/>
<connect gate="A" pin="TIMING_CAPACITOR" pad="3"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP3063BDR2G"/>
<attribute name="OC_FARNELL" value="1547126"/>
<attribute name="OC_NEWARK" value="04R7841"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP3065DR2G" prefix="U">
<description>Switching Regulator for LEDs</description>
<gates>
<gate name="A" symbol="NCP3065DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMPTR_NEG" pad="5"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IPK_SENSE" pad="7"/>
<connect gate="A" pin="N.C." pad="8"/>
<connect gate="A" pin="SW_C" pad="1"/>
<connect gate="A" pin="SW_E" pad="2"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP3065DR2G"/>
<attribute name="OC_FARNELL" value="1652395"/>
<attribute name="OC_NEWARK" value="57M9798"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP3065PG" prefix="U">
<description>Regulator for LEDs</description>
<gates>
<gate name="A" symbol="NCP3065PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="COMP_NEG" pad="5"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ISEN" pad="7"/>
<connect gate="A" pin="N.C" pad="8"/>
<connect gate="A" pin="SW_C" pad="1"/>
<connect gate="A" pin="SW_E" pad="2"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP3065PG"/>
<attribute name="OC_FARNELL" value="1652396"/>
<attribute name="OC_NEWARK" value="57M9800"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP3163BMNR2G" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="NCP3163BMNR2G"/>
</gates>
<devices>
<device name="" package="DFN600X500X100-19N">
<connects>
<connect gate="A" pin="BOOTSTRAP_INPUT" pad="14"/>
<connect gate="A" pin="DRIVER_COLLECTOR" pad="5"/>
<connect gate="A" pin="EPAD" pad="19"/>
<connect gate="A" pin="GND" pad="18"/>
<connect gate="A" pin="IPK_SENSE" pad="4"/>
<connect gate="A" pin="LVI_OUTPUT" pad="15"/>
<connect gate="A" pin="N/C" pad="2"/>
<connect gate="A" pin="SWITCH_COLLECTOR" pad="6"/>
<connect gate="A" pin="SWITCH_COLLECTOR_2" pad="7"/>
<connect gate="A" pin="SWITCH_COLLECTOR_3" pad="8"/>
<connect gate="A" pin="SWITCH_COLLECTOR_4" pad="9"/>
<connect gate="A" pin="SWITCH_EMITTER" pad="10"/>
<connect gate="A" pin="SWITCH_EMITTER_2" pad="11"/>
<connect gate="A" pin="SWITCH_EMITTER_3" pad="12"/>
<connect gate="A" pin="SWITCH_EMITTER_4" pad="13"/>
<connect gate="A" pin="TC" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK1" pad="17"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK_2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP3163BMNR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="27M2541"/>
<attribute name="PACKAGE" value="DFN-18"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP361SNT1G" prefix="U">
<description>USB Positive Overvoltage Protection Controller</description>
<gates>
<gate name="A" symbol="NCP361SNT1G"/>
</gates>
<devices>
<device name="" package="SOP95P275X110-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="~EN" pad="3"/>
<connect gate="A" pin="~FLAG" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP361SNT1G"/>
<attribute name="OC_FARNELL" value="1642242"/>
<attribute name="OC_NEWARK" value="01P0135"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4587DMX12TCG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4587DMX12TCG"/>
</gates>
<devices>
<device name="" package="DFN120X120X40-6N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4587DMX12TCG"/>
<attribute name="OC_FARNELL" value="1885122"/>
<attribute name="OC_NEWARK" value="41T0727"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4587DMX18TCG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4587DMX18TCG"/>
</gates>
<devices>
<device name="" package="DFN120X120X40-6N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4587DMX18TCG"/>
<attribute name="OC_FARNELL" value="1885123"/>
<attribute name="OC_NEWARK" value="41T0728"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4587DMX28TCG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4587DMX28TCG"/>
</gates>
<devices>
<device name="" package="DFN120X120X40-6N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4587DMX28TCG"/>
<attribute name="OC_FARNELL" value="1885124"/>
<attribute name="OC_NEWARK" value="41T0729"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4587DMX30TCG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4587DMX30TCG"/>
</gates>
<devices>
<device name="" package="DFN120X120X40-6N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4587DMX30TCG"/>
<attribute name="OC_FARNELL" value="1885125"/>
<attribute name="OC_NEWARK" value="41T0730"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4587DMX33TCG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4587DMX33TCG"/>
</gates>
<devices>
<device name="" package="DFN120X120X40-6N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4587DMX33TCG"/>
<attribute name="OC_FARNELL" value="1885126"/>
<attribute name="OC_NEWARK" value="41T0731"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4588DSQ10T1G" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4588DSQ10T1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4588DSQ10T1G"/>
<attribute name="OC_FARNELL" value="1885130"/>
<attribute name="OC_NEWARK" value="41T0735"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4588DSQ15T1G" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4588DSQ15T1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4588DSQ15T1G"/>
<attribute name="OC_FARNELL" value="1885131"/>
<attribute name="OC_NEWARK" value="41T0736"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4588DSQ25T1G" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4588DSQ25T1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4588DSQ25T1G"/>
<attribute name="OC_FARNELL" value="1885132"/>
<attribute name="OC_NEWARK" value="41T0737"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4589DMX12TCG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4589DMX12TCG"/>
</gates>
<devices>
<device name="" package="DFN120X120X40-6N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4589DMX12TCG"/>
<attribute name="OC_FARNELL" value="1885134"/>
<attribute name="OC_NEWARK" value="41T0738"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4589DMX18TCG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4589DMX18TCG"/>
</gates>
<devices>
<device name="" package="DFN120X120X40-6N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4589DMX18TCG"/>
<attribute name="OC_FARNELL" value="1885135"/>
<attribute name="OC_NEWARK" value="41T0739"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4589DMX28TCG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4589DMX28TCG"/>
</gates>
<devices>
<device name="" package="DFN120X120X40-6N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4589DMX28TCG"/>
<attribute name="OC_FARNELL" value="1885136"/>
<attribute name="OC_NEWARK" value="41T0740"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4589DMX30TCG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4589DMX30TCG"/>
</gates>
<devices>
<device name="" package="DFN120X120X40-6N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4589DMX30TCG"/>
<attribute name="OC_FARNELL" value="1885137"/>
<attribute name="OC_NEWARK" value="41T0741"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4589DMX33TCG" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4589DMX33TCG"/>
</gates>
<devices>
<device name="" package="DFN120X120X40-6N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4589DMX33TCG"/>
<attribute name="OC_FARNELL" value="1885138"/>
<attribute name="OC_NEWARK" value="41T0742"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4589DSQ12T1G" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4589DSQ12T1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="5"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4589DSQ12T1G"/>
<attribute name="OC_FARNELL" value="1885139"/>
<attribute name="OC_NEWARK" value="24T3414"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4589DSQ18T1G" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4589DSQ18T1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="5"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4589DSQ18T1G"/>
<attribute name="OC_FARNELL" value="1885140"/>
<attribute name="OC_NEWARK" value="41T0744"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4589DSQ25T1G" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4589DSQ25T1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="5"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4589DSQ25T1G"/>
<attribute name="OC_FARNELL" value="1885141"/>
<attribute name="OC_NEWARK" value="24T3416"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4589DSQ30T1G" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4589DSQ30T1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="5"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4589DSQ30T1G"/>
<attribute name="OC_FARNELL" value="1885142"/>
<attribute name="OC_NEWARK" value="24T3417"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP4589DSQ33T1G" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="NCP4589DSQ33T1G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="AE" pad="1"/>
<connect gate="A" pin="CE" pad="5"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP4589DSQ33T1G"/>
<attribute name="OC_FARNELL" value="1885143"/>
<attribute name="OC_NEWARK" value="24T3418"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP565MNADJT2G" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="NCP565MNADJT2G"/>
</gates>
<devices>
<device name="" package="DFN300X330X90-6N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP565MNADJT2G"/>
<attribute name="OC_FARNELL" value="1369744"/>
<attribute name="OC_NEWARK" value="53M9459"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP5810DMUTXG" prefix="U">
<description>Dual 1 W Output AMOLED Driver Supply</description>
<gates>
<gate name="A" symbol="NCP5810DMUTXG"/>
</gates>
<devices>
<device name="" package="DFN300X300X55-13N">
<connects>
<connect gate="A" pin="AGND" pad="4"/>
<connect gate="A" pin="AVIN" pad="8"/>
<connect gate="A" pin="EN" pad="9"/>
<connect gate="A" pin="EPAD" pad="13"/>
<connect gate="A" pin="FBN" pad="7"/>
<connect gate="A" pin="LXP" pad="12"/>
<connect gate="A" pin="PGND" pad="3"/>
<connect gate="A" pin="PVIN" pad="11"/>
<connect gate="A" pin="SWN" pad="10"/>
<connect gate="A" pin="SWP" pad="2"/>
<connect gate="A" pin="VOUTP" pad="1"/>
<connect gate="A" pin="VREF" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP5810DMUTXG"/>
<attribute name="OC_FARNELL" value="1578235"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DFN-12"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP699SN18T1G" prefix="U">
<description>CMOS Low Iq LDO</description>
<gates>
<gate name="A" symbol="NCP699SN18T1G"/>
</gates>
<devices>
<device name="" package="SOP95P275X110-5N">
<connects>
<connect gate="A" pin="ENABLE" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="N/C" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP699SN18T1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7848"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP699SN33T1G" prefix="U">
<description>150 mA CMOS Low Iq LDO with Enable</description>
<gates>
<gate name="A" symbol="NCP699SN33T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="N/C" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP699SN33T1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7849"/>
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP803SN263T1G" prefix="U">
<description>3-Pin Microprocessor</description>
<gates>
<gate name="A" symbol="NCP803SN263T1G"/>
</gates>
<devices>
<device name="" package="SOT95P240X111-3N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="~RESET" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCP803SN263T1G"/>
<attribute name="OC_FARNELL" value="1652406"/>
<attribute name="OC_NEWARK" value="42K2012"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCS2001SN1T1G" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="NCS2001SN1T1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCS2001SN1T1G"/>
<attribute name="OC_FARNELL" value="1364638"/>
<attribute name="OC_NEWARK" value="45J1978"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCV1124DG" prefix="U">
<description>Dual Variable-Reluctance Sensor Interface</description>
<gates>
<gate name="A" symbol="NCV1124DG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DIAG" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN1" pad="2"/>
<connect gate="A" pin="IN2" pad="3"/>
<connect gate="A" pin="INADJ" pad="1"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCV1124DG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="02M9852"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCV85082BPD33R2G" prefix="U">
<description>5.0 V and 3.3 V, 250 mA  LDO with Watchdog and ~RESET</description>
<gates>
<gate name="A" symbol="NCV85082BPD33R2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-9N">
<connects>
<connect gate="A" pin="DELAY" pad="1"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SENSE" pad="3"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="WAKEUP" pad="7"/>
<connect gate="A" pin="WDI" pad="6"/>
<connect gate="A" pin="~RESET" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCV85082BPD33R2G"/>
<attribute name="OC_FARNELL" value="1885144"/>
<attribute name="OC_NEWARK" value="41T0751"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCV8537MN180R2G" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="NCV8537MN180R2G"/>
</gates>
<devices>
<device name="" package="DFN300X300X100-10N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="10"/>
<connect gate="A" pin="IN_2" pad="9"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NR" pad="7"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="PWRG" pad="5"/>
<connect gate="A" pin="SENSE" pad="3"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCV8537MN180R2G"/>
<attribute name="OC_FARNELL" value="1885146"/>
<attribute name="OC_NEWARK" value="41T0753"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="On-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCV8537MN250R2G" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="NCV8537MN250R2G"/>
</gates>
<devices>
<device name="" package="DFN300X300X100-10N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="10"/>
<connect gate="A" pin="IN_2" pad="9"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NR" pad="7"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="PWRG" pad="5"/>
<connect gate="A" pin="SENSE" pad="3"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCV8537MN250R2G"/>
<attribute name="OC_FARNELL" value="1885147"/>
<attribute name="OC_NEWARK" value="41T0754"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="On-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCV8537MN330R2G" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="NCV8537MN330R2G"/>
</gates>
<devices>
<device name="" package="DFN300X300X100-10N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="10"/>
<connect gate="A" pin="IN_2" pad="9"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NR" pad="7"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="PWRG" pad="5"/>
<connect gate="A" pin="SENSE" pad="3"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCV8537MN330R2G"/>
<attribute name="OC_FARNELL" value="1885148"/>
<attribute name="OC_NEWARK" value="41T0755"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="On-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCV8537MN500R2G" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="NCV8537MN500R2G"/>
</gates>
<devices>
<device name="" package="DFN300X300X100-10N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="10"/>
<connect gate="A" pin="IN_2" pad="9"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NR" pad="7"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="PWRG" pad="5"/>
<connect gate="A" pin="SENSE" pad="3"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCV8537MN500R2G"/>
<attribute name="OC_FARNELL" value="1885149"/>
<attribute name="OC_NEWARK" value="41T0756"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="On-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCV8537MNADJR2G" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="NCV8537MNADJR2G"/>
</gates>
<devices>
<device name="" package="DFN300X300X100-10N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="10"/>
<connect gate="A" pin="IN_2" pad="9"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NR" pad="7"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="PWRG" pad="5"/>
<connect gate="A" pin="SENSE" pad="3"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NCV8537MNADJR2G"/>
<attribute name="OC_FARNELL" value="1885150"/>
<attribute name="OC_NEWARK" value="41T0752"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="On-Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE5532AD8G" prefix="U">
<description>Internally Compensated Dual Low Noise Operational Amplifier</description>
<gates>
<gate name="A" symbol="NE5532AD8G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NE5532AD8G"/>
<attribute name="OC_FARNELL" value="1426379"/>
<attribute name="OC_NEWARK" value="42K2208"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE5532ANG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="NE5532ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NE5532ANG"/>
<attribute name="OC_FARNELL" value="1426380"/>
<attribute name="OC_NEWARK" value="26K5043"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE5532DG" prefix="U">
<description>Internally Compensated Dual Low Noise Operational Amplifier</description>
<gates>
<gate name="A" symbol="NE5532DG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="+INA" pad="2"/>
<connect gate="A" pin="+INB" pad="7"/>
<connect gate="A" pin="-INA" pad="1"/>
<connect gate="A" pin="-INB" pad="8"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="NC_2" pad="16"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="10"/>
<connect gate="A" pin="NC_5" pad="14"/>
<connect gate="A" pin="NC_6" pad="15"/>
<connect gate="A" pin="NC_7" pad="5"/>
<connect gate="A" pin="NC_8" pad="6"/>
<connect gate="A" pin="OUTA" pad="13"/>
<connect gate="A" pin="OUTB" pad="11"/>
<connect gate="A" pin="V+" pad="12"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NE5532DG"/>
<attribute name="OC_FARNELL" value="1705907"/>
<attribute name="OC_NEWARK" value="42K2210"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE5532NG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="NE5532NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NE5532NG"/>
<attribute name="OC_FARNELL" value="1705909"/>
<attribute name="OC_NEWARK" value="42K2213"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE5534ANG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="NE5534ANG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OFS" pad="1"/>
<connect gate="A" pin="OFS/COMP" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NE5534ANG"/>
<attribute name="OC_FARNELL" value="1426386"/>
<attribute name="OC_NEWARK" value="42K2216"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE5534NG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="NE5534NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OFS" pad="1"/>
<connect gate="A" pin="OFS/COMP" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NE5534NG"/>
<attribute name="OC_FARNELL" value="1426388"/>
<attribute name="OC_NEWARK" value="42K2219"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE592D14G" prefix="U">
<description>Video Amplifier</description>
<gates>
<gate name="A" symbol="NE592D14G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="G1A_GAIN_SELECT" pad="11"/>
<connect gate="A" pin="G1B_GAIN_SELECT" pad="4"/>
<connect gate="A" pin="G2A_GAIN_SELECT" pad="12"/>
<connect gate="A" pin="G2B_GAIN_SELECT" pad="3"/>
<connect gate="A" pin="IN_1" pad="14"/>
<connect gate="A" pin="IN_2" pad="1"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="NC_3" pad="6"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="OUT_1" pad="8"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NE592D14G"/>
<attribute name="OC_FARNELL" value="1468773"/>
<attribute name="OC_NEWARK" value="42K2222"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE592D8G" prefix="U">
<description>Video Amplifier</description>
<gates>
<gate name="A" symbol="NE592D8G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="G1A_GAIN_SELECT" pad="7"/>
<connect gate="A" pin="G1B_GAIN_SELECT" pad="2"/>
<connect gate="A" pin="IN_1" pad="8"/>
<connect gate="A" pin="IN_2" pad="1"/>
<connect gate="A" pin="OUT_1" pad="5"/>
<connect gate="A" pin="OUT_2" pad="4"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NE592D8G"/>
<attribute name="OC_FARNELL" value="1426401"/>
<attribute name="OC_NEWARK" value="42K2224"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL17SZ07DFT2G" prefix="U">
<description>Single Non-Inverting Buffer with Open Drain Output</description>
<gates>
<gate name="A" symbol="NL17SZ07DFT2G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL17SZ07DFT2G"/>
<attribute name="OC_FARNELL" value="1705431"/>
<attribute name="OC_NEWARK" value="04R7799"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL17SZ125DFT2G" prefix="U">
<description>Non-Inverting 3-State Buffer</description>
<gates>
<gate name="A" symbol="NL17SZ125DFT2G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="OUT_Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~OE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL17SZ125DFT2G"/>
<attribute name="OC_FARNELL" value="1468775"/>
<attribute name="OC_NEWARK" value="83H7736"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL17SZ14DFT2G" prefix="U">
<description>Single Inverter with Schmitt Trigger</description>
<gates>
<gate name="A" symbol="NL17SZ14DFT2G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT_~Y" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL17SZ14DFT2G"/>
<attribute name="OC_FARNELL" value="1468776"/>
<attribute name="OC_NEWARK" value="88H5066"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL17SZ17DFT2G" prefix="U">
<description>Single Non-Inverting Buffer with Schmitt Trigger</description>
<gates>
<gate name="A" symbol="NL17SZ17DFT2G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL17SZ17DFT2G"/>
<attribute name="OC_FARNELL" value="1311236"/>
<attribute name="OC_NEWARK" value="45J2062"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL17SZ74USG" prefix="U">
<description>Single D Flip Flop</description>
<gates>
<gate name="A" symbol="NL17SZ74USG"/>
</gates>
<devices>
<device name="" package="SOP50P310X90-8N">
<connects>
<connect gate="A" pin="CP" pad="1"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="Q" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~CLR" pad="6"/>
<connect gate="A" pin="~PR" pad="7"/>
<connect gate="A" pin="~Q" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL17SZ74USG"/>
<attribute name="OC_FARNELL" value="1468778"/>
<attribute name="OC_NEWARK" value="83H7737"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL17SZU04DFT2G" prefix="U">
<description>Single Unbuffered Inverter</description>
<gates>
<gate name="A" symbol="NL17SZU04DFT2G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="Y" pad="4"/>
<connect gate="A" pin="~A" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL17SZU04DFT2G"/>
<attribute name="OC_FARNELL" value="1155818"/>
<attribute name="OC_NEWARK" value="98H0938"/>
<attribute name="PACKAGE" value="SOT-353-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL27WZ04DTT1G" prefix="U">
<description>Dual Inverter</description>
<gates>
<gate name="A" symbol="NL27WZ04DTT1G"/>
</gates>
<devices>
<device name="" package="SOP95P275X110-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN_A1" pad="1"/>
<connect gate="A" pin="IN_A2" pad="3"/>
<connect gate="A" pin="OUT_~Y1" pad="6"/>
<connect gate="A" pin="OUT_~Y2" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL27WZ04DTT1G"/>
<attribute name="OC_FARNELL" value="1607797"/>
<attribute name="OC_NEWARK" value="26K5079"/>
<attribute name="PACKAGE" value="TSOP-6"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL27WZ08USG" prefix="U">
<description>Dual 2-Input AND Gate</description>
<gates>
<gate name="A" symbol="NL27WZ08USG"/>
</gates>
<devices>
<device name="" package="SOP50P310X90-8N">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="Y1" pad="7"/>
<connect gate="A" pin="Y2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL27WZ08USG"/>
<attribute name="OC_FARNELL" value="1652022"/>
<attribute name="OC_NEWARK" value="83H7741"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL27WZ126USG" prefix="U">
<description>Dual Buffer with 3-State Outputs</description>
<gates>
<gate name="A" symbol="NL27WZ126USG"/>
</gates>
<devices>
<device name="" package="SOP50P310X90-8N">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OE1" pad="1"/>
<connect gate="A" pin="OE2" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="Y1" pad="6"/>
<connect gate="A" pin="Y2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL27WZ126USG"/>
<attribute name="OC_FARNELL" value="1651993"/>
<attribute name="OC_NEWARK" value="83H7743"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL27WZ14DTT1G" prefix="U">
<description>Dual Schmitt-Trigger Inverter</description>
<gates>
<gate name="A" symbol="NL27WZ14DTT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN_A1" pad="1"/>
<connect gate="A" pin="IN_A2" pad="3"/>
<connect gate="A" pin="OUT_~Y1" pad="6"/>
<connect gate="A" pin="OUT_~Y2" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL27WZ14DTT1G"/>
<attribute name="OC_FARNELL" value="1468780"/>
<attribute name="OC_NEWARK" value="71J6968"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL27WZ16DFT2G" prefix="U">
<description>Dual Buffer</description>
<gates>
<gate name="A" symbol="NL27WZ16DFT2G"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN_A1" pad="1"/>
<connect gate="A" pin="IN_A2" pad="3"/>
<connect gate="A" pin="OUT_Y1" pad="6"/>
<connect gate="A" pin="OUT_Y2" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL27WZ16DFT2G"/>
<attribute name="OC_FARNELL" value="1147928"/>
<attribute name="OC_NEWARK" value="88H5068"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL37WZ14USG" prefix="U">
<description>Triple Schmitt-Trigger Inverter</description>
<gates>
<gate name="A" symbol="NL37WZ14USG"/>
</gates>
<devices>
<device name="" package="SOP50P310X90-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN_A1" pad="1"/>
<connect gate="A" pin="IN_A2" pad="3"/>
<connect gate="A" pin="IN_A3" pad="6"/>
<connect gate="A" pin="OUT_~Y1" pad="7"/>
<connect gate="A" pin="OUT_~Y2" pad="5"/>
<connect gate="A" pin="OUT_~Y3" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL37WZ14USG"/>
<attribute name="OC_FARNELL" value="1365143"/>
<attribute name="OC_NEWARK" value="83H7749"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL37WZ17USG" prefix="U">
<description>Triple Noninverting  Schmitt-Trigger Buffer</description>
<gates>
<gate name="A" symbol="NL37WZ17USG"/>
</gates>
<devices>
<device name="" package="SOP50P310X90-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN_A1" pad="1"/>
<connect gate="A" pin="IN_A2" pad="3"/>
<connect gate="A" pin="IN_A3" pad="6"/>
<connect gate="A" pin="OUT__Y1" pad="7"/>
<connect gate="A" pin="OUT__Y2" pad="5"/>
<connect gate="A" pin="OUT__Y3" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NL37WZ17USG"/>
<attribute name="OC_FARNELL" value="1607624"/>
<attribute name="OC_NEWARK" value="83H7751"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NLAS4599DTT1G" prefix="U">
<description>Low Voltage Single Supply SPDT Analog Switch</description>
<gates>
<gate name="A" symbol="NLAS4599DTT1G"/>
</gates>
<devices>
<device name="" package="SOP95P275X110-6N">
<connects>
<connect gate="A" pin="COM" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NO" pad="6"/>
<connect gate="A" pin="SELECT" pad="1"/>
<connect gate="A" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NLAS4599DTT1G"/>
<attribute name="OC_FARNELL" value="1468781"/>
<attribute name="OC_NEWARK" value="71J6944"/>
<attribute name="PACKAGE" value="TSOP-6"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NLAST4599DTT1G" prefix="U">
<description>Low Voltage Single Supply SPDT Analog Switch</description>
<gates>
<gate name="A" symbol="NLAST4599DTT1G"/>
</gates>
<devices>
<device name="" package="SOP95P275X110-6N">
<connects>
<connect gate="A" pin="COM" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NO" pad="6"/>
<connect gate="A" pin="SELECT" pad="1"/>
<connect gate="A" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NLAST4599DTT1G"/>
<attribute name="OC_FARNELL" value="1311162"/>
<attribute name="OC_NEWARK" value="26K5050"/>
<attribute name="PACKAGE" value="TSOP-6"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUD3105DMT1G" prefix="U">
<description>Inductive Load Driver</description>
<gates>
<gate name="A" symbol="NUD3105DMT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-6N">
<connects>
<connect gate="A" pin="DRAIN1" pad="6"/>
<connect gate="A" pin="DRAIN2" pad="3"/>
<connect gate="A" pin="GATE1" pad="2"/>
<connect gate="A" pin="GATE2" pad="5"/>
<connect gate="A" pin="SOURCE1" pad="1"/>
<connect gate="A" pin="SOURCE2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NUD3105DMT1G"/>
<attribute name="OC_FARNELL" value="1880145"/>
<attribute name="OC_NEWARK" value="42K2469"/>
<attribute name="PACKAGE" value="SC-74-6"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUD3105LT1G" prefix="U">
<description>Integrated Relay,  Inductive Load Driver</description>
<gates>
<gate name="A" symbol="NUD3105LT1G"/>
</gates>
<devices>
<device name="" package="SOT95P240X110-3N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NUD3105LT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7853"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUD3112DMT1G" prefix="U">
<description>Inductive Load Driver</description>
<gates>
<gate name="A" symbol="NUD3112DMT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-6N">
<connects>
<connect gate="A" pin="DRAIN1" pad="6"/>
<connect gate="A" pin="DRAIN2" pad="3"/>
<connect gate="A" pin="GATE1" pad="2"/>
<connect gate="A" pin="GATE2" pad="5"/>
<connect gate="A" pin="SOURCE1" pad="1"/>
<connect gate="A" pin="SOURCE2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NUD3112DMT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7854"/>
<attribute name="PACKAGE" value="SC-74-6"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUD3112LT1G" prefix="U">
<description>Integrated Relay,  Inductive Load Driver</description>
<gates>
<gate name="A" symbol="NUD3112LT1G"/>
</gates>
<devices>
<device name="" package="SOT95P240X110-3N">
<connects>
<connect gate="A" pin="DRAIN" pad="3"/>
<connect gate="A" pin="GATE" pad="1"/>
<connect gate="A" pin="SOURCE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NUD3112LT1G"/>
<attribute name="OC_FARNELL" value="1705476"/>
<attribute name="OC_NEWARK" value="04R7855"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="OM SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUD3124LT1G" prefix="U">
<description>Driver</description>
<gates>
<gate name="A" symbol="NUD3124LT1G"/>
</gates>
<devices>
<device name="" package="SOT95P240X111-3N">
<connects>
<connect gate="A" pin="DRAIN" pad="3"/>
<connect gate="A" pin="GATE" pad="1"/>
<connect gate="A" pin="SOURCE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NUD3124LT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7856"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUD3160DMT1G" prefix="U">
<description>Inductive Load Driver</description>
<gates>
<gate name="A" symbol="NUD3160DMT1G"/>
</gates>
<devices>
<device name="" package="SOT95P275X110-6N">
<connects>
<connect gate="A" pin="DRAIN1" pad="6"/>
<connect gate="A" pin="DRAIN2" pad="3"/>
<connect gate="A" pin="GATE1" pad="2"/>
<connect gate="A" pin="GATE2" pad="5"/>
<connect gate="A" pin="SOURCE1" pad="1"/>
<connect gate="A" pin="SOURCE2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NUD3160DMT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7857"/>
<attribute name="PACKAGE" value="SC-74-6"/>
<attribute name="SUPPLIER" value="ON Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUD3160LT1G" prefix="U">
<description>Load Driver</description>
<gates>
<gate name="A" symbol="NUD3160LT1G"/>
</gates>
<devices>
<device name="" package="SOT95P240X111-3N">
<connects>
<connect gate="A" pin="DRAIN" pad="3"/>
<connect gate="A" pin="GATE" pad="1"/>
<connect gate="A" pin="SOURCE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NUD3160LT1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R7858"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUD4001DR2G" prefix="U">
<description>High Current LED Driver</description>
<gates>
<gate name="A" symbol="NUD4001DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BOOST" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IOUT" pad="5"/>
<connect gate="A" pin="IOUT_2" pad="6"/>
<connect gate="A" pin="IOUT_3" pad="7"/>
<connect gate="A" pin="IOUT_4" pad="8"/>
<connect gate="A" pin="REXT" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NUD4001DR2G"/>
<attribute name="OC_FARNELL" value="1547147"/>
<attribute name="OC_NEWARK" value="70K4034"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUD4011DR2G" prefix="U">
<description>Low Current LED Driver</description>
<gates>
<gate name="A" symbol="NUD4011DR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BOOST" pad="2"/>
<connect gate="A" pin="IOUT" pad="5"/>
<connect gate="A" pin="IOUT_2" pad="6"/>
<connect gate="A" pin="IOUT_3" pad="7"/>
<connect gate="A" pin="IOUT_4" pad="8"/>
<connect gate="A" pin="PWM" pad="4"/>
<connect gate="A" pin="REXT" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NUD4011DR2G"/>
<attribute name="OC_FARNELL" value="1547149"/>
<attribute name="OC_NEWARK" value="04R7859"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Onsemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P2782AF-08SR" prefix="U">
<description>General Purpose EMI Reduction IC</description>
<gates>
<gate name="A" symbol="P2782AF-08SR"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FS0" pad="7"/>
<connect gate="A" pin="FS1" pad="3"/>
<connect gate="A" pin="LF" pad="4"/>
<connect gate="A" pin="MODOUT" pad="6"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VSS" pad="5"/>
<connect gate="A" pin="XIN/CLKIN" pad="1"/>
<connect gate="A" pin="XOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="P2782AF-08SR"/>
<attribute name="OC_FARNELL" value="1903669"/>
<attribute name="OC_NEWARK" value="55T3865"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="On semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P2784AF-08SR" prefix="U">
<description>General Purpose EMI Reduction IC</description>
<gates>
<gate name="A" symbol="P2784AF-08SR"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FS0" pad="7"/>
<connect gate="A" pin="FS1" pad="3"/>
<connect gate="A" pin="LF" pad="4"/>
<connect gate="A" pin="MODOUT" pad="6"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VSS" pad="5"/>
<connect gate="A" pin="XIN/CLKIN" pad="1"/>
<connect gate="A" pin="XOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="P2784AF-08SR"/>
<attribute name="OC_FARNELL" value="1903670"/>
<attribute name="OC_NEWARK" value="55T3866"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="On semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCS3P25811AG08SR" prefix="U">
<description>Spread Spectrum Clock Generator</description>
<gates>
<gate name="A" symbol="PCS3P25811AG08SR"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FSEL" pad="6"/>
<connect gate="A" pin="MODOUT" pad="5"/>
<connect gate="A" pin="S0" pad="4"/>
<connect gate="A" pin="S1" pad="3"/>
<connect gate="A" pin="VDD" pad="7"/>
<connect gate="A" pin="VSS" pad="2"/>
<connect gate="A" pin="XIN_/_CLKIN" pad="1"/>
<connect gate="A" pin="XOUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="PCS3P25811AG08SR"/>
<attribute name="OC_FARNELL" value="1903671"/>
<attribute name="OC_NEWARK" value="55T3616"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA571DG" prefix="U">
<description>Compandor</description>
<gates>
<gate name="A" symbol="SA571DG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="G_CELL_IN_1" pad="3"/>
<connect gate="A" pin="G_CELL_IN_2" pad="14"/>
<connect gate="A" pin="INV._IN_1" pad="5"/>
<connect gate="A" pin="INV._IN_2" pad="12"/>
<connect gate="A" pin="OUT_1" pad="7"/>
<connect gate="A" pin="OUT_2" pad="10"/>
<connect gate="A" pin="RECT_CAP_1" pad="1"/>
<connect gate="A" pin="RECT_CAP_2" pad="16"/>
<connect gate="A" pin="RECT_IN_1" pad="2"/>
<connect gate="A" pin="RECT_IN_2" pad="15"/>
<connect gate="A" pin="RES._R3_1" pad="6"/>
<connect gate="A" pin="RES._R3_2" pad="11"/>
<connect gate="A" pin="THD_TRIM_1" pad="8"/>
<connect gate="A" pin="THD_TRIM_2" pad="9"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SA571DG"/>
<attribute name="OC_FARNELL" value="1426393"/>
<attribute name="OC_NEWARK" value="42K2600"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA571NG" prefix="U">
<description>Compandor</description>
<gates>
<gate name="A" symbol="SA571NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="G_CELL_IN_1" pad="3"/>
<connect gate="A" pin="G_CELL_IN_2" pad="14"/>
<connect gate="A" pin="INV._IN_1" pad="5"/>
<connect gate="A" pin="INV._IN_2" pad="12"/>
<connect gate="A" pin="OUTPUT_1" pad="7"/>
<connect gate="A" pin="OUTPUT_2" pad="10"/>
<connect gate="A" pin="RECT_CAP_1" pad="1"/>
<connect gate="A" pin="RECT_CAP_2" pad="16"/>
<connect gate="A" pin="RECT_IN_1" pad="2"/>
<connect gate="A" pin="RECT_IN_2" pad="15"/>
<connect gate="A" pin="RES._R3_1" pad="6"/>
<connect gate="A" pin="RES._R3_2" pad="11"/>
<connect gate="A" pin="THD_TRIM_1" pad="8"/>
<connect gate="A" pin="THD_TRIM_2" pad="9"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SA571NG"/>
<attribute name="OC_FARNELL" value="1364647"/>
<attribute name="OC_NEWARK" value="45J2245"/>
<attribute name="PACKAGE" value="DIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA572NG" prefix="U">
<description>Analog Comparator</description>
<gates>
<gate name="A" symbol="SA572NG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="ATTACK_CAP_A" pad="4"/>
<connect gate="A" pin="ATTACK_CAP_B" pad="12"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="G_INB" pad="9"/>
<connect gate="A" pin="G_IN_A" pad="7"/>
<connect gate="A" pin="G_OUT_A" pad="5"/>
<connect gate="A" pin="G_OUT_B" pad="11"/>
<connect gate="A" pin="RECOV._CAP_A" pad="2"/>
<connect gate="A" pin="RECOV._CAP_B" pad="14"/>
<connect gate="A" pin="RECT._IN_A" pad="3"/>
<connect gate="A" pin="RECT._IN_B" pad="13"/>
<connect gate="A" pin="THD_TRIM_A" pad="6"/>
<connect gate="A" pin="THD_TRIM_B" pad="10"/>
<connect gate="A" pin="TRACK_TRIM_A" pad="1"/>
<connect gate="A" pin="TRACK_TRIM_B" pad="15"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SA572NG"/>
<attribute name="OC_FARNELL" value="1426397"/>
<attribute name="OC_NEWARK" value="42K2602"/>
<attribute name="PACKAGE" value="DIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA575DTBG" prefix="U">
<description>Low Voltage Compandor</description>
<gates>
<gate name="A" symbol="SA575DTBG"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-20N">
<connects>
<connect gate="A" pin="+VIN1" pad="1"/>
<connect gate="A" pin="+VIN2" pad="19"/>
<connect gate="A" pin="-VIN1" pad="2"/>
<connect gate="A" pin="-VIN2" pad="18"/>
<connect gate="A" pin="COMP.IN2" pad="13"/>
<connect gate="A" pin="COMP._IN1" pad="7"/>
<connect gate="A" pin="CRECT1" pad="5"/>
<connect gate="A" pin="CRECT2" pad="15"/>
<connect gate="A" pin="GAIN_CELL_IN1" pad="9"/>
<connect gate="A" pin="GAIN_CELL_IN2" pad="11"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="RECT.IN2" pad="16"/>
<connect gate="A" pin="RECT._IN1" pad="4"/>
<connect gate="A" pin="SUM_NODE_2" pad="12"/>
<connect gate="A" pin="SUM_OUT2" pad="14"/>
<connect gate="A" pin="SUM_OUT_1" pad="6"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VOUT1" pad="3"/>
<connect gate="A" pin="VOUT2" pad="17"/>
<connect gate="A" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SA575DTBG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="70K4377"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCA0372DP1G" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="TCA0372DP1G"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="IN_A" pad="7"/>
<connect gate="A" pin="IN_A_2" pad="8"/>
<connect gate="A" pin="IN_B" pad="5"/>
<connect gate="A" pin="IN_B_2" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="3"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="VEE/GND" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TCA0372DP1G"/>
<attribute name="OC_FARNELL" value="1651877"/>
<attribute name="OC_NEWARK" value="88H5148"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCA0372DWG" prefix="U">
<description>1.0 A Output Current Dual Power OperationalAmplifiers</description>
<gates>
<gate name="A" symbol="TCA0372DWG"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="INPUTS_A" pad="9"/>
<connect gate="A" pin="INPUTS_A_2" pad="10"/>
<connect gate="A" pin="INPUTS_B" pad="7"/>
<connect gate="A" pin="INPUTS_B_2" pad="8"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="14"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="6"/>
<connect gate="A" pin="NC_5" pad="15"/>
<connect gate="A" pin="OUTPUT_A" pad="16"/>
<connect gate="A" pin="OUTPUT_B" pad="2"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VEE/GND" pad="13"/>
<connect gate="A" pin="VEE/GND_2" pad="12"/>
<connect gate="A" pin="VEE/GND_3" pad="4"/>
<connect gate="A" pin="VEE/GND_4" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TCA0372DWG"/>
<attribute name="OC_FARNELL" value="1468783"/>
<attribute name="OC_NEWARK" value="26K5198"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCA0372DWR2G" prefix="U">
<description>Analog Multiplexers/ Demultiplexers</description>
<gates>
<gate name="A" symbol="TCA0372DWR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="INPUTS_A" pad="10"/>
<connect gate="A" pin="INPUTS_A_2" pad="9"/>
<connect gate="A" pin="INPUTS_B" pad="7"/>
<connect gate="A" pin="INPUTS_B_2" pad="8"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="14"/>
<connect gate="A" pin="NC_5" pad="15"/>
<connect gate="A" pin="OUTPUT_A" pad="16"/>
<connect gate="A" pin="OUTPUT_B" pad="2"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VEE/GND" pad="4"/>
<connect gate="A" pin="VEE/GND_2" pad="12"/>
<connect gate="A" pin="VEE/GND_3" pad="13"/>
<connect gate="A" pin="VEE/GND_4" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TCA0372DWR2G"/>
<attribute name="OC_FARNELL" value="1277937"/>
<attribute name="OC_NEWARK" value="26K5199"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="On Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1085CG" prefix="U">
<description>Universal Motor Speed Controller</description>
<gates>
<gate name="A" symbol="TDA1085CG"/>
</gates>
<devices>
<device name="" package="DIP254P762X444-16">
<connects>
<connect gate="A" pin="+VCC" pad="9"/>
<connect gate="A" pin="ACTUAL_SPEED" pad="4"/>
<connect gate="A" pin="CLOSED_LOOP_STABILITY" pad="16"/>
<connect gate="A" pin="CURRENT_SYNCHRONIZATION" pad="1"/>
<connect gate="A" pin="DIGITAL_SPEED_SENSE" pad="12"/>
<connect gate="A" pin="F/VC_PUMP_CAPACITOR" pad="11"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="MOTOR_CURRENT_LIMIT" pad="3"/>
<connect gate="A" pin="RAMP_CURRENT_GEN._CONTROL" pad="6"/>
<connect gate="A" pin="RAMP_GEN._TIMING" pad="7"/>
<connect gate="A" pin="SAWTOOTH_CAPACITOR" pad="14"/>
<connect gate="A" pin="SAWTOOTH_SET_CURRENT" pad="15"/>
<connect gate="A" pin="SET_SPEED" pad="5"/>
<connect gate="A" pin="SHUNT_REGULATOR_BALLAST_RESISTOR" pad="10"/>
<connect gate="A" pin="TRIGGER_PULSE_OUTPUT" pad="13"/>
<connect gate="A" pin="VOLTAGE_SYNCHRONIZATION" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TDA1085CG"/>
<attribute name="OC_FARNELL" value="1468784"/>
<attribute name="OC_NEWARK" value="71J7907"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL431ACDG" prefix="U">
<description>Programmable Precision Reference / Shunt Regulator</description>
<gates>
<gate name="A" symbol="TL431ACDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ANODE" pad="3"/>
<connect gate="A" pin="ANODE_2" pad="2"/>
<connect gate="A" pin="ANODE_3" pad="6"/>
<connect gate="A" pin="ANODE_4" pad="7"/>
<connect gate="A" pin="CATHODE" pad="1"/>
<connect gate="A" pin="N/C" pad="5"/>
<connect gate="A" pin="N/C_2" pad="4"/>
<connect gate="A" pin="REF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TL431ACDG"/>
<attribute name="OC_FARNELL" value="1651199"/>
<attribute name="OC_NEWARK" value="45J2294"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL431AIDG" prefix="U">
<description>Programmable Precision Reference / Shunt Regulator</description>
<gates>
<gate name="A" symbol="TL431AIDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ANODE" pad="3"/>
<connect gate="A" pin="ANODE_2" pad="2"/>
<connect gate="A" pin="ANODE_3" pad="6"/>
<connect gate="A" pin="ANODE_4" pad="7"/>
<connect gate="A" pin="CATHODE" pad="1"/>
<connect gate="A" pin="N/C" pad="5"/>
<connect gate="A" pin="N/C_2" pad="4"/>
<connect gate="A" pin="REF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TL431AIDG"/>
<attribute name="OC_FARNELL" value="1651200"/>
<attribute name="OC_NEWARK" value="45J2295"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL431AIDR2G" prefix="U">
<description>Programmable Precision Reference / Shunt Regulator</description>
<gates>
<gate name="A" symbol="TL431AIDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ANODE" pad="3"/>
<connect gate="A" pin="ANODE_2" pad="2"/>
<connect gate="A" pin="ANODE_3" pad="6"/>
<connect gate="A" pin="ANODE_4" pad="7"/>
<connect gate="A" pin="CATHODE" pad="1"/>
<connect gate="A" pin="N/C" pad="5"/>
<connect gate="A" pin="N/C_2" pad="4"/>
<connect gate="A" pin="REF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TL431AIDR2G"/>
<attribute name="OC_FARNELL" value="1651202"/>
<attribute name="OC_NEWARK" value="98H0990"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL431BIDG" prefix="U">
<description>Programmable Precision Reference / Shunt Regulator</description>
<gates>
<gate name="A" symbol="TL431BIDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ANODE" pad="3"/>
<connect gate="A" pin="ANODE_2" pad="2"/>
<connect gate="A" pin="ANODE_3" pad="6"/>
<connect gate="A" pin="ANODE_4" pad="7"/>
<connect gate="A" pin="CATHODE" pad="1"/>
<connect gate="A" pin="N/C" pad="5"/>
<connect gate="A" pin="N/C_2" pad="4"/>
<connect gate="A" pin="REF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TL431BIDG"/>
<attribute name="OC_FARNELL" value="1652302"/>
<attribute name="OC_NEWARK" value="98H0994"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL431CDG" prefix="U">
<description>Programmable Precision Reference / Shunt Regulator</description>
<gates>
<gate name="A" symbol="TL431CDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ANODE" pad="3"/>
<connect gate="A" pin="ANODE_2" pad="2"/>
<connect gate="A" pin="ANODE_3" pad="6"/>
<connect gate="A" pin="ANODE_4" pad="7"/>
<connect gate="A" pin="CATHODE" pad="1"/>
<connect gate="A" pin="N/C" pad="5"/>
<connect gate="A" pin="N/C_2" pad="4"/>
<connect gate="A" pin="REF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TL431CDG"/>
<attribute name="OC_FARNELL" value="1104704"/>
<attribute name="OC_NEWARK" value="42K2696"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL431CDR2G" prefix="U">
<description>Programmable Precision Reference / Shunt Regulator</description>
<gates>
<gate name="A" symbol="TL431CDR2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="ANODE" pad="3"/>
<connect gate="A" pin="ANODE_2" pad="2"/>
<connect gate="A" pin="ANODE_3" pad="6"/>
<connect gate="A" pin="ANODE_4" pad="7"/>
<connect gate="A" pin="CATHODE" pad="1"/>
<connect gate="A" pin="N/C" pad="5"/>
<connect gate="A" pin="N/C_2" pad="4"/>
<connect gate="A" pin="REF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TL431CDR2G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="88H5153"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UAA2016PG" prefix="U">
<description>Power Controller</description>
<gates>
<gate name="A" symbol="UAA2016PG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="HYS._ADJ." pad="2"/>
<connect gate="A" pin="OUTPUT" pad="6"/>
<connect gate="A" pin="SENSOR" pad="3"/>
<connect gate="A" pin="SYNC" pad="8"/>
<connect gate="A" pin="TEMP._REDUC." pad="4"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="UAA2016PG"/>
<attribute name="OC_FARNELL" value="1192087"/>
<attribute name="OC_NEWARK" value="45J2359"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC2842BD1R2G" prefix="U">
<description>High Performance Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="UC2842BD1R2G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="CURRENT_SENSE" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="RT/CT" pad="4"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VOLTAGE_FB" pad="2"/>
<connect gate="A" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="UC2842BD1R2G"/>
<attribute name="OC_FARNELL" value="1293251"/>
<attribute name="OC_NEWARK" value="67H7336"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC2842BDG" prefix="U">
<description>High Performance Current Mode Controllers</description>
<gates>
<gate name="A" symbol="UC2842BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="CURRENT_SENSE" pad="5"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="NC_4" pad="4"/>
<connect gate="A" pin="OUT" pad="10"/>
<connect gate="A" pin="POWER_GND" pad="8"/>
<connect gate="A" pin="RT/CT" pad="7"/>
<connect gate="A" pin="VC" pad="11"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VOLTAGE_FB" pad="3"/>
<connect gate="A" pin="VREF" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="UC2842BDG"/>
<attribute name="OC_FARNELL" value="1278355"/>
<attribute name="OC_NEWARK" value="70K5973"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC2843BD1G" prefix="U">
<description>High Performance Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="UC2843BD1G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="CURRENT_SENSE" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="RT/CT" pad="4"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VOLTAGE_FB" pad="2"/>
<connect gate="A" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="UC2843BD1G"/>
<attribute name="OC_FARNELL" value="1104705"/>
<attribute name="OC_NEWARK" value="93K1068"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC2843BNG" prefix="U">
<description>Current Mode Controllers</description>
<gates>
<gate name="A" symbol="UC2843BNG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="COMPENSATION" pad="1"/>
<connect gate="A" pin="CURRENT_SENSE" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUTPUT" pad="6"/>
<connect gate="A" pin="RT/CT" pad="4"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK" pad="2"/>
<connect gate="A" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="UC2843BNG"/>
<attribute name="OC_FARNELL" value="1230088"/>
<attribute name="OC_NEWARK" value="45J2366"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC3842BNG" prefix="U">
<description>Current Mode Controllers</description>
<gates>
<gate name="A" symbol="UC3842BNG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="COMPENSATION" pad="1"/>
<connect gate="A" pin="CURRENT_SENSE" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUTPUT" pad="6"/>
<connect gate="A" pin="RT/CT" pad="4"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK" pad="2"/>
<connect gate="A" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="UC3842BNG"/>
<attribute name="OC_FARNELL" value="1652438"/>
<attribute name="OC_NEWARK" value="88H5155"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC3843BD1G" prefix="U">
<description>High Performance Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="UC3843BD1G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="CURRENT_SENSE" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="RT/CT" pad="4"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VOLTAGE_FB" pad="2"/>
<connect gate="A" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="UC3843BD1G"/>
<attribute name="OC_FARNELL" value="1705973"/>
<attribute name="OC_NEWARK" value="45J2379"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC3843BVD1G" prefix="U">
<description>High Performance Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="UC3843BVD1G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="CURRENT_SENSE" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="RT/CT" pad="4"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VOLTAGE_FB" pad="2"/>
<connect gate="A" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="UC3843BVD1G"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="71J8473"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC3844BNG" prefix="U">
<description>Current Mode Controllers</description>
<gates>
<gate name="A" symbol="UC3844BNG"/>
</gates>
<devices>
<device name="" package="DIP254P762X445-8">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="ISEN" pad="3"/>
<connect gate="A" pin="OUTPUT" pad="6"/>
<connect gate="A" pin="RT/CT" pad="4"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VOLTAGE_FEEDBACK" pad="2"/>
<connect gate="A" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="UC3844BNG"/>
<attribute name="OC_FARNELL" value="1652439"/>
<attribute name="OC_NEWARK" value="45J2386"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC3845BDG" prefix="U">
<description>High Performance Current Mode Controllers</description>
<gates>
<gate name="A" symbol="UC3845BDG"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="CURRENT_SENSE" pad="5"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="NC_4" pad="4"/>
<connect gate="A" pin="OUT" pad="10"/>
<connect gate="A" pin="POWER_GND" pad="8"/>
<connect gate="A" pin="RT/CT" pad="7"/>
<connect gate="A" pin="VC" pad="11"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VOLTAGE_FB" pad="3"/>
<connect gate="A" pin="VREF" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="UC3845BDG"/>
<attribute name="OC_FARNELL" value="1364584"/>
<attribute name="OC_NEWARK" value="42K2722"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC3845BVD1G" prefix="U">
<description>High Performance Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="UC3845BVD1G"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="CURRENT_SENSE" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="RT/CT" pad="4"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VOLTAGE_FB" pad="2"/>
<connect gate="A" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="UC3845BVD1G"/>
<attribute name="OC_FARNELL" value="1705923"/>
<attribute name="OC_NEWARK" value="42K2725"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="ON Semi"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
