<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>G717 Bus Terminator</text>
<text>G717 Bus Terminator</text>
<text>G717 Bus Terminator</text>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="SINGLE">
<description>Single-Height DEC board</description>
</package>
<package name="EDGE-CON1">
<description>Single-sided Edge Connector</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dec-con" package="SINGLE" value="OUTLINE-SINGLE"/>
<element name="U$3" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="R1" library="rcl" package="0207/10" value="100"/>
<element name="R2" library="rcl" package="0207/10" value="100"/>
<element name="R3" library="rcl" package="0207/10" value="100"/>
<element name="R4" library="rcl" package="0207/10" value="100"/>
<element name="R5" library="rcl" package="0207/10" value="100"/>
<element name="R6" library="rcl" package="0207/10" value="100"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="C2"/>
<contactref element="U$3" pad="U2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="U$3" pad="L2"/>
<contactref element="U$3" pad="N2"/>
<contactref element="U$3" pad="R2"/>
<contactref element="U$3" pad="F2"/>
<contactref element="U$3" pad="J2"/>
</signal>
<signal name="N$1">
<contactref element="U$3" pad="V2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$3" pad="T2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$3" pad="S2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$3" pad="P2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$3" pad="M2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$3" pad="K2"/>
<contactref element="R6" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
