<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>RELAY G851B</text>
<text>6-69</text>
<text>FLIP CHIP</text>
<hole x="26.67" y="15.24" drill="3.175"/>
<hole x="26.67" y="115.57" drill="3.175"/>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="DOUBLE">
<description>Double-Height DEC board</description>
</package>
<package name="EDGE-CON4">
<description>Double-Height DEC edge connector</description>
</package>
<package name="260-3A-12">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch, Omron</description>
</package>
<package name="133-022-03">
<description>Pseudo-edge connector with .156 inch spacing.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$3" library="dec-con" package="DOUBLE" value="OUTLINE-DOUBLE"/>
<element name="U$1" library="dec-con" package="EDGE-CON4" value=""/>
<element name="K1" library="dec-con" package="260-3A-12" value="260-3A-12"/>
<element name="K2" library="dec-con" package="260-3A-12" value="260-3A-12"/>
<element name="K3" library="dec-con" package="260-3A-12" value="260-3A-12"/>
<element name="K4" library="dec-con" package="260-3A-12" value="260-3A-12"/>
<element name="K5" library="dec-con" package="260-3A-12" value="260-3A-12"/>
<element name="U1" library="dec-con" package="133-022-03" value="133-022-03"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="AC2"/>
<contactref element="U1" pad="L1"/>
<contactref element="U1" pad="L2"/>
</signal>
<signal name="-15V">
<contactref element="U$1" pad="AB2"/>
<contactref element="K1" pad="2"/>
<contactref element="K2" pad="2"/>
<contactref element="K3" pad="2"/>
<contactref element="K4" pad="2"/>
<contactref element="K5" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="AD2"/>
<contactref element="U1" pad="A1"/>
<contactref element="U1" pad="A2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="AF2"/>
<contactref element="K1" pad="P1"/>
</signal>
<signal name="N$3">
<contactref element="K1" pad="P2"/>
<contactref element="U$1" pad="AH2"/>
</signal>
<signal name="N$4">
<contactref element="K1" pad="P3"/>
<contactref element="U$1" pad="AJ2"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="AN2"/>
<contactref element="K2" pad="P1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="AP2"/>
<contactref element="K2" pad="P2"/>
</signal>
<signal name="N$7">
<contactref element="K2" pad="P3"/>
<contactref element="U$1" pad="AR2"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="AK2"/>
<contactref element="U$1" pad="AS2"/>
<contactref element="U1" pad="E1"/>
<contactref element="U1" pad="K1"/>
<contactref element="U1" pad="E2"/>
<contactref element="U1" pad="K2"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="AT2"/>
<contactref element="U$1" pad="BE2"/>
<contactref element="U$1" pad="BL2"/>
<contactref element="U1" pad="M1"/>
<contactref element="U1" pad="S1"/>
<contactref element="U1" pad="W1"/>
<contactref element="U1" pad="W2"/>
<contactref element="U1" pad="S2"/>
<contactref element="U1" pad="M2"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="BM2"/>
<contactref element="K5" pad="P1"/>
</signal>
<signal name="N$11">
<contactref element="K5" pad="P2"/>
<contactref element="U$1" pad="BN2"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="BP2"/>
<contactref element="K5" pad="P3"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="BJ2"/>
<contactref element="K4" pad="P3"/>
</signal>
<signal name="N$14">
<contactref element="K4" pad="P2"/>
<contactref element="U$1" pad="BH2"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="BF2"/>
<contactref element="K4" pad="P1"/>
</signal>
<signal name="N$16">
<contactref element="K3" pad="P3"/>
<contactref element="U$1" pad="BD2"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="AV2"/>
<contactref element="K3" pad="P2"/>
</signal>
<signal name="N$18">
<contactref element="K3" pad="P1"/>
<contactref element="U$1" pad="AU2"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="AE2"/>
<contactref element="K5" pad="1"/>
<contactref element="K4" pad="1"/>
<contactref element="K3" pad="1"/>
<contactref element="K2" pad="1"/>
<contactref element="K1" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="K1" pad="S3"/>
<contactref element="U1" pad="D1"/>
<contactref element="U1" pad="D2"/>
</signal>
<signal name="N$21">
<contactref element="K1" pad="S2"/>
<contactref element="U1" pad="C1"/>
<contactref element="U1" pad="C2"/>
</signal>
<signal name="N$22">
<contactref element="K1" pad="S1"/>
<contactref element="U1" pad="B1"/>
<contactref element="U1" pad="B2"/>
</signal>
<signal name="N$23">
<contactref element="K5" pad="S2"/>
<contactref element="U1" pad="Y1"/>
<contactref element="U1" pad="Y2"/>
</signal>
<signal name="N$24">
<contactref element="K2" pad="S1"/>
<contactref element="U1" pad="F1"/>
<contactref element="U1" pad="F2"/>
</signal>
<signal name="N$25">
<contactref element="K2" pad="S2"/>
<contactref element="U1" pad="H1"/>
<contactref element="U1" pad="H2"/>
</signal>
<signal name="N$26">
<contactref element="K2" pad="S3"/>
<contactref element="U1" pad="J1"/>
<contactref element="U1" pad="J2"/>
</signal>
<signal name="N$27">
<contactref element="K3" pad="S1"/>
<contactref element="U1" pad="N1"/>
<contactref element="U1" pad="N2"/>
</signal>
<signal name="N$28">
<contactref element="K3" pad="S2"/>
<contactref element="U1" pad="P1"/>
<contactref element="U1" pad="P2"/>
</signal>
<signal name="N$29">
<contactref element="K3" pad="S3"/>
<contactref element="U1" pad="R1"/>
<contactref element="U1" pad="R2"/>
</signal>
<signal name="N$30">
<contactref element="K4" pad="S1"/>
<contactref element="U1" pad="T1"/>
<contactref element="U1" pad="T2"/>
</signal>
<signal name="N$31">
<contactref element="K4" pad="S2"/>
<contactref element="U1" pad="U1"/>
<contactref element="U1" pad="U2"/>
</signal>
<signal name="N$32">
<contactref element="K4" pad="S3"/>
<contactref element="U1" pad="V1"/>
<contactref element="U1" pad="V2"/>
</signal>
<signal name="N$33">
<contactref element="K5" pad="S1"/>
<contactref element="U1" pad="X1"/>
<contactref element="U1" pad="X2"/>
</signal>
<signal name="N$34">
<contactref element="K5" pad="S3"/>
<contactref element="U1" pad="Z1"/>
<contactref element="U1" pad="Z2"/>
</signal>
<signal name="N$35">
</signal>
</signals>
</board>
</drawing>
</eagle>
